<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="6.10235" y1="5.55625" x2="6.10235" y2="17.30375" width="0" layer="20"/>
<wire x1="6.10235" y1="17.30375" x2="42.5831" y2="17.30375" width="0" layer="20"/>
<wire x1="42.5831" y1="17.30375" x2="42.5831" y2="5.55625" width="0" layer="20"/>
<wire x1="42.5831" y1="5.55625" x2="6.10235" y2="5.55625" width="0" layer="20"/>
<text>DiXi</text>
<text>GND</text>
<text>+5</text>
<text>GND</text>
<text>32.768</text>
<text>user btn</text>
<text>+</text>
<text>PeMi</text>
<text>GND</text>
<text>+5</text>
<text>D11</text>
<text>2016</text>
<text>D+</text>
<text>D-</text>
<text>SamD11c14</text>
<text>+3.3</text>
<text>2</text>
<text>15</text>
<text>14</text>
<text>Reset</text>
<text>30.SWC</text>
<text>31.SWD</text>
<text>D11c14</text>
<text>Bobricius</text>
<text>15</text>
<text>FUSE</text>
<text>*</text>
<text>+</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="USB-A-PCB">
</package>
<package name="TACTILE-SWITCH-1101NE">
<description>Sparkfun SKU# COM-08229</description>
</package>
<package name="SOD-323">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="todstuff">
<packages>
<package name="MOLEX-48037-1000">
</package>
</packages>
</library>
<library name="resistor-dil">
<description>&lt;b&gt;Resistors in DIL Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EXB38V">
<description>&lt;b&gt;Chip Resistor Array 0603x4&lt;/b&gt; 4 resistors in 3.2 mm x 1.6 mm size (EXB38V, V8V)&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
</packages>
</library>
<library name="eclibrary">
<packages>
<package name="10_PIN_EDGE">
</package>
</packages>
</library>
<library name="samd11">
<packages>
<package name="SO14">
</package>
</packages>
</library>
<library name="es">
<packages>
<package name="KX-327LT">
</package>
</packages>
</library>
<library name="okie">
<packages>
<package name="SOT23">
</package>
</packages>
</library>
<library name="rc-master-smd">
<packages>
<package name="C0603">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt; - 0603</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-TRICOLOR-SMD">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X3" library="todstuff" package="MOLEX-48037-1000" value="USB"/>
<element name="X4" library="SparkFun" package="USB-A-PCB" value="USBPCB"/>
<element name="U$2" library="eclibrary" package="10_PIN_EDGE" value="10_PIN_EDGE10_PIN_EDGE"/>
<element name="BTN" library="SparkFun" package="TACTILE-SWITCH-1101NE" value="">
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun" package="SOD-323" value="">
<attribute name="VALUE"/>
</element>
<element name="JUMPER1" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="U$3" library="samd11" package="SO14" value="ATSAMD11C14">
<attribute name="PROD_ID" value="IC-11285"/>
</element>
<element name="32,768KHZ" library="es" package="KX-327LT" value="32768KHz"/>
<element name="3V3" library="okie" package="SOT23" value="3V3"/>
<element name="C7" library="rc-master-smd" package="C0603" value="100n"/>
<element name="C1" library="rc-master-smd" package="C0603" value="100n"/>
<element name="C2" library="rc-master-smd" package="C0603" value="100n"/>
<element name="C3" library="rc-master-smd" package="C0603" value="22p"/>
<element name="C4" library="rc-master-smd" package="C0603" value="22p"/>
<element name="U$6" library="SparkFun-LED" package="LED-TRICOLOR-SMD" value="LED-TRICOLOR"/>
<element name="LED2" library="led" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="RN2" library="resistor-dil" package="EXB38V" value="1k5">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="3V3" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U$3" pad="12"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$6" pad="A"/>
</signal>
<signal name="GND">
<contactref element="X3" pad="4"/>
<contactref element="X3" pad="4"/>
<contactref element="X4" pad="GND"/>
<contactref element="U$2" pad="2"/>
<contactref element="BTN" pad="P$1"/>
<contactref element="3V3" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U$3" pad="11"/>
<contactref element="U$2" pad="1"/>
<contactref element="RN2" pad="1"/>
</signal>
<signal name="USBP">
<contactref element="U$3" pad="10"/>
<contactref element="X3" pad="3"/>
<contactref element="X4" pad="USB_P"/>
</signal>
<signal name="USBM">
<contactref element="U$3" pad="9"/>
<contactref element="X3" pad="2"/>
<contactref element="X4" pad="USB_M"/>
</signal>
<signal name="RES">
<contactref element="U$3" pad="6"/>
<contactref element="U$2" pad="9"/>
</signal>
<signal name="VUSB">
<contactref element="X3" pad="1"/>
<contactref element="X4" pad="5V"/>
<contactref element="D3" pad="1"/>
<contactref element="JUMPER1" pad="2"/>
</signal>
<signal name="USB2">
<contactref element="D3" pad="2"/>
<contactref element="3V3" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="JUMPER1" pad="1"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="32,768KHZ" pad="4"/>
<contactref element="U$3" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U$3" pad="3"/>
<contactref element="32,768KHZ" pad="1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="PA04">
<contactref element="U$3" pad="14"/>
<contactref element="RN2" pad="4"/>
</signal>
<signal name="PA02">
<contactref element="U$3" pad="13"/>
<contactref element="U$2" pad="6"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="SWD">
<contactref element="U$3" pad="8"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="PA05">
<contactref element="U$3" pad="1"/>
<contactref element="RN2" pad="3"/>
</signal>
<signal name="PA14">
<contactref element="U$3" pad="4"/>
<contactref element="U$2" pad="10"/>
<contactref element="RN2" pad="2"/>
</signal>
<signal name="PA15">
<contactref element="U$3" pad="5"/>
<contactref element="BTN" pad="P$2"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="SWC">
<contactref element="U$3" pad="7"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="U$6" pad="R"/>
<contactref element="RN2" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="U$6" pad="B"/>
<contactref element="RN2" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="U$6" pad="G"/>
<contactref element="RN2" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="LED2" pad="C"/>
<contactref element="RN2" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
