{"text_format":"1","workbook":"xls","n_sheets":3,"sheets":["Test Data","Reformatted","Tests"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Test Data","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[[0,7,0,8],[1,0,5,0],[6,0,9,0],[10,0,12,0],[13,0,14,0],[19,0,19,2],[20,0,20,2],[21,0,21,2]],"flags":["formulas_cached_only"]}
["Node 1","Node 2","Measured res.","Actual res.",null,null,null,"Other data"]
["C2 – PWR","ORNG-CBM",1.47,1.0699999999999998,null,null,null,"Resistance of test circuit",0.4]
[null,"C1-Red",7.69,7.29,null,null,null,"Resistance of vice coil",1.1600000000000001]
[null,"C1-Brown",0.43,0.02999999999999997]
[null,"Relay “J”",2.86,2.46]
[null,"Relay “B”",1.43,1.0299999999999998]
["ORNG-CBM","C1-Red",6.67,6.27]
[null,"C1-Brown",1.4,0.9999999999999999]
[null,"Relay “J”",1.82,1.42]
[null,"Relay “B”",0.59,0.18999999999999995]
["C1-Red","C1-Brown",7.69,7.29]
[null,"Relay “J”",5.26,4.859999999999999]
[null,"Relay “B”",6.67,6.27]
["C1-Brown","Relay “J”",2.86,2.46]
[null,"Relay “B”",1.49,1.0899999999999999]
["Relay “J”","Relay “B”",1.85,1.4500000000000002]
[]
[]
[]
["Observations"]
["C1 red is only connected to Relay (J)"]
["Proof that C2 and C1 (brown) are the same"]
[null,"C1 (brown)","C2"]
["ORNG-CBM",1,1.07]
["C1-Red",7.29,7.29]
["Relay “J”",2.46,2.46]
["Relay “B”",1.09,1.03]

{"sheet":"Reformatted","index":1,"n_rows":9,"n_cols":9,"rows_kept":9,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"T1","T2","T3","T4","T5","T6","T7","T8"]
["T1",null,7.29,7.29,6.27,4.859999999999999,"-",6.27,"-"]
["T2",null,null,0.02999999999999997,1.0899999999999999,2.46,"-",0.9999999999999999,"-"]
["T3",null,null,null,1.07,2.46,"-",0.9999999999999999,"-"]
["T4",null,null,null,null,1.4500000000000002,"-","0.19 (1.03)","-"]
["T5",null,null,null,null,null,"-",1.42,"-"]
["T6",null,null,null,null,null,null,"-",1.16]
["T7",null,null,null,null,null,null,null,"-"]
["T8"]

{"sheet":"Tests","index":2,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[[2,0,3,0],[4,0,7,0],[10,5,11,5]],"flags":["formulas_cached_only"]}
["Purpose","Config","Voltage Position","Disconnected nodes","Current","Comment","Relay Coil Voltage"]
["To test the pump in its original configuration","All wires connected and pump attached",110,"-","-","Won't start, even with a “push”","Not measured."]
["To test the motor without the pump","No pump",110,"-","4.62 A","Run 1. Motor works normally. Relay engages","152 VAC"]
[null,"No pump",110,"-","4.58 A","Run 2. Motor works normally. Relay engages","152 VAC"]
["To test at lower power","No pump",220,"-","Not measured","Worked fine.","77.8 VAC"]
[null,"No pump",220,"-","0.84 A","Motor spins at lower speed. Relay keeps clicking.","77.8 VAC"]
[null,"No pump",220,"-","0.84 A","Motor spins at lower speed. Relay  does not engage.","77.8 VAC"]
[null,"No pump",220,"-","0.84 A","Motor spins at lower speed. Relay keeps clicking.","77.8 VAC"]
["To test at lower power, without starting capacitor","No pump",220,"B","0.84 A","Motor spins at lower speed. Relay keeps clicking.","77.8 VAC"]
["Test vice coil ONLY","No pump",110,"B, C","4.20 A","Motor spins at lower speed. Relay fully engages.","146 VAC"]
["Test main coil","No pump",110,"A","4.64 A","Motor works fine, more “full” than vice coil only","152 VAC"]
["Test main coil without vice coil or starting cap / relay (only relevant to initial startup)","No pump",110,"A, B","4.64 A",null,"152 VAC"]
["Test both coils without starter","No pump",110,"D","> 15 A","Motor spins with difficulty and draws huge current","Not measured."]
["More thorough version of above test","No pump",110,"D, B","> 15 A","Motor spins with difficulty and draws huge current","~6 VAC","Could this be proof that the main coil is busted?"]
["Try the starter coil by itself","No pump. Disconnect 2 and 3, and wire the ends to each other",110,"A, B","1.48 A","Motor buzzes but no torque at all"]