USB:

    USB High-Speed Bus:

      Host Controller Location: Built-in USB
      Host Controller Driver: AppleUSBEHCI
      PCI Device ID: 0x1c2d 
      PCI Revision ID: 0x0005 
      PCI Vendor ID: 0x8086 
      Bus Number: 0xfa 

        Hub:

          Product ID: 0x2513
          Vendor ID: 0x0424  (SMSC)
          Version:  b.b3
          Speed: Up to 480 Mb/sec
          Location ID: 0xfa100000 / 2
          Current Available (mA): 500
          Current Required (mA): 2

            Trans-It Drive:

              Capacity: 3.99 GB (3,992,977,408 bytes)
              Removable Media: Yes
              Detachable Drive: Yes
              BSD Name: disk1
              Product ID: 0x0622
              Vendor ID: 0x0718  (Imation Corp.)
              Version: 1.10
              Serial Number: 0792181A2BDD
              Speed: Up to 480 Mb/sec
              Manufacturer: TDKMedia
              Location ID: 0xfa130000 / 6
              Current Available (mA): 500
              Current Required (mA): 300
              Partition Map Type: MBR (Master Boot Record)
              S.M.A.R.T. status: Not Supported
              Volumes:
                Untitled:
                  Capacity: 3.99 GB (3,990,379,520 bytes)
                  Available: 1.99 GB (1,986,838,528 bytes)
                  Writable: Yes
                  File System: MS-DOS FAT32
                  BSD Name: disk1s1
                  Mount Point: /Volumes/Untitled
                  Content: Windows_FAT_32

            Arduino Mega ADK:

              Product ID: 0x0044
              Vendor ID: 0x2341
              Version: 0.01
              Serial Number: 64936333936351500000
              Speed: Up to 12 Mb/sec
              Manufacturer: Arduino (www.arduino.cc)
              Location ID: 0xfa120000 / 5
              Current Available (mA): 500
              Current Required (mA): 100

            BRCM20702 Hub:

              Product ID: 0x4500
              Vendor ID: 0x0a5c  (Broadcom Corp.)
              Version: 1.00
              Speed: Up to 12 Mb/sec
              Manufacturer: Apple Inc.
              Location ID: 0xfa110000 / 3
              Current Available (mA): 500
              Current Required (mA): 94

                Bluetooth USB Host Controller:

                  Product ID: 0x8281
                  Vendor ID: 0x05ac  (Apple Inc.)
                  Version: 0.97
                  Speed: Up to 12 Mb/sec
                  Manufacturer: Apple Inc.
                  Location ID: 0xfa113000 / 4
                  Current Available (mA): 500
                  Current Required (mA): 0

    USB High-Speed Bus:

      Host Controller Location: Built-in USB
      Host Controller Driver: AppleUSBEHCI
      PCI Device ID: 0x7ffc00001c26 
      PCI Revision ID: 0x7ffc00000005 
      PCI Vendor ID: 0x7ffc00008086 
      Bus Number: 0xfd 

        Hub:

          Product ID: 0x2513
          Vendor ID: 0x0424  (SMSC)
          Version:  b.b3
          Speed: Up to 480 Mb/sec
          Location ID: 0xfd100000 / 2
          Current Available (mA): 500
          Current Required (mA): 2

            USB Multimedia Keyboard:

              Product ID: 0xc311
              Vendor ID: 0x046d  (Logitech Inc.)
              Version: 1.30
              Speed: Up to 1.5 Mb/sec
              Manufacturer: BTC
              Location ID: 0xfd120000 / 5
              Current Available (mA): 500
              Current Required (mA): 100

            USB-PS/2 Optical Mouse:

              Product ID: 0xc050
              Vendor ID: 0x046d  (Logitech Inc.)
              Version: 27.20
              Speed: Up to 1.5 Mb/sec
              Manufacturer: Logitech
              Location ID: 0xfd130000 / 4
              Current Available (mA): 500
              Current Required (mA): 98

            IR Receiver:

              Product ID: 0x8242
              Vendor ID: 0x05ac  (Apple Inc.)
              Version: 0.16
              Speed: Up to 1.5 Mb/sec
              Manufacturer: Apple Computer, Inc.
              Location ID: 0xfd110000 / 3
              Current Available (mA): 500
              Current Required (mA): 100

