This is a library for the Adafruit CC3000 WiFi Breakouts etc

Designed specifically to work with the Adafruit CC3000 Breakout 
  ----> https://www.adafruit.com/products/1469

These modules use SPI to communicate, 6 pins are required to interface

Adafruit invests time and resources providing this open source code, 
please support Adafruit and open-source hardware by purchasing 
products from Adafruit!

Check out the links above for our tutorials and wiring diagrams 

Arduino library Written by Limor Fried & Kevin Townsend for Adafruit Industries.  
CC3000 host core written by TI

To download. click the DOWNLOADS button in the top right corner, rename the uncompressed folder Adafruit_CC3000 
Check that the Adafruit_CC3000 folder contains Adafruit_CC3000.cpp and Adafruit_CC3000.h

Place the Adafruit_CC3000 library folder your *arduinosketchfolder*/libraries/ folder. 
You may need to create the libraries subfolder if its your first library. Restart the IDE.

NOTE: the 'SendTweet' example currently DOES NOT WORK due to Twitter API changes. The code is being kept for posterity in case a workaround can be developed.

