This is a 3d-printable shell I'm working on for my working Tricorder that I've been designing for the past couple years.

Project details here: https://hackaday.io/project/132098-science-tricorder-by-olympus-heavy-industries
Thingiverse page: https://www.thingiverse.com/thing:3796426

The main body part comes in 2 variants, one with a space for a magnetic reed switch (it would be triggered by a magnet in the door assy), and one without.

The door's control panel is designed to allow very thin wire to be run into and glued down, then connected to a capacitive controller.

The main body allows a mainboard 70x80mm.

Parts needed -

    2x Hinges (https://www.rockler.com/butt-hinges-for-small-boxes-3-4quot-height ,Item #44445)
    10x m2 10mm buttoncap screws (I used Torx t-6 for this)
    2x m2 15mm socket head screws (same Torx t-6)
    8x small nylon washers
    8x 2mm nut

Included is the 123dx file if anyone wants to make any changes, just let me know!

--------------------
Print Settings

Printer Brand:

Creality

Printer:

CR-10

Rafts:

No

Supports:

Yes

Resolution:

0.1mm

Infill:

65%

Filament: Hatchbox PLA Gray

Notes:

Printing the main body and door either requires a lot of support or printed on-edge as in the images.