<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>GND</text>
<text>EN</text>
<text>SVP</text>
<text>SVN</text>
<text>IO34</text>
<text>IO35</text>
<text>IO32</text>
<text>IO33</text>
<text>IO25</text>
<text>IO26</text>
<text>IO27</text>
<text>IO14</text>
<text>IO12</text>
<text>IO13</text>
<text>IO15</text>
<text>IO2</text>
<text>IO0</text>
<text>IO4</text>
<text>IO16</text>
<text>GND</text>
<text>IO21</text>
<text>U0TX</text>
<text>U0RX</text>
<text>IO22</text>
<text>IO19</text>
<text>IO23</text>
<text>IO18</text>
<text>IO5</text>
<text>IO17</text>
<text>3V3</text>
<wire x1="0.065" y1="2.335" x2="0.065" y2="38" width="0" layer="20"/>
<wire x1="0.065" y1="38" x2="2.065" y2="40" width="0" layer="20" curve="-90"/>
<wire x1="2.065" y1="40" x2="27" y2="40" width="0" layer="20"/>
<wire x1="27" y1="40" x2="29" y2="38" width="0" layer="20" curve="-90"/>
<wire x1="29" y1="38" x2="29" y2="12" width="0" layer="20"/>
<wire x1="29" y1="11" x2="29" y2="12" width="0" layer="20"/>
<wire x1="29" y1="11" x2="29" y2="9" width="0" layer="20"/>
<wire x1="23" y1="1" x2="23.665" y2="0.335" width="0" layer="20" curve="90"/>
<wire x1="23.665" y1="0.335" x2="27" y2="0.335" width="0" layer="20"/>
<wire x1="27" y1="0.335" x2="29" y2="2.335" width="0" layer="20" curve="90"/>
<wire x1="29" y1="2.335" x2="29" y2="9" width="0" layer="20"/>
<wire x1="6" y1="1.171571875" x2="5.163428125" y2="0.335" width="0" layer="20" curve="-90"/>
<wire x1="5.163428125" y1="0.335" x2="2.065" y2="0.335" width="0" layer="20"/>
<wire x1="2.065" y1="0.335" x2="0.065" y2="2.335" width="0" layer="20" curve="-90"/>
<wire x1="6.5857875" y1="2.5857875" x2="13.0857875" y2="9.0857875" width="0" layer="20"/>
<wire x1="13.0857875" y1="9.0857875" x2="15.9142125" y2="9.0857875" width="0" layer="20" curve="-90"/>
<wire x1="15.9142125" y1="9.0857875" x2="22.4142125" y2="2.5857875" width="0" layer="20"/>
<wire x1="6.5857875" y1="2.5857875" x2="6" y2="1.171571875" width="0" layer="20" curve="45.00009"/>
<wire x1="22.4142125" y1="2.5857875" x2="23" y2="1.171571875" width="0" layer="20" curve="-45.00009"/>
<wire x1="23" y1="1.171571875" x2="23" y2="1" width="0" layer="20"/>
</plain>
<libraries>
<library name="esp3212-ptw">
<packages>
<package name="ESP3212_NOPINLABELS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X15">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="esp3212-ptw" package="ESP3212_NOPINLABELS" value="ESP3212NOLABELS"/>
<element name="JP1" library="SparkFun-Connectors" package="1X15" value="M15"/>
<element name="JP2" library="SparkFun-Connectors" package="1X15" value="M15"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="U$1" pad="EN"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="SVP"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="SVN"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="IO34"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="IO35"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="IO32"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="IO33"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="IO25"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="IO26"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="IO27"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="IO21"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="U0TX"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="U0RX"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="IO22"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="IO19"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="IO23"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="IO18"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="IO5"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="IO17"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="3V3"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="IO14"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="N$24">
<contactref element="JP1" pad="13"/>
<contactref element="U$1" pad="IO12"/>
</signal>
<signal name="N$25">
<contactref element="JP1" pad="14"/>
<contactref element="U$1" pad="IO13"/>
</signal>
<signal name="N$26">
<contactref element="JP1" pad="15"/>
<contactref element="U$1" pad="IO15"/>
</signal>
<signal name="N$27">
<contactref element="JP2" pad="12"/>
<contactref element="U$1" pad="IO16"/>
</signal>
<signal name="N$28">
<contactref element="JP2" pad="13"/>
<contactref element="U$1" pad="IO4"/>
</signal>
<signal name="N$29">
<contactref element="JP2" pad="14"/>
<contactref element="U$1" pad="IO0"/>
</signal>
<signal name="N$30">
<contactref element="JP2" pad="15"/>
<contactref element="U$1" pad="IO2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND_B"/>
<contactref element="U$1" pad="GND_L"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="GND_R"/>
<contactref element="JP2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
