<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="58.42" y1="7.62" x2="58.42" y2="17.78" width="0" layer="20"/>
<wire x1="58.42" y1="21.59" x2="58.42" y2="106.68" width="0" layer="20"/>
<wire x1="-6.35" y1="106.68" x2="-6.35" y2="7.62" width="0" layer="20"/>
<wire x1="-6.35" y1="7.62" x2="58.42" y2="7.62" width="0" layer="20"/>
<wire x1="-6.35" y1="106.68" x2="58.42" y2="106.68" width="0" layer="20"/>
<wire x1="58.42" y1="21.59" x2="46.99" y2="21.59" width="0" layer="20"/>
<wire x1="46.99" y1="21.59" x2="46.99" y2="17.78" width="0" layer="20"/>
<wire x1="46.99" y1="17.78" x2="58.42" y2="17.78" width="0" layer="20"/>
<hole x="57.15" y="16.51" drill="1"/>
<hole x="57.15" y="8.89" drill="1"/>
<hole x="49.53" y="8.89" drill="1"/>
<hole x="49.53" y="16.51" drill="1"/>
<hole x="46.99" y="16.51" drill="0.5"/>
<hole x="46.99" y="15.24" drill="0.5"/>
<hole x="46.99" y="13.97" drill="0.5"/>
<hole x="46.99" y="12.7" drill="0.5"/>
<hole x="46.99" y="11.43" drill="0.5"/>
<hole x="46.99" y="10.16" drill="0.5"/>
<hole x="46.99" y="8.89" drill="0.5"/>
<text>MBOT</text>
<text>BOBRICIUS
Made in Slovakia
www.PeMi.Technology</text>
<text>PeMi Technology - Factory For Materializing Dreams</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>D</text>
<text>E</text>
<text>F</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>HOME</text>
<text>GND</text>
<text>+5V</text>
<text>OFF</text>
<text>ON</text>
<text>MISO</text>
<text>DETACHABLE
MICRO
ROBOT</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="0309/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="JVN">
<packages>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO214AC">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="rc-master-smd">
<packages>
<package name="C0603">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt; - 0603</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - Long Pads without Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="ppeter">
<packages>
<package name="6_PIN_EDGE">
</package>
</packages>
</library>
<library name="transistor-small-signal">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SMT-8585-BUZZER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="T2" library="JVN" package="TO252" value="IRLR110-ND"/>
<element name="R5" library="rcl" package="R0603" value="4.7k"/>
<element name="LED2" library="led" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="DO214AC" value="">
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0603" value="4.7k"/>
<element name="T3" library="JVN" package="TO252" value="IRLR110-ND"/>
<element name="R10" library="rcl" package="R0603" value="4.7k"/>
<element name="LED3" library="led" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode" package="DO214AC" value="">
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0603" value="4.7k"/>
<element name="T4" library="JVN" package="TO252" value="IRLR110-ND"/>
<element name="R12" library="rcl" package="R0603" value="4.7k"/>
<element name="LED4" library="led" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D4" library="diode" package="DO214AC" value="">
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0603" value="4.7k"/>
<element name="T6" library="JVN" package="TO252" value="IRLR110-ND"/>
<element name="R16" library="rcl" package="R0603" value="4.7k"/>
<element name="LED6" library="led" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D6" library="diode" package="DO214AC" value="">
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R0603" value="4.7k"/>
<element name="T7" library="JVN" package="TO252" value="IRLR110-ND"/>
<element name="R18" library="rcl" package="R0603" value="4.7k"/>
<element name="LED7" library="led" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D7" library="diode" package="DO214AC" value="">
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="R0603" value="4.7k"/>
<element name="T8" library="JVN" package="TO252" value="IRLR110-ND"/>
<element name="R22" library="rcl" package="R0603" value="4.7k"/>
<element name="LED8" library="led" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D8" library="diode" package="DO214AC" value="">
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="R0603" value="4.7k"/>
<element name="R3" library="rcl" package="0309/12" value="10R"/>
<element name="R4" library="rcl" package="0309/12" value="10R"/>
<element name="C1" library="rcl" package="E2,5-7" value="10uF"/>
<element name="C2" library="rcl" package="E2,5-7" value="10uF"/>
<element name="C4" library="rcl" package="E2,5-7" value="10uF"/>
<element name="LOGO3" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="C14" library="rc-master-smd" package="C0603" value="100nF"/>
<element name="C15" library="rc-master-smd" package="C0603" value="100nF"/>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="pb22">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S3" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="pb22">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S4" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="pb22">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="JP4" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="S5" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="pb22">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S6" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="pb22">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="VINZ" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="VINZ1" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="VINZ2" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="VINZ3" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="VINZ4" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="VINZ5" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="IC1" library="atmel" package="TQFP32-08" value="ATMEGA328P">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8-16AU"/>
<attribute name="OC_FARNELL" value="9171371"/>
<attribute name="OC_NEWARK" value="73M8863"/>
</element>
<element name="ISP_HEADER" library="ppeter" package="6_PIN_EDGE" value="6_PIN_ISPEDGE-NORM"/>
<element name="R1" library="rcl" package="R0603" value="4k7"/>
<element name="J5" library="SparkFun-Connectors" package="1X02_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0603" value="1k"/>
<element name="Q1" library="transistor-small-signal" package="SOT23" value="BSS123"/>
<element name="U$2" library="adafruit" package="SMT-8585-BUZZER" value="BUZZER"/>
<element name="VINZ6" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
</elements>
<signals>
<signal name="GND">
<contactref element="R5" pad="1"/>
<contactref element="T2" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="T3" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="T4" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="T6" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="T7" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="T8" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="C2" pad="-"/>
<contactref element="C1" pad="-"/>
<contactref element="C4" pad="-"/>
<contactref element="S1" pad="1"/>
<contactref element="S3" pad="1"/>
<contactref element="S4" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="S5" pad="1"/>
<contactref element="S6" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="21"/>
<contactref element="ISP_HEADER" pad="6"/>
<contactref element="J5" pad="1"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="C2" pad="+"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="ISP_HEADER" pad="2"/>
<contactref element="IC1" pad="18"/>
<contactref element="R1" pad="1"/>
<contactref element="JP4" pad="6"/>
<contactref element="JP4" pad="5"/>
<contactref element="U$2" pad="+"/>
<contactref element="VINZ6" pad="1"/>
</signal>
<signal name="A3">
<contactref element="IC1" pad="26"/>
<contactref element="S5" pad="3"/>
</signal>
<signal name="X2">
<contactref element="T3" pad="3"/>
<contactref element="D3" pad="A"/>
<contactref element="VINZ4" pad="1"/>
</signal>
<signal name="X3">
<contactref element="T4" pad="3"/>
<contactref element="D4" pad="A"/>
<contactref element="VINZ3" pad="1"/>
</signal>
<signal name="Y1">
<contactref element="T6" pad="3"/>
<contactref element="D6" pad="A"/>
<contactref element="VINZ" pad="1"/>
</signal>
<signal name="Y3">
<contactref element="T8" pad="3"/>
<contactref element="D8" pad="A"/>
<contactref element="VINZ2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R9" pad="2"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$10">
<contactref element="R17" pad="2"/>
<contactref element="LED6" pad="C"/>
</signal>
<signal name="N$12">
<contactref element="R11" pad="2"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="N$14">
<contactref element="R21" pad="2"/>
<contactref element="LED7" pad="C"/>
</signal>
<signal name="N$19">
<contactref element="R13" pad="2"/>
<contactref element="LED4" pad="C"/>
</signal>
<signal name="N$21">
<contactref element="R23" pad="2"/>
<contactref element="LED8" pad="C"/>
</signal>
<signal name="N$4">
</signal>
<signal name="X1">
<contactref element="T2" pad="3"/>
<contactref element="D2" pad="A"/>
<contactref element="VINZ5" pad="1"/>
</signal>
<signal name="Y2">
<contactref element="T7" pad="3"/>
<contactref element="D7" pad="A"/>
<contactref element="VINZ1" pad="1"/>
</signal>
<signal name="D4">
<contactref element="IC1" pad="2"/>
<contactref element="T4" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="D3">
<contactref element="IC1" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="D2">
<contactref element="IC1" pad="32"/>
<contactref element="S6" pad="3"/>
</signal>
<signal name="D5">
<contactref element="IC1" pad="9"/>
<contactref element="T3" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="D8">
<contactref element="IC1" pad="12"/>
<contactref element="T7" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="D9">
<contactref element="IC1" pad="13"/>
<contactref element="T8" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="23"/>
<contactref element="S4" pad="3"/>
</signal>
<signal name="D10">
<contactref element="IC1" pad="14"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="VUSB">
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="VINZ6" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="IC1" pad="29"/>
<contactref element="R1" pad="2"/>
<contactref element="ISP_HEADER" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="27"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="28"/>
</signal>
<signal name="VINX">
<contactref element="D3" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="C4" pad="+"/>
<contactref element="R3" pad="1"/>
<contactref element="VINZ5" pad="2"/>
<contactref element="VINZ4" pad="2"/>
<contactref element="VINZ3" pad="2"/>
</signal>
<signal name="VINY">
<contactref element="D6" pad="C"/>
<contactref element="D7" pad="C"/>
<contactref element="D8" pad="C"/>
<contactref element="C1" pad="+"/>
<contactref element="R4" pad="1"/>
<contactref element="VINZ" pad="2"/>
<contactref element="VINZ1" pad="2"/>
<contactref element="VINZ2" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="JP4" pad="4"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="D7">
<contactref element="IC1" pad="11"/>
<contactref element="T6" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="24"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="A2">
<contactref element="IC1" pad="25"/>
<contactref element="S3" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="15"/>
<contactref element="ISP_HEADER" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="16"/>
<contactref element="ISP_HEADER" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="17"/>
<contactref element="ISP_HEADER" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="PB6">
<contactref element="IC1" pad="7"/>
</signal>
<signal name="PB7">
<contactref element="IC1" pad="8"/>
</signal>
<signal name="AREF">
<contactref element="IC1" pad="20"/>
</signal>
<signal name="RXD">
<contactref element="IC1" pad="30"/>
</signal>
<signal name="TXD">
<contactref element="IC1" pad="31"/>
</signal>
<signal name="D6">
<contactref element="IC1" pad="10"/>
<contactref element="T2" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="ADC6">
<contactref element="IC1" pad="19"/>
</signal>
<signal name="ADC7">
<contactref element="IC1" pad="22"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="OUT">
<contactref element="Q1" pad="3"/>
<contactref element="U$2" pad="-"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
