<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>0</text>
<wire x1="0" y1="3.175" x2="3.175" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.175" y1="0" x2="41.275" y2="0" width="0" layer="20"/>
<wire x1="41.275" y1="0" x2="44.45" y2="3.81" width="0" layer="20" curve="90"/>
<wire x1="44.45" y1="3.81" x2="44.45" y2="93.345" width="0" layer="20"/>
<wire x1="44.45" y1="93.345" x2="41.275" y2="96.52" width="0" layer="20" curve="90"/>
<wire x1="41.275" y1="96.52" x2="38.1" y2="93.345" width="0" layer="20" curve="90"/>
<wire x1="38.1" y1="93.345" x2="38.1" y2="86.36" width="0" layer="20"/>
<wire x1="38.1" y1="86.36" x2="36.83" y2="85.09" width="0" layer="20" curve="-90"/>
<wire x1="36.83" y1="85.09" x2="31.75" y2="85.09" width="0" layer="20"/>
<wire x1="31.75" y1="85.09" x2="30.48" y2="86.36" width="0" layer="20" curve="-90"/>
<wire x1="30.48" y1="86.36" x2="30.48" y2="95.25" width="0" layer="20"/>
<wire x1="30.48" y1="95.25" x2="29.21" y2="96.52" width="0" layer="20" curve="90"/>
<wire x1="29.21" y1="96.52" x2="3.81" y2="96.52" width="0" layer="20"/>
<wire x1="3.81" y1="96.52" x2="0" y2="93.345" width="0" layer="20" curve="90"/>
<wire x1="0" y1="93.345" x2="0" y2="3.175" width="0" layer="20"/>
<wire x1="0" y1="52.07" x2="0" y2="42.545" width="0" layer="20"/>
<wire x1="48.895" y1="-1.27" x2="94.615" y2="-1.27" width="0" layer="20"/>
<wire x1="94.615" y1="-1.27" x2="95.885" y2="0" width="0" layer="20" curve="90"/>
<wire x1="95.885" y1="0" x2="95.885" y2="97.155" width="0" layer="20"/>
<wire x1="95.885" y1="97.155" x2="94.615" y2="98.425" width="0" layer="20" curve="90"/>
<wire x1="94.615" y1="98.425" x2="48.895" y2="98.425" width="0" layer="20"/>
<wire x1="48.895" y1="98.425" x2="47.625" y2="97.155" width="0" layer="20" curve="90"/>
<wire x1="47.625" y1="97.155" x2="47.625" y2="0" width="0" layer="20"/>
<wire x1="47.625" y1="0" x2="48.895" y2="-1.27" width="0" layer="20" curve="90"/>
<circle x="61.595" y="11.43" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="71.755" y="11.43" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="81.915" y="11.43" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="61.595" y="46.99" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="71.755" y="43.18" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="81.915" y="19.05" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="71.755" y="19.05" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="61.595" y="19.05" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="61.595" y="26.67" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="71.755" y="26.67" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="81.915" y="26.67" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="71.755" y="50.8" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="81.915" y="46.99" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="81.915" y="34.29" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="71.755" y="34.29" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="61.595" y="34.29" radius="1.767765625" width="0.002540625" layer="20"/>
<wire x1="49.53" y1="59.055" x2="52.07" y2="56.515" width="0" layer="20"/>
<wire x1="52.07" y1="56.515" x2="93.98" y2="56.515" width="0" layer="20"/>
<wire x1="93.98" y1="56.515" x2="93.98" y2="69.215" width="0" layer="20"/>
<wire x1="93.98" y1="69.215" x2="49.53" y2="69.215" width="0" layer="20"/>
<wire x1="49.53" y1="69.215" x2="49.53" y2="59.055" width="0" layer="20"/>
<text>1</text>
<text>?
.
,</text>
<text>4</text>
<text>G
H
I</text>
<text>7</text>
<text>P
Q
R
S</text>
<text>8</text>
<text>T
U
V</text>
<text>*</text>
<text>5</text>
<text>J
K
L</text>
<text>2</text>
<text>A
B
C</text>
<text>#</text>
<text>9</text>
<text>W
X
Y
Z</text>
<text>6</text>
<text>M
N
O</text>
<text>3</text>
<text>D
E
F</text>
<text>OK</text>
<text>&gt;</text>
<text>&lt;</text>
<text>X</text>
<hole x="71.755" y="85.09" drill="1.1"/>
<hole x="75.565" y="85.09" drill="1.1"/>
<hole x="78.105" y="85.09" drill="1.1"/>
<hole x="67.945" y="85.09" drill="1.1"/>
<hole x="65.405" y="85.09" drill="1.1"/>
<hole x="71.755" y="88.9" drill="1.1"/>
<hole x="71.755" y="91.44" drill="1.1"/>
<hole x="71.755" y="81.28" drill="1.1"/>
<hole x="71.755" y="78.74" drill="1.1"/>
<hole x="69.215" y="82.55" drill="1.1"/>
<hole x="69.215" y="87.63" drill="1.1"/>
<hole x="74.295" y="87.63" drill="1.1"/>
<hole x="74.295" y="82.55" drill="1.1"/>
<hole x="76.2" y="80.645" drill="1.1"/>
<hole x="67.31" y="89.535" drill="1.1"/>
<hole x="76.2" y="89.535" drill="1.1"/>
<hole x="67.31" y="80.645" drill="1.1"/>
<hole x="69.215" y="79.375" drill="1.1"/>
<hole x="74.295" y="79.375" drill="1.1"/>
<hole x="77.47" y="82.55" drill="1.1"/>
<hole x="66.04" y="82.55" drill="1.1"/>
<hole x="66.04" y="87.63" drill="1.1"/>
<hole x="69.215" y="90.805" drill="1.1"/>
<hole x="74.295" y="90.805" drill="1.1"/>
<hole x="77.47" y="87.63" drill="1.1"/>
<hole x="61.595" y="5.715" drill="1.1"/>
<hole x="61.595" y="3.81" drill="1.1"/>
<hole x="61.595" y="1.905" drill="1.1"/>
<hole x="63.5" y="3.81" drill="1.1"/>
<hole x="59.69" y="3.81" drill="1.1"/>
<text>+5V</text>
<text>GND</text>
<text>GND</text>
<text>+BAT</text>
<text>33p</text>
<text>10p</text>
<text>SPEAKER</text>
<text>4</text>
<text>1</text>
<text>2</text>
<text>5</text>
<text>3</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>#</text>
<text>0</text>
<text>*</text>
<text>OK</text>
<text>X</text>
<text>Down</text>
<text>Up</text>
<text>RX</text>
<text>TX</text>
<text>BAT</text>
<text>Reset</text>
</plain>
<libraries>
<library name="microbuilder">
<packages>
<package name="MOUNTINGHOLE_2.0_PLATED">
</package>
<package name="0805-NO">
</package>
<package name="0603-NO">
</package>
<package name="CHIPLED_0805_NOOUTLINE">
</package>
<package name="4UCONN_20329_V2">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="OSHW-LOGO-L">
</package>
<package name="TACTILE-SWITCH-1101NE">
<description>Sparkfun SKU# COM-08229</description>
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="buzzer">
<description>&lt;b&gt;Speakers and Buzzers&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;Distributors:
&lt;li&gt;Buerklin
&lt;li&gt;Spoerle
&lt;li&gt;Schukat
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="F/QMX">
<description>&lt;b&gt;BUZZER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="microphon">
<description>&lt;b&gt;Microphon&lt;/b&gt; from&lt;p&gt;
JLI Electronics - www.jlielectronics.com&lt;br&gt;
Panansonic - http://industrial.panasonic.com&lt;br&gt;
&lt;p&gt;
&lt;author&gt;librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="WM-64PC/64PK">
<description>&lt;b&gt;Omnidirectional Back Electret Condenser Microphone Cartridge&lt;/b&gt;&lt;p&gt;
Source: http://industrial.panasonic.com/www-data/pdf/ABA5000/ABA5000CE10.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_NO_SILK">
</package>
<package name="2X3-NS">
</package>
</packages>
</library>
<library name="cellphone">
<packages>
<package name="HCMS-[23]97X">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rc-master-smd">
<packages>
<package name="C0603">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt; - 0603</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="R0603@1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun_20110922_my">
<packages>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-small-signal">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SMT-8585-BUZZER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$6" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$8" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$9" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$7" library="SparkFun" package="OSHW-LOGO-L" value="OSHW-LOGOL"/>
<element name="X6" library="microbuilder" package="4UCONN_20329_V2" value="microUSB"/>
<element name="U1" library="microbuilder" package="SOT23-5" value="MCP73831T-2ACI/OT"/>
<element name="CHG1" library="microbuilder" package="CHIPLED_0805_NOOUTLINE" value="RED"/>
<element name="R6" library="microbuilder" package="0603-NO" value="1K"/>
<element name="C25" library="microbuilder" package="0805-NO" value="10µF"/>
<element name="R7" library="microbuilder" package="0603-NO" value="10K\"/>
<element name="U$4" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$5" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$12" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$15" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="SIM1" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="SIIM2" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="RES" library="SparkFun" package="TACTILE-SWITCH-1101NE" value="">
<attribute name="VALUE"/>
</element>
<element name="U$13" library="cellphone" package="HCMS-[23]97X" value="HCMS-[23]97X"/>
<element name="MIC" library="microphon" package="WM-64PC/64PK" value="ELECTRET_MICROPHON-WM-64PC/64PK"/>
<element name="JP2" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="RX" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="TX" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="C2" library="rc-master-smd" package="C0603" value="100n"/>
<element name="RRST" library="rcl" package="R0603@1" value="10k"/>
<element name="IC2" library="atmel" package="TQFP32-08" value="ATMEGA328P">
<attribute name="OC_FARNELL" value="9171371"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8-16AU"/>
<attribute name="OC_NEWARK" value="73M8863"/>
</element>
<element name="C4" library="rc-master-smd" package="C0603" value="18pF"/>
<element name="C1" library="rc-master-smd" package="C0603" value="18pF"/>
<element name="8MHZ" library="SparkFun_20110922_my" package="HC49UP" value="8MHz"/>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S3" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S4" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S5" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S6" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S7" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S8" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S9" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S10" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S11" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S12" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S13" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S14" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S15" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S17" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="Q1" library="transistor-small-signal" package="SOT23" value="BSS123"/>
<element name="U$2" library="adafruit" package="SMT-8585-BUZZER" value="BUZZER"/>
<element name="SG1" library="buzzer" package="F/QMX" value="F/QMX">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="JP3" library="pinhead" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="PWR" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="BAT" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="FTDI" library="pinhead" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="QI" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="C3" library="rc-master-smd" package="C0603" value="10p"/>
<element name="C5" library="rc-master-smd" package="C0603" value="10p"/>
<element name="C6" library="rc-master-smd" package="C0603" value="10p"/>
<element name="C8" library="rc-master-smd" package="C0603" value="33p"/>
<element name="C9" library="rc-master-smd" package="C0603" value="33p"/>
<element name="C10" library="rc-master-smd" package="C0603" value="33p"/>
<element name="U$11" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$14" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="JP1" library="SparkFun-Connectors" package="2X3-NS" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="X6" pad="SPRT@1"/>
<contactref element="X6" pad="BASE@2"/>
<contactref element="X6" pad="SPRT@2"/>
<contactref element="X6" pad="GND"/>
<contactref element="X6" pad="SPRT@4"/>
<contactref element="X6" pad="BASE@1"/>
<contactref element="X6" pad="SPRT@3"/>
<contactref element="C25" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="RES" pad="P$1"/>
<contactref element="U$13" pad="7"/>
<contactref element="U$13" pad="20"/>
<contactref element="U$13" pad="19"/>
<contactref element="SIIM2" pad="6"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="5"/>
<contactref element="IC2" pad="21"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="BAT" pad="1"/>
<contactref element="FTDI" pad="1"/>
<contactref element="QI" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="VBUS">
<contactref element="X6" pad="VBUS"/>
<contactref element="U1" pad="4"/>
<contactref element="CHG1" pad="A"/>
<contactref element="QI" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="U1" pad="3"/>
<contactref element="C25" pad="1"/>
<contactref element="SIIM2" pad="2"/>
<contactref element="PWR" pad="1"/>
<contactref element="BAT" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="CHG1" pad="C"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R6" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="U1" pad="5"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="D5">
<contactref element="IC2" pad="9"/>
<contactref element="TX" pad="2"/>
</signal>
<signal name="D4">
<contactref element="IC2" pad="2"/>
<contactref element="S9" pad="1"/>
<contactref element="S10" pad="1"/>
<contactref element="S11" pad="1"/>
<contactref element="S12" pad="1"/>
</signal>
<signal name="A3">
<contactref element="IC2" pad="26"/>
<contactref element="S4" pad="3"/>
<contactref element="S8" pad="3"/>
<contactref element="S12" pad="3"/>
<contactref element="S17" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="U$13" pad="3"/>
<contactref element="U$13" pad="10"/>
<contactref element="U$13" pad="22"/>
<contactref element="U$13" pad="21"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="6"/>
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="18"/>
<contactref element="RRST" pad="2"/>
<contactref element="U$2" pad="+"/>
<contactref element="SG1" pad="-"/>
<contactref element="JP3" pad="1"/>
<contactref element="PWR" pad="2"/>
<contactref element="FTDI" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="D10">
<contactref element="IC2" pad="14"/>
<contactref element="U$13" pad="15"/>
</signal>
<signal name="DP">
<contactref element="X6" pad="D+"/>
</signal>
<signal name="DM">
<contactref element="X6" pad="D-"/>
</signal>
<signal name="RESET">
<contactref element="RES" pad="P$2"/>
<contactref element="IC2" pad="29"/>
<contactref element="RRST" pad="1"/>
<contactref element="FTDI" pad="2"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="D3">
<contactref element="IC2" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="D9_RST">
<contactref element="SIIM2" pad="3"/>
</signal>
<signal name="DISPLAY_DATA_OUT">
<contactref element="U$13" pad="26"/>
</signal>
<signal name="DISPLAY_OSC">
<contactref element="U$13" pad="25"/>
</signal>
<signal name="RING">
<contactref element="SIM1" pad="1"/>
<contactref element="IC2" pad="32"/>
</signal>
<signal name="DTR">
<contactref element="SIM1" pad="2"/>
</signal>
<signal name="MCP">
<contactref element="SIM1" pad="3"/>
<contactref element="MIC" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="MCN">
<contactref element="SIM1" pad="4"/>
<contactref element="MIC" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="SPKP">
<contactref element="SIM1" pad="5"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="SPKN">
<contactref element="SIM1" pad="6"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="NET">
<contactref element="SIIM2" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="IC2" pad="30"/>
<contactref element="FTDI" pad="4"/>
</signal>
<signal name="TXD">
<contactref element="IC2" pad="31"/>
<contactref element="FTDI" pad="5"/>
</signal>
<signal name="DISPLAY_RESET">
<contactref element="IC2" pad="13"/>
<contactref element="U$13" pad="24"/>
</signal>
<signal name="D7">
<contactref element="IC2" pad="11"/>
<contactref element="S13" pad="1"/>
<contactref element="S14" pad="1"/>
<contactref element="S15" pad="1"/>
<contactref element="S17" pad="1"/>
</signal>
<signal name="D6">
<contactref element="IC2" pad="10"/>
<contactref element="RX" pad="2"/>
</signal>
<signal name="A0">
<contactref element="IC2" pad="23"/>
<contactref element="S1" pad="3"/>
<contactref element="S5" pad="3"/>
<contactref element="S9" pad="3"/>
<contactref element="S13" pad="3"/>
</signal>
<signal name="A1">
<contactref element="IC2" pad="24"/>
<contactref element="S2" pad="3"/>
<contactref element="S6" pad="3"/>
<contactref element="S10" pad="3"/>
<contactref element="S14" pad="3"/>
</signal>
<signal name="A2">
<contactref element="IC2" pad="25"/>
<contactref element="S15" pad="3"/>
<contactref element="S11" pad="3"/>
<contactref element="S7" pad="3"/>
<contactref element="S3" pad="3"/>
</signal>
<signal name="GSM_RESET">
<contactref element="IC2" pad="12"/>
</signal>
<signal name="MOSI">
<contactref element="IC2" pad="15"/>
<contactref element="U$13" pad="14"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="IC2" pad="16"/>
<contactref element="U$13" pad="18"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC2" pad="17"/>
<contactref element="U$13" pad="17"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="PB6">
<contactref element="IC2" pad="7"/>
<contactref element="C1" pad="1"/>
<contactref element="8MHZ" pad="1"/>
</signal>
<signal name="PB7">
<contactref element="IC2" pad="8"/>
<contactref element="C4" pad="1"/>
<contactref element="8MHZ" pad="2"/>
</signal>
<signal name="AREF">
<contactref element="IC2" pad="20"/>
</signal>
<signal name="ADC6">
<contactref element="IC2" pad="19"/>
</signal>
<signal name="ADC7">
<contactref element="IC2" pad="22"/>
</signal>
<signal name="A4">
<contactref element="IC2" pad="27"/>
<contactref element="S1" pad="1"/>
<contactref element="S2" pad="1"/>
<contactref element="S3" pad="1"/>
<contactref element="S4" pad="1"/>
</signal>
<signal name="A5">
<contactref element="IC2" pad="28"/>
<contactref element="S8" pad="1"/>
<contactref element="S7" pad="1"/>
<contactref element="S6" pad="1"/>
<contactref element="S5" pad="1"/>
</signal>
<signal name="RXDM">
<contactref element="SIIM2" pad="4"/>
<contactref element="RX" pad="1"/>
</signal>
<signal name="TXDM">
<contactref element="SIIM2" pad="5"/>
<contactref element="TX" pad="1"/>
</signal>
<signal name="OUT">
<contactref element="Q1" pad="3"/>
<contactref element="U$2" pad="-"/>
<contactref element="SG1" pad="+"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
