(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 28)
    (no_connects 0)
    (area 134.924999 93.174999 145.075001 108.825001)
    (thickness 1.6)
    (drawings 40)
    (tracks 54)
    (zones 0)
    (modules 14)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4572)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.4 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.15)
    (pcb_text_size 0.75 0.75)
    (mod_edge_width 0.15)
    (mod_text_size 0.75 0.75)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J3-Pad1)")
  (net 5 "Net-(J4-Pad1)")
  (net 6 "Net-(J6-Pad1)")
  (net 7 "Net-(J10-Pad1)")
  (net 8 "Net-(U1-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(U1-Pad6)")
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B1D69B0)
    (at 136.25 97.25 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 3 270) (layer F.Fab))
    (fp_text value 0.1u (at 0 4.25 270) (layer F.Fab))
    (fp_text user %R (at 0 3 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B1D69A7)
    (at 143.75 98.5 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -14.75 270) (layer F.Fab))
    (fp_text value 0.1u (at 0 -13.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -14.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module testpads:PAD_1.6MM (layer F.Cu) (tedit 5B1D6993)
    (at 140.5 94.5)
    (fp_text reference J1 (at -0.5 -2.5) (layer F.Fab))
    (fp_text value VBAT+ (at 0 -3.75) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.6 1.6) (layers F.Cu F.Mask)
      (net 3 "Net-(J1-Pad1)") (solder_mask_margin 0.07))
  )
  (module testpads:PAD_1.6MM (layer F.Cu) (tedit 5B1D6998)
    (at 143.75 94.5)
    (fp_text reference J2 (at 1 -2.5) (layer F.Fab))
    (fp_text value VBAT- (at 1.5 -3.75) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.6 1.6) (layers F.Cu F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
  )
  (module testpads:PAD_1.6MM (layer F.Cu) (tedit 5B1D69B5)
    (at 136.5 101.25)
    (fp_text reference J3 (at -3.75 0.5) (layer F.Fab))
    (fp_text value FM+ (at -3.5 -0.75) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.6 1.6) (layers F.Cu F.Mask)
      (net 4 "Net-(J3-Pad1)") (solder_mask_margin 0.07))
  )
  (module testpads:PAD_1.6MM (layer F.Cu) (tedit 5B1D69BA)
    (at 136.5 104)
    (fp_text reference J4 (at -3.75 0.75) (layer F.Fab))
    (fp_text value FM- (at -3.5 -0.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.6 1.6) (layers F.Cu F.Mask)
      (net 5 "Net-(J4-Pad1)") (solder_mask_margin 0.07))
  )
  (module testpads:PAD_1.6MM (layer F.Cu) (tedit 5B1D69D3)
    (at 143.75 102.5)
    (fp_text reference J5 (at 18 1.25) (layer F.Fab))
    (fp_text value PWSW1 (at 18 0) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.6 1.6) (layers F.Cu F.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.07))
  )
  (module testpads:PAD_1.6MM (layer F.Cu) (tedit 5B1D69CD)
    (at 141 107.5)
    (fp_text reference J6 (at 14.5 1.25) (layer F.Fab))
    (fp_text value PWSW2 (at 14.5 0) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.6 1.6) (layers F.Cu F.Mask)
      (net 6 "Net-(J6-Pad1)") (solder_mask_margin 0.07))
  )
  (module testpads:PAD_1.6MM (layer F.Cu) (tedit 5B1D69DA)
    (at 143.75 105)
    (fp_text reference J7 (at 18 1.25) (layer F.Fab))
    (fp_text value SHSW1 (at 18 0) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.6 1.6) (layers F.Cu F.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.07))
  )
  (module testpads:PAD_1.6MM (layer F.Cu) (tedit 5B1D69C6)
    (at 141 105)
    (fp_text reference J8 (at 14.5 1.25) (layer F.Fab))
    (fp_text value SHSW2 (at 14.5 0) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.6 1.6) (layers F.Cu F.Mask)
      (net 7 "Net-(J10-Pad1)") (solder_mask_margin 0.07))
  )
  (module testpads:PAD_1.6MM (layer F.Cu) (tedit 5B1D69DF)
    (at 143.75 107.5)
    (fp_text reference J9 (at 18 1.25) (layer F.Fab))
    (fp_text value PSSW1 (at 18 0) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.6 1.6) (layers F.Cu F.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.07))
  )
  (module testpads:PAD_1.6MM (layer F.Cu) (tedit 5B1D69C3)
    (at 138.25 107.5)
    (fp_text reference J10 (at 11.25 1.25) (layer F.Fab))
    (fp_text value PSSW2 (at 11 0) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.6 1.6) (layers F.Cu F.Mask)
      (net 7 "Net-(J10-Pad1)") (solder_mask_margin 0.07))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5B1D699D)
    (at 139.75 98)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 10 0) (layer F.Fab))
    (fp_text value DMG2305UX (at 10.75 -1.25) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module testpads:DRV8838_WSON (layer F.Cu) (tedit 5B1D69BF)
    (at 140 102.5)
    (fp_text reference U1 (at 9.5 0.25) (layer F.Fab))
    (fp_text value DRV8838 (at 9.5 -1) (layer F.Fab))
    (pad 9 smd rect (at 0 0) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07) (clearance 0.07))
    (pad 1 smd rect (at -1.2 -0.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 2 smd rect (at -1.2 -0.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J3-Pad1)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 3 smd rect (at -1.2 0.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J4-Pad1)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 4 smd rect (at -1.2 0.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07) (clearance 0.07))
    (pad 5 smd rect (at 1.2 0.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J10-Pad1)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 6 smd rect (at 1.2 0.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad6)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 7 smd rect (at 1.2 -0.25) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J6-Pad1)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 8 smd rect (at 1.2 -0.75) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 1 smd circle (at -1.7 -0.75) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 2 smd circle (at -1.7 -0.25) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J3-Pad1)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 3 smd circle (at -1.7 0.25) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J4-Pad1)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 4 smd circle (at -1.7 0.75) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07) (clearance 0.07))
    (pad 5 smd circle (at 1.7 0.75) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J10-Pad1)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 6 smd circle (at 1.7 0.25) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad6)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 7 smd circle (at 1.7 -0.25) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J6-Pad1)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 8 smd circle (at 1.7 -0.75) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)") (solder_mask_margin 0.07) (clearance 0.07))
    (pad 9 thru_hole circle (at 0 -0.55) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0 0.55) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_text "KADOOKA C.W.\nINSTAX EJECT \nCIRCUIT MK.II" (at 140 98.25) (layer B.SilkS))
  (gr_text MOTOR (at 138 102.25 90) (layer B.SilkS))
  (gr_text SW (at 138.25 106) (layer B.SilkS))
  (gr_text BAT (at 138.5 94.5) (layer B.SilkS))
  (gr_text PS (at 138.25 107.5) (layer B.SilkS))
  (gr_text PW (at 141 107.5) (layer B.SilkS))
  (gr_text SH (at 141 105) (layer B.SilkS))
  (gr_text VCC (at 143.75 105 90) (layer B.SilkS))
  (gr_text - (at 143.75 94.5) (layer B.SilkS))
  (gr_text + (at 140.5 94.5) (layer B.SilkS))
  (gr_text - (at 136.5 104) (layer B.SilkS))
  (gr_text + (at 136.5 101.25) (layer B.SilkS))
  (gr_text U1 (at 141.25 100.5) (layer F.SilkS))
  (gr_text Q1 (at 139.75 95.75) (layer F.SilkS))
  (gr_text C2 (at 142.25 98.5 90) (layer F.SilkS))
  (gr_text C1 (at 137.5 94.25) (layer F.SilkS))
  (dimension 10 (width 0.1875) (layer F.Fab)
    (gr_text "10.000 mm" (at 140 111.25) (layer F.Fab))
    (feature1 (pts (xy 145 109.25) (xy 145 112)))
    (feature2 (pts (xy 135 109.25) (xy 135 112)))
    (crossbar (pts (xy 135 110.5) (xy 145 110.5)))
    (arrow1a (pts (xy 145 110.5) (xy 143.873496 111.086421)))
    (arrow1b (pts (xy 145 110.5) (xy 143.873496 109.913579)))
    (arrow2a (pts (xy 135 110.5) (xy 136.126504 111.086421)))
    (arrow2b (pts (xy 135 110.5) (xy 136.126504 109.913579)))
  )
  (dimension 15.5 (width 0.1875) (layer F.Fab)
    (gr_text "15.500 mm" (at 129.25 101 270) (layer F.Fab))
    (feature1 (pts (xy 134.25 108.75) (xy 128.5 108.75)))
    (feature2 (pts (xy 134.25 93.25) (xy 128.5 93.25)))
    (crossbar (pts (xy 130 93.25) (xy 130 108.75)))
    (arrow1a (pts (xy 130 108.75) (xy 129.413579 107.623496)))
    (arrow1b (pts (xy 130 108.75) (xy 130.586421 107.623496)))
    (arrow2a (pts (xy 130 93.25) (xy 129.413579 94.376504)))
    (arrow2b (pts (xy 130 93.25) (xy 130.586421 94.376504)))
  )
  (gr_line (start 135 108.75) (end 135 93.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145 108.75) (end 135 108.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145 93.25) (end 145 108.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135 93.25) (end 145 93.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name "Net-(J3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 138.1 102.125) (xy 139.3 102.125) (xy 139.3 102.375) (xy 135.375 102.375) (xy 135.375 100.125)
        (xy 137.5 100.125)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J4-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 139.3 102.875) (xy 138.1 102.875) (xy 137.5 105.125) (xy 135.375 105.125) (xy 135.375 102.625)
        (xy 139.3 102.625)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 145 108.75) (xy 135 108.75) (xy 135 93.25) (xy 145 93.25)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 141.425 95.3) (xy 141.2 97.6) (xy 141.2 98.4) (xy 140.3 98.4) (xy 140.3 97.6)
        (xy 139.575 95.3) (xy 139.575 93.575) (xy 141.425 93.575)
      )
    )
  )
  (zone (net 2) (net_name "Net-(C1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 138.3 98.55) (xy 139.2 98.55) (xy 139.2 99.35) (xy 139.3 101.625) (xy 139.3 101.875)
        (xy 138.3 101.875) (xy 138.175 101.75) (xy 137.45 99.25) (xy 135.625 99.25) (xy 135.625 97.75)
        (xy 136.875 97.75)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 139.3 103.575) (xy 145 103.575) (xy 145 108.75) (xy 135 108.75) (xy 135 103.125)
        (xy 139.3 103.125)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 145 102.5) (xy 135 102.5) (xy 135 93.25) (xy 145 93.25)
      )
    )
  )
)
