<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="91.44" y2="0" width="0" layer="20"/>
<wire x1="91.44" y1="0" x2="91.44" y2="91.44" width="0" layer="20"/>
<wire x1="91.44" y1="91.44" x2="0" y2="91.44" width="0" layer="20"/>
<wire x1="0" y1="91.44" x2="0" y2="0" width="0" layer="20"/>
<hole x="7.62" y="7.62" drill="3.2"/>
<hole x="83.82" y="7.62" drill="3.2"/>
<hole x="7.62" y="83.82" drill="3.2"/>
<circle x="45.72" y="45.72" radius="8" width="0.0254" layer="20"/>
<text>Axail generator stator
2 layers, 3 phase, 4 coil, 22 turns
0.25-in magnet Halback array </text>
<text>Rev C 2018-06-26</text>
<text>Silicon Farmers</text>
<text>1P</text>
<text>1N</text>
<text>2P</text>
<text>2N</text>
<text>3P</text>
<text>3N</text>
</plain>
<libraries>
<library name="SparkFun">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="1X06-SMD">
</package>
</packages>
</library>
<library name="AxialGenerator">
<packages>
<package name="MAGNET0.25INCH_2LAYER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun" package="1X06-SMD" value=""/>
<element name="P1A" library="AxialGenerator" package="MAGNET0.25INCH_2LAYER" value="COIL12MAG16_0.25INMAGNET0.25INCH2LAYER"/>
<element name="P3B" library="AxialGenerator" package="MAGNET0.25INCH_2LAYER" value="COIL12MAG16_0.25INMAGNET0.25INCH2LAYER"/>
<element name="P3C" library="AxialGenerator" package="MAGNET0.25INCH_2LAYER" value="COIL12MAG16_0.25INMAGNET0.25INCH2LAYER"/>
<element name="P3D" library="AxialGenerator" package="MAGNET0.25INCH_2LAYER" value="COIL12MAG16_0.25INMAGNET0.25INCH2LAYER"/>
<element name="P1B" library="AxialGenerator" package="MAGNET0.25INCH_2LAYER" value="COIL12MAG16_0.25INMAGNET0.25INCH2LAYER"/>
<element name="P1C" library="AxialGenerator" package="MAGNET0.25INCH_2LAYER" value="COIL12MAG16_0.25INMAGNET0.25INCH2LAYER"/>
<element name="P1D" library="AxialGenerator" package="MAGNET0.25INCH_2LAYER" value="COIL12MAG16_0.25INMAGNET0.25INCH2LAYER"/>
<element name="P2A" library="AxialGenerator" package="MAGNET0.25INCH_2LAYER" value="COIL12MAG16_0.25INMAGNET0.25INCH2LAYER"/>
<element name="P2B" library="AxialGenerator" package="MAGNET0.25INCH_2LAYER" value="COIL12MAG16_0.25INMAGNET0.25INCH2LAYER"/>
<element name="P2C" library="AxialGenerator" package="MAGNET0.25INCH_2LAYER" value="COIL12MAG16_0.25INMAGNET0.25INCH2LAYER"/>
<element name="P2D" library="AxialGenerator" package="MAGNET0.25INCH_2LAYER" value="COIL12MAG16_0.25INMAGNET0.25INCH2LAYER"/>
<element name="P3A" library="AxialGenerator" package="MAGNET0.25INCH_2LAYER" value="COIL12MAG16_0.25INMAGNET0.25INCH2LAYER"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="P1A" pad="OUT"/>
<contactref element="P1B" pad="IN"/>
</signal>
<signal name="N$2">
<contactref element="P1B" pad="OUT"/>
<contactref element="P1C" pad="IN"/>
</signal>
<signal name="N$3">
<contactref element="P1C" pad="OUT"/>
<contactref element="P1D" pad="IN"/>
</signal>
<signal name="N$4">
<contactref element="P2A" pad="OUT"/>
<contactref element="P2B" pad="IN"/>
</signal>
<signal name="N$5">
<contactref element="P2B" pad="OUT"/>
<contactref element="P2C" pad="IN"/>
</signal>
<signal name="N$6">
<contactref element="P2C" pad="OUT"/>
<contactref element="P2D" pad="IN"/>
</signal>
<signal name="N$7">
<contactref element="P3A" pad="OUT"/>
<contactref element="P3B" pad="IN"/>
</signal>
<signal name="N$8">
<contactref element="P3B" pad="OUT"/>
<contactref element="P3C" pad="IN"/>
</signal>
<signal name="N$9">
<contactref element="P3C" pad="OUT"/>
<contactref element="P3D" pad="IN"/>
</signal>
<signal name="POLE1+">
<contactref element="P1A" pad="IN"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="POLE1-">
<contactref element="P1D" pad="OUT"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="POLE2-">
<contactref element="P2D" pad="OUT"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="POLE2+">
<contactref element="P2A" pad="IN"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="POLE3+">
<contactref element="P3A" pad="IN"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="POLE3-">
<contactref element="P3D" pad="OUT"/>
<contactref element="JP1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
