<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="5.207" y1="6.604" x2="16.942" y2="6.477" width="0" layer="20"/>
<wire x1="16.942" y1="6.477" x2="16.942" y2="28.565" width="0" layer="20"/>
<wire x1="16.942" y1="28.565" x2="5.207" y2="28.565" width="0" layer="20"/>
<wire x1="5.207" y1="28.565" x2="5.207" y2="6.604" width="0" layer="20"/>
<text>NEOPIXEL
CONTROL</text>
<hole x="15.367" y="27.178" drill="2"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="genLib">
<packages>
<package name="QFN-24-NO-THERMAL">
</package>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="3-SLIDESWITCH">
</package>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
<library name="M0plus_breakout">
<description>Generated from &lt;b&gt;M0plus_breakout.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="ADAFRUIT_KMR2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="SOIC1" library="genLib" package="QFN-24-NO-THERMAL" value="ATSAMD10"/>
<element name="J2" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="PROD_ID" value="CONN-11566"/>
</element>
<element name="C2" library="genLib" package="0603" value="0.1uF">
<attribute name="PROD_ID" value="CAP-12380"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="genLib" package="0603" value="0.1uF">
<attribute name="PROD_ID" value="CAP-12380"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="genLib" package="3-SLIDESWITCH" value="3-SLIDESWITCH"/>
<element name="J3" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="genLib" package="SOT23-3" value="MCP1700"/>
<element name="C4" library="genLib" package="0603" value="1uF">
<attribute name="PROD_ID" value="CAP-12380"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="genLib" package="0603" value="1uF">
<attribute name="PROD_ID" value="CAP-12380"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="M0plus_breakout" package="ADAFRUIT_KMR2" value="ADAFRUIT_SPST_TACT-KMR2"/>
<element name="R1" library="genLib" package="0603" value="100k">
<attribute name="PROD_ID" value="RES-09333"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="1"/>
<contactref element="SOIC1" pad="23"/>
<contactref element="J2" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="U$2" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="SOIC1" pad="24"/>
<contactref element="J2" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="U$2" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="TX">
<contactref element="J1" pad="3"/>
<contactref element="SOIC1" pad="9"/>
</signal>
<signal name="RX">
<contactref element="J1" pad="2"/>
<contactref element="SOIC1" pad="10"/>
</signal>
<signal name="RST">
<contactref element="J2" pad="5"/>
<contactref element="SOIC1" pad="18"/>
</signal>
<signal name="SCLK">
<contactref element="J2" pad="6"/>
<contactref element="SOIC1" pad="19"/>
</signal>
<signal name="DIO">
<contactref element="J2" pad="4"/>
<contactref element="SOIC1" pad="20"/>
</signal>
<signal name="SWO">
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="SOIC1" pad="2"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="V_BATT">
<contactref element="J1" pad="4"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="NEODAT">
<contactref element="SOIC1" pad="15"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="BUTTON">
<contactref element="SOIC1" pad="22"/>
<contactref element="SW1" pad="2"/>
<contactref element="SW1" pad="4"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
