(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 104)
    (no_connects 0)
    (area 203.924999 58.924999 284.075001 101.075001)
    (thickness 1.6)
    (drawings 23)
    (tracks 542)
    (zones 0)
    (modules 59)
    (nets 61)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 186.69 101.6)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory cad/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 LED1)
  (net 6 LED2)
  (net 7 LED3)
  (net 8 LED4)
  (net 9 LED5)
  (net 10 LED6)
  (net 11 LED7)
  (net 12 LED8)
  (net 13 LED9)
  (net 14 LED10)
  (net 15 LED11)
  (net 16 LED12)
  (net 17 LED13)
  (net 18 LED14)
  (net 19 LED15)
  (net 20 LED16)
  (net 21 /leds/CLOCK)
  (net 22 /leds/Latch)
  (net 23 /leds/DATA)
  (net 24 "Net-(R1-Pad1)")
  (net 25 "Net-(R2-Pad1)")
  (net 26 "Net-(R3-Pad1)")
  (net 27 "Net-(U1-Pad9)")
  (net 28 "Net-(U2-Pad9)")
  (net 29 "Net-(U4-Pad3)")
  (net 30 VCC)
  (net 31 GND)
  (net 32 min+)
  (net 33 hour+)
  (net 34 "Net-(SW2-Pad2)")
  (net 35 EN)
  (net 36 "Net-(J2-Pad3)")
  (net 37 "Net-(J4-Pad1)")
  (net 38 "Net-(J4-Pad2)")
  (net 39 "Net-(J4-Pad3)")
  (net 40 "Net-(TP2-Pad1)")
  (net 41 "Net-(TP4-Pad1)")
  (net 42 "Net-(TP5-Pad1)")
  (net 43 "Net-(TP6-Pad1)")
  (net 44 "Net-(D2-Pad1)")
  (net 45 "Net-(D3-Pad1)")
  (net 46 "Net-(D4-Pad1)")
  (net 47 "Net-(D5-Pad1)")
  (net 48 "Net-(D6-Pad1)")
  (net 49 "Net-(D7-Pad1)")
  (net 50 "Net-(D8-Pad1)")
  (net 51 "Net-(D9-Pad1)")
  (net 52 "Net-(D10-Pad1)")
  (net 53 "Net-(D11-Pad1)")
  (net 54 "Net-(D12-Pad1)")
  (net 55 "Net-(D13-Pad1)")
  (net 56 "Net-(D14-Pad1)")
  (net 57 "Net-(D15-Pad1)")
  (net 58 "Net-(D16-Pad1)")
  (net 59 "Net-(R10-Pad2)")
  (net 60 "Net-(RV1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /leds/CLOCK)
    (add_net /leds/DATA)
    (add_net /leds/Latch)
    (add_net EN)
    (add_net LED1)
    (add_net LED10)
    (add_net LED11)
    (add_net LED12)
    (add_net LED13)
    (add_net LED14)
    (add_net LED15)
    (add_net LED16)
    (add_net LED2)
    (add_net LED3)
    (add_net LED4)
    (add_net LED5)
    (add_net LED6)
    (add_net LED7)
    (add_net LED8)
    (add_net LED9)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(RV1-Pad1)")
    (add_net "Net-(SW2-Pad2)")
    (add_net "Net-(TP2-Pad1)")
    (add_net "Net-(TP4-Pad1)")
    (add_net "Net-(TP5-Pad1)")
    (add_net "Net-(TP6-Pad1)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U4-Pad3)")
    (add_net hour+)
    (add_net min+)
  )
  (net_class .0156 ""
    (clearance 0.199898)
    (trace_width 0.499872)
    (via_dia 1.1684)
    (via_drill 0.79756)
    (uvia_dia 0.59944)
    (uvia_drill 0.199644)
    (add_net GND)
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B22C889)
    (at 217.17 79.06 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value C_Small (at 1.27 2.54 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 217.17 75.25 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 252.73 76.2)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 LED1))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 252.73 80.01)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 LED2))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 257.98 68.58)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D3 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 LED3))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 257.81 72.39)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D4 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 LED4))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 257.81 76.2)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D5 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 LED5))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 257.81 80.01)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D6 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 LED6))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 266.7 72.39)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D7 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 LED7))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 266.7 76.2)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D8 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 LED8))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 266.7 80.01)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D9 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 LED9))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 271.95 68.58)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D10 (at 0 -1.27) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 LED10))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 271.78 72.39)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D11 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 LED11))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 271.78 76.2)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D12 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 LED12))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 271.78 80.01)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D13 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 LED13))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer B.Cu) (tedit 595FC9C0)
    (at 280.67 80.01 270)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D14 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value LED (at 0 -1.55 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(D14-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 18 LED14))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer B.Cu) (tedit 595FC9C0)
    (at 263.06 62.23)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D15 (at 0 1.45) (layer B.SilkS))
    (fp_text value LED (at 0 -1.55) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(D15-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 19 LED15))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer B.Cu) (tedit 595FC9C0)
    (at 245.11 80.18 270)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D16 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value LED (at 0 -1.55 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 20 LED16))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 226.06 82.55)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 260.35 87.63 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /leds/CLOCK))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /leds/Latch))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /leds/DATA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 217.17 73.49 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.45 90) (layer B.SilkS))
    (fp_text value R_Small (at 0 -1.55 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 30 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 222.25 77.64 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.45 90) (layer B.SilkS))
    (fp_text value R_Small (at 0 -1.55 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 30 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module switch:74HC595D (layer F.Cu) (tedit 0)
    (at 253.9619 89.535)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value 74HC595 (at -5.0419 -6.985) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -2.5019 -4.445) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 6 LED2))
    (pad 2 smd rect (at -2.5019 -3.175) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 7 LED3))
    (pad 3 smd rect (at -2.5019 -1.905) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 8 LED4))
    (pad 4 smd rect (at -2.5019 -0.635) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 9 LED5))
    (pad 5 smd rect (at -2.5019 0.635) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 10 LED6))
    (pad 6 smd rect (at -2.5019 1.905) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 11 LED7))
    (pad 7 smd rect (at -2.5019 3.175) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 12 LED8))
    (pad 8 smd rect (at -2.5019 4.445) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 31 GND))
    (pad 9 smd rect (at 2.5019 4.445) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at 2.5019 3.175) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 11 smd rect (at 2.5019 1.905) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 21 /leds/CLOCK))
    (pad 12 smd rect (at 2.5019 0.635) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 22 /leds/Latch))
    (pad 13 smd rect (at 2.5019 -0.635) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 35 EN))
    (pad 14 smd rect (at 2.5019 -1.905) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 23 /leds/DATA))
    (pad 15 smd rect (at 2.5019 -3.175) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 5 LED1))
    (pad 16 smd rect (at 2.5019 -4.445) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
  )
  (module switch:74HC595D (layer F.Cu) (tedit 0)
    (at 270.5481 89.535 180)
    (fp_text reference U2 (at 0 0 180) (layer F.SilkS))
    (fp_text value 74HC595 (at -6.3119 5.715 180) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 180) (layer Cmts.User))
    (pad 1 smd rect (at -2.5019 -4.445 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 14 LED10))
    (pad 2 smd rect (at -2.5019 -3.175 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 15 LED11))
    (pad 3 smd rect (at -2.5019 -1.905 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 16 LED12))
    (pad 4 smd rect (at -2.5019 -0.635 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 17 LED13))
    (pad 5 smd rect (at -2.5019 0.635 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 18 LED14))
    (pad 6 smd rect (at -2.5019 1.905 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 19 LED15))
    (pad 7 smd rect (at -2.5019 3.175 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 20 LED16))
    (pad 8 smd rect (at -2.5019 4.445 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 31 GND))
    (pad 9 smd rect (at 2.5019 4.445 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U2-Pad9)"))
    (pad 10 smd rect (at 2.5019 3.175 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 11 smd rect (at 2.5019 1.905 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 21 /leds/CLOCK))
    (pad 12 smd rect (at 2.5019 0.635 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 22 /leds/Latch))
    (pad 13 smd rect (at 2.5019 -0.635 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 35 EN))
    (pad 14 smd rect (at 2.5019 -1.905 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad9)"))
    (pad 15 smd rect (at 2.5019 -3.175 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 13 LED9))
    (pad 16 smd rect (at 2.5019 -4.445 180) (size 1.905 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
  )
  (module SMD_Packages:SOIC-14_N (layer B.Cu) (tedit 0)
    (at 212.09 80.772)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U3 (at 0 1.27) (layer B.SilkS))
    (fp_text value ATTINY84A-SSUR (at 0 -1.27) (layer B.Fab))
    (pad 1 smd rect (at -3.81 -3.302) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 30 VCC))
    (pad 2 smd rect (at -2.54 -3.302) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 hour+))
    (pad 3 smd rect (at -1.27 -3.302) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(R3-Pad1)"))
    (pad 4 smd rect (at 0 -3.302) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(TP6-Pad1)"))
    (pad 5 smd rect (at 1.27 -3.302) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(R2-Pad1)"))
    (pad 6 smd rect (at 2.54 -3.302) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(R1-Pad1)"))
    (pad 7 smd rect (at 3.81 -3.302) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(TP5-Pad1)"))
    (pad 8 smd rect (at 3.81 3.048) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(TP4-Pad1)"))
    (pad 9 smd rect (at 2.54 3.048) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(TP2-Pad1)"))
    (pad 11 smd rect (at 0 3.048) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J4-Pad2)"))
    (pad 12 smd rect (at -1.27 3.048) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(J4-Pad1)"))
    (pad 13 smd rect (at -2.54 3.048) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 32 min+))
    (pad 14 smd rect (at -3.81 3.048) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 31 GND))
    (pad 10 smd rect (at 1.27 3.048) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J4-Pad3)"))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 0)
    (at 211.455 76.835)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U4 (at 0 -1.27) (layer F.SilkS))
    (fp_text value MCP7940M-I/SN (at 0 1.27) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 7 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R3-Pad1)"))
    (pad 6 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R2-Pad1)"))
    (pad 5 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R1-Pad1)"))
    (pad 4 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 31 GND))
    (pad 3 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U4-Pad3)"))
    (pad 2 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module switch:crystal (layer F.Cu) (tedit 5B1FFECB)
    (at 225.31 79.87)
    (fp_text reference Y1 (at 3.6 -2.5) (layer F.SilkS))
    (fp_text value Crystal (at 3.6 -3.5) (layer F.Fab))
    (pad 1 smd trapezoid (at -5.6 -3.6) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 smd trapezoid (at -5.6 -2.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 smd trapezoid (at 0.5 -2.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd trapezoid (at 0.5 -3.6) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask))
  )
  (module switch:battery1 (layer B.Cu) (tedit 5B207AE1)
    (at 235.775 46.61 90)
    (fp_text reference BT1 (at 0 -0.5 90) (layer B.SilkS))
    (fp_text value Battery_Cell (at 0 0.5 90) (layer B.Fab))
    (pad 2 smd circle (at -21.97 -10.985 90) (size 12.7 12.7) (layers B.Cu B.Paste B.Mask)
      (net 31 GND))
    (pad 1 smd rect (at -21.97 0 90) (size 5.08 2.79) (layers B.Cu B.Paste B.Mask)
      (net 30 VCC))
    (pad 1 smd rect (at -21.97 -21.97 90) (size 5.08 2.79) (layers B.Cu B.Paste B.Mask)
      (net 30 VCC))
  )
  (module switch:button (layer B.Cu) (tedit 5B2C65CD)
    (at 239.91 88.44)
    (fp_text reference SW2 (at 0 -0.5) (layer B.SilkS))
    (fp_text value SW_Push (at -5.1 1.4) (layer B.Fab))
    (pad 1 smd rect (at -7.5 3) (size 1.4 2.2) (layers B.Cu B.Paste B.Mask)
      (net 32 min+))
    (pad 2 smd rect (at -7.5 -0.5) (size 1.4 2.2) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(SW2-Pad2)"))
    (pad 3 smd rect (at -3.1 -0.5) (size 1.4 2.2) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -3.1 3) (size 1.4 2.2) (layers B.Cu B.Paste B.Mask))
  )
  (module switch:button (layer B.Cu) (tedit 5B2C65CD)
    (at 230 94)
    (fp_text reference SW3 (at 0 -0.5) (layer B.SilkS))
    (fp_text value SW_Push (at -5.1 1.4) (layer B.Fab))
    (pad 1 smd rect (at -7.5 3) (size 1.4 2.2) (layers B.Cu B.Paste B.Mask)
      (net 33 hour+))
    (pad 2 smd rect (at -7.5 -0.5) (size 1.4 2.2) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(SW2-Pad2)"))
    (pad 3 smd rect (at -3.1 -0.5) (size 1.4 2.2) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -3.1 3) (size 1.4 2.2) (layers B.Cu B.Paste B.Mask))
  )
  (module switch:button (layer B.Cu) (tedit 5B2C65CD)
    (at 209.67 90.94 180)
    (fp_text reference SW4 (at 0.12 2.04 180) (layer B.SilkS))
    (fp_text value SW_Push (at -5.1 1.4 180) (layer B.Fab))
    (pad 1 smd rect (at -7.5 3 180) (size 1.4 2.2) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(SW2-Pad2)"))
    (pad 2 smd rect (at -7.5 -0.5 180) (size 1.4 2.2) (layers B.Cu B.Paste B.Mask)
      (net 31 GND))
    (pad 3 smd rect (at -3.1 -0.5 180) (size 1.4 2.2) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -3.1 3 180) (size 1.4 2.2) (layers B.Cu B.Paste B.Mask))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 233.68 78.57 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.45 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.55 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 31 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module switch:limit (layer F.Cu) (tedit 5B340F0C)
    (at 237.49 81.28 270)
    (fp_text reference SW1 (at 0 0.5 270) (layer F.SilkS))
    (fp_text value SW_Push (at 0 -0.5 270) (layer F.Fab))
    (pad 1 smd rect (at -4 0 270) (size 1.8 2.5) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at -0.5 0 270) (size 1.8 2.5) (layers B.Cu B.Paste B.Mask)
      (net 31 GND))
    (pad "" np_thru_hole circle (at -2.25 -2.25 270) (size 1.2 1.2) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.25 -5 270) (size 1.2 1.2) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.05 -5 270) (size 1.2 1.2) (drill 1.1) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 264.16 87.63 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 EN))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 VCC))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 222.25 82.55)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 218.9 95.98)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP1 (at -5.08 20.32) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 31 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 221.44 95.98)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP2 (at -2.54 20.32) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 40 "Net-(TP2-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 223.98 95.98)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP3 (at 0 20.32) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 30 VCC))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 226.52 95.98)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP4 (at 0 20.32) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 41 "Net-(TP4-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 229.06 95.98)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP5 (at 0 20.32) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 42 "Net-(TP5-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 231.6 95.98)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP6 (at 0 20.32) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 43 "Net-(TP6-Pad1)"))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 216.9 80)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.45) (layer B.SilkS))
    (fp_text value R_Small (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 30 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 249.09 74.93)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.45) (layer B.SilkS))
    (fp_text value R (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 249.09 78.74 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value R (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 253.83 67.31 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value R (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 254.17 71.12)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 1.45) (layer B.SilkS))
    (fp_text value R (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 254.17 74.93 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value R (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 254.17 78.74 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value R (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 263.06 69.85 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value R (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 263.06 73.66 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value R (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 263.06 77.47 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value R (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 267.8 67.31 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value R (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 267.8 71.12 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value R (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 267.8 74.93 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value R (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 267.8 78.74 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value R (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 276.86 80.18 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(D14-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 263.06 64.77)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 0 1.45) (layer B.SilkS))
    (fp_text value R (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(D15-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 248.75 81.28)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0 1.45) (layer B.SilkS))
    (fp_text value R (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module switch:pot (layer F.Cu) (tedit 5B372DE7)
    (at 251.4 88.4 180)
    (fp_text reference RV1 (at 0 0.5 180) (layer F.SilkS))
    (fp_text value POT (at 0 -0.5 180) (layer F.Fab))
    (pad 2 smd rect (at 3.75 -0.5 180) (size 1.6002 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 31 GND))
    (pad 1 smd rect (at 2.75 2.75 180) (size 1.1938 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(RV1-Pad1)"))
    (pad 3 smd rect (at 4.75 2.75 180) (size 1.1938 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R10-Pad2)"))
  )
  (gr_text Diodes (at 243.84 62.23) (layer F.SilkS))
  (gr_text - (at 248.896394 62.129814 180) (layer F.SilkS))
  (gr_text + (at 251.436394 62.129814 180) (layer F.SilkS))
  (gr_line (start 204 101) (end 204 59) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 284 101) (end 204 101) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 284 59) (end 284 101) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204 59) (end 284 59) (layer Edge.Cuts) (width 0.15))
  (gr_text MM (at 266.7 68.58) (layer F.SilkS))
  (gr_text HH (at 252.73 72.39) (layer F.SilkS))
  (zone (net 30) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 204 59) (xy 284 59) (xy 284 101) (xy 204 101)
      )
    )
  )
  (zone (net 31) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 204 59) (xy 284 59) (xy 284 101) (xy 204 101)
      )
    )
  )
)
