<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="25.4" y1="24.13" x2="24.13" y2="25.4" width="0" layer="20" curve="90"/>
<wire x1="24.13" y1="25.4" x2="1.27" y2="25.4" width="0" layer="20"/>
<wire x1="1.27" y1="25.4" x2="0" y2="24.13" width="0" layer="20" curve="90"/>
<wire x1="0" y1="24.13" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="24.13" y2="0" width="0" layer="20"/>
<wire x1="24.13" y1="0" x2="25.4" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="25.4" y1="1.27" x2="25.4" y2="24.13" width="0" layer="20"/>
<text>(Bobricius) - PeMi Technology
Factory For Materializing Dreams</text>
<text>https://www.youtube.com/bobricius
https://hackaday.io/bobricius
www.tindie.com/stores/bobricius/
www.tindie.com/stores/kitsforkids/</text>
<text>www.pemi.technology</text>
<text>+

-</text>
<text>+

-</text>
<text>www.pemi.technology</text>
<text>IN</text>
</plain>
<libraries>
<library name="led">
<packages>
<package name="KA-3528ASYC">
<description>&lt;b&gt;SURFACE MOUNT LED LAMP&lt;/b&gt; 3.5x2.8mm&lt;p&gt;
Source: http://www.kingbright.com/manager/upload/pdf/KA-3528ASYC(Ver1189474662.1)</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
</packages>
</library>
<library name="transistor-npn">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP07R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-SMD">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library="rcl" package="R1206W" value="1K5"/>
<element name="TP1" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP2" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP3" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP4" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="LED" library="led" package="KA-3528ASYC" value="">
<attribute name="VALUE"/>
</element>
<element name="TP5" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP6" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP7" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP8" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="Q2" library="transistor-npn" package="SOT23" value="MMBT2222ALTG1"/>
<element name="J1" library="SparkFun-Connectors" package="JST-2-SMD" value="">
<attribute name="VALUE"/>
<attribute name="PROD_ID" value="CONN-11443"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="N$3">
<contactref element="TP8" pad="TP"/>
<contactref element="LED" pad="A"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="TP3" pad="TP"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="N$5">
<contactref element="TP1" pad="TP"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="GND">
<contactref element="LED" pad="C"/>
<contactref element="Q2" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="TP6" pad="TP"/>
<contactref element="TP7" pad="TP"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
</signals>
</board>
</drawing>
</eagle>
