(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 77)
    (no_connects 0)
    (area 142.164999 86.284999 167.715001 111.835001)
    (thickness 1.6)
    (drawings 19)
    (tracks 341)
    (zones 0)
    (modules 27)
    (nets 47)
  )
  (page A)
  (title_block
    (title "Beetje 32U4 Blok")
    (date 2018-08-10)
    (rev 0.0)
    (company www.MakersBox.us)
    (comment 1 648.ken@gmail.com)
  )
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (trace_clearance 0.2)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 0.508)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /AREF)
  (net 3 VBUS)
  (net 4 +BATT)
  (net 5 /D4)
  (net 6 /D6)
  (net 7 /D8)
  (net 8 /D13)
  (net 9 /D12)
  (net 10 /D11)
  (net 11 /D10)
  (net 12 /D9)
  (net 13 /D7)
  (net 14 /SCL)
  (net 15 /SDA)
  (net 16 /D1)
  (net 17 /D0)
  (net 18 /A0)
  (net 19 /A1)
  (net 20 /A2)
  (net 21 /A3)
  (net 22 /A4)
  (net 23 /A5)
  (net 24 /SCK)
  (net 25 /MOSI)
  (net 26 /MISO)
  (net 27 "Net-(R4-Pad2)")
  (net 28 "Net-(R5-Pad2)")
  (net 29 "Net-(R9-Pad1)")
  (net 30 "Net-(U1-Pad2)")
  (net 31 "Net-(U1-Pad16)")
  (net 32 "Net-(U1-Pad17)")
  (net 33 /D5)
  (net 34 "Net-(U2-Pad4)")
  (net 35 "Net-(X3-Pad4)")
  (net 36 /RXLED)
  (net 37 /TXLED)
  (net 38 /VHI)
  (net 39 /~RESET)
  (net 40 /D+)
  (net 41 /D-)
  (net 42 VCC)
  (net 43 "Net-(D13-Pad2)")
  (net 44 "Net-(F1-Pad2)")
  (net 45 "Net-(D3-Pad1)")
  (net 46 "Net-(D5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /AREF)
    (add_net /D+)
    (add_net /D-)
    (add_net /D0)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RXLED)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TXLED)
    (add_net /VHI)
    (add_net /~RESET)
    (add_net GND)
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(X3-Pad4)")
    (add_net VBUS)
    (add_net VCC)
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 5B6DEFF3)
    (at 161.29 109.855 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0 -0.127 270) (layer F.SilkS) hide)
    (fp_text value TX (at -2.413 0 270) (layer F.SilkS))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module footprints:Resonator_SMD_CTSC_1.3mmx3.2mm (layer F.Cu) (tedit 5B6DD41E)
    (at 156.464 106.172 180)
    (descr "SMD Resomator/Filter Murata TPSKA, http://cdn-reichelt.de/documents/datenblatt/B400/SFECV-107.pdf, hand-soldering, 7.9x3.8mm^2 package")
    (tags "SMD SMT ceramic resonator filter filter hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at -0.127 -1.27 180) (layer F.SilkS) hide)
    (fp_text value "8 Mhz" (at 0 1.397 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.2 0 180) (size 0.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad17)"))
    (pad 2 smd rect (at 0 0 180) (size 0.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.2 0 180) (size 0.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad16)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Resonator_SMD_muRata_TPSKA-3pin_7.9x3.8mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:EVQ-P7A (layer F.Cu) (tedit 5B6DD3F6)
    (at 166.116 92.075 90)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (attr smd)
    (fp_text reference SW1 (at -0.127 0.127 180) (layer F.SilkS))
    (fp_text value RESET (at -3.429 -0.127 180) (layer F.SilkS))
    (fp_text user %R (at 0 -2.45 90) (layer F.Fab))
    (pad 2 smd rect (at 1.8 0.725 90) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 39 /~RESET))
    (pad 2 smd rect (at -1.8 0.725 90) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 39 /~RESET))
    (pad 1 smd rect (at 1.8 -0.7 90) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.8 -0.7 90) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_KMR2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/Maker's Box/Downloads/3d_switch (1)/walter/switch/smd_push2.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Jumper (layer B.Cu) (tedit 5B6DF181)
    (at 149.606 93.599 180)
    (attr smd)
    (fp_text reference JMP1 (at 0 -1.143 180) (layer B.SilkS) hide)
    (fp_text value 5V (at 0 -1.25 180) (layer B.SilkS))
    (fp_text user %R (at 0 1.2 180) (layer B.Fab))
    (pad 1 smd rect (at -0.3 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 42 VCC))
    (pad 2 smd rect (at 0.3 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 VBUS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:MadeInOregonRev25 (layer F.Cu) (tedit 0)
    (at 164.084 97.409)
    (fp_text reference VAL (at 0 0) (layer F.SilkS) hide)
    (fp_text value MadeInOregonRev25 (at 0 0) (layer F.SilkS) hide)
  )
  (module footprints:KiCad-Logo2_8mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 158.623 104.267 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_8mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module footprints:C_0805 (layer F.Cu) (tedit 5B6DF131)
    (at 147.32 92.71 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.397 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 38 /VHI))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0603 (layer F.Cu) (tedit 5B6DF0BC)
    (at 147.32 96.52 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -0.127 1.27 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 151.13 106.045 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0805 (layer F.Cu) (tedit 5B6DF0C6)
    (at 144.272 96.774 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Pin_Header_Straight_2x03_Pitch2.54mm (layer B.Cu) (tedit 5B6DE115)
    (at 159.385 99.06 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference CON1 (at 1.27 2.33 90) (layer B.SilkS) hide)
    (fp_text value AVR-ISP-6 (at 1.27 -7.41 90) (layer B.Fab))
    (fp_text user %R (at 1.27 -2.54 360) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 0.508) (layers *.Cu *.Mask)
      (net 26 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 0.508) (layers *.Cu *.Mask)
      (net 42 VCC))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 0.508) (layers *.Cu *.Mask)
      (net 24 /SCK))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7 1.7) (drill 0.508) (layers *.Cu *.Mask)
      (net 25 /MOSI))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 0.508) (layers *.Cu *.Mask)
      (net 39 /~RESET))
    (pad 6 thru_hole oval (at 2.54 -5.08 90) (size 1.7 1.7) (drill 0.508) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module footprints:D_SOD-123F (layer B.Cu) (tedit 5B6DF1BB)
    (at 144.78 90.424 180)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D1 (at 0.127 -1.651 180) (layer B.SilkS))
    (fp_text value MBR120 (at 0 -2.1 180) (layer B.Fab))
    (fp_text user %R (at -0.127 1.905 180) (layer B.Fab))
    (pad 1 smd rect (at -1.4 0 180) (size 1.1 1.1) (layers B.Cu B.Paste B.Mask)
      (net 38 /VHI))
    (pad 2 smd rect (at 1.4 0 180) (size 1.1 1.1) (layers B.Cu B.Paste B.Mask)
      (net 3 VBUS))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:D_SOD-123F (layer B.Cu) (tedit 5B6DF1A5)
    (at 149.86 90.424)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D4 (at 0 1.651) (layer B.SilkS))
    (fp_text value MBR120 (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at -0.127 1.905) (layer B.Fab))
    (pad 1 smd rect (at -1.4 0) (size 1.1 1.1) (layers B.Cu B.Paste B.Mask)
      (net 38 /VHI))
    (pad 2 smd rect (at 1.4 0) (size 1.1 1.1) (layers B.Cu B.Paste B.Mask)
      (net 4 +BATT))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 5B6DEFD7)
    (at 163.195 109.855 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value RX (at -2.413 -0.127 270) (layer F.SilkS))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 5B6DEFA4)
    (at 165.1 109.855 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D13 (at -2.921 -0.127 270) (layer F.SilkS))
    (fp_text value D13 (at 0 -0.127 270) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module footprints:R_1206 (layer B.Cu) (tedit 5B6DF1D0)
    (at 144.78 93.853 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference F1 (at 0.127 -1.778 180) (layer B.SilkS))
    (fp_text value Polyfuse (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 3 VBUS))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(F1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5B6DE62D)
    (at 158.75 110.49 270)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 2.286 -1.27 360) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 2.286 9.525 360) (layer F.Fab))
    (fp_text user %R (at 0 6.35 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /D9))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /SDA))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /SCL))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /MISO))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /MOSI))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /SCK))
  )
  (module footprints:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 5B6DE634)
    (at 163.83 87.63 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J4 (at -2.286 0.127 360) (layer F.SilkS) hide)
    (fp_text value Conn_01x08 (at -2.413 14.605 360) (layer F.Fab))
    (fp_text user %R (at 0 8.89 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /~RESET))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /D10))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /A0))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /A1))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +BATT))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 VCC))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VBUS))
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 5B6DF016)
    (at 166.116 101.092 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.508 1.27 270) (layer F.SilkS))
    (fp_text value 180 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 /TXLED))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 5B6DF008)
    (at 166.116 104.648 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -0.508 1.27 270) (layer F.SilkS))
    (fp_text value 180 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 /RXLED))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 5B6DF066)
    (at 148.844 103.505 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 1.905 -0.127 270) (layer F.SilkS))
    (fp_text value 22 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 /D+))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 5B6DF079)
    (at 148.844 100.33 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.778 0 270) (layer F.SilkS))
    (fp_text value 22 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 /D-))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 5B6DF02D)
    (at 166.116 97.536 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0.635 -1.27 90) (layer F.SilkS))
    (fp_text value 180 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D13-Pad2)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /D13))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 5B6DF0EE)
    (at 143.891 90.297)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 100K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 /VHI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:TQFP-44_10x10mm_Pitch0.8mm (layer F.Cu) (tedit 5B6DF053)
    (at 156.845 97.79)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 5.461 6.223) (layer F.SilkS))
    (fp_text value ATMEGA32U4-AU (at 0.127 4.445) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 /D7))
    (pad 2 smd rect (at -5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 /D-))
    (pad 4 smd rect (at -5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 /D+))
    (pad 5 smd rect (at -5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (pad 7 smd rect (at -5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 VBUS))
    (pad 8 smd rect (at -5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 /RXLED))
    (pad 9 smd rect (at -5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 /SCK))
    (pad 10 smd rect (at -5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 /MOSI))
    (pad 11 smd rect (at -5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 /MISO))
    (pad 12 smd rect (at -4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 /D11))
    (pad 13 smd rect (at -3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 /~RESET))
    (pad 14 smd rect (at -2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (pad 15 smd rect (at -1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at 0 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at 0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /SCL))
    (pad 19 smd rect (at 1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 /SDA))
    (pad 20 smd rect (at 2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 /D0))
    (pad 21 smd rect (at 3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /D1))
    (pad 22 smd rect (at 4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 /TXLED))
    (pad 23 smd rect (at 5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (pad 25 smd rect (at 5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 /D4))
    (pad 26 smd rect (at 5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 /D12))
    (pad 27 smd rect (at 5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /D6))
    (pad 28 smd rect (at 5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 /D8))
    (pad 29 smd rect (at 5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /D9))
    (pad 30 smd rect (at 5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /D10))
    (pad 31 smd rect (at 5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 /D5))
    (pad 32 smd rect (at 5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 /D13))
    (pad 33 smd rect (at 5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (pad 34 smd rect (at 4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (pad 35 smd rect (at 3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 /A0))
    (pad 37 smd rect (at 1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /A1))
    (pad 38 smd rect (at 0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /A2))
    (pad 39 smd rect (at 0 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 /A3))
    (pad 40 smd rect (at -0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 /A4))
    (pad 41 smd rect (at -1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 /A5))
    (pad 42 smd rect (at -2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 /AREF))
    (pad 43 smd rect (at -3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 44 smd rect (at -4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SOT-23-5 (layer F.Cu) (tedit 5B6DF0E4)
    (at 144.145 93.345 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 1.143 0 270) (layer F.SilkS))
    (fp_text value MIC5225-3.3 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 38 /VHI))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R9-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:USB_Micro-B_Molex-105017-0001 (layer F.Cu) (tedit 5B6DF08E)
    (at 144.145 102.87 270)
    (descr http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf)
    (tags "Micro-USB SMD Typ-B")
    (attr smd)
    (fp_text reference X3 (at 3.302 -3.556 270) (layer F.SilkS))
    (fp_text value USB_OTG (at 0.3 3.45 270) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 1.8 270) (layer Dwgs.User))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 6 smd rect (at 1 0.35 270) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -2.5 -2.35 270) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.65 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R5-Pad2)"))
    (pad 1 smd rect (at -1.3 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(F1-Pad2)"))
    (pad 5 smd rect (at 1.3 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(X3-Pad4)"))
    (pad 3 smd rect (at 0 -2.35 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R4-Pad2)"))
    (pad 6 thru_hole circle (at 2.5 -2.35 270) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -1 0.35 270) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -3.5 0.35 90) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 3.5 0.35 270) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.9 0.35 270) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.9 0.35 270) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_USB.3dshapes/USB_Micro-B_Molex-105017-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ../../../../../../Users/kolsen/Documents/git/KiCad/projects/Beetje/design_files_32U4/usb_B_micro_smd.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Rev 0.0\nAug 2018" (at 148.336 102.997) (layer B.SilkS))
  (gr_text "VBUS GND VCC BAT  A1  A0  D10 RST" (at 144.907 89.535) (layer F.SilkS))
  (gr_line (start 142.24 109.22) (end 142.24 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.1 111.76) (end 144.78 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 88.9) (end 167.64 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 86.36) (end 165.1 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.78 88.9) (end 142.24 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.78 109.22) (end 144.78 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 165.1 109.22) (end 167.64 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 165.1 88.9) (end 165.1 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 25.4 (width 0.3) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 176.61 99.06 270) (layer Dwgs.User))
    (feature1 (pts (xy 167.64 111.76) (xy 177.96 111.76)))
    (feature2 (pts (xy 167.64 86.36) (xy 177.96 86.36)))
    (crossbar (pts (xy 175.26 86.36) (xy 175.26 111.76)))
    (arrow1a (pts (xy 175.26 111.76) (xy 174.673579 110.633496)))
    (arrow1b (pts (xy 175.26 111.76) (xy 175.846421 110.633496)))
    (arrow2a (pts (xy 175.26 86.36) (xy 174.673579 87.486504)))
    (arrow2b (pts (xy 175.26 86.36) (xy 175.846421 87.486504)))
  )
  (dimension 25.4 (width 0.3) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 154.94 79.930001) (layer Dwgs.User))
    (feature1 (pts (xy 142.24 86.36) (xy 142.24 78.580001)))
    (feature2 (pts (xy 167.64 86.36) (xy 167.64 78.580001)))
    (crossbar (pts (xy 167.64 81.280001) (xy 142.24 81.280001)))
    (arrow1a (pts (xy 142.24 81.280001) (xy 143.366504 80.69358)))
    (arrow1b (pts (xy 142.24 81.280001) (xy 143.366504 81.866422)))
    (arrow2a (pts (xy 167.64 81.280001) (xy 166.513496 80.69358)))
    (arrow2b (pts (xy 167.64 81.280001) (xy 166.513496 81.866422)))
  )
  (gr_text "- ISP +" (at 156.845 94.234) (layer B.SilkS))
  (gr_text www.MakersBox.us (at 166.751 108.204) (layer B.SilkS))
  (gr_text "Beetje Blok\n32U4" (at 167.132 91.44) (layer B.SilkS))
  (gr_text ~ (at 135.636 90.678) (layer B.SilkS))
  (gr_text ~ (at 135.128 90.551) (layer B.SilkS))
  (gr_text "SCK MO  MI  SCL SDA D9" (at 144.78 108.712) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.18 113.03) (xy 127 113.03) (xy 127 82.55) (xy 170.18 82.55)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 114.3) (xy 125.73 114.3) (xy 125.73 81.28) (xy 171.45 81.28)
      )
    )
  )
)
