(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 64)
    (no_connects 1)
    (area 16.5 13.5 53.5 76.250001)
    (thickness 1.6)
    (drawings 22)
    (tracks 301)
    (zones 0)
    (modules 30)
    (nets 43)
  )
  (page A4 portrait)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.2)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 1.35)
    (pad_drill 0.1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFCEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 RESET)
  (net 4 /SCK)
  (net 5 "Net-(D1-Pad1)")
  (net 6 LED)
  (net 7 "Net-(IC1-Pad19)")
  (net 8 "Net-(IC1-Pad20)")
  (net 9 "Net-(IC1-Pad23)")
  (net 10 /SDA)
  (net 11 /SCL)
  (net 12 "Net-(IC1-Pad30)")
  (net 13 TX)
  (net 14 BTN)
  (net 15 "Net-(P3-Pad1)")
  (net 16 "Net-(P3-Pad3)")
  (net 17 "Net-(P3-Pad5)")
  (net 18 "Net-(P3-Pad2)")
  (net 19 "Net-(P3-Pad4)")
  (net 20 "Net-(P4-Pad1)")
  (net 21 "Net-(P4-Pad3)")
  (net 22 "Net-(P4-Pad5)")
  (net 23 "Net-(P4-Pad2)")
  (net 24 "Net-(P4-Pad4)")
  (net 25 ACCEL-VCC)
  (net 26 RIGHT-EYE-1)
  (net 27 RIGHT-EYE-2)
  (net 28 RIGHT-EYE-3)
  (net 29 RIGHT-EYE-4)
  (net 30 RIGHT-LED-5)
  (net 31 LEFT-LED-1)
  (net 32 LEFT-LED-2)
  (net 33 LEFT-LED-3)
  (net 34 LEFT-LED-4)
  (net 35 LEFT-LED-5)
  (net 36 CE)
  (net 37 "Net-(U1-Pad3)")
  (net 38 "Net-(D2-Pad1)")
  (net 39 "Net-(IC1-Pad7)")
  (net 40 "Net-(IC1-Pad8)")
  (net 41 +BATT)
  (net 42 "Net-(P1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 1.2)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net +BATT)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net ACCEL-VCC)
    (add_net BTN)
    (add_net CE)
    (add_net GND)
    (add_net LED)
    (add_net LEFT-LED-1)
    (add_net LEFT-LED-2)
    (add_net LEFT-LED-3)
    (add_net LEFT-LED-4)
    (add_net LEFT-LED-5)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad30)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P4-Pad5)")
    (add_net "Net-(U1-Pad3)")
    (add_net RESET)
    (add_net RIGHT-EYE-1)
    (add_net RIGHT-EYE-2)
    (add_net RIGHT-EYE-3)
    (add_net RIGHT-EYE-4)
    (add_net RIGHT-LED-5)
    (add_net TX)
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59D4FFBB)
    (at 48.4 38.42 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P5 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value CONN_4 (at 0 9.95 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 ACCEL-VCC))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 3 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 3 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /SCL))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 3 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /SDA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 35 54 225)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 -6.05 225) (layer F.SilkS))
    (fp_text value ATMEGA328P-A (at 0 6.05 225) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 26 RIGHT-EYE-1))
    (pad 2 smd rect (at -4.25 -2 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 RIGHT-EYE-2))
    (pad 3 smd rect (at -4.25 -1.2 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -4.25 -0.4 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 5 smd rect (at -4.25 0.4 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -4.25 1.2 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 7 smd rect (at -4.25 2 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.25 2.8 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -2.8 4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 RIGHT-EYE-3))
    (pad 10 smd rect (at -2 4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 RIGHT-EYE-4))
    (pad 11 smd rect (at -1.2 4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 30 RIGHT-LED-5))
    (pad 12 smd rect (at -0.4 4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 31 LEFT-LED-1))
    (pad 13 smd rect (at 0.4 4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 LEFT-LED-2))
    (pad 14 smd rect (at 1.2 4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 LEFT-LED-3))
    (pad 15 smd rect (at 2 4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 LEFT-LED-4))
    (pad 16 smd rect (at 2.8 4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 LEFT-LED-5))
    (pad 17 smd rect (at 4.25 2.8 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCK))
    (pad 18 smd rect (at 4.25 2 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 19 smd rect (at 4.25 1.2 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 4.25 -1.2 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 +BATT))
    (pad 23 smd rect (at 4.25 -2 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad23)"))
    (pad 24 smd rect (at 4.25 -2.8 225) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 LED))
    (pad 25 smd rect (at 2.8 -4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 36 CE))
    (pad 26 smd rect (at 2 -4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 ACCEL-VCC))
    (pad 27 smd rect (at 1.2 -4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 /SDA))
    (pad 28 smd rect (at 0.4 -4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCL))
    (pad 29 smd rect (at -0.4 -4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 RESET))
    (pad 30 smd rect (at -1.2 -4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad30)"))
    (pad 31 smd rect (at -2 -4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 TX))
    (pad 32 smd rect (at -2.8 -4.25 315) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 14 BTN))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer F.Cu) (tedit 5936E9F8)
    (at 24.6 47.2 180)
    (attr smd)
    (fp_text reference R10 (at 0 -0.7 180) (layer F.SilkS))
    (fp_text value 47Ω (at 0 0.8 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 LEFT-LED-3))
    (pad 2 smd rect (at 1 0 180) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P4-Pad3)"))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer F.Cu) (tedit 5936E9F8)
    (at 24.6 45.2 180)
    (attr smd)
    (fp_text reference R9 (at 0 -0.7 180) (layer F.SilkS))
    (fp_text value 47Ω (at 0 0.8 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 LEFT-LED-2))
    (pad 2 smd rect (at 1 0 180) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P4-Pad2)"))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer F.Cu) (tedit 5936E9F8)
    (at 24.6 43.2 180)
    (attr smd)
    (fp_text reference R8 (at 0 -0.7 180) (layer F.SilkS))
    (fp_text value 47Ω (at 0 0.8 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 LEFT-LED-1))
    (pad 2 smd rect (at 1 0 180) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P4-Pad1)"))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer F.Cu) (tedit 5936E9F8)
    (at 24.6 51.2 180)
    (attr smd)
    (fp_text reference R12 (at 0 -0.7 180) (layer F.SilkS))
    (fp_text value 47Ω (at 0 0.8 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 LEFT-LED-5))
    (pad 2 smd rect (at 1 0 180) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P4-Pad5)"))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer F.Cu) (tedit 5936E9F8)
    (at 24.6 49.2 180)
    (attr smd)
    (fp_text reference R11 (at 0 -0.7 180) (layer F.SilkS))
    (fp_text value 47Ω (at 0 0.8 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 LEFT-LED-4))
    (pad 2 smd rect (at 1 0 180) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P4-Pad4)"))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.00mm (layer F.Cu) (tedit 59D50013)
    (at 21.4 43.2)
    (descr "Through hole straight pin header, 1x05, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.00mm single row")
    (fp_text reference P4 (at 0 -2.06) (layer F.SilkS))
    (fp_text value CONN_5 (at 0 10.06) (layer F.Fab))
    (fp_text user %R (at 0 4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3 1.35) (drill 0.1) (layers *.Cu *.Mask)
      (net 20 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2) (size 3 1.35) (drill 0.1) (layers *.Cu *.Mask)
      (net 23 "Net-(P4-Pad2)"))
    (pad 3 thru_hole oval (at 0 4) (size 3 1.35) (drill 0.1) (layers *.Cu *.Mask)
      (net 21 "Net-(P4-Pad3)"))
    (pad 4 thru_hole oval (at 0 6) (size 3 1.35) (drill 0.1) (layers *.Cu *.Mask)
      (net 24 "Net-(P4-Pad4)"))
    (pad 5 thru_hole oval (at 0 8) (size 3 1.35) (drill 0.1) (layers *.Cu *.Mask)
      (net 22 "Net-(P4-Pad5)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:ISP-edge-connector (layer B.Cu) (tedit 580D053D)
    (at 31.6 62 180)
    (fp_text reference CON1 (at 5.8 -10.1 180) (layer B.SilkS))
    (fp_text value AVR-ISP6 (at 5.8 -12.3 180) (layer B.SilkS))
    (pad 6 smd rect (at 9.68 -4 180) (size 1.5 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 9.68 -4 180) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 3 RESET))
    (pad 4 smd rect (at 7.14 -4 180) (size 1.5 4) (layers B.Cu B.Paste B.Mask)
      (net 34 LEFT-LED-4))
    (pad 3 smd rect (at 7.14 -4 180) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCK))
    (pad 2 smd rect (at 4.6 -4 180) (size 1.5 4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at 4.6 -4 180) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 35 LEFT-LED-5))
    (model ../3d_models/ab2_header/AB2_HDR_M01-1V.wrl
      (at (xyz -0.1 -0.05 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
    (model ../3d_models/ab2_header/AB2_HDR_M01-1V.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
    (model ../3d_models/ab2_header/AB2_HDR_M01-1V.wrl
      (at (xyz 0.1 -0.05 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
    (model ../3d_models/ab2_header/AB2_HDR_M01-1V.wrl
      (at (xyz -0.1 0.05 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
    (model ../3d_models/ab2_header/AB2_HDR_M01-1V.wrl
      (at (xyz 0 0.05 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
    (model ../3d_models/ab2_header/AB2_HDR_M01-1V.wrl
      (at (xyz 0.1 0.05 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0805 (layer F.Cu) (tedit 54D7CFF6)
    (at 30 28.4)
    (attr smd)
    (fp_text reference C1 (at 0 -0.3175) (layer F.SilkS))
    (fp_text value 10µF (at 0 0.381) (layer F.SilkS))
    (pad 1 smd rect (at -1.2 0) (size 1.4 1.397) (layers F.Cu F.Paste F.Mask)
      (net 41 +BATT))
    (pad 2 smd rect (at 1.2 0) (size 1.4 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0805 (layer F.Cu) (tedit 54D7CFF6)
    (at 39.2 47.4)
    (attr smd)
    (fp_text reference C3 (at 0 -0.3175) (layer F.SilkS))
    (fp_text value C (at 0 0.381) (layer F.SilkS))
    (pad 1 smd rect (at -1.2 0) (size 1.4 1.397) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.2 0) (size 1.4 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0805 (layer F.Cu) (tedit 54D7CFF6)
    (at 39.2 45.2)
    (attr smd)
    (fp_text reference C4 (at 0 -0.3175) (layer F.SilkS))
    (fp_text value C (at 0 0.381) (layer F.SilkS))
    (pad 1 smd rect (at -1.2 0) (size 1.4 1.397) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.2 0) (size 1.4 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer F.Cu) (tedit 5936E9F8)
    (at 35 66.2 270)
    (attr smd)
    (fp_text reference D2 (at 0 -0.7 270) (layer F.SilkS))
    (fp_text value LED (at 0 0.8 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:HEADER-1 placed (layer F.Cu) (tedit 55322239)
    (at 27 24)
    (fp_text reference P1 (at 0 2.54) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 -2.54) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 1.6764 3.3528) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P1-Pad1)"))
    (model ../3d_models/ab2_header/AB2_HDR_M01-1V.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:HEADER-1 placed (layer F.Cu) (tedit 55322239)
    (at 30.2 24)
    (fp_text reference P2 (at 0 2.54) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 -2.54) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 1.6764 3.3528) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model ../3d_models/ab2_header/AB2_HDR_M01-1V.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer B.Cu) (tedit 5936E9F8)
    (at 34.2 63.6 270)
    (attr smd)
    (fp_text reference R1 (at 0 0.7 270) (layer B.SilkS))
    (fp_text value 4k7 (at 0 -0.8 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 RESET))
    (pad 2 smd rect (at 1 0 270) (size 1 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer F.Cu) (tedit 5936E9F8)
    (at 33.8 63.4)
    (attr smd)
    (fp_text reference R2 (at 0 -0.7) (layer F.SilkS))
    (fp_text value 1k (at 0 0.8) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 LED))
    (pad 2 smd rect (at 1 0) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D2-Pad1)"))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer F.Cu) (tedit 5936E9F8)
    (at 45 51.2)
    (attr smd)
    (fp_text reference R3 (at 0 -0.7) (layer F.SilkS))
    (fp_text value 47Ω (at 0 0.8) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 RIGHT-EYE-1))
    (pad 2 smd rect (at 1 0) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P3-Pad1)"))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer F.Cu) (tedit 5936E9F8)
    (at 45 49.2)
    (attr smd)
    (fp_text reference R4 (at 0 -0.7) (layer F.SilkS))
    (fp_text value 47Ω (at 0 0.8) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 RIGHT-EYE-2))
    (pad 2 smd rect (at 1 0) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P3-Pad2)"))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer F.Cu) (tedit 5936E9F8)
    (at 45 47.2)
    (attr smd)
    (fp_text reference R5 (at 0 -0.7) (layer F.SilkS))
    (fp_text value 47Ω (at 0 0.8) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 RIGHT-EYE-3))
    (pad 2 smd rect (at 1 0) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P3-Pad3)"))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer F.Cu) (tedit 5936E9F8)
    (at 45 45.2)
    (attr smd)
    (fp_text reference R6 (at 0 -0.7) (layer F.SilkS))
    (fp_text value 47Ω (at 0 0.8) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 RIGHT-EYE-4))
    (pad 2 smd rect (at 1 0) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P3-Pad4)"))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer F.Cu) (tedit 5936E9F8)
    (at 45 43.2)
    (attr smd)
    (fp_text reference R7 (at 0 -0.7) (layer F.SilkS))
    (fp_text value 47Ω (at 0 0.8) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 RIGHT-LED-5))
    (pad 2 smd rect (at 1 0) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P3-Pad5)"))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-23-5 (layer F.Cu) (tedit 58CE4E80)
    (at 29.6 32.2 90)
    (descr "5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf")
    (tags TSOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0 -2.45 90) (layer F.SilkS))
    (fp_text value NCP1402 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0.2 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.31 -0.95 90) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 36 CE))
    (pad 2 smd rect (at -1.31 0 90) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at -1.31 0.95 90) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at 1.31 0.95 90) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.31 -0.95 90) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TSOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Wave (layer F.Cu) (tedit 58CC8C08)
    (at 31.4 37.2)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Wave soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C2 (at 0 -3.15) (layer F.SilkS))
    (fp_text value 68µF (at 0 3.15) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.625 0) (size 2.15 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.625 0) (size 2.15 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-B_EIA-3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-60xx (layer F.Cu) (tedit 574C3AE3)
    (at 24 31 90)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-60xx, 6.0mmx6.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L1 (at 0 -4 90) (layer F.SilkS))
    (fp_text value INDUCTOR (at 0 4.5 90) (layer F.Fab))
    (pad 1 smd rect (at -2.35 0 90) (size 1.6 5.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2.35 0 90) (size 1.6 5.9) (layers F.Cu F.Paste F.Mask)
      (net 41 +BATT))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-60xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.00mm (layer F.Cu) (tedit 59D4FFEB)
    (at 48.4 51.2 180)
    (descr "Through hole straight pin header, 1x05, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.00mm single row")
    (fp_text reference P3 (at 0 -2.06 180) (layer F.SilkS))
    (fp_text value CONN_5 (at 0 10.06 180) (layer F.Fab))
    (fp_text user %R (at 0 4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 1.35) (drill 0.1) (layers *.Cu *.Mask)
      (net 15 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2 180) (size 3 1.35) (drill 0.1) (layers *.Cu *.Mask)
      (net 18 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 4 180) (size 3 1.35) (drill 0.1) (layers *.Cu *.Mask)
      (net 16 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at 0 6 180) (size 3 1.35) (drill 0.1) (layers *.Cu *.Mask)
      (net 19 "Net-(P3-Pad4)"))
    (pad 5 thru_hole oval (at 0 8 180) (size 3 1.35) (drill 0.1) (layers *.Cu *.Mask)
      (net 17 "Net-(P3-Pad5)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:Diode_SMB (layer F.Cu) (tedit 59D4EDA6)
    (at 24.4 37.2)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (attr smd)
    (fp_text reference D1 (at 0 -3) (layer F.SilkS))
    (fp_text value ~ (at 0 3.1) (layer F.Fab) hide)
    (fp_text user %R (at 0 -3) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2.15 0) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SM0603 (layer F.Cu) (tedit 5936E9F8)
    (at 26.6 58.4 315)
    (attr smd)
    (fp_text reference R13 (at 0 -0.7 315) (layer F.SilkS))
    (fp_text value 0 (at 0 0.8 315) (layer F.Fab))
    (pad 1 smd rect (at -1 0 315) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 LEFT-LED-5))
    (pad 2 smd rect (at 1 0 315) (size 1 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 LEFT-LED-5))
    (model "/Library/Application Support/kicad/packages3d/Resistors_SMD.3dshapes/R_0805.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun2:SW_PUSH_SMD (layer F.Cu) (tedit 53EFA8FB)
    (at 42.3 65.5)
    (descr "Bouton poussoir")
    (tags "SWITCH DEV")
    (autoplace_cost180 10)
    (fp_text reference SW1 (at 0 -4) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 5) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3.1 -1.85) (size 1.8 1) (layers F.Cu F.Paste F.Mask)
      (net 14 BTN))
    (pad 1 smd rect (at 3.1 -1.85) (size 1.8 1) (layers F.Cu F.Paste F.Mask)
      (net 14 BTN))
    (pad 2 smd rect (at -3.1 1.85) (size 1.8 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.1 1.85) (size 1.8 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model device/switch_push.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module beargun:SOT23 (layer F.Cu) (tedit 549C2C89)
    (at 23.4 23.2 270)
    (fp_text reference Q1 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value AO3401 (at 0 2.54 270) (layer F.SilkS) hide)
    (pad 3 smd rect (at 0 -1.35 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(P1-Pad1)"))
    (pad 1 smd rect (at -0.95 1.35 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 1.35 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 41 +BATT))
  )
  (gr_line (start 30.8 69.6) (end 49.2 69.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 30.8 62) (end 30.8 69.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 29.6 62) (end 30.8 62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 29.6 69.6) (end 29.6 62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 29.6 69.6) (end 20.8 69.6) (layer Edge.Cuts) (width 0.15))
  (gr_text "charieplexed\neyelashes v1" (at 49 22.6) (layer F.Cu))
  (gr_text "charlieplex eyelashes" (at 35 15) (layer F.Cu))
  (gr_text R (at 48.4 41) (layer F.Cu))
  (gr_text L (at 21.4 40.8) (layer F.Cu))
  (gr_text bat (at 33.6 21.2) (layer F.Cu))
  (target plus (at 51 70.6) (size 5) (width 0.15) (layer Edge.Cuts))
  (target plus (at 19 19) (size 5) (width 0.15) (layer Edge.Cuts))
  (target plus (at 51 19) (size 5) (width 0.15) (layer Edge.Cuts))
  (gr_arc (start 20.8 20.8) (end 20 20.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 20.8 68.8) (end 20.8 69.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 49.2 68.8) (end 50 68.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 49.2 20.8) (end 49.2 20) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20 68.8) (end 20 20.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50 20.8) (end 50 68.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20.8 20) (end 49.2 20) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20 20) (xy 50 20) (xy 50 69.6) (xy 20 69.6)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20 20) (xy 50 20) (xy 50 69.6) (xy 20 69.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.4 20.4) (xy 30 20.4) (xy 30 27.2) (xy 27.8 27.2) (xy 27.8 39.2)
        (xy 20.2 39.2) (xy 20.2 20.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.7 69.6) (xy 30.7 62.1) (xy 29.6 62.1) (xy 29.6 69.6) (xy 29.6 68.3)
        (xy 20.6 68.3) (xy 20.6 70.6) (xy 30.7 70.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.7 69.6) (xy 30.7 62.2) (xy 29.6 62.2) (xy 29.6 68.3) (xy 20.6 68.3)
        (xy 20.6 70.6) (xy 30.7 70.6)
      )
    )
  )
)
