(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.5748)
    (drawings 16)
    (tracks 466)
    (zones 0)
    (modules 60)
    (nets 41)
  )
  (page A)
  (title_block
    (title "7th Area QSO Party Pixie Plaque")
    (date 2017-03-14)
    (rev A)
    (company "Central Oregon DX Club")
    (comment 1 "Design by Martin Held, AE7EU")
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.889)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.635)
    (via_min_drill 0.381)
    (user_via 0.635 0.381)
    (user_via 0.635 0.381)
    (user_via 0.889 0.635)
    (user_via 0.889 0.635)
    (user_via 1.27 0.889)
    (user_via 1.27 0.889)
    (user_via 1.905 1.524)
    (user_via 1.905 1.524)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.1524)
    (pad_size 0.9906 0.9906)
    (pad_drill 0.9906)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 RST)
  (net 3 "Net-(C5-Pad1)")
  (net 4 "Net-(C6-Pad1)")
  (net 5 +3.3V)
  (net 6 VDDA)
  (net 7 SWDIO)
  (net 8 SWCLK)
  (net 9 "Net-(C7-Pad1)")
  (net 10 +15V)
  (net 11 -15V)
  (net 12 "Net-(C13-Pad1)")
  (net 13 DAC)
  (net 14 "Net-(C16-Pad1)")
  (net 15 "Net-(D1-Pad2)")
  (net 16 SENSE_I)
  (net 17 SENSE_V)
  (net 18 "Net-(R8-Pad2)")
  (net 19 "Net-(R10-Pad2)")
  (net 20 VREF)
  (net 21 "Net-(R12-Pad1)")
  (net 22 CURRENT)
  (net 23 "Net-(R14-Pad1)")
  (net 24 VOLTAGE)
  (net 25 GNDF)
  (net 26 +5V)
  (net 27 IN_SDA)
  (net 28 IN_SCL)
  (net 29 "Net-(I1-Pad4)")
  (net 30 "Net-(I1-Pad1)")
  (net 31 "Net-(I1-Pad3)")
  (net 32 "Net-(Q1-Pad1)")
  (net 33 "Net-(Q3-Pad3)")
  (net 34 SDA_MSTR)
  (net 35 SCL_MSTR)
  (net 36 OUT_EN)
  (net 37 "Net-(R20-Pad1)")
  (net 38 "Net-(R21-Pad1)")
  (net 39 "Net-(R22-Pad1)")
  (net 40 "Net-(R23-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +15V)
    (add_net +3.3V)
    (add_net +5V)
    (add_net -15V)
    (add_net CURRENT)
    (add_net DAC)
    (add_net GND)
    (add_net GNDF)
    (add_net IN_SCL)
    (add_net IN_SDA)
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(I1-Pad1)")
    (add_net "Net-(I1-Pad3)")
    (add_net "Net-(I1-Pad4)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R21-Pad1)")
    (add_net "Net-(R22-Pad1)")
    (add_net "Net-(R23-Pad1)")
    (add_net "Net-(R8-Pad2)")
    (add_net OUT_EN)
    (add_net RST)
    (add_net SCL_MSTR)
    (add_net SDA_MSTR)
    (add_net SENSE_I)
    (add_net SENSE_V)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net VDDA)
    (add_net VOLTAGE)
    (add_net VREF)
  )
  (module mheld_std:C0603 (layer B.Cu) (tedit 5408865B)
    (at 45.466 39.624 90)
    (descr "SMT capacitor, 0603")
    (fp_text reference C1 (at 0.9144 1.4732 180) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -0.635 90) (layer B.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 5 +3.3V))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer B.Cu) (tedit 5408865B)
    (at 36.5252 36.7538)
    (descr "SMT capacitor, 0603")
    (fp_text reference C2 (at -0.3048 -1.1684) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -0.635) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 5 +3.3V))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer F.Cu) (tedit 5408865B)
    (at 45.72 33.528)
    (descr "SMT capacitor, 0603")
    (fp_text reference C3 (at 0 -1.1938) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer F.Cu) (tedit 5408865B)
    (at 45.72 34.798 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C4 (at 1.8034 0.1016 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 6 VDDA))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer B.Cu) (tedit 5408865B)
    (at 38.1 33.528 270)
    (descr "SMT capacitor, 0603")
    (fp_text reference C5 (at 0.762 1.1938 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -0.635 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 270) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 270) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer B.Cu) (tedit 5408865B)
    (at 42.672 32.258 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C6 (at -0.762 -1.2446 180) (layer B.SilkS))
    (fp_text value 12p (at 0 -0.635 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer B.Cu) (tedit 5408865B)
    (at 40.64 36.322 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C7 (at -2.286 -0.508 180) (layer B.SilkS))
    (fp_text value 12p (at 0 -0.635 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer F.Cu) (tedit 5408865B)
    (at 47.752 30.48)
    (descr "SMT capacitor, 0603")
    (fp_text reference C8 (at -0.762 -1.27) (layer F.SilkS))
    (fp_text value 1.0u (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 10 +15V))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer F.Cu) (tedit 5408865B)
    (at 49.276 35.814)
    (descr "SMT capacitor, 0603")
    (fp_text reference C9 (at 0.254 1.27) (layer F.SilkS))
    (fp_text value 1.0u (at 0 0.635) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer B.Cu) (tedit 5408865B)
    (at 32.258 44.958)
    (descr "SMT capacitor, 0603")
    (fp_text reference C11 (at 0 -1.27) (layer B.SilkS))
    (fp_text value 0.001u (at 0 -0.635) (layer B.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 20 VREF))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer F.Cu) (tedit 541C5381)
    (at 45.72 36.068)
    (descr "SMT Resistor, 0603")
    (fp_text reference L1 (at -1.8034 0.0508 90) (layer F.SilkS))
    (fp_text value FB (at -0.00254 1.55448) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 6 VDDA))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer F.Cu) (tedit 541C5381)
    (at 45.72 37.338 180)
    (descr "SMT Resistor, 0603")
    (fp_text reference R1 (at -2.286 0 180) (layer F.SilkS))
    (fp_text value 47k (at -0.00254 1.55448 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 RST))
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:PTS810_42x32 (layer B.Cu) (tedit 59B7260E)
    (at 46.99 34.798 90)
    (fp_text reference S1 (at 1.9304 2.3876) (layer B.SilkS))
    (fp_text value pushbutton (at 0 2.3 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 RST))
    (pad 2 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 RST))
  )
  (module mheld_std:TH0-80 (layer F.Cu) (tedit 5AA09487)
    (at 49.276 46.736)
    (fp_text reference TH1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value TP (at 0 -2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.9464 2.9464) (drill 1.6002) (layers *.Cu *.Mask)
      (net 17 SENSE_V))
  )
  (module mheld_std:TH0-80 (layer F.Cu) (tedit 5AA09487)
    (at 49.276 40.64 180)
    (fp_text reference TH2 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text value TP (at 0 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 2.9464 2.9464) (drill 1.6002) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module mheld_std:TH0-80 (layer F.Cu) (tedit 5AA09487)
    (at 26.924 26.924)
    (fp_text reference TH3 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value TP (at 0 -2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.9464 2.9464) (drill 1.6002) (layers *.Cu *.Mask)
      (net 26 +5V))
  )
  (module mheld_std:TH0-80 (layer F.Cu) (tedit 5AA09487)
    (at 26.924 40.64)
    (fp_text reference TH4 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value TP (at 0 -2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.9464 2.9464) (drill 1.6002) (layers *.Cu *.Mask)
      (net 25 GNDF))
  )
  (module mheld_std:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm (layer F.Cu) (tedit 5B85E6A0)
    (at 40.64 35.052 90)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U2 (at 3.2004 -2.7432 180) (layer F.SilkS))
    (fp_text value ATSAMD21E (at 0 3.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.4 -1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at -2.4 -1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C7-Pad1)"))
    (pad 3 smd rect (at -2.4 -0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 DAC))
    (pad 4 smd rect (at -2.4 -0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.4 0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.4 0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.4 1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 VOLTAGE))
    (pad 8 smd rect (at -2.4 1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 CURRENT))
    (pad 9 smd rect (at -1.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 VDDA))
    (pad 10 smd rect (at -1.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -0.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -0.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 OUT_EN))
    (pad 13 smd rect (at 0.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R20-Pad1)"))
    (pad 14 smd rect (at 0.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 1.25 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R21-Pad1)"))
    (pad 16 smd rect (at 1.75 2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 2.4 1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R22-Pad1)"))
    (pad 18 smd rect (at 2.4 1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 2.4 0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R23-Pad1)"))
    (pad 20 smd rect (at 2.4 0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 2.4 -0.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 SDA_MSTR))
    (pad 22 smd rect (at 2.4 -0.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 SCL_MSTR))
    (pad 23 smd rect (at 2.4 -1.25 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 2.4 -1.75 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 1.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 1.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 RST))
    (pad 27 smd rect (at 0.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 0.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at -0.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (pad 30 smd rect (at -0.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (pad 31 smd rect (at -1.25 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 SWCLK))
    (pad 32 smd rect (at -1.75 -2.4 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 SWDIO))
    (pad "" smd rect (at 1.15 1.15 90) (size 0.92 0.92) (layers F.Paste))
    (pad 33 smd rect (at 0 0 90) (size 3.45 3.45) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad "" smd rect (at 0 1.15 90) (size 0.92 0.92) (layers F.Paste))
    (pad "" smd rect (at -1.15 1.15 90) (size 0.92 0.92) (layers F.Paste))
    (pad "" smd rect (at -1.15 0 90) (size 0.92 0.92) (layers F.Paste))
    (pad "" smd rect (at 0 0 90) (size 0.92 0.92) (layers F.Paste))
    (pad "" smd rect (at 1.15 0 90) (size 0.92 0.92) (layers F.Paste))
    (pad "" smd rect (at -1.15 -1.15 90) (size 0.92 0.92) (layers F.Paste))
    (pad "" smd rect (at 0 -1.15 90) (size 0.92 0.92) (layers F.Paste))
    (pad "" smd rect (at 1.15 -1.15 90) (size 0.92 0.92) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RB_DCDC (layer B.Cu) (tedit 5407A5A4)
    (at 30.48 30.226)
    (fp_text reference U6 (at 18.542 -4.064) (layer B.SilkS))
    (fp_text value RB0515D (at 0.762 -4.064) (layer B.SilkS))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 11 -15V))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 10 +15V))
    (pad 1 thru_hole rect (at 0 0) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 26 +5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 25 GNDF))
  )
  (module mheld_std:SOT23 (layer F.Cu) (tedit 54FE24D9)
    (at 49.022 33.02)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U7 (at -1.27 -1.27) (layer F.SilkS))
    (fp_text value MCP1754ST-SOT23 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 10 +15V))
    (model Housings_SOT-23_SOT-143_TSOT-6/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:Crystal_SMD-2pin_3.2x1.5mm (layer B.Cu) (tedit 5B85E6B3)
    (at 40.132 33.528 270)
    (descr "SMD Crystal EuroQuartz EQ161 series http://cdn-reichelt.de/documents/datenblatt/B400/PG32768C.pdf, 3.2x1.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference X1 (at 0.9652 -1.6002) (layer B.SilkS))
    (fp_text value 32.768kHz (at 0 -1.95 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_EuroQuartz_EQ161-2pin_3.2x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:SOIC8N (layer F.Cu) (tedit 55BFD478)
    (at 32.512 34.544)
    (descr "Small outline package, narrow (150mil)")
    (fp_text reference U5 (at -3.429 3.2004) (layer F.SilkS))
    (fp_text value SI8600AC (at -2.54 -3.302) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.6035 -1.905) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 26 +5V))
    (pad 2 smd rect (at -2.6035 -0.635) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 27 IN_SDA))
    (pad 3 smd rect (at -2.6035 0.635) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 28 IN_SCL))
    (pad 4 smd rect (at -2.6035 1.905) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 25 GNDF))
    (pad 5 smd rect (at 2.6035 1.905 180) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.6035 0.635 180) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 35 SCL_MSTR))
    (pad 7 smd rect (at 2.6035 -0.635 180) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 34 SDA_MSTR))
    (pad 8 smd rect (at 2.6035 -1.905 180) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
  )
  (module mheld_std:C0603 (layer F.Cu) (tedit 5408865B)
    (at 42.164 28.448)
    (descr "SMT capacitor, 0603")
    (fp_text reference C10 (at 0.254 -1.27) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 10 +15V))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer F.Cu) (tedit 5408865B)
    (at 39.116 28.448 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C12 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 11 -15V))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer B.Cu) (tedit 5408865B)
    (at 27.178 46.482 90)
    (descr "SMT capacitor, 0603")
    (fp_text reference C13 (at 0.0508 1.27 90) (layer B.SilkS))
    (fp_text value 0.001u (at 0 -0.635 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer F.Cu) (tedit 5408865B)
    (at 31.75 28.448 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C14 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 25 GNDF))
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 26 +5V))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer B.Cu) (tedit 5408865B)
    (at 40.894 37.846 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C15 (at 0 -1.27 180) (layer B.SilkS))
    (fp_text value 0.001u (at 0 -0.635 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 13 DAC))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C0603 (layer F.Cu) (tedit 5408865B)
    (at 49.276 42.926)
    (descr "SMT capacitor, 0603")
    (fp_text reference C16 (at -2.5146 0) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:TC2030-MCP-NL (layer B.Cu) (tedit 50632EA8)
    (at 34.29 38.862 180)
    (descr http://www.tag-connect.com/Materials/TC2030-MCP-NL%20PCB%20Footprint.pdf)
    (fp_text reference J1 (at 0 4.064 180) (layer B.SilkS) hide)
    (fp_text value ICSP (at 0 -3.048 180) (layer B.SilkS) hide)
    (pad 1 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 5 +3.3V) (clearance 0.4826))
    (pad 2 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 SWDIO) (clearance 0.4826))
    (pad 3 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND) (clearance 0.4826))
    (pad 4 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 SWCLK) (clearance 0.4826))
    (pad 5 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND) (clearance 0.4318))
    (pad 6 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 2 RST) (clearance 0.4318))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  )
  (module mheld_std:R0603 (layer F.Cu) (tedit 541C5381)
    (at 27.178 43.688 90)
    (descr "SMT Resistor, 0603")
    (fp_text reference R3 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 5k (at -0.00254 1.55448 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer F.Cu) (tedit 541C5381)
    (at 27.178 46.482 270)
    (descr "SMT Resistor, 0603")
    (fp_text reference R4 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 5k (at -0.00254 1.55448 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 1 smd rect (at 0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer F.Cu) (tedit 541C5381)
    (at 42.672 46.736 90)
    (descr "SMT Resistor, 0603")
    (fp_text reference R5 (at 2.286 0 90) (layer F.SilkS))
    (fp_text value 5k (at -0.00254 1.55448 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 16 SENSE_I))
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(Q1-Pad1)"))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer F.Cu) (tedit 541C5381)
    (at 46.228 46.736 180)
    (descr "SMT Resistor, 0603")
    (fp_text reference R6 (at -0.5334 1.143 180) (layer F.SilkS))
    (fp_text value 1 (at -0.00254 1.55448 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 16 SENSE_I))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 17 SENSE_V))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer F.Cu) (tedit 541C5381)
    (at 49.276 44.196 180)
    (descr "SMT Resistor, 0603")
    (fp_text reference R7 (at 2.286 0 180) (layer F.SilkS))
    (fp_text value 1 (at -0.00254 1.55448 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C16-Pad1)"))
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 17 SENSE_V))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer F.Cu) (tedit 541C5381)
    (at 34.544 40.894)
    (descr "SMT Resistor, 0603")
    (fp_text reference R8 (at -2.286 0) (layer F.SilkS))
    (fp_text value 5k (at -0.00254 1.55448) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R8-Pad2)"))
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 13 DAC))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer F.Cu) (tedit 541C5381)
    (at 37.338 43.18 270)
    (descr "SMT Resistor, 0603")
    (fp_text reference R9 (at -2.286 0 270) (layer F.SilkS))
    (fp_text value 50k (at -0.00254 1.55448 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R8-Pad2)"))
    (pad 2 smd rect (at -0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(Q3-Pad3)"))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer B.Cu) (tedit 541C5381)
    (at 32.258 47.498)
    (descr "SMT Resistor, 0603")
    (fp_text reference R10 (at 0.381 -1.1684) (layer B.SilkS))
    (fp_text value 75k (at -0.00254 -1.55448) (layer B.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(R10-Pad2)"))
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 20 VREF))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer B.Cu) (tedit 541C5381)
    (at 41.148 48.514 180)
    (descr "SMT Resistor, 0603")
    (fp_text reference R11 (at -2.6924 0 180) (layer B.SilkS))
    (fp_text value 5k (at -0.00254 -1.55448 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(R10-Pad2)"))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 16 SENSE_I))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer B.Cu) (tedit 541C5381)
    (at 41.148 50.038 180)
    (descr "SMT Resistor, 0603")
    (fp_text reference R12 (at -2.7178 0 180) (layer B.SilkS))
    (fp_text value 5k (at -0.00254 -1.55448 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 17 SENSE_V))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer F.Cu) (tedit 541C5381)
    (at 27.178 49.276 270)
    (descr "SMT Resistor, 0603")
    (fp_text reference R13 (at -0.01016 1.27 270) (layer F.SilkS))
    (fp_text value 75k (at -0.00254 1.55448 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 22 CURRENT))
    (pad 2 smd rect (at -0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R12-Pad1)"))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer F.Cu) (tedit 541C5381)
    (at 39.624 48.768 180)
    (descr "SMT Resistor, 0603")
    (fp_text reference R14 (at 1.27 1.27) (layer F.SilkS))
    (fp_text value 10k (at -0.00254 1.55448 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R14-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 17 SENSE_V))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer F.Cu) (tedit 541C5381)
    (at 39.624 50.038 180)
    (descr "SMT Resistor, 0603")
    (fp_text reference R15 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 1.2k (at -0.00254 1.55448 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R14-Pad1)"))
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 24 VOLTAGE))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:SOIC14N (layer F.Cu) (tedit 56D62FA6)
    (at 32.258 46.228)
    (descr "Small outline package, narrow (150mil)")
    (fp_text reference U3 (at -2.667 -5.207) (layer F.SilkS))
    (fp_text value ISL28345 (at -2.667 5.334) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.6035 -3.81) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 20 VREF))
    (pad 2 smd rect (at -2.6035 -2.54) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 20 VREF) (solder_mask_margin 0.127) (clearance 0.127))
    (pad 3 smd rect (at -2.6035 -1.27) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C13-Pad1)") (solder_mask_margin 0.127) (clearance 0.127))
    (pad 4 smd rect (at -2.6035 0) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 10 +15V) (solder_mask_margin 0.127) (clearance 0.127))
    (pad 5 smd rect (at -2.6035 1.27) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R10-Pad2)") (solder_mask_margin 0.127) (clearance 0.127))
    (pad 6 smd rect (at -2.6035 2.54) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R12-Pad1)") (solder_mask_margin 0.127) (clearance 0.127))
    (pad 7 smd rect (at -2.6035 3.81) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 22 CURRENT) (solder_mask_margin 0.127) (clearance 0.127))
    (pad 8 smd rect (at 2.6035 3.81 180) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 24 VOLTAGE) (solder_mask_margin 0.127) (clearance 0.127))
    (pad 9 smd rect (at 2.6035 2.54 180) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R14-Pad1)") (solder_mask_margin 0.127) (clearance 0.127))
    (pad 10 smd rect (at 2.6035 1.27 180) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 20 VREF) (solder_mask_margin 0.127) (clearance 0.127))
    (pad 11 smd rect (at 2.6035 0 180) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 11 -15V) (solder_mask_margin 0.127) (clearance 0.127))
    (pad 12 smd rect (at 2.6035 -1.27 180) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 20 VREF) (solder_mask_margin 0.127) (clearance 0.127))
    (pad 13 smd rect (at 2.6035 -2.54 180) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R8-Pad2)") (solder_mask_margin 0.127) (clearance 0.127))
    (pad 14 smd rect (at 2.6035 -3.81 180) (size 2.159 0.508) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(Q3-Pad3)") (solder_mask_margin 0.127) (clearance 0.127))
  )
  (module mheld_std:C0603 (layer B.Cu) (tedit 5408865B)
    (at 29.21 38.354 90)
    (descr "SMT capacitor, 0603")
    (fp_text reference C17 (at -0.0762 1.27 90) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -0.635 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 26 +5V))
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 25 GNDF))
    (model smd/capacitors/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:HDR4X1_P1 (layer F.Cu) (tedit 5B85B38F)
    (at 26.924 37.592 180)
    (fp_text reference P1 (at -1.9558 8.3312 90) (layer F.SilkS))
    (fp_text value HDR4X1 (at 0.47 -1.94 180) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 0 5.08 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 27 IN_SDA))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 26 +5V))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 28 IN_SCL))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 25 GNDF))
  )
  (module mheld_std:R0603 (layer B.Cu) (tedit 541C5381)
    (at 29.464 33.02 90)
    (descr "SMT Resistor, 0603")
    (fp_text reference R2 (at -2.286 0 90) (layer B.SilkS))
    (fp_text value 5k (at -0.00254 -1.55448 90) (layer B.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 27 IN_SDA))
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 26 +5V))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer B.Cu) (tedit 541C5381)
    (at 30.988 33.02 90)
    (descr "SMT Resistor, 0603")
    (fp_text reference R16 (at -2.54 0 90) (layer B.SilkS))
    (fp_text value 5k (at -0.00254 -1.55448 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 26 +5V))
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 28 IN_SCL))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer B.Cu) (tedit 541C5381)
    (at 33.528 33.528 90)
    (descr "SMT Resistor, 0603")
    (fp_text reference R17 (at -2.5146 0.5588 90) (layer B.SilkS))
    (fp_text value 5k (at -0.00254 -1.55448 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 5 +3.3V))
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 35 SCL_MSTR))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer B.Cu) (tedit 541C5381)
    (at 35.052 33.528 90)
    (descr "SMT Resistor, 0603")
    (fp_text reference R18 (at 0.889 1.2446 90) (layer B.SilkS))
    (fp_text value 5k (at -0.00254 -1.55448 90) (layer B.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 34 SDA_MSTR))
    (pad 1 smd rect (at 0.75184 0 90) (size 0.89916 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 5 +3.3V))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:SOT23 (layer F.Cu) (tedit 54FE24D9)
    (at 44.704 49.276)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.3114 -0.3048) (layer F.SilkS))
    (fp_text value DMN3730U (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 16 SENSE_I))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D1-Pad2)"))
    (model Housings_SOT-23_SOT-143_TSOT-6/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:SOT23 (layer F.Cu) (tedit 54FE24D9)
    (at 44.704 44.196)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -1.2446 -1.27) (layer F.SilkS))
    (fp_text value BSH203,215 (at 0 2.54) (layer F.SilkS) hide)
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 11 -15V))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 16 SENSE_I))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(Q1-Pad1)"))
    (model Housings_SOT-23_SOT-143_TSOT-6/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0603 (layer F.Cu) (tedit 541C5381)
    (at 39.878 39.37 180)
    (descr "SMT Resistor, 0603")
    (fp_text reference R19 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 1k (at -0.00254 1.55448 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(I1-Pad1)"))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3V))
    (model smd/resistors/R0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:SOT23 (layer F.Cu) (tedit 54FE24D9)
    (at 40.132 43.18)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 1.4224 -1.2954) (layer F.SilkS))
    (fp_text value 2n7002_sot23 (at 0 2.54) (layer F.SilkS) hide)
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(Q3-Pad3)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(I1-Pad3)"))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(I1-Pad4)"))
    (model Housings_SOT-23_SOT-143_TSOT-6/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:SOT23 (layer F.Cu) (tedit 54FE24D9)
    (at 40.132 46.228 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at -1.143 -1.3462 180) (layer F.SilkS))
    (fp_text value 2n7002_sot23 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(I1-Pad4)"))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(I1-Pad3)"))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(Q1-Pad1)"))
    (model Housings_SOT-23_SOT-143_TSOT-6/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:SOD-323 (layer F.Cu) (tedit 59F3CCBC)
    (at 48.26 49.784)
    (descr DIODE)
    (tags DIODE)
    (attr smd)
    (fp_text reference D1 (at -0.635 -1.3208) (layer F.SilkS))
    (fp_text value S1M (at -0.2159 0.7366) (layer B.SilkS) hide)
    (pad 1 smd rect (at 1.0922 0) (size 0.7874 0.7874) (layers F.Cu F.Paste F.Mask)
      (net 10 +15V))
    (pad 2 smd rect (at -1.0922 0) (size 0.7874 0.7874) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D1-Pad2)"))
  )
  (module SSOP4 (layer B.Cu) (tedit 5B118AA3)
    (at 39.878 42.164 270)
    (fp_text reference I1 (at 0 2.032 90) (layer B.SilkS))
    (fp_text value APV2111 (at 0.127 -2.159 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.175 0.635 270) (size 0.9 0.7) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(I1-Pad1)"))
    (pad 2 smd rect (at -2.175 -0.635 270) (size 0.9 0.7) (layers B.Cu B.Paste B.Mask)
      (net 36 OUT_EN))
    (pad 3 smd rect (at 2.175 -0.635 270) (size 0.9 0.7) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(I1-Pad3)"))
    (pad 4 smd rect (at 2.175 0.635 270) (size 0.9 0.7) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(I1-Pad4)"))
  )
  (module mheld_std:R0201 (layer F.Cu) (tedit 5B86FD36)
    (at 43.8912 34.798)
    (descr "Resistor SMD 0201, reflow soldering, Vishay (see crcw0201e3.pdf)")
    (tags "resistor 0201")
    (attr smd)
    (fp_text reference R20 (at 0 -0.889) (layer F.SilkS) hide)
    (fp_text value DNI (at 0 0.889) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.26 0) (size 0.28 0.43) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R20-Pad1)"))
    (pad 2 smd rect (at 0.26 0) (size 0.28 0.43) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0201.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0201 (layer F.Cu) (tedit 5B86FD36)
    (at 43.8912 33.782)
    (descr "Resistor SMD 0201, reflow soldering, Vishay (see crcw0201e3.pdf)")
    (tags "resistor 0201")
    (attr smd)
    (fp_text reference R21 (at 0 -0.889) (layer F.SilkS) hide)
    (fp_text value DNI (at 0 0.889) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.26 0) (size 0.28 0.43) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.26 0) (size 0.28 0.43) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R21-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0201.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0201 (layer F.Cu) (tedit 5B86FD36)
    (at 42.3926 31.6992 90)
    (descr "Resistor SMD 0201, reflow soldering, Vishay (see crcw0201e3.pdf)")
    (tags "resistor 0201")
    (attr smd)
    (fp_text reference R22 (at 0 -0.889 90) (layer F.SilkS) hide)
    (fp_text value DNI (at 0 0.889 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.26 0 90) (size 0.28 0.43) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R22-Pad1)"))
    (pad 2 smd rect (at 0.26 0 90) (size 0.28 0.43) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0201.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R0201 (layer F.Cu) (tedit 5B86FD36)
    (at 41.3766 31.6992 90)
    (descr "Resistor SMD 0201, reflow soldering, Vishay (see crcw0201e3.pdf)")
    (tags "resistor 0201")
    (attr smd)
    (fp_text reference R23 (at 0 -0.889 90) (layer F.SilkS) hide)
    (fp_text value DNI (at 0 0.889 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.26 0 90) (size 0.28 0.43) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.26 0 90) (size 0.28 0.43) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R23-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0201.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "1sqin 4quad PSU" (at 45.3136 26.162) (layer F.SilkS))
  (gr_text martin.held@gmail.com (at 39.1668 50.1142) (layer B.SilkS))
  (gr_text GNDIN (at 29.1592 42.6466) (layer B.SilkS))
  (gr_text +5IN (at 28.6258 28.829) (layer B.SilkS))
  (gr_text -OUT (at 50.927 42.6974) (layer B.SilkS))
  (gr_text +OUT (at 50.7238 48.9204) (layer B.SilkS))
  (gr_text "AE7EU\n4Quad\nPSU\n" (at 46.863 44.9834) (layer B.SilkS))
  (gr_line (start 25.4 50.8) (end 25.4 25.4) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.8 50.8) (end 25.4 50.8) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.8 25.4) (end 50.8 50.8) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 25.4 25.4) (end 50.8 25.4) (layer Edge.Cuts) (width 0.1))
  (dimension 0.113592 (width 0.3) (layer Dwgs.User)
    (gr_text "0.0045 in" (at 58.48174 36.681118 333.4349488) (layer Dwgs.User))
    (feature1 (pts (xy 59.1566 35.4584) (xy 57.928801 37.913998)))
    (feature2 (pts (xy 59.055 35.4076) (xy 57.827201 37.863198)))
    (crossbar (pts (xy 59.03468 35.448239) (xy 59.13628 35.499039)))
    (arrow1a (pts (xy 59.13628 35.499039) (xy 57.866449 35.519762)))
    (arrow1b (pts (xy 59.13628 35.499039) (xy 58.39096 34.470741)))
    (arrow2a (pts (xy 59.03468 35.448239) (xy 59.78 36.476537)))
    (arrow2b (pts (xy 59.03468 35.448239) (xy 60.304511 35.427516)))
  )
  (dimension 14.528822 (width 0.3) (layer Dwgs.User)
    (gr_text "0.5720 in" (at 21.887117 34.305045 270.1001673) (layer Dwgs.User))
    (feature1 (pts (xy 30.5054 41.5544) (xy 20.549819 41.571805)))
    (feature2 (pts (xy 30.48 27.0256) (xy 20.524419 27.043005)))
    (crossbar (pts (xy 23.224415 27.038285) (xy 23.249815 41.567085)))
    (arrow1a (pts (xy 23.249815 41.567085) (xy 22.661426 40.441608)))
    (arrow1b (pts (xy 23.249815 41.567085) (xy 23.834265 40.439558)))
    (arrow2a (pts (xy 23.224415 27.038285) (xy 22.639965 28.165812)))
    (arrow2b (pts (xy 23.224415 27.038285) (xy 23.812804 28.163762)))
  )
  (dimension 58.42 (width 0.3) (layer Dwgs.User)
    (gr_text "2.3000 in" (at 59.69 21.510001) (layer Dwgs.User))
    (feature1 (pts (xy 30.48 25.4) (xy 30.48 20.160001)))
    (feature2 (pts (xy 88.9 25.4) (xy 88.9 20.160001)))
    (crossbar (pts (xy 88.9 22.860001) (xy 30.48 22.860001)))
    (arrow1a (pts (xy 30.48 22.860001) (xy 31.606504 22.27358)))
    (arrow1b (pts (xy 30.48 22.860001) (xy 31.606504 23.446422)))
    (arrow2a (pts (xy 88.9 22.860001) (xy 87.773496 22.27358)))
    (arrow2b (pts (xy 88.9 22.860001) (xy 87.773496 23.446422)))
  )
  (dimension 17.78 (width 0.3) (layer Dwgs.User)
    (gr_text "0.7000 in" (at 100.41 34.29 270) (layer Dwgs.User))
    (feature1 (pts (xy 92.202 43.18) (xy 101.76 43.18)))
    (feature2 (pts (xy 92.202 25.4) (xy 101.76 25.4)))
    (crossbar (pts (xy 99.06 25.4) (xy 99.06 43.18)))
    (arrow1a (pts (xy 99.06 43.18) (xy 98.473579 42.053496)))
    (arrow1b (pts (xy 99.06 43.18) (xy 99.646421 42.053496)))
    (arrow2a (pts (xy 99.06 25.4) (xy 98.473579 26.526504)))
    (arrow2b (pts (xy 99.06 25.4) (xy 99.646421 26.526504)))
  )
  (dimension 66.802 (width 0.3) (layer Dwgs.User)
    (gr_text "2.6300 in" (at 58.801 16.43) (layer Dwgs.User))
    (feature1 (pts (xy 25.4 25.4) (xy 25.4 15.08)))
    (feature2 (pts (xy 92.202 25.4) (xy 92.202 15.08)))
    (crossbar (pts (xy 92.202 17.78) (xy 25.4 17.78)))
    (arrow1a (pts (xy 25.4 17.78) (xy 26.526504 17.193579)))
    (arrow1b (pts (xy 25.4 17.78) (xy 26.526504 18.366421)))
    (arrow2a (pts (xy 92.202 17.78) (xy 91.075496 17.193579)))
    (arrow2b (pts (xy 92.202 17.78) (xy 91.075496 18.366421)))
  )
  (zone (net 5) (net_name +3.3V) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.228 32.512) (xy 47.752 32.512) (xy 47.752 36.83) (xy 46.228 36.83) (xy 46.228 40.386)
        (xy 37.592 40.386) (xy 37.592 31.496) (xy 46.228 31.496)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.8 50.8) (xy 25.4 50.8) (xy 25.4 41.656) (xy 33.782 41.656) (xy 33.782 38.862)
        (xy 33.782 31.75) (xy 38.862 31.75) (xy 38.862 25.4) (xy 50.8 25.4)
      )
    )
  )
  (zone (net 10) (net_name +15V) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.8 50.8) (xy 47.244 50.8) (xy 28.194 50.546) (xy 28.194 44.704) (xy 31.496 44.704)
        (xy 31.496 47.244) (xy 44.45 47.244) (xy 46.736 45.466) (xy 46.736 30.988) (xy 41.91 30.988)
        (xy 41.91 25.4) (xy 50.8 25.4)
      )
    )
  )
  (zone (net 11) (net_name -15V) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39.37 25.4) (xy 39.37 30.988) (xy 36.068 30.988) (xy 36.068 40.894) (xy 42.164 40.894)
        (xy 45.466 40.894) (xy 45.466 43.942) (xy 37.084 43.942) (xy 37.084 46.482) (xy 33.02 46.482)
        (xy 33.02 40.894) (xy 34.798 40.894) (xy 34.798 25.4)
      )
    )
  )
)
