<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0.935" y1="0.935" x2="19.31" y2="0.935" width="0" layer="20"/>
<wire x1="19.31" y1="0.935" x2="19.31" y2="31.365" width="0" layer="20"/>
<wire x1="19.31" y1="31.365" x2="0.935" y2="31.365" width="0" layer="20"/>
<wire x1="0.935" y1="31.365" x2="0.935" y2="0.935" width="0" layer="20"/>
<text>R1</text>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>R2</text>
<text>R3</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>1</text>
<text>0</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>sjm4306</text>
<text>Arduino Pico</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-SMD-5X3.2-2PAD">
<description>&lt;h3&gt;5x3.2mm 2-pad SMD Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.txccrystal.com/images/pdf/7a.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="sjm4306_LOGO">
<packages>
<package name="SJM4306_LOGO_SMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C0805" value="0.1uF"/>
<element name="C2" library="adafruit" package="C0805" value="22pF"/>
<element name="C3" library="adafruit" package="C0805" value="22pF"/>
<element name="P" library="adafruit" package="CHIP-LED0805" value="Red">
<attribute name="NAME"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="10K"/>
<element name="R2" library="adafruit" package="M0805" value="1K"/>
<element name="U1" library="SparkFun-IC-Microcontroller" package="TQFP32-08" value="ATMEGA328P_TQFP">
<attribute name="PROD_ID" value="IC-09069"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-Clocks" package="CRYSTAL-SMD-5X3.2-2PAD" value="16MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X3" value="ICSP">
<attribute name="PROD_ID" value="CONN-09701"/>
<attribute name="VALUE"/>
</element>
<element name="L" library="adafruit" package="CHIP-LED0805" value="Green">
<attribute name="NAME"/>
</element>
<element name="R3" library="adafruit" package="M0805" value="1K"/>
<element name="J2" library="SparkFun-Connectors" package="1X08" value="Digital">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X08" value="Analog">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X06" value="Digital">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X01" value="Vcc">
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X01" value="Reset">
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X01" value="Gnd">
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X01" value="Vcc">
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X01" value="Gnd">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="sjm4306_LOGO" package="SJM4306_LOGO_SMALL" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="J1" pad="6"/>
<contactref element="R3" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J7" pad="1"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="20"/>
<contactref element="C1" pad="1"/>
<contactref element="P" pad="A"/>
<contactref element="J1" pad="2"/>
<contactref element="J5" pad="1"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="29"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="5"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="8"/>
<contactref element="Y1" pad="P$1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="7"/>
<contactref element="Y1" pad="P$2"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="P" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="J1" pad="4"/>
<contactref element="U1" pad="15"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="17"/>
<contactref element="L" pad="A"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="A0">
<contactref element="U1" pad="23"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="A1">
<contactref element="U1" pad="24"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="25"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="A3">
<contactref element="U1" pad="26"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="27"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="28"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="A6">
<contactref element="U1" pad="19"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="A7">
<contactref element="U1" pad="22"/>
<contactref element="J3" pad="8"/>
</signal>
<signal name="D0">
<contactref element="U1" pad="30"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="31"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="32"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="1"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="2"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="9"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="10"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="11"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="D8">
<contactref element="U1" pad="12"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="D9">
<contactref element="U1" pad="13"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="D10">
<contactref element="U1" pad="14"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="L" pad="C"/>
<contactref element="R3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
