(module 000EigeneFootprints:Atmega328P-MU_Pogoadapter (layer F.Cu) (tedit 5BD0A964)
  (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
  (tags "QFN 0.5")
  (attr smd)
  (fp_text reference REF** (at 0 -5.7785) (layer F.SilkS))
  (fp_text value "Atmega328P-MU QFN-32 with additional pads for 1mm diameter pogo pins" (at 0 5.9055) (layer F.Fab))
  (pad 2 thru_hole oval (at -3.25 0.75 270) (size 1.5 2) (drill 1.05 (offset 0 0.3)) (layers *.Mask F.Cu)
    (zone_connect 1))
  (pad 6 thru_hole oval (at -3.25 -0.75 270) (size 1.5 2) (drill 1.05 (offset 0 0.3)) (layers *.Mask B.Cu)
    (zone_connect 1))
  (pad 1 thru_hole oval (at 2.5 3.25) (size 1.5 2) (drill 1.05 (offset 0 0.3)) (layers *.Mask F.Cu)
    (zone_connect 1))
  (pad 5 thru_hole circle (at -0.25 -3.25) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
    (zone_connect 1))
  (pad 3 thru_hole circle (at 3.25 1.75) (size 1.5 1.5) (drill 1.05) (layers *.Cu *.Mask)
    (zone_connect 1))
  (pad 4 thru_hole oval (at 1 3.25) (size 1.5 2) (drill 1.05 (offset 0 0.3)) (layers *.Mask B.Cu)
    (zone_connect 1))
  (pad "" thru_hole circle (at 3 -3) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
    (solder_mask_margin 0.05) (zone_connect 1))
  (pad "" thru_hole circle (at -3 3) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
    (solder_mask_margin 0.05) (zone_connect 1))
)
