(module 000EigeneFootprints:VQFN-32_5x5mm_0.5mm_Atmega328P-MU_rundePads_incl.ICSPHeader (layer F.Cu) (tedit 5BC0DDBC)
  (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
  (tags "QFN 0.5")
  (attr smd)
  (fp_text reference U2 (at 1.524 -7.874) (layer F.SilkS) hide)
  (fp_text value ATmega328P-MU (at -10.8585 -7.239) (layer F.Fab) hide)
  (pad 6 smd circle (at -3.25 0.75) (size 0.5 0.5) (layers F.Cu F.Mask)
    (zone_connect 1))
  (pad 3 smd circle (at -3.25 -0.75) (size 0.5 0.5) (layers F.Cu F.Mask)
    (zone_connect 1))
  (pad 29 smd circle (at -0.25 -3.25) (size 0.5 0.5) (layers F.Cu F.Mask)
    (zone_connect 1))
  (pad 17 smd circle (at 3.25 1.75) (size 0.5 0.5) (layers F.Cu F.Mask)
    (zone_connect 1))
  (pad 16 smd circle (at 2.5 3.25) (size 0.5 0.5) (layers F.Cu F.Mask)
    (zone_connect 1))
  (pad 15 smd circle (at 1 3.25) (size 0.5 0.5) (layers F.Cu F.Mask)
    (zone_connect 1))
  (pad 33 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin_ratio -0.2) (clearance 0.2) (zone_connect 0))
  (pad 32 smd oval (at -1.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 31 smd oval (at -1.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 30 smd oval (at -0.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 29 smd oval (at -0.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 28 smd oval (at 0.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 27 smd oval (at 0.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 26 smd oval (at 1.25 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 25 smd oval (at 1.75 -2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 24 smd oval (at 2.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 23 smd oval (at 2.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 22 smd oval (at 2.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 21 smd oval (at 2.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 20 smd oval (at 2.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 19 smd oval (at 2.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 18 smd oval (at 2.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 17 smd oval (at 2.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 16 smd oval (at 1.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 15 smd oval (at 1.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 14 smd oval (at 0.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 13 smd oval (at 0.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 12 smd oval (at -0.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 11 smd oval (at -0.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 10 smd oval (at -1.25 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 9 smd oval (at -1.75 2.4 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 8 smd oval (at -2.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 7 smd oval (at -2.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 6 smd oval (at -2.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 5 smd oval (at -2.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 4 smd oval (at -2.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 3 smd oval (at -2.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 2 smd oval (at -2.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad 1 smd oval (at -2.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
    (zone_connect 1))
  (pad "" np_thru_hole circle (at 3 -3) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask)
    (solder_mask_margin 0.05) (zone_connect 1))
  (pad "" np_thru_hole circle (at -3 3) (size 0.95 0.95) (drill 0.9) (layers *.Cu *.Mask)
    (solder_mask_margin 0.05) (zone_connect 1))
  (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
