<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="61.194" y2="0" width="0" layer="20"/>
<wire x1="61.194" y1="0" x2="61.194" y2="54.28" width="0" layer="20"/>
<wire x1="61.194" y1="54.28" x2="0" y2="54.28" width="0" layer="20"/>
<wire x1="0" y1="54.28" x2="0" y2="0" width="0" layer="20"/>
<hole x="58.674" y="52.07" drill="3.1"/>
<hole x="2.286" y="51.816" drill="3.1"/>
<hole x="58.674" y="2.286" drill="3.1"/>
<hole x="2.286" y="2.286" drill="3.1"/>
<text>EasyFlip v2.0</text>
<text>sjm4306 121218</text>
<text>+</text>
<text>+</text>
<text>PIC16F887</text>
<text>D1</text>
<text>D2</text>
<text>PWR</text>
<text>sjm4306</text>
<text>Serial</text>
<text>PWR</text>
<text>Test</text>
<text>S7S</text>
<text>S7S</text>
<text>o</text>
<text>D1</text>
<text>D2</text>
<text>D3</text>
<text>gnd</text>
<text>gnd</text>
<text>12V</text>
<text>12V</text>
<text>5V</text>
<text>5V</text>
<text>&gt;</text>
<text>TX</text>
<text>RX</text>
<text>gnd</text>
<text>o</text>
<text>o</text>
<text>o</text>
<text>o</text>
<text>o</text>
<text>o</text>
<text>o</text>
<text>o</text>
<text>o</text>
<text>o</text>
<text>o</text>
<text>o</text>
<text>o</text>
</plain>
<libraries>
<library name="sjm4306-custom">
<packages>
<package name="EM_7_SEG">
</package>
<package name="SO8">
<description>&lt;B&gt;SO8: plastic small outline package; 8 leads; body width 3.9 mm&lt;/B&gt;&lt;p&gt;
Source: http://www.nxp.com/documents/data_sheet/PCA82C250.pdf</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="1X03-CLEANBIG">
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="sjm4306_LOGO">
<packages>
<package name="SJM4306_LOGO_MEDIUM">
</package>
<package name="SJM4306_LOGO_SMALL">
</package>
</packages>
</library>
<library name="Microchip_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 11:22:31</description>
<packages>
<package name="QFP80P1200X1200X120-44N">
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE05-1">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C5B2.5">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 2.5 mm, grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="BeagleBone_Blue_R3">
<description>Generated from &lt;b&gt;BeagleBone_Blue.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="TP16R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="sjm4306-custom" package="EM_7_SEG" value="ELECTROMECHANICAL_7_SEG"/>
<element name="C1" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="U$2" library="sjm4306-custom" package="EM_7_SEG" value="ELECTROMECHANICAL_7_SEG"/>
<element name="U$3" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="U$11" library="sjm4306_LOGO" package="SJM4306_LOGO_MEDIUM" value=""/>
<element name="U$13" library="sjm4306_LOGO" package="SJM4306_LOGO_SMALL" value=""/>
<element name="ICSP" library="con-lsta" package="FE05-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="JP1" library="adafruit" package="1X03-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="C2" library="capacitor-wima" package="C5B2.5" value="100uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="capacitor-wima" package="C5B2.5" value="100uF">
<attribute name="NAME"/>
</element>
<element name="JP2" library="adafruit" package="1X03-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="adafruit" package="1X03-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="M0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="M0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="BeagleBone_Blue_R3" package="TP16R" value="TPTP16R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="U$17" library="Microchip_By_element14_Batch_1" package="QFP80P1200X1200X120-44N" value="PIC16F887-I/PT">
<attribute name="MPN" value="PIC16F887-I/PT"/>
<attribute name="OC_FARNELL" value="1439542"/>
<attribute name="OC_NEWARK" value="74K8587"/>
<attribute name="PACKAGE" value="QFP-44"/>
<attribute name="SUPPLIER" value="Microchip"/>
</element>
<element name="U$4" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="U$5" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="U$6" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="U$7" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="U$8" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="U$9" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="U$10" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="U$140" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="U$150" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="U$160" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="U$14" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="U$15" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="U$16" library="sjm4306-custom" package="SO8" value="L9110SOP8"/>
<element name="TP2" library="BeagleBone_Blue_R3" package="TP16R" value="TPTP16R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP3" library="BeagleBone_Blue_R3" package="TP16R" value="TPTP16R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$3" pad="8"/>
<contactref element="U$3" pad="5"/>
<contactref element="ICSP" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="S1" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="U$17" pad="6"/>
<contactref element="U$17" pad="29"/>
<contactref element="U$4" pad="8"/>
<contactref element="U$4" pad="5"/>
<contactref element="U$5" pad="8"/>
<contactref element="U$5" pad="5"/>
<contactref element="U$6" pad="8"/>
<contactref element="U$6" pad="5"/>
<contactref element="U$7" pad="8"/>
<contactref element="U$7" pad="5"/>
<contactref element="U$8" pad="8"/>
<contactref element="U$8" pad="5"/>
<contactref element="U$9" pad="8"/>
<contactref element="U$9" pad="5"/>
<contactref element="U$10" pad="8"/>
<contactref element="U$10" pad="5"/>
<contactref element="U$140" pad="8"/>
<contactref element="U$140" pad="5"/>
<contactref element="U$150" pad="8"/>
<contactref element="U$150" pad="5"/>
<contactref element="U$160" pad="8"/>
<contactref element="U$160" pad="5"/>
<contactref element="U$14" pad="8"/>
<contactref element="U$14" pad="5"/>
<contactref element="U$15" pad="8"/>
<contactref element="U$15" pad="5"/>
<contactref element="U$16" pad="8"/>
<contactref element="U$16" pad="5"/>
</signal>
<signal name="5V">
<contactref element="ICSP" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="U$17" pad="28"/>
<contactref element="U$17" pad="7"/>
</signal>
<signal name="12V">
<contactref element="U$3" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="U$3" pad="3"/>
<contactref element="U$7" pad="2"/>
<contactref element="U$7" pad="3"/>
<contactref element="U$8" pad="3"/>
<contactref element="U$8" pad="2"/>
<contactref element="U$6" pad="2"/>
<contactref element="U$6" pad="3"/>
<contactref element="U$5" pad="3"/>
<contactref element="U$5" pad="2"/>
<contactref element="U$9" pad="2"/>
<contactref element="U$9" pad="3"/>
<contactref element="U$4" pad="3"/>
<contactref element="U$4" pad="2"/>
<contactref element="U$10" pad="2"/>
<contactref element="U$10" pad="3"/>
<contactref element="U$14" pad="2"/>
<contactref element="U$14" pad="3"/>
<contactref element="U$15" pad="3"/>
<contactref element="U$15" pad="2"/>
<contactref element="U$160" pad="2"/>
<contactref element="U$160" pad="3"/>
<contactref element="U$150" pad="3"/>
<contactref element="U$150" pad="2"/>
<contactref element="U$16" pad="2"/>
<contactref element="U$16" pad="3"/>
<contactref element="U$140" pad="3"/>
<contactref element="U$140" pad="2"/>
</signal>
<signal name="ICSP_DATA">
<contactref element="ICSP" pad="4"/>
<contactref element="U$17" pad="17"/>
<contactref element="S1" pad="1"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="MCLR">
<contactref element="ICSP" pad="1"/>
<contactref element="TP1" pad="TP"/>
<contactref element="U$17" pad="18"/>
</signal>
<signal name="TX">
<contactref element="JP3" pad="1"/>
<contactref element="U$17" pad="44"/>
</signal>
<signal name="RX">
<contactref element="JP3" pad="2"/>
<contactref element="U$17" pad="1"/>
</signal>
<signal name="DBG0">
<contactref element="R1" pad="2"/>
<contactref element="U$17" pad="25"/>
</signal>
<signal name="DBG1">
<contactref element="R2" pad="2"/>
<contactref element="U$17" pad="26"/>
</signal>
<signal name="DBG2">
<contactref element="R3" pad="2"/>
<contactref element="U$17" pad="27"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="LED3" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="E2-2">
<contactref element="U$2" pad="E2"/>
<contactref element="U$14" pad="4"/>
</signal>
<signal name="F2-2">
<contactref element="U$2" pad="F2"/>
<contactref element="U$15" pad="4"/>
</signal>
<signal name="G2-2">
<contactref element="U$2" pad="G2"/>
<contactref element="U$16" pad="4"/>
</signal>
<signal name="A2-2">
<contactref element="U$2" pad="A2"/>
<contactref element="U$10" pad="4"/>
</signal>
<signal name="B2-2">
<contactref element="U$2" pad="B2"/>
<contactref element="U$140" pad="4"/>
</signal>
<signal name="C2-2">
<contactref element="U$2" pad="C2"/>
<contactref element="U$150" pad="4"/>
</signal>
<signal name="D2-2">
<contactref element="U$2" pad="D2"/>
<contactref element="U$160" pad="4"/>
</signal>
<signal name="A1-1">
<contactref element="U$1" pad="A1"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="B1-1">
<contactref element="U$1" pad="B1"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="C1-1">
<contactref element="U$1" pad="C1"/>
<contactref element="U$5" pad="1"/>
</signal>
<signal name="D1-1">
<contactref element="U$1" pad="D1"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="E1-1">
<contactref element="U$1" pad="E1"/>
<contactref element="U$7" pad="1"/>
</signal>
<signal name="F1-1">
<contactref element="U$1" pad="F1"/>
<contactref element="U$8" pad="1"/>
</signal>
<signal name="G1-1">
<contactref element="U$1" pad="G1"/>
<contactref element="U$9" pad="1"/>
</signal>
<signal name="A2-1">
<contactref element="U$1" pad="A2"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="B1-2">
<contactref element="U$2" pad="B1"/>
<contactref element="U$140" pad="1"/>
</signal>
<signal name="C1-2">
<contactref element="U$2" pad="C1"/>
<contactref element="U$150" pad="1"/>
</signal>
<signal name="D1-2">
<contactref element="U$2" pad="D1"/>
<contactref element="U$160" pad="1"/>
</signal>
<signal name="E1-2">
<contactref element="U$2" pad="E1"/>
<contactref element="U$14" pad="1"/>
</signal>
<signal name="G2-1">
<contactref element="U$1" pad="G2"/>
<contactref element="U$9" pad="4"/>
</signal>
<signal name="A1-2">
<contactref element="U$2" pad="A1"/>
<contactref element="U$10" pad="1"/>
</signal>
<signal name="F1-2">
<contactref element="U$2" pad="F1"/>
<contactref element="U$15" pad="1"/>
</signal>
<signal name="B2-1">
<contactref element="U$1" pad="B2"/>
<contactref element="U$4" pad="4"/>
</signal>
<signal name="C2-1">
<contactref element="U$1" pad="C2"/>
<contactref element="U$5" pad="4"/>
</signal>
<signal name="D2-1">
<contactref element="U$1" pad="D2"/>
<contactref element="U$6" pad="4"/>
</signal>
<signal name="E2-1">
<contactref element="U$1" pad="E2"/>
<contactref element="U$7" pad="4"/>
</signal>
<signal name="F2-1">
<contactref element="U$1" pad="F2"/>
<contactref element="U$8" pad="4"/>
</signal>
<signal name="G1-2">
<contactref element="U$2" pad="G1"/>
<contactref element="U$16" pad="1"/>
</signal>
<signal name="SE2-2">
<contactref element="U$17" pad="2"/>
<contactref element="U$14" pad="7"/>
</signal>
<signal name="SF2-2">
<contactref element="U$17" pad="3"/>
<contactref element="U$15" pad="7"/>
</signal>
<signal name="SG2-2">
<contactref element="U$17" pad="4"/>
<contactref element="U$16" pad="7"/>
</signal>
<signal name="SG1-2">
<contactref element="U$17" pad="5"/>
<contactref element="U$16" pad="6"/>
</signal>
<signal name="SA2-1">
<contactref element="U$17" pad="8"/>
<contactref element="U$3" pad="7"/>
</signal>
<signal name="SB2-1">
<contactref element="U$17" pad="9"/>
<contactref element="U$4" pad="7"/>
</signal>
<signal name="SC2-1">
<contactref element="U$17" pad="10"/>
<contactref element="U$5" pad="7"/>
</signal>
<signal name="SD2-1">
<contactref element="U$17" pad="11"/>
<contactref element="U$6" pad="7"/>
</signal>
<signal name="SE2-1">
<contactref element="U$17" pad="14"/>
<contactref element="U$7" pad="7"/>
</signal>
<signal name="SF2-1">
<contactref element="U$17" pad="15"/>
<contactref element="U$8" pad="7"/>
</signal>
<signal name="SG2-1">
<contactref element="U$17" pad="16"/>
<contactref element="U$9" pad="7"/>
<contactref element="ICSP" pad="5"/>
</signal>
<signal name="SA1-1">
<contactref element="U$17" pad="19"/>
<contactref element="U$3" pad="6"/>
</signal>
<signal name="SB1-1">
<contactref element="U$17" pad="20"/>
<contactref element="U$4" pad="6"/>
</signal>
<signal name="SC1-1">
<contactref element="U$17" pad="21"/>
<contactref element="U$5" pad="6"/>
</signal>
<signal name="SD1-1">
<contactref element="U$17" pad="22"/>
<contactref element="U$6" pad="6"/>
</signal>
<signal name="SE1-1">
<contactref element="U$17" pad="23"/>
<contactref element="U$7" pad="6"/>
</signal>
<signal name="SF1-1">
<contactref element="U$17" pad="24"/>
<contactref element="U$8" pad="6"/>
</signal>
<signal name="SG1-1">
<contactref element="U$17" pad="31"/>
<contactref element="U$9" pad="6"/>
</signal>
<signal name="SA1-2">
<contactref element="U$17" pad="32"/>
<contactref element="U$10" pad="6"/>
</signal>
<signal name="SB1-2">
<contactref element="U$17" pad="35"/>
<contactref element="U$140" pad="6"/>
</signal>
<signal name="SC1-2">
<contactref element="U$17" pad="36"/>
<contactref element="U$150" pad="6"/>
</signal>
<signal name="SD1-2">
<contactref element="U$17" pad="37"/>
<contactref element="U$160" pad="6"/>
</signal>
<signal name="SE1-2">
<contactref element="U$17" pad="42"/>
<contactref element="U$14" pad="6"/>
</signal>
<signal name="SF1-2">
<contactref element="U$17" pad="43"/>
<contactref element="U$15" pad="6"/>
</signal>
<signal name="SA2-2">
<contactref element="U$17" pad="38"/>
<contactref element="U$10" pad="7"/>
</signal>
<signal name="SB2-2">
<contactref element="U$17" pad="39"/>
<contactref element="U$140" pad="7"/>
</signal>
<signal name="SC2-2">
<contactref element="U$17" pad="40"/>
<contactref element="U$150" pad="7"/>
</signal>
<signal name="SD2-2">
<contactref element="U$17" pad="41"/>
<contactref element="U$160" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="U$17" pad="30"/>
<contactref element="TP2" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
