Telescoping Yagi

Thumb screws 10-24 1/2" tunable/adjustable impedance matching "U" bridge

Straighten 0.125" copper pipe or find salvage wire/pipe for tunable/adjustable impedance matching "U" bridge

Solder Terminal Lug's together for 3/4" spacing of two wire/pipe for tunable/adjustable impedance matching "U" bridge

Completed Tasks:

Drill out telescoping antennas to #32 diameter