<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="-0.19" y1="-0.19" x2="55.995" y2="-0.19" width="0" layer="20"/>
<wire x1="55.995" y1="-0.19" x2="55.995" y2="35.265" width="0" layer="20"/>
<wire x1="55.995" y1="35.265" x2="-0.19" y2="35.265" width="0" layer="20"/>
<wire x1="-0.19" y1="35.265" x2="-0.19" y2="-0.19" width="0" layer="20"/>
<hole x="4.445" y="29.36" drill="3.2"/>
<hole x="51.36" y="29.36" drill="3.2"/>
<text>by K.Jacobs</text>
<text>HTTPS://www.GrauTier.com</text>
<text>CC-by-nc-sa</text>
<text>Ver. 1.0</text>
</plain>
<libraries>
<library name="v-reg-3">
<packages>
<package name="SOT223">
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="SMC_D">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X20/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="neoway_m590">
<packages>
<package name="M590">
<description>&lt;b&gt; Neoway M590 &lt;/b&gt; &lt;br/&gt;
GSM Module &lt;br/&gt;
Library created by Konrad Połys (k13.pl)</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SIMHOLDER">
</package>
</packages>
</library>
<library name="transistor-neu-to92">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="v-reg-3" package="SOT223" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="resistor" package="C0805K" value="100n">
<attribute name="NAME"/>
</element>
<element name="C2" library="resistor" package="C0805K" value="100n">
<attribute name="NAME"/>
</element>
<element name="C3" library="rcl" package="C1206K" value="10µ">
<attribute name="NAME"/>
</element>
<element name="C4" library="rcl" package="C1206K" value="10µ">
<attribute name="NAME"/>
</element>
<element name="JP2" library="pinhead" package="2X20/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="neoway_m590" package="M590" value="NEOWAY_M590"/>
<element name="PWR" library="led" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RUN" library="led" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R2" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R3" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="SIMHOLDER" value="">
<attribute name="PROD_ID" value="CONN-08536"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="C5" library="rcl" package="SMC_D" value="47µ">
<attribute name="NAME"/>
</element>
<element name="RING" library="led" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R6" library="rcl" package="R0805" value="4k7">
<attribute name="NAME"/>
</element>
<element name="T1" library="transistor-neu-to92" package="SOT23" value="BC847">
<attribute name="NAME"/>
</element>
<element name="C6" library="rcl" package="SMC_D" value="220µ">
<attribute name="NAME"/>
</element>
<element name="C7" library="rcl" package="SMC_D" value="220µ">
<attribute name="NAME"/>
</element>
<element name="GND" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="ANT" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="JP2" pad="5"/>
<contactref element="JP2" pad="13"/>
<contactref element="JP2" pad="19"/>
<contactref element="JP2" pad="29"/>
<contactref element="JP2" pad="33"/>
<contactref element="JP2" pad="26"/>
<contactref element="JP2" pad="40"/>
<contactref element="JP2" pad="10"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="U$1" pad="P$15"/>
<contactref element="U$1" pad="P$20"/>
<contactref element="U$1" pad="P$9"/>
<contactref element="RUN" pad="C"/>
<contactref element="PWR" pad="C"/>
<contactref element="J1" pad="C5"/>
<contactref element="C5" pad="-"/>
<contactref element="T1" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="C7" pad="-"/>
<contactref element="C6" pad="-"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="IC1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="V+">
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="C5" pad="+"/>
<contactref element="C6" pad="+"/>
<contactref element="C7" pad="+"/>
<contactref element="RING" pad="C"/>
</signal>
<signal name="LED">
<contactref element="U$1" pad="P$5"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="U$1" pad="P$7"/>
<contactref element="JP2" pad="14"/>
</signal>
<signal name="TXD">
<contactref element="U$1" pad="P$8"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="RING">
<contactref element="U$1" pad="P$10"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="RUN" pad="A"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="PWR" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="ON">
<contactref element="JP2" pad="16"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="SVCC">
<contactref element="U$1" pad="P$14"/>
<contactref element="J1" pad="C1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="SRST">
<contactref element="U$1" pad="P$13"/>
<contactref element="J1" pad="C2"/>
</signal>
<signal name="SCLK">
<contactref element="U$1" pad="P$12"/>
<contactref element="J1" pad="C3"/>
</signal>
<signal name="SIO">
<contactref element="U$1" pad="P$11"/>
<contactref element="J1" pad="C7"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="RING" pad="A"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="2"/>
<contactref element="T1" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="ON_E">
<contactref element="T1" pad="3"/>
<contactref element="U$1" pad="P$19"/>
</signal>
<signal name="ANT">
<contactref element="U$1" pad="P$21"/>
<contactref element="ANT" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
