<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.5.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="71.1" y2="0" width="0" layer="20"/>
<wire x1="71.1" y1="0" x2="71.1" y2="60.63" width="0" layer="20"/>
<wire x1="71.1" y1="60.63" x2="0" y2="60.63" width="0" layer="20"/>
<wire x1="0" y1="60.63" x2="0" y2="0" width="0" layer="20"/>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>A6</text>
<text>A7</text>
<text>31</text>
<text>30</text>
<text>29</text>
<text>28</text>
<text>27</text>
<text>26</text>
<text>25</text>
<text>DIGITAL</text>
<text>23</text>
<text>22</text>
<text>21</text>
<text>20</text>
<text>19</text>
<text>18</text>
<text>17</text>
<text>16</text>
<text>15</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>24</text>
<text>Decker Electronics PLP-1.0</text>
<text>SS</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
<text>VCC</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>TDI</text>
<text>TDO</text>
<text>TMS</text>
<text>TCK</text>
<text>RESET</text>
<text>INTERRUPT</text>
</plain>
<libraries>
<library name="1284p">
<packages>
<package name="DIL40">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL-KIT">
<description>&lt;h3&gt;CAP-PTH-SMALL-KIT&lt;/h3&gt;
Commonly used for small ceramic capacitors. Like our 0.1uF (http://www.sparkfun.com/products/8375) or 22pF caps (http://www.sparkfun.com/products/8571).&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="CAP-PTH-2.54">
<description>2 PTH spaced 0.1" apart</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49US">
<description>&lt;h3&gt;HC49/US 11.6x4.6mm PTH Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.digikey.com/Web%20Export/Supplier%20Content/Citizen_300/PDF/Citizen_HC49US.pdf?redirected=1"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X10">
<description>&lt;h3&gt;Plated Through Hole -10 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X09">
<description>&lt;h3&gt;Plated Through Hole -9 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electromechanical Parts&lt;/h3&gt;
This library contains electromechanical devices, like motors, speakers,servos, and relays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BUZZER-12MM">
<description>&lt;h3&gt;12mm Buzzer - PTH&lt;/h3&gt;
&lt;p&gt;This is a small 12mm round speaker that operates around the audible 2kHz range. You can use these speakers to create simple music or user interfaces.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/General/cem-1203-42-.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BUZZER&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ATMEGA1284" library="1284p" package="DIL40" value="ATmega 1284">
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H2" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H3" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H4" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="PWR5V" library="adafruit" package="DCJACK_2MM_PTH" value="jack">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="CAP-PTH-SMALL-KIT" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08370"/>
</element>
<element name="R4" library="adafruit" package="0207/10" value="10k">
<attribute name="VALUE"/>
</element>
<element name="SW_RESET" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="Y1" library="SparkFun-Clocks" package="HC49US" value="16MHz">
<attribute name="PROD_ID" value="XTAL-08181"/>
<attribute name="SF_ID" value="COM-00536"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-2.54" value="22pF">
<attribute name="PROD_ID" value="CAP-09128"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-2.54" value="22pF">
<attribute name="PROD_ID" value="CAP-09128"/>
<attribute name="VALUE"/>
</element>
<element name="FTDI_HEADER_TOP" library="SparkFun-Connectors" package="1X06_LONGPADS" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="CAP-PTH-SMALL-KIT" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08370"/>
</element>
<element name="R1" library="adafruit" package="0207/10" value="10k">
<attribute name="VALUE"/>
</element>
<element name="SW_INT0" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="R2" library="adafruit" package="0207/10" value="1k">
<attribute name="VALUE"/>
</element>
<element name="LS1" library="SparkFun-Electromechanical" package="BUZZER-12MM" value="BUZZER-PTH">
<attribute name="PROD_ID" value="COMP-08253"/>
<attribute name="SF_SKU" value="COM-07950"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="adafruit" package="0207/10" value="220">
<attribute name="VALUE"/>
</element>
<element name="RESET" library="adafruit" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0207/10" value="1k">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X09" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="SW_RESET" pad="1"/>
<contactref element="PWR5V" pad="GNDBREAK"/>
<contactref element="PWR5V" pad="GND"/>
<contactref element="ATMEGA1284" pad="11"/>
<contactref element="ATMEGA1284" pad="31"/>
<contactref element="FTDI_HEADER_TOP" pad="6"/>
<contactref element="C4" pad="1"/>
<contactref element="SW_INT0" pad="3"/>
<contactref element="R13" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="J1" pad="10"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="ATMEGA1284" pad="32"/>
<contactref element="ATMEGA1284" pad="10"/>
<contactref element="ATMEGA1284" pad="30"/>
<contactref element="R4" pad="1"/>
<contactref element="PWR5V" pad="PWR"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="N$1">
<contactref element="SW_RESET" pad="3"/>
<contactref element="ATMEGA1284" pad="9"/>
<contactref element="C3" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="DTR">
<contactref element="C3" pad="1"/>
<contactref element="FTDI_HEADER_TOP" pad="1"/>
</signal>
<signal name="TXO">
<contactref element="FTDI_HEADER_TOP" pad="3"/>
<contactref element="ATMEGA1284" pad="14"/>
</signal>
<signal name="RXI">
<contactref element="FTDI_HEADER_TOP" pad="2"/>
<contactref element="ATMEGA1284" pad="15"/>
</signal>
<signal name="N$4">
<contactref element="ATMEGA1284" pad="16"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="SW_INT0" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="LS1" pad="-"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="O_BUZZ">
<contactref element="LS1" pad="+"/>
<contactref element="ATMEGA1284" pad="20"/>
</signal>
<signal name="N$6">
<contactref element="RESET" pad="K"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="R_LED">
<contactref element="RESET" pad="A"/>
<contactref element="ATMEGA1284" pad="1"/>
</signal>
<signal name="A0">
<contactref element="ATMEGA1284" pad="40"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="A1">
<contactref element="ATMEGA1284" pad="39"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="A2">
<contactref element="ATMEGA1284" pad="38"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="A3">
<contactref element="ATMEGA1284" pad="37"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="A4">
<contactref element="ATMEGA1284" pad="36"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="A5">
<contactref element="ATMEGA1284" pad="35"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="A6">
<contactref element="ATMEGA1284" pad="34"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="A7">
<contactref element="ATMEGA1284" pad="33"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="D1">
<contactref element="ATMEGA1284" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="D2">
<contactref element="ATMEGA1284" pad="3"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="D3">
<contactref element="ATMEGA1284" pad="4"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="D4">
<contactref element="ATMEGA1284" pad="5"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="D5">
<contactref element="ATMEGA1284" pad="6"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="D6">
<contactref element="ATMEGA1284" pad="7"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="D7">
<contactref element="ATMEGA1284" pad="8"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="D11">
<contactref element="ATMEGA1284" pad="17"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="D12">
<contactref element="ATMEGA1284" pad="18"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="D13">
<contactref element="ATMEGA1284" pad="19"/>
<contactref element="J2" pad="10"/>
</signal>
<signal name="D16">
<contactref element="ATMEGA1284" pad="22"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="D17">
<contactref element="ATMEGA1284" pad="23"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="D18">
<contactref element="ATMEGA1284" pad="24"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="D19">
<contactref element="ATMEGA1284" pad="25"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="D20">
<contactref element="ATMEGA1284" pad="26"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="D21">
<contactref element="ATMEGA1284" pad="27"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="D22">
<contactref element="ATMEGA1284" pad="28"/>
<contactref element="J3" pad="8"/>
</signal>
<signal name="D23">
<contactref element="ATMEGA1284" pad="29"/>
<contactref element="J3" pad="9"/>
</signal>
<signal name="D15">
<contactref element="ATMEGA1284" pad="21"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="2"/>
<contactref element="ATMEGA1284" pad="13"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="C2" pad="2"/>
<contactref element="ATMEGA1284" pad="12"/>
<contactref element="Y1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
