(kicad_pcb (version 20171130) (host pcbnew 5.0.1)
  (general
    (thickness 1.6)
    (drawings 42)
    (tracks 380)
    (zones 0)
    (modules 36)
    (nets 35)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.7)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.6)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1)
    (via_drill 0.8)
    (via_min_size 1)
    (via_min_drill 0.6)
    (uvia_size 0.6)
    (uvia_drill 0.4)
    (uvias_allowed no)
    (uvia_min_size 0.6)
    (uvia_min_drill 0.4)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8796 1.8796)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 78.08 130.5)
    (grid_origin 78.08 130.5)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Exports/"))
  )
  (net 0 "")
  (net 1 N$1)
  (net 2 N$2)
  (net 3 N$4)
  (net 4 N$5)
  (net 5 N$7)
  (net 6 N$6)
  (net 7 N$8)
  (net 8 N$9)
  (net 9 N$10)
  (net 10 N$11)
  (net 11 N$13)
  (net 12 N$17)
  (net 13 N$12)
  (net 14 N$14)
  (net 15 N$15)
  (net 16 N$16)
  (net 17 N$19)
  (net 18 N$27)
  (net 19 N$21)
  (net 20 N$24)
  (net 21 N$20)
  (net 22 N$18)
  (net 23 N$26)
  (net 24 N$22)
  (net 25 N$23)
  (net 26 N$29)
  (net 27 N$28)
  (net 28 N$30)
  (net 29 N$31)
  (net 30 N$32)
  (net 31 N$33)
  (net 32 N$35)
  (net 33 N$36)
  (net 34 N$38)
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.7)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.6)
    (uvia_drill 0.4)
    (add_net N$1)
    (add_net N$10)
    (add_net N$11)
    (add_net N$12)
    (add_net N$13)
    (add_net N$14)
    (add_net N$15)
    (add_net N$16)
    (add_net N$17)
    (add_net N$18)
    (add_net N$19)
    (add_net N$2)
    (add_net N$20)
    (add_net N$21)
    (add_net N$22)
    (add_net N$23)
    (add_net N$24)
    (add_net N$26)
    (add_net N$27)
    (add_net N$28)
    (add_net N$29)
    (add_net N$30)
    (add_net N$31)
    (add_net N$32)
    (add_net N$33)
    (add_net N$35)
    (add_net N$36)
    (add_net N$38)
    (add_net N$4)
    (add_net N$5)
    (add_net N$6)
    (add_net N$7)
    (add_net N$8)
    (add_net N$9)
  )
  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer Top) (tedit 5C437BDD)
    (at 95.26 83.731)
    (fp_text reference H1 (at -1.698 -0.508) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_2-5mmDrill (at 1.27 5.08) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.76 -5.731) (size 5.99948 5.99948) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module tacx_library:Arduino_Nano (layer Top) (tedit 5C76E37B)
    (at 115.545 86.812 270)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (fp_text reference NANO (at 7.62 17.907) (layer F.SilkS))
    (fp_text value Arduino_Nano (at 8.89 19.05) (layer F.Fab))
    (fp_text user VIN (at 12.5 0 270) (layer F.SilkS))
    (fp_text user GND (at 12.3 2.6 270) (layer F.SilkS))
    (fp_text user RST (at 12.5 5.2 270) (layer F.SilkS))
    (fp_text user 5v (at 13 7.6 270) (layer F.SilkS))
    (fp_text user A7 (at 12.9 10.1 270) (layer F.SilkS))
    (fp_text user A6 (at 12.9 12.8 270) (layer F.SilkS))
    (fp_text user A5 (at 12.9 15.3 270) (layer F.SilkS))
    (fp_text user A4 (at 12.9 17.8 270) (layer F.SilkS))
    (fp_text user A3 (at 12.9 20.4 270) (layer F.SilkS))
    (fp_text user A2 (at 12.9 22.9 270) (layer F.SilkS))
    (fp_text user A1 (at 13 25.5 270) (layer F.SilkS))
    (fp_text user A0 (at 12.9 27.9 270) (layer F.SilkS))
    (fp_text user AREF (at 12 30.5 270) (layer F.SilkS))
    (fp_text user 3.3v (at 12.4 33 270) (layer F.SilkS))
    (fp_text user D13 (at 12.4 35.6 270) (layer F.SilkS))
    (fp_text user D12 (at 2.8 35.6 270) (layer F.SilkS))
    (fp_text user D11 (at 2.8 33 270) (layer F.SilkS))
    (fp_text user D10 (at 2.8 30.5 270) (layer F.SilkS))
    (fp_text user D9 (at 2.3 28 270) (layer F.SilkS))
    (fp_text user D8 (at 2.3 25.4 270) (layer F.SilkS))
    (fp_text user D7 (at 2.3 22.9 270) (layer F.SilkS))
    (fp_text user D6 (at 2.3 20.3 270) (layer F.SilkS))
    (fp_text user D5 (at 2.3 17.8 270) (layer F.SilkS))
    (fp_text user D4 (at 2.3 15.3 270) (layer F.SilkS))
    (fp_text user D3 (at 2.3 12.7 270) (layer F.SilkS))
    (fp_text user D2 (at 2.3 10.2 270) (layer F.SilkS))
    (fp_text user GND (at 2.9 7.6 270) (layer F.SilkS))
    (fp_text user RST (at 2.7 5.1 270) (layer F.SilkS))
    (fp_text user "RX 0" (at 3.2 2.6 270) (layer F.SilkS))
    (fp_text user " TX 1" (at 3.429 -0.127 270) (layer F.SilkS))
    (fp_text user %R (at 6.35 19.05) (layer F.Fab))
    (pad 16 thru_hole oval (at 15.24 35.56 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 N$11))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 N$13))
    (pad 30 thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 N$30))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 N$5))
    (pad 29 thru_hole oval (at 15.24 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 N$26))
    (pad 28 thru_hole oval (at 15.24 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 N$12))
    (pad 27 thru_hole oval (at 15.24 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 N$2))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 N$7))
    (pad 26 thru_hole oval (at 15.24 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 N$10))
    (pad 25 thru_hole oval (at 15.24 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 N$9))
    (pad 24 thru_hole oval (at 15.24 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 N$17))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 N$8))
    (pad 23 thru_hole oval (at 15.24 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 N$32))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 N$6))
    (pad 22 thru_hole oval (at 15.24 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 N$29))
    (pad 21 thru_hole oval (at 15.24 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 N$16))
    (pad 20 thru_hole oval (at 15.24 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 19 thru_hole oval (at 15.24 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 15.24 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 N$28))
    (pad 17 thru_hole oval (at 15.24 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 N$24))
    (model ${KISYS3DMOD}/Module.3dshapes/Arduino_Nano_WithMountingHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tacx_library:TO-92_Inline_Narrow_Oval (layer Top) (tedit 5C424D1A)
    (at 130.912 125.42 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference 2N4401 (at 1.016 -3.429 180) (layer F.SilkS))
    (fp_text value TO-92_Inline_Narrow_Oval (at 1.27 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.2 0) (size 1.1 1.1) (drill 0.6) (layers *.Cu *.Mask)
      (net 25 N$23))
    (pad 3 thru_hole circle (at 2.7 0) (size 1.1 1.1) (drill 0.6) (layers *.Cu *.Mask)
      (net 24 N$22))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.1 1.1) (drill 0.6) (layers *.Cu *.Mask)
      (net 34 N$38))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module AXIAL-0.3 (layer Top) (tedit 5C432D7C)
    (at 133.706 115.26 180)
    (descr "<h3>AXIAL-0.3</h3>\n<p>Commonly used for 1/4W through-hole resistors. 0.3\" pitch between holes.</p>")
    (fp_text reference R11 (at -2.921 -1.14 180) (layer F.SilkS))
    (fp_text value 10K (at 0.381 1.905 180) (layer F.SilkS))
    (fp_text user "" (at 0 1.016 180) (layer F.SilkS))
    (fp_text user "" (at 0 -1.016 180) (layer F.SilkS))
    (pad P$2 thru_hole circle (at 3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 N$22))
    (pad P$1 thru_hole circle (at -3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 N$38))
  )
  (module AXIAL-0.3 (layer Top) (tedit 5C432DEA)
    (at 133.706 119.07 180)
    (descr "<h3>AXIAL-0.3</h3>\n<p>Commonly used for 1/4W through-hole resistors. 0.3\" pitch between holes.</p>")
    (fp_text reference R12 (at -2.921 -1.143 180) (layer F.SilkS))
    (fp_text value 10K (at 0.381 1.905 180) (layer F.SilkS))
    (fp_text user "" (at 0 1.016 180) (layer F.SilkS))
    (fp_text user "" (at 0 -1.016 180) (layer F.SilkS))
    (pad P$2 thru_hole circle (at 3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 N$38))
    (pad P$1 thru_hole circle (at -3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 N$1))
  )
  (module Pin_Headers:Pin_Header_Straight_1x09_Pitch2.54mm (layer Top) (tedit 5C169B62)
    (at 126.594 71.064 90)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x09_Pitch2.54mm (at 0 22.65 90) (layer F.Fab))
    (fp_text user %R (at 0 10.16 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 N$2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 N$29))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 N$32))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 N$14))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 N$15))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 N$24))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 N$28))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 N$26))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AXIAL-0.3 (layer Top) (tedit 5C168688)
    (at 152 83 180)
    (descr "<h3>AXIAL-0.3</h3>\n<p>Commonly used for 1/4W through-hole resistors. 0.3\" pitch between holes.</p>")
    (fp_text reference R9 (at -2.788 -1.328 180) (layer F.SilkS))
    (fp_text value 10K (at -0.502 2.0866 180) (layer F.SilkS))
    (fp_text user "" (at 0 1.016 180) (layer F.SilkS))
    (fp_text user "" (at 0 -1.016 180) (layer F.SilkS))
    (pad P$2 thru_hole circle (at 3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 N$31))
    (pad P$1 thru_hole circle (at -3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 N$2))
  )
  (module My_Tacx_Library:AP2_MODULE_2 (layer Top) (tedit 5C76E342)
    (at 91.669 107.005 270)
    (fp_text reference U$1 (at 7.493 2.794 270) (layer F.SilkS) hide)
    (fp_text value AP2 (at 9.144 6.35) (layer F.SilkS))
    (fp_text user "" (at 7.5 19.3 270) (layer F.SilkS))
    (pad 11 thru_hole rect (at 20 12 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 N$20))
    (pad 12 thru_hole rect (at 20 10 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 N$21))
    (pad 13 thru_hole rect (at 20 8 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 14 thru_hole rect (at 20 6 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 15 thru_hole rect (at 20 4 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 16 thru_hole rect (at 20 2 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 17 thru_hole rect (at 20 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 N$18))
    (pad 1 thru_hole rect (at 12 -1 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 2 thru_hole rect (at 10 -1 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole rect (at 8 -1 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 N$27))
    (pad 10 thru_hole rect (at 0 12 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 9 thru_hole rect (at 0 10 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 8 thru_hole rect (at 0 8 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole rect (at 0 6 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 6 thru_hole rect (at 0 4 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 N$27))
    (pad 5 thru_hole rect (at 0 2 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 N$1))
  )
  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer Top) (tedit 5C444229)
    (at 157.444 133.223)
    (fp_text reference H4 (at -1.698 -0.508) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_2-5mmDrill (at 1.27 5.08) (layer F.Fab))
    (pad 4 thru_hole circle (at -2.444 -5.723) (size 5.99948 5.99948) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer Top) (tedit 5C437BFB)
    (at 155.158 74.549)
    (fp_text reference H2 (at -1.698 -0.508) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_2-5mmDrill (at 1.27 5.08) (layer F.Fab))
    (pad 2 thru_hole circle (at -0.158 -2.049) (size 5.99948 5.99948) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer Top) (tedit 5C437CF8)
    (at 176.159 132.626)
    (fp_text reference H5 (at -1.698 -0.508) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_2-5mmDrill (at 1.27 5.08) (layer F.Fab))
    (pad 5 thru_hole circle (at -2.159 -5.126) (size 5.99948 5.99948) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_2-5mmDrill (layer Top) (tedit 5C437F93)
    (at 84 132.525)
    (fp_text reference H3 (at -1.698 -0.508) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_2-5mmDrill (at 1.27 5.08) (layer F.Fab))
    (pad 3 thru_hole circle (at 16 -5.025) (size 5.99948 5.99948) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Potentiometers:Potentiometer_Trimmer_ACP_CA6h_Vertical (layer Top) (tedit 5C8025AF)
    (at 81.763 82.113 180)
    (descr "Potentiometer, vertically mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, Suntan TSR-3386H Single, Suntan TSR-3386P Single, Vishay T73XX Single, Vishay T73XX Single, Vishay T73YP Single, Piher PT-6h Single, Piher PT-6v Single, Piher PT-6v Single, Piher PT-10h2.5 Single, Piher PT-10h5 Single, Piher PT-101h3.8 Single, Piher PT-10v10 Single, Piher PT-10v10 Single, Piher PT-10v5 Single, Piher PT-15h5 Single, Piher PT-15h2.5 Single, Piher PT-15B Single, Piher PT-15hc5 Single, Piher PT-15v12.5 Single, Piher PT-15v12.5 Single, Piher PT-15v15 Single, Piher PT-15v15 Single, ACP CA6h Single, http://www.acptechnologies.com/wp-content/uploads/2016/12/ACP-CAT%C3%81LOGO-ENTERO-2016.pdf")
    (tags "Potentiometer vertical  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single  Suntan TSR-3386H Single  Suntan TSR-3386P Single  Vishay T73XX Single  Vishay T73XX Single  Vishay T73YP Single  Piher PT-6h Single  Piher PT-6v Single  Piher PT-6v Single  Piher PT-10h2.5 Single  Piher PT-10h5 Single  Piher PT-101h3.8 Single  Piher PT-10v10 Single  Piher PT-10v10 Single  Piher PT-10v5 Single  Piher PT-15h5 Single  Piher PT-15h2.5 Single  Piher PT-15B Single  Piher PT-15hc5 Single  Piher PT-15v12.5 Single  Piher PT-15v12.5 Single  Piher PT-15v15 Single  Piher PT-15v15 Single  ACP CA6h Single")
    (fp_text reference 10K (at 1.778 -1.778 180) (layer F.SilkS))
    (fp_text value Potentiometer_Trimmer_ACP_CA6h_Vertical (at 0 7.06 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 5 180) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 N$2))
    (pad 2 thru_hole circle (at 2.5 2.5 180) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 N$4))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 N$1))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_ACP_CA6h_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer Top) (tedit 5C1686AB)
    (at 141.58 83.002 270)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference CD40106BE (at 3.81 7.62) (layer F.SilkS))
    (fp_text value DIP-14_W7.62mm (at 3.81 17.57 270) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 N$19))
    (pad 8 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 N$29))
    (pad 9 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 N$31))
    (pad 10 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 N$32))
    (pad 11 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 14 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 N$27))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Tacx_Library:TACX_LOGIC_LEVEL_CONVERTER (layer Top) (tedit 5C76E47D)
    (at 116.053 116.276)
    (descr "<h3>SparkFun Logic Level Converter</h3>\n<p>Specifications:\n<ul><li>Pin count:12</li>\n<li>Pin pitch: 0.1\"</li>\n<li>Area: 0.6x 0.5 \"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>SparkFun Logic Level Converter</li>\n</ul></p>")
    (fp_text reference "3.3V <> 5V" (at -0.254 -7.874) (layer F.SilkS))
    (fp_text value "LOGIC LEVEL CONVERTER" (at 0 8.1026) (layer F.SilkS))
    (fp_text user HV4 (at 2.921 6.731) (layer F.SilkS))
    (fp_text user HV3 (at 2.921 4.318) (layer F.SilkS))
    (fp_text user GND (at 2.794 1.778) (layer F.SilkS))
    (fp_text user HV (at 3.556 -0.889) (layer F.SilkS))
    (fp_text user LV4 (at -5.207 6.6802) (layer F.SilkS) hide)
    (fp_text user LV3 (at -5.207 4.191) (layer F.SilkS) hide)
    (fp_text user GND (at -5.207 1.651) (layer F.SilkS) hide)
    (fp_text user LV (at -5.207 -0.889) (layer F.SilkS) hide)
    (fp_text user HV2 (at 2.921 -3.429) (layer F.SilkS))
    (fp_text user HV1 (at 3.048 -5.842) (layer F.SilkS))
    (fp_text user LV2 (at -5.207 -3.429) (layer F.SilkS) hide)
    (fp_text user LV1 (at -5.207 -5.842) (layer F.SilkS) hide)
    (pad HV1 thru_hole circle (at 6.5 -6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 N$36))
    (pad HV2 thru_hole circle (at 6.5 -3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 N$24))
    (pad HV thru_hole circle (at 6.5 -1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 N$2))
    (pad GND2 thru_hole circle (at 6.5 1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad HV3 thru_hole circle (at 6.5 3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 N$26))
    (pad HV4 thru_hole circle (at 6.5 6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask))
    (pad LV4 thru_hole circle (at -6.5 6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 N$33))
    (pad LV3 thru_hole circle (at -6.5 3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 N$18))
    (pad GND1 thru_hole circle (at -6.5 1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad LV thru_hole circle (at -6.5 -1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 N$27))
    (pad LV2 thru_hole circle (at -6.5 -3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 N$21))
    (pad LV1 thru_hole circle (at -6.5 -6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 N$35))
  )
  (module tacx_library:my_slide_switch (layer Top) (tedit 5C10129C)
    (at 176.378 116.122 270)
    (fp_text reference "Power Switch" (at 0.1778 2.4638 270) (layer F.SilkS))
    (fp_text value slide_switch (at 0 -2 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 2.1 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 N$30))
    (pad 1 thru_hole circle (at -1.9 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0.1 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 N$23))
    (pad 5 thru_hole circle (at 4.2 0 270) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -4 0 270) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
  )
  (module DO41Z10 (layer Top) (tedit 5BF84AAA)
    (at 137.77 108.192 180)
    (descr "<B>DIODE</B><p>\ndiameter 2.54 mm, horizontal, grid 10.16 mm")
    (fp_text reference D1 (at 0.762 -1.6218 180) (layer F.SilkS))
    (fp_text value 4.3v (at -3.302 -1.6218 180) (layer F.SilkS))
    (pad C thru_hole circle (at -5.08 0 180) (size 2.34696 2.34696) (drill 1.1176) (layers *.Cu *.Mask)
      (net 16 N$16))
    (pad A thru_hole circle (at 5.08 0 180) (size 2.34696 2.34696) (drill 1.1176) (layers *.Cu *.Mask)
      (net 1 N$1))
  )
  (module DO41Z10 (layer Top) (tedit 5BF84A5D)
    (at 151.74 118 180)
    (descr "<B>DIODE</B><p>\ndiameter 2.54 mm, horizontal, grid 10.16 mm")
    (fp_text reference D2 (at 2.794 -2.536 180) (layer F.SilkS))
    (fp_text value 4.3v (at 0 -2.57 180) (layer F.SilkS))
    (pad C thru_hole circle (at -5.08 0 180) (size 2.34696 2.34696) (drill 1.1176) (layers *.Cu *.Mask)
      (net 14 N$14))
    (pad A thru_hole circle (at 5.08 0 180) (size 2.34696 2.34696) (drill 1.1176) (layers *.Cu *.Mask)
      (net 1 N$1))
  )
  (module RJ11-6 (layer Top) (tedit 5C17FC9E)
    (at 174.6 77.16 90)
    (descr "<h3>RJ11 6-Pin Socket with PCB Mounting Post</h3>\n<p>Specifications:\n<ul><li>Pin count: 6</li>\n</ul></p>\n<p><a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/RJ11-Datasheet.pdf”>Datasheet referenced for footprint</a></p>\n<p>Example device(s):\n<ul><li>RJ11-6</li>\n</ul></p>")
    (fp_text reference RJ12 (at 6.096 4.652 180) (layer F.SilkS) hide)
    (fp_text value RJ12 (at 0.3302 0.889 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 -8.89 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 N$31))
    (pad 2 thru_hole circle (at -1.905 -6.35 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 3 thru_hole circle (at -0.635 -8.89 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 N$14))
    (pad 4 thru_hole circle (at 0.635 -6.35 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 N$15))
    (pad 5 thru_hole circle (at 1.905 -8.89 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 N$22))
    (pad 6 thru_hole circle (at 3.175 -6.35 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 N$19))
    (pad "" np_thru_hole circle (at -5.08 0 90) (size 3.8 3.8) (drill 3.4) (layers *.Cu))
    (pad "" np_thru_hole circle (at 5.08 0 90) (size 3.8 3.8) (drill 3.4) (layers *.Cu))
  )
  (module LCD-16X2_NOHOLESNOSILK (layer Top) (tedit 5C8025C8)
    (at 112.421 87.9602)
    (descr "<h3>LCD-16x2 No silk or mounting holes</h3>\n<p>For Standard hitatchi type LCDs with backlight.  Has 16 pin connection and outline on docu, but no silk or mounting holes.</p>\n\n<p>Specifications:\n<ul><li>Pin count: 16</li>\n<li>Pin pitch: 0.1\"</li>\n<li>Area: </li>\n</ul></p>\n<p><b>Datasheet referenced for footprint:</b></p>\n<p>Example device(s): \n<ul><li><a href=\"https://www.sparkfun.com/products/255\">Basic 16x2 LCD</a></li>\n</ul></p>")
    (fp_text reference 16x4 (at 1.727 -13.2132) (layer F.SilkS))
    (fp_text value LCD (at 5.664 -13.2132) (layer F.SilkS))
    (fp_text user 1 (at -34.29 -15.24) (layer Dwgs.User))
    (fp_text user "" (at -31.75 -19.05) (layer F.SilkS))
    (fp_text user "" (at -31.75 19.05) (layer F.SilkS))
    (pad 1 thru_hole rect (at -32 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 2 thru_hole circle (at -29.46 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 N$2))
    (pad 3 thru_hole circle (at -26.92 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 N$4))
    (pad 4 thru_hole circle (at -24.38 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 N$5))
    (pad 5 thru_hole circle (at -21.84 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 6 thru_hole circle (at -19.3 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 N$7))
    (pad 7 thru_hole circle (at -16.76 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -14.22 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -11.68 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -9.14 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at -6.6 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 N$10))
    (pad 12 thru_hole circle (at -4.06 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 N$9))
    (pad 13 thru_hole circle (at -1.52 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 N$8))
    (pad 14 thru_hole circle (at 1.02 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 N$6))
    (pad 15 thru_hole circle (at 3.56 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 N$2))
    (pad 16 thru_hole circle (at 6.1 -15.5) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 N$1))
  )
  (module AXIAL-0.3 (layer Top) (tedit 5BF55C69)
    (at 152 88 180)
    (descr "<h3>AXIAL-0.3</h3>\n<p>Commonly used for 1/4W through-hole resistors. 0.3\" pitch between holes.</p>")
    (fp_text reference R1 (at -2.788 -1.328 180) (layer F.SilkS))
    (fp_text value 10K (at -0.502 2.0866 180) (layer F.SilkS))
    (fp_text user "" (at 0 -1.016 180) (layer F.SilkS))
    (fp_text user "" (at 0 1.016 180) (layer F.SilkS))
    (pad P$1 thru_hole circle (at -3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad P$2 thru_hole circle (at 3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 N$11))
  )
  (module AXIAL-0.3 (layer Top) (tedit 5BF55C0B)
    (at 152 103)
    (descr "<h3>AXIAL-0.3</h3>\n<p>Commonly used for 1/4W through-hole resistors. 0.3\" pitch between holes.</p>")
    (fp_text reference R2 (at 1.772 1.672) (layer F.SilkS))
    (fp_text value 10K (at -1.276 -1.63) (layer F.SilkS))
    (fp_text user "" (at 0 -1.016) (layer F.SilkS))
    (fp_text user "" (at 0 1.016) (layer F.SilkS))
    (pad P$1 thru_hole circle (at -3.81 0) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad P$2 thru_hole circle (at 3.81 0) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 N$13))
  )
  (module AXIAL-0.3 (layer Top) (tedit 5BF55C23)
    (at 152 98)
    (descr "<h3>AXIAL-0.3</h3>\n<p>Commonly used for 1/4W through-hole resistors. 0.3\" pitch between holes.</p>")
    (fp_text reference R3 (at 1.772 1.742) (layer F.SilkS))
    (fp_text value 10K (at -1.276 -1.5278) (layer F.SilkS))
    (fp_text user "" (at 0 -1.016) (layer F.SilkS))
    (fp_text user "" (at 0 1.016) (layer F.SilkS))
    (pad P$1 thru_hole circle (at -3.81 0) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad P$2 thru_hole circle (at 3.81 0) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 N$17))
  )
  (module AXIAL-0.3 (layer Top) (tedit 5BF55C8F)
    (at 152 93 180)
    (descr "<h3>AXIAL-0.3</h3>\n<p>Commonly used for 1/4W through-hole resistors. 0.3\" pitch between holes.</p>")
    (fp_text reference R4 (at -2.788 -1.1646 180) (layer F.SilkS))
    (fp_text value 220 (at -0.248 2.1374 180) (layer F.SilkS))
    (fp_text user "" (at 0 -1.016 180) (layer F.SilkS))
    (fp_text user "" (at 0 1.016 180) (layer F.SilkS))
    (pad P$1 thru_hole circle (at -3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 N$14))
    (pad P$2 thru_hole circle (at 3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 N$12))
  )
  (module AXIAL-0.3 (layer Top) (tedit 5BF55CD3)
    (at 137.762 103.192)
    (descr "<h3>AXIAL-0.3</h3>\n<p>Commonly used for 1/4W through-hole resistors. 0.3\" pitch between holes.</p>")
    (fp_text reference R5 (at 2.946 1.317) (layer F.SilkS))
    (fp_text value 1K2 (at 0.152 -1.985) (layer F.SilkS))
    (fp_text user "" (at 0 -1.016) (layer F.SilkS))
    (fp_text user "" (at 0 1.016) (layer F.SilkS))
    (pad P$1 thru_hole circle (at -3.81 0) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad P$2 thru_hole circle (at 3.81 0) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 N$14))
  )
  (module AXIAL-0.3 (layer Top) (tedit 5BF55BE6)
    (at 152 113)
    (descr "<h3>AXIAL-0.3</h3>\n<p>Commonly used for 1/4W through-hole resistors. 0.3\" pitch between holes.</p>")
    (fp_text reference R6 (at 1.772 1.728) (layer F.SilkS))
    (fp_text value 1K (at -1.784 -1.574) (layer F.SilkS))
    (fp_text user "" (at -1.5748 -1.5494) (layer F.SilkS))
    (fp_text user "" (at 0 1.016) (layer F.SilkS))
    (pad P$1 thru_hole circle (at -3.81 0) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 N$16))
    (pad P$2 thru_hole circle (at 3.81 0) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 N$15))
  )
  (module AXIAL-0.3 (layer Top) (tedit 5BF55BD6)
    (at 152 108 180)
    (descr "<h3>AXIAL-0.3</h3>\n<p>Commonly used for 1/4W through-hole resistors. 0.3\" pitch between holes.</p>")
    (fp_text reference R7 (at -2.788 -1.14 180) (layer F.SilkS))
    (fp_text value 10K (at -0.248 2.162 180) (layer F.SilkS))
    (fp_text user "" (at 0 -1.016 180) (layer F.SilkS))
    (fp_text user "" (at 0 1.016 180) (layer F.SilkS))
    (pad P$1 thru_hole circle (at -3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 N$16))
    (pad P$2 thru_hole circle (at 3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 N$1))
  )
  (module TACTILE_SWITCH_PTH_6.0MM (layer Top) (tedit 5BF136E2)
    (at 167.5 90)
    (descr "<h3>Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square</h3>\n<p>Normally-open (NO) SPST momentary switches (buttons, pushbuttons).</p>\n<p><a href=\"https://www.omron.com/ecb/products/pdf/en-b3f.pdf\">Datasheet</a> (B3F-1000)</p>")
    (fp_text reference S1 (at -4.456 -0.053 90) (layer F.SilkS))
    (fp_text value Up (at 0.08 5.334) (layer F.SilkS))
    (fp_text user "" (at 0 -3.302) (layer F.SilkS))
    (fp_text user "" (at 0 3.175) (layer F.SilkS))
    (pad 1 thru_hole circle (at -0.0512 -3.0606) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 N$11))
    (pad 3 thru_hole circle (at 0.0488 2.9606) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 N$2))
  )
  (module TACTILE_SWITCH_PTH_6.0MM (layer Top) (tedit 5BF136D2)
    (at 167.5 116)
    (descr "<h3>Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square</h3>\n<p>Normally-open (NO) SPST momentary switches (buttons, pushbuttons).</p>\n<p><a href=\"https://www.omron.com/ecb/products/pdf/en-b3f.pdf\">Datasheet</a> (B3F-1000)</p>")
    (fp_text reference S2 (at -4.456 0.014 90) (layer F.SilkS))
    (fp_text value Down (at 0.207 5.334) (layer F.SilkS))
    (fp_text user "" (at 0 -3.302) (layer F.SilkS))
    (fp_text user "" (at 0 3.175) (layer F.SilkS))
    (pad 1 thru_hole circle (at -0.0512 -3.0606) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 N$13))
    (pad 3 thru_hole circle (at 0.0488 2.9606) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 N$2))
  )
  (module TACTILE_SWITCH_PTH_6.0MM (layer Top) (tedit 5BF136B2)
    (at 167.5 103)
    (descr "<h3>Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square</h3>\n<p>Normally-open (NO) SPST momentary switches (buttons, pushbuttons).</p>\n<p><a href=\"https://www.omron.com/ecb/products/pdf/en-b3f.pdf\">Datasheet</a> (B3F-1000)</p>")
    (fp_text reference S3 (at -4.456 0.044 90) (layer F.SilkS))
    (fp_text value Select (at 0.007 5.461) (layer F.SilkS))
    (fp_text user "" (at 0 -3.302) (layer F.SilkS))
    (fp_text user "" (at 0 3.175) (layer F.SilkS))
    (pad 1 thru_hole circle (at -0.0512 -3.0606) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 N$17))
    (pad 3 thru_hole circle (at 0.0488 2.9606) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 N$2))
  )
  (module AXIAL-0.3 (layer Top) (tedit 5C07F07C)
    (at 137.762 98.192 180)
    (descr "<h3>AXIAL-0.3</h3>\n<p>Commonly used for 1/4W through-hole resistors. 0.3\" pitch between holes.</p>")
    (fp_text reference R8 (at -2.794 -1.2154 180) (layer F.SilkS))
    (fp_text value 10K (at -0.262 2.0866 180) (layer F.SilkS))
    (fp_text user "" (at 0 -1.016 180) (layer F.SilkS))
    (fp_text user "" (at 0 1.016 180) (layer F.SilkS))
    (pad P$1 thru_hole circle (at -3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 N$2))
    (pad P$2 thru_hole circle (at 3.81 0 180) (size 1.8796 1.8796) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 N$19))
  )
  (module tacx_library:my_slide_switch (layer Top) (tedit 5C76E8A3)
    (at 176.378 97.734 270)
    (fp_text reference "TX Switch" (at 0 2.286 270) (layer F.SilkS))
    (fp_text value slide_switch (at 0 -2 270) (layer F.Fab))
    (pad 4 thru_hole circle (at -4 0 270) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 4.2 0 270) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0.1 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 N$28))
    (pad 1 thru_hole circle (at -1.9 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 N$20))
    (pad 3 thru_hole circle (at 2.1 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask))
  )
  (module t2_lib:SPARKFUN_LOGIC_LEVEL_CONVERTER (layer Top) (tedit 5C76E370)
    (at 117.45 116.276)
    (descr "<h3>SparkFun Logic Level Converter</h3>\n<p>Specifications:\n<ul><li>Pin count:12</li>\n<li>Pin pitch: 0.1\"</li>\n<li>Area: 0.6x 0.5 \"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>SparkFun Logic Level Converter</li>\n</ul></p>")
    (fp_text reference "3V <> 5V" (at 0 -7.874) (layer F.SilkS) hide)
    (fp_text value "LOGIC LEVEL CONVERTER" (at 0 8.1026) (layer F.SilkS) hide)
    (fp_text user LV1 (at -3.7084 -5.9182) (layer F.SilkS))
    (fp_text user LV2 (at -3.7084 -3.429) (layer F.SilkS))
    (fp_text user HV1 (at 1.6256 -6.1214) (layer F.SilkS) hide)
    (fp_text user HV2 (at 1.524 -3.429) (layer F.SilkS) hide)
    (fp_text user LV (at -3.7084 -0.889) (layer F.SilkS))
    (fp_text user GND (at -3.6576 1.651) (layer F.SilkS))
    (fp_text user LV3 (at -3.7084 4.191) (layer F.SilkS))
    (fp_text user LV4 (at -3.7084 6.6802) (layer F.SilkS))
    (fp_text user HV (at 2.1336 -0.889) (layer F.SilkS) hide)
    (fp_text user GND (at 1.3716 1.651) (layer F.SilkS) hide)
    (fp_text user HV3 (at 1.524 4.2926) (layer F.SilkS) hide)
    (fp_text user HV4 (at 1.4732 6.6802) (layer F.SilkS) hide)
    (pad LV1 thru_hole circle (at -5.08 -6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 N$35))
    (pad LV2 thru_hole circle (at -5.08 -3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 N$21))
    (pad LV thru_hole circle (at -5.08 -1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 N$27))
    (pad GND1 thru_hole circle (at -5.08 1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad LV3 thru_hole circle (at -5.08 3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 N$18))
    (pad LV4 thru_hole circle (at -5.08 6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 N$33))
    (pad HV4 thru_hole circle (at 5.08 6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask))
    (pad HV3 thru_hole circle (at 5.08 3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 N$26))
    (pad GND2 thru_hole circle (at 5.08 1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad HV thru_hole circle (at 5.08 -1.27) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 N$2))
    (pad HV2 thru_hole circle (at 5.08 -3.81) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 N$24))
    (pad HV1 thru_hole circle (at 5.08 -6.35) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 N$36))
  )
  (module tacx_library:LOGO2 (layer Top) (tedit 0)
    (at 104.496 79.573)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO2 (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer Top) (tedit 5C434EC2)
    (at 137.516 126.563 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference "100uF 25v" (at -2.921 0.127 180) (layer F.SilkS))
    (fp_text value CP_Radial_D6.3mm_P2.50mm (at 1.25 4.46 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 N$38))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 N$1))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "tacx_library:3.3v Regulator" (layer Top) (tedit 5C77EC99)
    (at 101.194 119.832)
    (fp_text reference VReg (at 0.2 -8.2) (layer F.SilkS) hide)
    (fp_text value "3.3v Regulator" (at 0.2 2.2) (layer F.Fab))
    (fp_text user GND (at 2.5 -2.1 90) (layer F.SilkS))
    (fp_text user "Vo 3.3v" (at 0.1 -3.1 90) (layer F.SilkS))
    (fp_text user Vi (at -2.4 -1.9 90) (layer F.SilkS))
    (pad 3 thru_hole circle (at 2.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 N$1))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 N$27))
    (pad 1 thru_hole circle (at -2.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 N$2))
  )
  (gr_text SYN (at 139.294 73.985 90) (layer F.SilkS))
  (gr_text +5V (at 129.261 74.239 90) (layer F.SilkS))
  (gr_text RTS (at 146.914 73.858 90) (layer F.SilkS))
  (gr_text RX (at 144.374 73.604 90) (layer F.SilkS))
  (gr_text TX (at 141.834 73.477 90) (layer F.SilkS))
  (gr_text CDN (at 134.214 74.112 90) (layer F.SilkS))
  (gr_text BRK (at 136.754 74.112 90) (layer F.SilkS))
  (gr_text SPD (at 131.801 74.112 90) (layer F.SilkS))
  (gr_text GND (at 126.721 74.112 90) (layer F.SilkS))
  (gr_text Prg (at 176.378 104.084) (layer F.SilkS))
  (gr_text Run (at 176.378 91.638) (layer F.SilkS))
  (gr_text USB (at 176.378 110.18) (layer F.SilkS))
  (gr_text Int (at 176.378 122.372) (layer F.SilkS))
  (gr_text bug@randomcode.co.uk (at 115.418 128.976) (layer F.SilkS))
  (gr_text v1.2c (at 164.694 128.087) (layer F.SilkS))
  (gr_text VR1 (at 83.287 80.081) (layer F.SilkS))
  (gr_line (start 78 69.5) (end 78 130.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 1 (at 80.366 70.556) (layer F.SilkS))
  (gr_text 17 (at 91.669 128.849) (layer F.SilkS))
  (gr_text 11 (at 79.731 128.849) (layer F.SilkS))
  (gr_text 10 (at 79.731 105.354) (layer F.SilkS))
  (gr_text 4 (at 91.796 105.354) (layer F.SilkS))
  (gr_text 3 (at 94.209 115.006) (layer F.SilkS))
  (gr_text 2 (at 94.209 117.038) (layer F.SilkS))
  (gr_text 1 (at 94.209 119.07) (layer F.SilkS))
  (gr_line (start 78 69.5) (end 178 69.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178 69.5) (end 178 130.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 5 (at 164.948 73.35) (layer F.SilkS))
  (gr_text 6 (at 169.7482 72.4916) (layer F.SilkS))
  (gr_text 3 (at 163.6522 77.8256) (layer F.SilkS))
  (gr_text 1 (at 164.948 82.24) (layer F.SilkS))
  (gr_text 2 (at 169.8752 80.6196) (layer F.SilkS))
  (gr_text 4 (at 170.2562 76.5556) (layer F.SilkS))
  (gr_text 3 (at 163.5252 77.8256) (layer B.SilkS))
  (gr_text 5 (at 164.948 73.35) (layer B.SilkS))
  (gr_text 2 (at 169.7736 80.6196) (layer B.SilkS))
  (gr_text 4 (at 170.3832 76.5048) (layer B.SilkS))
  (gr_text 6 (at 169.8244 72.4916) (layer B.SilkS))
  (gr_text "T_Flow ANT+ Transceiver" (at 118.72 79.065) (layer F.SilkS))
  (gr_text 1 (at 164.948 82.24) (layer B.SilkS))
  (gr_text 1 (at 143.231 83.002) (layer F.SilkS))
  (gr_line (start 78 130.5) (end 178 130.5) (angle 90) (layer Edge.Cuts) (width 0.15))
)
