(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.2)
    (pcbplotparams
      (layerselection 0x00030f0_80000001)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber2/")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D3-Pad1)")
  (net 5 "/VS")
  (net 6 "/HS")
  (net 7 "GND")
  (net 8 "Net-(P1-Pad1)")
  (net 9 "Net-(P1-Pad6)")
  (net 10 "Net-(P1-Pad7)")
  (net 11 "Net-(P1-Pad8)")
  (net 12 "Net-(P1-Pad9)")
  (net 13 "Net-(P1-Pad10)")
  (net 14 "Net-(P1-Pad11)")
  (net 15 "Net-(P1-Pad12)")
  (net 16 "Net-(P1-Pad13)")
  (net 17 "Net-(P1-Pad14)")
  (net 18 "+5V")
  (net 19 "Net-(P1-Pad16)")
  (net 20 "Net-(P1-Pad17)")
  (net 21 "Net-(R1-Pad2)")
  (net 22 "Net-(R2-Pad2)")
  (net 23 "Net-(R3-Pad2)")
  (net 24 "Net-(R4-Pad2)")
  (net 25 "Net-(R5-Pad2)")
  (net 26 "Net-(U5-Pad10)")
  (net 27 "Net-(U5-Pad9)")
  (net 28 "Net-(U11-Pad22)")
  (net 29 "Net-(U5-Pad6)")
  (net 30 "Net-(U3-Pad13)")
  (net 31 "Net-(U13-Pad9)")
  (net 32 "Net-(U13-Pad10)")
  (net 33 "Net-(U5-Pad1)")
  (net 34 "Net-(U11-Pad27)")
  (net 35 "Net-(U5-Pad2)")
  (net 36 "Net-(U4-Pad12)")
  (net 37 "Net-(U4-Pad2)")
  (net 38 "/AD0")
  (net 39 "/AD1")
  (net 40 "/AD2")
  (net 41 "/BLANK")
  (net 42 "/AD3")
  (net 43 "/AD4")
  (net 44 "/AD5")
  (net 45 "/AD6")
  (net 46 "/AD7")
  (net 47 "/AD8")
  (net 48 "/AD9")
  (net 49 "/AD10")
  (net 50 "/AD11")
  (net 51 "/AD12")
  (net 52 "/AD13")
  (net 53 "/AD14")
  (net 54 "/AD15")
  (net 55 "Net-(U6-Pad12)")
  (net 56 "/A0")
  (net 57 "/A1")
  (net 58 "/A2")
  (net 59 "/A3")
  (net 60 "/A4")
  (net 61 "/A5")
  (net 62 "/A6")
  (net 63 "/A7")
  (net 64 "/A8")
  (net 65 "/A9")
  (net 66 "/A10")
  (net 67 "/A11")
  (net 68 "/A12")
  (net 69 "/A13")
  (net 70 "/A14")
  (net 71 "Net-(J1-Pad14)")
  (net 72 "Net-(J1-Pad13)")
  (net 73 "Net-(U13-Pad1)")
  (net 74 "Net-(U10-Pad7)")
  (net 75 "Net-(U3-Pad6)")
  (net 76 "Net-(U4-Pad9)")
  (net 77 "unconnected-(J1-Pad4)")
  (net 78 "unconnected-(J1-Pad9)")
  (net 79 "unconnected-(J1-Pad11)")
  (net 80 "unconnected-(J1-Pad12)")
  (net 81 "unconnected-(J1-Pad15)")
  (net 82 "unconnected-(P1-Pad2)")
  (net 83 "unconnected-(P1-Pad3)")
  (net 84 "unconnected-(P1-Pad18)")
  (net 85 "unconnected-(U1-Pad1)")
  (net 86 "unconnected-(U1-Pad2)")
  (net 87 "unconnected-(U1-Pad3)")
  (net 88 "unconnected-(U2-Pad1)")
  (net 89 "unconnected-(U2-Pad2)")
  (net 90 "unconnected-(U2-Pad10)")
  (net 91 "unconnected-(U2-Pad11)")
  (net 92 "unconnected-(U3-Pad1)")
  (net 93 "unconnected-(U3-Pad2)")
  (net 94 "unconnected-(U3-Pad3)")
  (net 95 "unconnected-(U5-Pad7)")
  (net 96 "unconnected-(U5-Pad21)")
  (net 97 "unconnected-(U5-Pad38)")
  (net 98 "unconnected-(U5-Pad39)")
  (net 99 "unconnected-(U6-Pad6)")
  (net 100 "unconnected-(U6-Pad9)")
  (net 101 "/A15")
  (net 102 "unconnected-(U13-Pad11)")
  (net 103 "unconnected-(U13-Pad13)")
  (net 104 "unconnected-(U13-Pad14)")
  (net 105 "unconnected-(U13-Pad15)")
  (net 106 "unconnected-(U14-Pad11)")
  (net 107 "unconnected-(U14-Pad13)")
  (net 108 "unconnected-(U14-Pad14)")
  (net 109 "unconnected-(U14-Pad15)")
  (net 110 "unconnected-(U15-Pad11)")
  (net 111 "unconnected-(U15-Pad13)")
  (net 112 "unconnected-(U15-Pad14)")
  (net 113 "unconnected-(U15-Pad15)")
  (net 114 "unconnected-(U16-Pad11)")
  (net 115 "unconnected-(U16-Pad13)")
  (net 116 "unconnected-(U16-Pad14)")
  (net 117 "unconnected-(U16-Pad15)")
  (footprint "Diodes_THT:D_A-405_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5921392E)
    (at 170.43 118.23 180)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 3.81 -2.41 180) (layer "F.SilkS"))
    (fp_text value "diode" (at 3.81 2.41 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diodes_THT:D_A-405_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5921392E)
    (at 170.68 121.92 180)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at 3.81 -2.41 180) (layer "F.SilkS"))
    (fp_text value "diode" (at 3.81 2.41 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diodes_THT:D_A-405_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5921392E)
    (at 170.56 125.73 180)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at 3.81 -2.41 180) (layer "F.SilkS"))
    (fp_text value "diode" (at 3.81 2.41 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "NTI:VGA" (layer "F.Cu")
    (tedit 58CC9ED8)
    (at 165.1 100.27 90)
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -6.35 -7.62 90) (layer "F.SilkS"))
    (fp_text value "VGA" (at 6.35 -7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 4.325 -2.54 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)") (pinfunction "RED") (pintype "input"))
    (pad "2" thru_hole circle locked (at 2.035 -2.54 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)") (pinfunction "GREEN") (pintype "input"))
    (pad "3" thru_hole circle locked (at -0.255 -2.54 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)") (pinfunction "BLUE") (pintype "input"))
    (pad "4" thru_hole circle locked (at -2.545 -2.54 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 77 "unconnected-(J1-Pad4)") (pinfunction "ID2/RES") (pintype "input+no_connect"))
    (pad "5" thru_hole circle locked (at 12.5 0 90) (size 4.2 4.2) (drill 3.26) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND_HSYNC") (pintype "input"))
    (pad "5" thru_hole circle locked (at -12.49 0 90) (size 4.2 4.2) (drill 3.26) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND_HSYNC") (pintype "input"))
    (pad "5" thru_hole circle locked (at -4.835 -2.54 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND_HSYNC") (pintype "input"))
    (pad "6" thru_hole circle locked (at 5.47 0 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "RED_RTN") (pintype "input"))
    (pad "7" thru_hole circle locked (at 3.18 0 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GREEN_RTN") (pintype "input"))
    (pad "8" thru_hole circle locked (at 0.89 0 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "BLUE_RTN") (pintype "input"))
    (pad "9" thru_hole circle locked (at -1.4 0 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 78 "unconnected-(J1-Pad9)") (pinfunction "KEY/PWR") (pintype "input+no_connect"))
    (pad "10" thru_hole circle locked (at -3.69 0 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND_VSYNC") (pintype "input"))
    (pad "11" thru_hole circle locked (at 4.325 2.54 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 79 "unconnected-(J1-Pad11)") (pinfunction "ID0/RES") (pintype "input+no_connect"))
    (pad "12" thru_hole circle locked (at 2.035 2.54 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 80 "unconnected-(J1-Pad12)") (pinfunction "ID1/SDA") (pintype "input+no_connect"))
    (pad "13" thru_hole circle locked (at -0.255 2.54 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 72 "Net-(J1-Pad13)") (pinfunction "HSYNC") (pintype "input"))
    (pad "14" thru_hole circle locked (at -2.545 2.54 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 71 "Net-(J1-Pad14)") (pinfunction "VSYNC") (pintype "input"))
    (pad "15" thru_hole circle locked (at -4.835 2.54 90) (size 2 2) (drill 1.24) (layers *.Cu *.Mask)
      (net 81 "unconnected-(J1-Pad15)") (pinfunction "ID3/SCL") (pintype "input+no_connect"))
  )
  (footprint "Pin_Headers:Pin_Header_Angled_1x18_Pitch2.54mm" (layer "F.Cu")
    (tedit 59D30B88)
    (at 122.61 154.51 -90)
    (descr "Through hole angled pin header, 1x18, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x18 2.54mm single row")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P1" (at 4.385 -2.27 -90) (layer "F.SilkS"))
    (fp_text value "CONN_01X18" (at 4.385 45.45 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 21.59) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad1)") (pinfunction "P1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "unconnected-(P1-Pad2)") (pinfunction "P2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval locked (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "unconnected-(P1-Pad3)") (pinfunction "P3") (pintype "passive+no_connect"))
    (pad "5" thru_hole oval locked (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "P5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad6)") (pinfunction "P6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad7)") (pinfunction "P7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(P1-Pad8)") (pinfunction "P8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad9)") (pinfunction "P9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad10)") (pinfunction "P10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad11)") (pinfunction "P11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad12)") (pinfunction "P12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(P1-Pad13)") (pinfunction "P13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P1-Pad14)") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole oval locked (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "P15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(P1-Pad16)") (pinfunction "P16") (pintype "passive"))
    (pad "17" thru_hole oval locked (at 0 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(P1-Pad17)") (pinfunction "P17") (pintype "passive"))
    (pad "18" thru_hole oval locked (at 0 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "unconnected-(P1-Pad18)") (pinfunction "P18") (pintype "passive+no_connect"))
    (model "${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x18_Pitch2.54mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 59D30E85)
    (at 127.57 145.53 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 5.08 -2.31 90) (layer "F.Fab"))
    (fp_text value "10k" (at 5.08 2.31 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R1-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 59D30DCC)
    (at 171.2 130.94 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 5.08 -2.31 180) (layer "F.Fab"))
    (fp_text value "1k" (at 5.08 2.31 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 59D30DE3)
    (at 171.32 134.49 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 5.08 -2.31 180) (layer "F.Fab"))
    (fp_text value "1k" (at 5.2 0.23 180) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5874F706)
    (at 171.32 138.05 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 5.08 -2.31 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 5.08 2.31 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 59D30DB0)
    (at 157.49 123.82 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R5" (at 5.08 -2.31 -90) (layer "F.SilkS"))
    (fp_text value "820 OHM" (at 5.08 -0.11 -90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 59D30C22)
    (at 60.07 135.26)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS32" (at 3.81 17.57) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "unconnected-(U1-Pad1)") (pintype "input+no_connect"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 "unconnected-(U1-Pad2)") (pintype "input+no_connect"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "unconnected-(U1-Pad3)") (pintype "output+no_connect"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(P1-Pad17)") (pintype "input"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(P1-Pad14)") (pintype "input"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(U5-Pad10)") (pintype "output"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(U5-Pad9)") (pintype "output"))
    (pad "9" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(P1-Pad16)") (pintype "input"))
    (pad "10" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(P1-Pad14)") (pintype "input"))
    (pad "11" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(U11-Pad22)") (pintype "output"))
    (pad "12" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U5-Pad6)") (pintype "input"))
    (pad "13" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U3-Pad13)") (pintype "input"))
    (pad "14" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 59D30EE2)
    (at 129.91 89.13)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS04" (at 3.81 17.57) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "unconnected-(U2-Pad1)") (pintype "input+no_connect"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 "unconnected-(U2-Pad2)") (pintype "output+no_connect"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/VS") (pintype "input"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(J1-Pad14)") (pintype "output"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "/HS") (pintype "input"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(J1-Pad13)") (pintype "output"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(U13-Pad1)") (pintype "output"))
    (pad "9" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "/BLANK") (pintype "input"))
    (pad "10" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "unconnected-(U2-Pad10)") (pintype "output+no_connect"))
    (pad "11" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 "unconnected-(U2-Pad11)") (pintype "input+no_connect"))
    (pad "12" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(U10-Pad7)") (pintype "output"))
    (pad "13" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U5-Pad6)") (pintype "input"))
    (pad "14" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 59D30EE7)
    (at 145.24 88.85)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "7400" (at 3.81 17.57) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 "unconnected-(U3-Pad1)") (pintype "input+no_connect"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 "unconnected-(U3-Pad2)") (pintype "input+no_connect"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 "unconnected-(U3-Pad3)") (pintype "output+no_connect"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U5-Pad1)") (pintype "input"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U5-Pad2)") (pintype "input"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(U3-Pad6)") (pintype "output"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U13-Pad9)") (pintype "output"))
    (pad "9" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(U4-Pad9)") (pintype "input"))
    (pad "10" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(U3-Pad6)") (pintype "input"))
    (pad "11" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U11-Pad27)") (pintype "output"))
    (pad "12" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U5-Pad1)") (pintype "input"))
    (pad "13" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U3-Pad13)") (pintype "input"))
    (pad "14" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 59D30F0F)
    (at 57.36 98.32)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS74" (at 3.81 17.57) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "~{R}") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U4-Pad2)") (pinfunction "D") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U13-Pad10)") (pinfunction "C") (pintype "input"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "~{S}") (pintype "input"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U5-Pad1)") (pinfunction "Q") (pintype "output"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U4-Pad2)") (pinfunction "~{Q}") (pintype "output"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U4-Pad12)") (pinfunction "~{Q}") (pintype "output"))
    (pad "9" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(U4-Pad9)") (pinfunction "Q") (pintype "output"))
    (pad "10" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "~{S}") (pintype "input"))
    (pad "11" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U5-Pad1)") (pinfunction "C") (pintype "input"))
    (pad "12" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U4-Pad12)") (pinfunction "D") (pintype "input"))
    (pad "13" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(U10-Pad7)") (pinfunction "~{R}") (pintype "input"))
    (pad "14" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-40_W15.24mm" (layer "F.Cu")
    (tedit 59D30E8E)
    (at 123.14 133.1 -90)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at 7.62 -2.33 -90) (layer "F.Fab"))
    (fp_text value "uPD7220" (at 7.62 50.59 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 7.62 24.13 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U5-Pad1)") (pinfunction "CKx2") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U5-Pad2)") (pinfunction "!DBIN") (pintype "output"))
    (pad "3" thru_hole oval locked (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "/HS") (pinfunction "HSYNC") (pintype "output"))
    (pad "4" thru_hole oval locked (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/VS") (pinfunction "VSYNC") (pintype "output"))
    (pad "5" thru_hole oval locked (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "/BLANK") (pinfunction "BLANK") (pintype "output"))
    (pad "6" thru_hole oval locked (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U5-Pad6)") (pinfunction "ALE") (pintype "output"))
    (pad "7" thru_hole oval locked (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "unconnected-(U5-Pad7)") (pinfunction "DRQ") (pintype "output+no_connect"))
    (pad "8" thru_hole oval locked (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R1-Pad2)") (pinfunction "DACK") (pintype "input"))
    (pad "9" thru_hole oval locked (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(U5-Pad9)") (pinfunction "!RD") (pintype "input"))
    (pad "10" thru_hole oval locked (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(U5-Pad10)") (pinfunction "!WE") (pintype "input"))
    (pad "11" thru_hole oval locked (at 0 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad1)") (pinfunction "iA0") (pintype "input"))
    (pad "12" thru_hole oval locked (at 0 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad6)") (pinfunction "DB0") (pintype "bidirectional"))
    (pad "13" thru_hole oval locked (at 0 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad7)") (pinfunction "DB1") (pintype "bidirectional"))
    (pad "14" thru_hole oval locked (at 0 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(P1-Pad8)") (pinfunction "DB2") (pintype "bidirectional"))
    (pad "15" thru_hole oval locked (at 0 35.56 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad9)") (pinfunction "DB3") (pintype "bidirectional"))
    (pad "16" thru_hole oval locked (at 0 38.1 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad10)") (pinfunction "DB4") (pintype "bidirectional"))
    (pad "17" thru_hole oval locked (at 0 40.64 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad11)") (pinfunction "DB5") (pintype "bidirectional"))
    (pad "18" thru_hole oval locked (at 0 43.18 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad12)") (pinfunction "DB6") (pintype "bidirectional"))
    (pad "19" thru_hole oval locked (at 0 45.72 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(P1-Pad13)") (pinfunction "DB7") (pintype "bidirectional"))
    (pad "20" thru_hole oval locked (at 0 48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "21" thru_hole oval locked (at 15.24 48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 "unconnected-(U5-Pad21)") (pinfunction "LPEN") (pintype "unspecified+no_connect"))
    (pad "22" thru_hole oval locked (at 15.24 45.72 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "/AD0") (pinfunction "AD0") (pintype "bidirectional"))
    (pad "23" thru_hole oval locked (at 15.24 43.18 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "/AD1") (pinfunction "AD1") (pintype "bidirectional"))
    (pad "24" thru_hole oval locked (at 15.24 40.64 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "/AD2") (pinfunction "AD2") (pintype "bidirectional"))
    (pad "25" thru_hole oval locked (at 15.24 38.1 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "/AD3") (pinfunction "AD3") (pintype "bidirectional"))
    (pad "26" thru_hole oval locked (at 15.24 35.56 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "/AD4") (pinfunction "AD4") (pintype "bidirectional"))
    (pad "27" thru_hole oval locked (at 15.24 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "/AD5") (pinfunction "AD5") (pintype "bidirectional"))
    (pad "28" thru_hole oval locked (at 15.24 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "/AD6") (pinfunction "AD6") (pintype "bidirectional"))
    (pad "29" thru_hole oval locked (at 15.24 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "/AD7") (pinfunction "AD7") (pintype "bidirectional"))
    (pad "30" thru_hole oval locked (at 15.24 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/AD8") (pinfunction "AD8") (pintype "bidirectional"))
    (pad "31" thru_hole oval locked (at 15.24 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "/AD9") (pinfunction "AD9") (pintype "bidirectional"))
    (pad "32" thru_hole oval locked (at 15.24 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "/AD10") (pinfunction "AD10") (pintype "bidirectional"))
    (pad "33" thru_hole oval locked (at 15.24 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "/AD11") (pinfunction "AD11") (pintype "bidirectional"))
    (pad "34" thru_hole oval locked (at 15.24 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "/AD12") (pinfunction "AD12") (pintype "bidirectional"))
    (pad "35" thru_hole oval locked (at 15.24 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "/AD13") (pinfunction "AD13") (pintype "bidirectional"))
    (pad "36" thru_hole oval locked (at 15.24 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "/AD14") (pinfunction "AD14") (pintype "bidirectional"))
    (pad "37" thru_hole oval locked (at 15.24 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "/AD15") (pinfunction "AD15") (pintype "bidirectional"))
    (pad "38" thru_hole oval locked (at 15.24 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 "unconnected-(U5-Pad38)") (pinfunction "A16") (pintype "output+no_connect"))
    (pad "39" thru_hole oval locked (at 15.24 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 "unconnected-(U5-Pad39)") (pinfunction "A17") (pintype "output+no_connect"))
    (pad "40" thru_hole oval locked (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "+5V") (pintype "power_in"))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-40_W15.24mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 59D30F1A)
    (at 45.49 98.35)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U6" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS74" (at 3.81 17.57) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "~{R}") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U5-Pad2)") (pinfunction "D") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U5-Pad1)") (pinfunction "C") (pintype "input"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "~{S}") (pintype "input"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(U6-Pad12)") (pinfunction "Q") (pintype "output"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 "unconnected-(U6-Pad6)") (pinfunction "~{Q}") (pintype "output+no_connect"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "8" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U3-Pad13)") (pinfunction "~{Q}") (pintype "output"))
    (pad "9" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 "unconnected-(U6-Pad9)") (pinfunction "Q") (pintype "output+no_connect"))
    (pad "10" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "~{S}") (pintype "input"))
    (pad "11" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U5-Pad1)") (pinfunction "C") (pintype "input"))
    (pad "12" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(U6-Pad12)") (pinfunction "D") (pintype "input"))
    (pad "13" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "~{R}") (pintype "input"))
    (pad "14" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (tedit 59D30F25)
    (at 68.12 107.28)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U7" (at 3.81 -2.33) (layer "F.Fab"))
    (fp_text value "74LS173" (at 3.81 20.11) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "Oe1") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "Oe2") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "/A0") (pinfunction "Q0") (pintype "tri_state"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "/A1") (pinfunction "Q1") (pintype "tri_state"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "/A2") (pinfunction "Q2") (pintype "tri_state"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "/A3") (pinfunction "Q3") (pintype "tri_state"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(U10-Pad7)") (pinfunction "Cp") (pintype "input"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval locked (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "E1") (pintype "input"))
    (pad "10" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "E2") (pintype "input"))
    (pad "11" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "/AD3") (pinfunction "D3") (pintype "input"))
    (pad "12" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "/AD2") (pinfunction "D2") (pintype "input"))
    (pad "13" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "/AD1") (pinfunction "D1") (pintype "input"))
    (pad "14" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "/AD0") (pinfunction "D0") (pintype "input"))
    (pad "15" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "Mr") (pintype "input"))
    (pad "16" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (tedit 59D30EFE)
    (at 68.32 85.26)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U8" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS173" (at 3.81 20.11) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "Oe1") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "Oe2") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "/A4") (pinfunction "Q0") (pintype "tri_state"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "/A5") (pinfunction "Q1") (pintype "tri_state"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "/A6") (pinfunction "Q2") (pintype "tri_state"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "/A7") (pinfunction "Q3") (pintype "tri_state"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(U10-Pad7)") (pinfunction "Cp") (pintype "input"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval locked (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "E1") (pintype "input"))
    (pad "10" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "E2") (pintype "input"))
    (pad "11" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "/AD7") (pinfunction "D3") (pintype "input"))
    (pad "12" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "/AD6") (pinfunction "D2") (pintype "input"))
    (pad "13" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "/AD5") (pinfunction "D1") (pintype "input"))
    (pad "14" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "/AD4") (pinfunction "D0") (pintype "input"))
    (pad "15" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "Mr") (pintype "input"))
    (pad "16" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (tedit 59D30EF8)
    (at 78.88 85.37)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U9" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS173" (at 3.81 20.11) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "Oe1") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "Oe2") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "/A8") (pinfunction "Q0") (pintype "tri_state"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "/A9") (pinfunction "Q1") (pintype "tri_state"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "/A10") (pinfunction "Q2") (pintype "tri_state"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "/A11") (pinfunction "Q3") (pintype "tri_state"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(U10-Pad7)") (pinfunction "Cp") (pintype "input"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval locked (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "E1") (pintype "input"))
    (pad "10" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "E2") (pintype "input"))
    (pad "11" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "/AD11") (pinfunction "D3") (pintype "input"))
    (pad "12" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "/AD10") (pinfunction "D2") (pintype "input"))
    (pad "13" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "/AD9") (pinfunction "D1") (pintype "input"))
    (pad "14" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/AD8") (pinfunction "D0") (pintype "input"))
    (pad "15" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "Mr") (pintype "input"))
    (pad "16" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (tedit 59D30F2C)
    (at 79.37 107.79)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U10" (at 3.81 -2.33) (layer "F.Fab"))
    (fp_text value "74LS173" (at 3.81 20.11) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "Oe1") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "Oe2") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "/A12") (pinfunction "Q0") (pintype "tri_state"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "/A13") (pinfunction "Q1") (pintype "tri_state"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "/A14") (pinfunction "Q2") (pintype "tri_state"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 "/A15") (pinfunction "Q3") (pintype "tri_state+no_connect"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(U10-Pad7)") (pinfunction "Cp") (pintype "input"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval locked (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "E1") (pintype "input"))
    (pad "10" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "E2") (pintype "input"))
    (pad "11" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "/AD15") (pinfunction "D3") (pintype "input"))
    (pad "12" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "/AD14") (pinfunction "D2") (pintype "input"))
    (pad "13" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "/AD13") (pinfunction "D1") (pintype "input"))
    (pad "14" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "/AD12") (pinfunction "D0") (pintype "input"))
    (pad "15" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "Mr") (pintype "input"))
    (pad "16" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-28_W7.62mm" (layer "F.Cu")
    (tedit 59D30EDB)
    (at 115.19 93.35)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U11" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "RAM32KiB" (at 3.81 35.35) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 16.51) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "/A14") (pinfunction "A14") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "/A12") (pinfunction "A12") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "/A7") (pinfunction "A7") (pintype "input"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "/A6") (pinfunction "A6") (pintype "input"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "/A5") (pinfunction "A5") (pintype "input"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "/A4") (pinfunction "A4") (pintype "input"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "/A3") (pinfunction "A3") (pintype "input"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "/A2") (pinfunction "A2") (pintype "input"))
    (pad "9" thru_hole oval locked (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "/A1") (pinfunction "A1") (pintype "input"))
    (pad "10" thru_hole oval locked (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "/A0") (pinfunction "A0") (pintype "input"))
    (pad "11" thru_hole oval locked (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "/AD0") (pinfunction "D0") (pintype "tri_state"))
    (pad "12" thru_hole oval locked (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "/AD1") (pinfunction "D1") (pintype "tri_state"))
    (pad "13" thru_hole oval locked (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "/AD2") (pinfunction "D2") (pintype "tri_state"))
    (pad "14" thru_hole oval locked (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "15" thru_hole oval locked (at 7.62 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "/AD3") (pinfunction "D3") (pintype "tri_state"))
    (pad "16" thru_hole oval locked (at 7.62 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "/AD4") (pinfunction "D4") (pintype "tri_state"))
    (pad "17" thru_hole oval locked (at 7.62 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "/AD5") (pinfunction "D5") (pintype "tri_state"))
    (pad "18" thru_hole oval locked (at 7.62 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "/AD6") (pinfunction "D6") (pintype "tri_state"))
    (pad "19" thru_hole oval locked (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "/AD7") (pinfunction "D7") (pintype "tri_state"))
    (pad "20" thru_hole oval locked (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "CS") (pintype "input"))
    (pad "21" thru_hole oval locked (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "/A10") (pinfunction "A10") (pintype "input"))
    (pad "22" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(U11-Pad22)") (pinfunction "OE") (pintype "input"))
    (pad "23" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "/A11") (pinfunction "A11") (pintype "input"))
    (pad "24" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "/A9") (pinfunction "A9") (pintype "input"))
    (pad "25" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "/A8") (pinfunction "A8") (pintype "input"))
    (pad "26" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "/A13") (pinfunction "A13") (pintype "input"))
    (pad "27" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U11-Pad27)") (pinfunction "WE") (pintype "input"))
    (pad "28" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-28_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-28_W7.62mm" (layer "F.Cu")
    (tedit 59D30E53)
    (at 97.59 93.1)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U12" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "RAM32KiB" (at 3.81 35.35) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 16.51) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "/A14") (pinfunction "A14") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "/A12") (pinfunction "A12") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "/A7") (pinfunction "A7") (pintype "input"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "/A6") (pinfunction "A6") (pintype "input"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "/A5") (pinfunction "A5") (pintype "input"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "/A4") (pinfunction "A4") (pintype "input"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "/A3") (pinfunction "A3") (pintype "input"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "/A2") (pinfunction "A2") (pintype "input"))
    (pad "9" thru_hole oval locked (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "/A1") (pinfunction "A1") (pintype "input"))
    (pad "10" thru_hole oval locked (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "/A0") (pinfunction "A0") (pintype "input"))
    (pad "11" thru_hole oval locked (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/AD8") (pinfunction "D0") (pintype "tri_state"))
    (pad "12" thru_hole oval locked (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "/AD9") (pinfunction "D1") (pintype "tri_state"))
    (pad "13" thru_hole oval locked (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "/AD10") (pinfunction "D2") (pintype "tri_state"))
    (pad "14" thru_hole oval locked (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "15" thru_hole oval locked (at 7.62 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "/AD11") (pinfunction "D3") (pintype "tri_state"))
    (pad "16" thru_hole oval locked (at 7.62 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "/AD12") (pinfunction "D4") (pintype "tri_state"))
    (pad "17" thru_hole oval locked (at 7.62 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "/AD13") (pinfunction "D5") (pintype "tri_state"))
    (pad "18" thru_hole oval locked (at 7.62 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "/AD14") (pinfunction "D6") (pintype "tri_state"))
    (pad "19" thru_hole oval locked (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "/AD15") (pinfunction "D7") (pintype "tri_state"))
    (pad "20" thru_hole oval locked (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "CS") (pintype "input"))
    (pad "21" thru_hole oval locked (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "/A10") (pinfunction "A10") (pintype "input"))
    (pad "22" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(U11-Pad22)") (pinfunction "OE") (pintype "input"))
    (pad "23" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "/A11") (pinfunction "A11") (pintype "input"))
    (pad "24" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "/A9") (pinfunction "A9") (pintype "input"))
    (pad "25" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "/A8") (pinfunction "A8") (pintype "input"))
    (pad "26" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "/A13") (pinfunction "A13") (pintype "input"))
    (pad "27" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U11-Pad27)") (pinfunction "WE") (pintype "input"))
    (pad "28" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-28_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (tedit 59D30EA7)
    (at 146.09 110.41)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U13" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS195" (at 3.81 20.11) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(U13-Pad1)") (pinfunction "Mr") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "J") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "~{K}") (pintype "input"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "/AD0") (pinfunction "P0") (pintype "input"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "/AD1") (pinfunction "P1") (pintype "input"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "/AD2") (pinfunction "P2") (pintype "input"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "/AD3") (pinfunction "P3") (pintype "input"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval locked (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U13-Pad9)") (pinfunction "Pe") (pintype "input"))
    (pad "10" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U13-Pad10)") (pinfunction "Cp") (pintype "input"))
    (pad "11" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 "unconnected-(U13-Pad11)") (pinfunction "~{Q3}") (pintype "output+no_connect"))
    (pad "12" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R2-Pad2)") (pinfunction "Q3") (pintype "output"))
    (pad "13" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 "unconnected-(U13-Pad13)") (pinfunction "Q2") (pintype "output+no_connect"))
    (pad "14" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "unconnected-(U13-Pad14)") (pinfunction "Q1") (pintype "output+no_connect"))
    (pad "15" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 "unconnected-(U13-Pad15)") (pinfunction "Q0") (pintype "output+no_connect"))
    (pad "16" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (tedit 59D30EAD)
    (at 132.23 110.47)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U14" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS195" (at 3.81 20.11) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(U13-Pad1)") (pinfunction "Mr") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "J") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "~{K}") (pintype "input"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "/AD4") (pinfunction "P0") (pintype "input"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "/AD5") (pinfunction "P1") (pintype "input"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "/AD6") (pinfunction "P2") (pintype "input"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "/AD7") (pinfunction "P3") (pintype "input"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval locked (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U13-Pad9)") (pinfunction "Pe") (pintype "input"))
    (pad "10" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U13-Pad10)") (pinfunction "Cp") (pintype "input"))
    (pad "11" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 "unconnected-(U14-Pad11)") (pinfunction "~{Q3}") (pintype "output+no_connect"))
    (pad "12" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R3-Pad2)") (pinfunction "Q3") (pintype "output"))
    (pad "13" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 "unconnected-(U14-Pad13)") (pinfunction "Q2") (pintype "output+no_connect"))
    (pad "14" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 "unconnected-(U14-Pad14)") (pinfunction "Q1") (pintype "output+no_connect"))
    (pad "15" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 "unconnected-(U14-Pad15)") (pinfunction "Q0") (pintype "output+no_connect"))
    (pad "16" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (tedit 59D30E96)
    (at 132.13 134.66)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U15" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS195" (at 3.81 20.11) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(U13-Pad1)") (pinfunction "Mr") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "J") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "~{K}") (pintype "input"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/AD8") (pinfunction "P0") (pintype "input"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "/AD9") (pinfunction "P1") (pintype "input"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "/AD10") (pinfunction "P2") (pintype "input"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "/AD11") (pinfunction "P3") (pintype "input"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval locked (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U13-Pad9)") (pinfunction "Pe") (pintype "input"))
    (pad "10" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U13-Pad10)") (pinfunction "Cp") (pintype "input"))
    (pad "11" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "unconnected-(U15-Pad11)") (pinfunction "~{Q3}") (pintype "output+no_connect"))
    (pad "12" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R4-Pad2)") (pinfunction "Q3") (pintype "output"))
    (pad "13" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "unconnected-(U15-Pad13)") (pinfunction "Q2") (pintype "output+no_connect"))
    (pad "14" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "unconnected-(U15-Pad14)") (pinfunction "Q1") (pintype "output+no_connect"))
    (pad "15" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 "unconnected-(U15-Pad15)") (pinfunction "Q0") (pintype "output+no_connect"))
    (pad "16" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Housings_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (tedit 59D30E9E)
    (at 146.1 134.38)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "updgfx_r0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U16" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "74LS195" (at 3.81 20.11) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(U13-Pad1)") (pinfunction "Mr") (pintype "input"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "J") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "~{K}") (pintype "input"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "/AD12") (pinfunction "P0") (pintype "input"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "/AD13") (pinfunction "P1") (pintype "input"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "/AD14") (pinfunction "P2") (pintype "input"))
    (pad "7" thru_hole oval locked (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "/AD15") (pinfunction "P3") (pintype "input"))
    (pad "8" thru_hole oval locked (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval locked (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U13-Pad9)") (pinfunction "Pe") (pintype "input"))
    (pad "10" thru_hole oval locked (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U13-Pad10)") (pinfunction "Cp") (pintype "input"))
    (pad "11" thru_hole oval locked (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 "unconnected-(U16-Pad11)") (pinfunction "~{Q3}") (pintype "output+no_connect"))
    (pad "12" thru_hole oval locked (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R5-Pad2)") (pinfunction "Q3") (pintype "output"))
    (pad "13" thru_hole oval locked (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 "unconnected-(U16-Pad13)") (pinfunction "Q2") (pintype "output+no_connect"))
    (pad "14" thru_hole oval locked (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 "unconnected-(U16-Pad14)") (pinfunction "Q1") (pintype "output+no_connect"))
    (pad "15" thru_hole oval locked (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "unconnected-(U16-Pad15)") (pinfunction "Q0") (pintype "output+no_connect"))
    (pad "16" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Oscillators:Oscillator_DIP-8" (layer "F.Cu")
    (tedit 5C9971DC)
    (at 50.7 130.18)
    (descr "Oscillator, DIP8,http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf")
    (tags "oscillator")
    (attr through_hole)
    (fp_text reference "X1" (at 3.81 -11.26) (layer "F.SilkS"))
    (fp_text value "IQXO/7X" (at 3.81 3.74) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 -3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "2" thru_hole circle locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "GND"))
    (pad "3" thru_hole circle locked (at 7.62 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U13-Pad10)"))
    (pad "4" thru_hole circle locked (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+5V"))
    (model "${KISYS3DMOD}/Oscillators.3dshapes/Oscillator_DIP-8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 42.545 80.28) (end 173.99 80.28) (layer "Edge.Cuts") (width 0.0254))
  (gr_line (start 42.5704 80.264) (end 42.5704 80.2894) (layer "Edge.Cuts") (width 0.0254))
  (gr_line (start 173.99 160.655) (end 42.545 160.655) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 173.99 81.28) (end 173.99 160.655) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 42.545 160.655) (end 42.545 81.28) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 42.5704 81.2546) (end 42.5704 80.264) (layer "Edge.Cuts") (width 0.0254))
  (gr_line (start 173.99 81.28) (end 173.99 80.264) (layer "Edge.Cuts") (width 0.0254))
  (gr_text "NUCLAER TECH\nuPD7220 GRAPHICS CARD\nV2.0 SHOULD WORK\nFOR USE WITH Z80 MOBO\n" (at 54.61 88.9) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Eco2.User")
    (pts (xy 38.735 160.655) (xy 38.735 81.28))
    (height -1.27)
    (gr_text "79.3750 mm" (at 35.665 120.9675 90) (layer "Eco2.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Eco2.User")
    (pts (xy 42.545 79.375) (xy 173.99 79.375))
    (height -0.635)
    (gr_text "131.4450 mm" (at 108.2675 76.94) (layer "Eco2.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "F.Fab")
    (pts (xy 31.75 81.28) (xy 31.75 160.655))
    (height -1.905)
    (gr_text "79.3750 mm" (at 31.855 120.9675 90) (layer "F.Fab"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "F.Fab")
    (pts (xy 173.99 73.66) (xy 42.545 73.66))
    (height 1.905)
    (gr_text "131.4450 mm" (at 108.2675 69.955) (layer "F.Fab"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (zone (net 7) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.355 160.02)
        (xy 43.18 160.02)
        (xy 43.18 80.7466)
        (xy 173.355 80.7466)
      )
    )
  )
  (zone (net 7) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.355 160.02)
        (xy 43.18 160.02)
        (xy 43.18 80.7466)
        (xy 173.355 80.7466)
      )
    )
  )
)
