(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 1401)
    (zones 0)
    (modules 51)
    (nets 58)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +2V8)
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C4-Pad2)")
  (net 6 "Net-(D1-Pad2)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(D3-Pad2)")
  (net 9 "Net-(D4-Pad2)")
  (net 10 "Net-(D5-Pad2)")
  (net 11 "Net-(D6-Pad2)")
  (net 12 "Net-(D7-Pad2)")
  (net 13 "Net-(D8-Pad2)")
  (net 14 "Net-(D9-Pad2)")
  (net 15 "Net-(D10-Pad2)")
  (net 16 "Net-(D11-Pad2)")
  (net 17 "Net-(D12-Pad2)")
  (net 18 "Net-(D13-Pad2)")
  (net 19 "Net-(D14-Pad2)")
  (net 20 "Net-(D15-Pad2)")
  (net 21 "Net-(D16-Pad2)")
  (net 22 "Net-(POT1-Pad3)")
  (net 23 "Net-(POT1-Pad1)")
  (net 24 "Net-(R1-Pad1)")
  (net 25 "Net-(R2-Pad1)")
  (net 26 "Net-(R3-Pad1)")
  (net 27 "Net-(R4-Pad1)")
  (net 28 "Net-(R5-Pad1)")
  (net 29 "Net-(R6-Pad1)")
  (net 30 "Net-(R7-Pad1)")
  (net 31 "Net-(R8-Pad1)")
  (net 32 "Net-(R9-Pad1)")
  (net 33 "Net-(R10-Pad1)")
  (net 34 "Net-(R11-Pad1)")
  (net 35 "Net-(R12-Pad1)")
  (net 36 "Net-(R13-Pad1)")
  (net 37 "Net-(R14-Pad1)")
  (net 38 "Net-(R15-Pad1)")
  (net 39 "Net-(R16-Pad1)")
  (net 40 "Net-(R17-Pad2)")
  (net 41 "Net-(R19-Pad2)")
  (net 42 "Net-(U1-Pad8)")
  (net 43 "Net-(U1-Pad5)")
  (net 44 "Net-(U3-Pad11)")
  (net 45 "Net-(U3-Pad12)")
  (net 46 "Net-(U3-Pad13)")
  (net 47 "Net-(U3-Pad14)")
  (net 48 "Net-(U3-Pad2)")
  (net 49 "Net-(U3-Pad15)")
  (net 50 "Net-(U4-Pad4)")
  (net 51 "Net-(U4-Pad1)")
  (net 52 "Net-(U7-Pad13)")
  (net 53 "Net-(U7-Pad11)")
  (net 54 "Net-(U7-Pad9)")
  (net 55 "Net-(U7-Pad6)")
  (net 56 "Net-(U7-Pad4)")
  (net 57 "Net-(U7-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +2V8)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(POT1-Pad1)")
    (add_net "Net-(POT1-Pad3)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U7-Pad11)")
    (add_net "Net-(U7-Pad13)")
    (add_net "Net-(U7-Pad2)")
    (add_net "Net-(U7-Pad4)")
    (add_net "Net-(U7-Pad6)")
    (add_net "Net-(U7-Pad9)")
  )
  (module Package_SO:TSSOP-14_4.4x5mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 144.2 62.6)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U7 (at 0 -3.55) (layer F.SilkS))
    (fp_text value TLC555CPW (at 0 3.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 14 smd rect (at 2.95 -1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
    (pad 13 smd rect (at 2.95 -1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U7-Pad13)"))
    (pad 12 smd rect (at 2.95 -0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R19-Pad2)"))
    (pad 11 smd rect (at 2.95 0) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U7-Pad11)"))
    (pad 10 smd rect (at 2.95 0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 9 smd rect (at 2.95 1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U7-Pad9)"))
    (pad 8 smd rect (at 2.95 1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 7 smd rect (at -2.95 1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
    (pad 6 smd rect (at -2.95 1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U7-Pad6)"))
    (pad 5 smd rect (at -2.95 0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U3-Pad2)"))
    (pad 4 smd rect (at -2.95 0) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U7-Pad4)"))
    (pad 3 smd rect (at -2.95 -0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at -2.95 -1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U7-Pad2)"))
    (pad 1 smd rect (at -2.95 -1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module led_coaster:74HC238D (layer F.Cu) (tedit 0)
    (at 175.8 102 270)
    (attr smd)
    (fp_text reference U6 (at -6.245 0) (layer F.SilkS))
    (fp_text value 74HC238 (at 0 0 270) (layer F.Fab))
    (pad 8 smd rect (at 4.445 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 4.445 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R15-Pad1)"))
    (pad 7 smd rect (at 3.175 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R16-Pad1)"))
    (pad 10 smd rect (at 3.175 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R14-Pad1)"))
    (pad 6 smd rect (at 1.905 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U3-Pad11)"))
    (pad 11 smd rect (at 1.905 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R13-Pad1)"))
    (pad 5 smd rect (at 0.635 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 0.635 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R12-Pad1)"))
    (pad 4 smd rect (at -0.635 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -0.635 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R11-Pad1)"))
    (pad 3 smd rect (at -1.905 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U3-Pad12)"))
    (pad 14 smd rect (at -1.905 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at -3.175 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U3-Pad13)"))
    (pad 15 smd rect (at -3.175 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R9-Pad1)"))
    (pad 1 smd rect (at -4.445 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U3-Pad14)"))
    (pad 16 smd rect (at -4.445 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
  )
  (module led_coaster:74HC238D (layer F.Cu) (tedit 0)
    (at 176 83.2 270)
    (attr smd)
    (fp_text reference U5 (at -6.245 0) (layer F.SilkS))
    (fp_text value 74HC238 (at 0 0 270) (layer F.Fab))
    (pad 8 smd rect (at 4.445 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 4.445 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R7-Pad1)"))
    (pad 7 smd rect (at 3.175 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R8-Pad1)"))
    (pad 10 smd rect (at 3.175 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R6-Pad1)"))
    (pad 6 smd rect (at 1.905 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U4-Pad4)"))
    (pad 11 smd rect (at 1.905 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R5-Pad1)"))
    (pad 5 smd rect (at 0.635 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 0.635 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R4-Pad1)"))
    (pad 4 smd rect (at -0.635 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -0.635 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R3-Pad1)"))
    (pad 3 smd rect (at -1.905 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U3-Pad12)"))
    (pad 14 smd rect (at -1.905 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at -3.175 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U3-Pad13)"))
    (pad 15 smd rect (at -3.175 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R1-Pad1)"))
    (pad 1 smd rect (at -4.445 3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U3-Pad14)"))
    (pad 16 smd rect (at -4.445 -3 270) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
  )
  (module Package_TO_SOT_SMD:SOT-553 (layer F.Cu) (tedit 5A02FF57)
    (at 165.6 75.8 90)
    (descr SOT553)
    (tags SOT-553)
    (attr smd)
    (fp_text reference U4 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 74LVC1GU04DRL (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 4 smd rect (at 0.7 0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U4-Pad4)"))
    (pad 2 smd rect (at -0.7 0 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U3-Pad11)"))
    (pad 5 smd rect (at 0.7 -0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
    (pad 3 smd rect (at -0.7 0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7 -0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U4-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-553.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module led_coaster:SN74HC163DR (layer F.Cu) (tedit 0)
    (at 159 65.4 270)
    (attr smd)
    (fp_text reference U3 (at -6.22 0) (layer F.SilkS))
    (fp_text value SN74HC163 (at 0.125 0 270) (layer F.Fab))
    (pad 8 smd rect (at 4.445 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 4.445 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
    (pad 7 smd rect (at 3.175 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
    (pad 10 smd rect (at 3.175 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
    (pad 6 smd rect (at 1.905 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 1.905 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U3-Pad11)"))
    (pad 5 smd rect (at 0.635 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 0.635 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U3-Pad12)"))
    (pad 4 smd rect (at -0.635 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -0.635 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U3-Pad13)"))
    (pad 3 smd rect (at -1.905 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -1.905 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U3-Pad14)"))
    (pad 2 smd rect (at -3.175 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U3-Pad2)"))
    (pad 15 smd rect (at -3.175 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U3-Pad15)"))
    (pad 1 smd rect (at -4.445 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
    (pad 16 smd rect (at -4.445 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 115.4 115)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -3.5) (layer F.SilkS))
    (fp_text value LM317L_SO8 (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad8)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R17-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module led_coaster:supercap (layer F.Cu) (tedit 5CEB6920)
    (at 143.2 132.4)
    (attr smd)
    (fp_text reference SC3 (at 20 -0.2) (layer F.SilkS))
    (fp_text value 15F (at 0 -3.1) (layer F.Fab))
    (fp_text user + (at -17 -11.4) (layer F.SilkS))
    (pad 2 smd rect (at 14 0) (size 4 3.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -14 0) (size 4 3.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
  )
  (module led_coaster:supercap (layer F.Cu) (tedit 5CEB6920)
    (at 143.2 127.6)
    (attr smd)
    (fp_text reference SC2 (at 20 0) (layer F.SilkS))
    (fp_text value 15F (at 0 -3.1) (layer F.Fab))
    (fp_text user + (at -17 3) (layer F.SilkS))
    (pad 2 smd rect (at 14 0) (size 4 3.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -14 0) (size 4 3.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
  )
  (module led_coaster:supercap (layer F.Cu) (tedit 5CEB6920)
    (at 143.2 122.8)
    (attr smd)
    (fp_text reference SC1 (at 20 -0.2) (layer F.SilkS))
    (fp_text value 15F (at 0 -3.1) (layer F.Fab))
    (fp_text user + (at -17 3) (layer F.SilkS))
    (pad 2 smd rect (at 14 0) (size 4 3.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -14 0) (size 4 3.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +2V8))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 143.8 55.8 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0 -1.82 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 23 "Net-(POT1-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 41 "Net-(R19-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 149.2 56.6 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 41 "Net-(R19-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 +2V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 117.8 121.4)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 680 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 40 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 111.8 121.4)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0.4 -2) (layer F.SilkS))
    (fp_text value 560 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 40 "Net-(R17-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 +2V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 132.4 51.2 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 21 "Net-(D16-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 39 "Net-(R16-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 116.6 59.4 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 20 "Net-(D15-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 38 "Net-(R15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 102.4 71.2 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 19 "Net-(D14-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 37 "Net-(R14-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 97.6 89 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 18 "Net-(D13-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 36 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 98 106 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 "Net-(D12-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 35 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 105 121.8 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 16 "Net-(D11-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 34 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.6 134.6 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 15 "Net-(D10-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 33 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 137.6 140 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 "Net-(D9-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 32 "Net-(R9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 154.4 140 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 13 "Net-(D8-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 31 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 171.4 131.2 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(D7-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 30 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 183.4 117.6 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 "Net-(D6-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 29 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 188.8 101.6 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 10 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 28 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 187 83.8 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 27 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 179.4 68 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 26 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 165.8 56.6 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 25 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 149 50.4 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 24 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module led_coaster:POT_10K (layer F.Cu) (tedit 0)
    (at 128.2 60 180)
    (fp_text reference POT1 (at 0 -4 180) (layer F.SilkS))
    (fp_text value 10k (at 0 4 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 2.5 1.25 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "Net-(POT1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -1.25 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 1 thru_hole oval (at -2.5 1.25 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(POT1-Pad1)"))
  )
  (module led_coaster:pwr (layer F.Cu) (tedit 5CEB6B06)
    (at 109.4 108.4 180)
    (fp_text reference J1 (at 0 2.75 180) (layer F.SilkS))
    (fp_text value "5V PWR INPUT" (at 0 -2.75 180) (layer F.Fab))
    (fp_text user + (at -3.56 2.56 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 +5V))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 125.208511 52.602231 25)
    (attr smd)
    (fp_text reference D16 (at 0 2.7 25) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 25) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 25) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D16-Pad2)"))
    (pad 1 smd rect (at -1.425 0 25) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 110.5 62.492373 45)
    (attr smd)
    (fp_text reference D15 (at 0 2.7 45) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 45) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 45) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at -1.425 0 45) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 100.5 77.5 70)
    (attr smd)
    (fp_text reference D14 (at 0 2.7 70) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 70) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 70) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D14-Pad2)"))
    (pad 1 smd rect (at -1.425 0 70) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 97 95.075 90)
    (attr smd)
    (fp_text reference D13 (at -2.525 2.7 90) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 90) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 90) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -1.425 0 90) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 100.512621 111.5 110)
    (attr smd)
    (fp_text reference D12 (at 0 2.7 110) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 110) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 110) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D12-Pad2)"))
    (pad 1 smd rect (at -1.425 0 110) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 109.492373 126.992373 135)
    (attr smd)
    (fp_text reference D11 (at 0 2.7 135) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 135) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 135) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -1.425 0 135) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 125.160938 137.512621 160)
    (attr smd)
    (fp_text reference D10 (at 0 2.7 160) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 160) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 160) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -1.425 0 160) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 143 141 180)
    (attr smd)
    (fp_text reference D9 (at 0 2.7 180) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 180) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 180) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D9-Pad2)"))
    (pad 1 smd rect (at -1.425 0 180) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 160.708511 137.897769 205)
    (attr smd)
    (fp_text reference D8 (at 0 2.7 205) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 205) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 205) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at -1.425 0 205) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 176.992373 126.992373 225)
    (attr smd)
    (fp_text reference D7 (at 0 2.7 225) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 225) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 225) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -1.425 0 225) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 185.987379 111.660938 250)
    (attr smd)
    (fp_text reference D6 (at 0 2.7 250) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 250) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 250) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -1.425 0 250) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 189.5 95.075 270)
    (attr smd)
    (fp_text reference D5 (at 0 2.7 270) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 270) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 270) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -1.425 0 270) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 185.512621 76.765914 290)
    (attr smd)
    (fp_text reference D4 (at -4.038875 -0.498839 290) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 290) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 290) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.425 0 290) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 175.492373 62.492373 315)
    (attr smd)
    (fp_text reference D3 (at 0 2.7 315) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 315) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 315) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.425 0 315) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 160.660938 53.012621 340)
    (attr smd)
    (fp_text reference D2 (at 0 2.7 340) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7 340) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0 340) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.425 0 340) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module led_coaster:coaster_led (layer F.Cu) (tedit 0)
    (at 142.925 49)
    (attr smd)
    (fp_text reference D1 (at 0 2.7) (layer F.SilkS))
    (fp_text value LED (at 0 -2.7) (layer F.Fab))
    (pad 2 smd rect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 136 62.2 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 "Net-(C4-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 149.2 68.4 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 "Net-(C3-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 115.6 125)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 +2V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 107.6 113.2 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.82 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "By\nScott \nClandinin" (at 170.2 116.8) (layer F.SilkS))
  (gr_text "Charging Module" (at 120 68.2 -20) (layer F.SilkS))
  (gr_circle (center 142.92 95.27) (end 166.92 95.27) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 142.92 95.27) (end 106.7 60.8) (layer Edge.Cuts) (width 0.05))
)
