(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 88)
    (no_connects 0)
    (area 44.903429 78.837 141.80181 137.163)
    (thickness 1.6)
    (drawings 21)
    (tracks 541)
    (zones 0)
    (modules 24)
    (nets 67)
  )
  (page A3)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.305)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 1.1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 49.53 135.89)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory PiPlaydrill/))
  )
  (net 0 "")
  (net 1 +3.3V)
  (net 2 +5V)
  (net 3 "/(SPI_CE0_N)GPIO08")
  (net 4 /GPIO05)
  (net 5 /GPIO06)
  (net 6 "/GPIO09(SPI_MISO)")
  (net 7 "/GPIO10(SPI_MOSI)")
  (net 8 "/GPIO11(SPI_CLK)")
  (net 9 /GPIO12)
  (net 10 /GPIO13)
  (net 11 /GPIO19)
  (net 12 /GPIO20)
  (net 13 /GPIO21)
  (net 14 GND)
  (net 15 "Net-(C1-Pad2)")
  (net 16 "Net-(C2-Pad1)")
  (net 17 "Net-(P1-Pad1)")
  (net 18 "Net-(P1-Pad2)")
  (net 19 "Net-(P1-Pad3)")
  (net 20 "Net-(P1-Pad4)")
  (net 21 "Net-(P1-Pad5)")
  (net 22 "Net-(P1-Pad6)")
  (net 23 "Net-(P1-Pad7)")
  (net 24 "Net-(P1-Pad8)")
  (net 25 "Net-(P2-Pad1)")
  (net 26 "Net-(P2-Pad2)")
  (net 27 "Net-(P2-Pad3)")
  (net 28 "Net-(P2-Pad4)")
  (net 29 "Net-(P2-Pad5)")
  (net 30 "Net-(P2-Pad6)")
  (net 31 "Net-(P2-Pad7)")
  (net 32 "Net-(P2-Pad8)")
  (net 33 "Net-(P3-Pad1)")
  (net 34 "Net-(P3-Pad2)")
  (net 35 "Net-(P3-Pad3)")
  (net 36 "Net-(P3-Pad4)")
  (net 37 "Net-(P3-Pad5)")
  (net 38 "Net-(P3-Pad6)")
  (net 39 "Net-(P3-Pad7)")
  (net 40 "Net-(P3-Pad8)")
  (net 41 "Net-(P4-Pad1)")
  (net 42 "Net-(P4-Pad2)")
  (net 43 "Net-(P4-Pad3)")
  (net 44 "Net-(P4-Pad4)")
  (net 45 "Net-(P4-Pad5)")
  (net 46 "Net-(P4-Pad6)")
  (net 47 "Net-(P4-Pad7)")
  (net 48 "Net-(P4-Pad8)")
  (net 49 "/GPIO17(GPIO_GEN0)")
  (net 50 "/GPIO27(GPIO_GEN2)")
  (net 51 "/GPIO22(GPIO_GEN3)")
  (net 52 "/(TXD0)GPIO14")
  (net 53 "/(RXD0)GPIO15")
  (net 54 "/(GPIO_GEN1)GPIO18")
  (net 55 "/(GPIO_GEN4)GPIO23")
  (net 56 "/(GPIO_GEN5)GPIO24")
  (net 57 "/ID_SD(I2CID EEPROM)")
  (net 58 "/(GPIO_GEN6)GPIO25")
  (net 59 "/(SPI_CE1_N)GPIO07")
  (net 60 "/(I2CID EEPROM)ID_SC")
  (net 61 /GPIO16)
  (net 62 /GPIO26)
  (net 63 "/GPIO02(SDA1,I2C)")
  (net 64 "/GPIO03(SCL1,I2C)")
  (net 65 "/GPIO04(GPIO_GCLK)")
  (net 66 "Net-(U3-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3.3V)
    (add_net +5V)
    (add_net "/(GPIO_GEN1)GPIO18")
    (add_net "/(GPIO_GEN4)GPIO23")
    (add_net "/(GPIO_GEN5)GPIO24")
    (add_net "/(GPIO_GEN6)GPIO25")
    (add_net "/(I2CID EEPROM)ID_SC")
    (add_net "/(RXD0)GPIO15")
    (add_net "/(SPI_CE0_N)GPIO08")
    (add_net "/(SPI_CE1_N)GPIO07")
    (add_net "/(TXD0)GPIO14")
    (add_net "/GPIO02(SDA1,I2C)")
    (add_net "/GPIO03(SCL1,I2C)")
    (add_net "/GPIO04(GPIO_GCLK)")
    (add_net /GPIO05)
    (add_net /GPIO06)
    (add_net "/GPIO09(SPI_MISO)")
    (add_net "/GPIO10(SPI_MOSI)")
    (add_net "/GPIO11(SPI_CLK)")
    (add_net /GPIO12)
    (add_net /GPIO13)
    (add_net /GPIO16)
    (add_net "/GPIO17(GPIO_GEN0)")
    (add_net /GPIO19)
    (add_net /GPIO20)
    (add_net /GPIO21)
    (add_net "/GPIO22(GPIO_GEN3)")
    (add_net /GPIO26)
    (add_net "/GPIO27(GPIO_GEN2)")
    (add_net "/ID_SD(I2CID EEPROM)")
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad6)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P3-Pad8)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P4-Pad5)")
    (add_net "Net-(P4-Pad6)")
    (add_net "Net-(P4-Pad7)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(U3-Pad6)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.762)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Mounting_Holes:MountingHole_2.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 53.086 132.334)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module TSSOP14 (layer F.Cu) (tedit 4E43F187)
    (at 91.567 119.38 90)
    (attr smd)
    (fp_text reference U3 (at 0 -0.762 90) (layer F.SilkS))
    (fp_text value MAX31856 (at 0 0.508 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.9304 2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 2 smd rect (at -1.2954 2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (pad 3 smd rect (at -0.635 2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (pad 4 smd rect (at 0 2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at 0.6604 2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 6 smd rect (at 1.3081 2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at 1.9558 2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 4 /GPIO05))
    (pad 8 smd rect (at 1.9558 -2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 9 smd rect (at 1.3081 -2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 3 "/(SPI_CE0_N)GPIO08"))
    (pad 10 smd rect (at 0.6604 -2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 8 "/GPIO11(SPI_CLK)"))
    (pad 11 smd rect (at 0 -2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 6 "/GPIO09(SPI_MISO)"))
    (pad 12 smd rect (at -0.6477 -2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 7 "/GPIO10(SPI_MOSI)"))
    (pad 13 smd rect (at -1.2954 -2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 10 /GPIO13))
    (pad 14 smd rect (at -1.9431 -2.794 90) (size 0.29972 1.30048) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model smd\smd_dil\tssop-14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tssop-28 (layer F.Cu) (tedit 4E57952B)
    (at 69.85 113.03 180)
    (descr TSSOP-28)
    (attr smd)
    (fp_text reference U1 (at 0 0.508 180) (layer F.SilkS))
    (fp_text value ADG1607 (at 0 -1.143 180) (layer F.SilkS))
    (pad 7 smd rect (at -0.32512 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(P3-Pad2)"))
    (pad 8 smd rect (at 0.32512 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P1-Pad8)"))
    (pad 9 smd rect (at 0.97536 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P1-Pad6)"))
    (pad 10 smd rect (at 1.6256 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P1-Pad4)"))
    (pad 25 smd rect (at -2.26568 -2.794 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(P3-Pad5)"))
    (pad 4 smd rect (at -2.27584 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(P3-Pad8)"))
    (pad 5 smd rect (at -1.6256 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(P3-Pad6)"))
    (pad 6 smd rect (at -0.97536 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(P3-Pad4)"))
    (pad 18 smd rect (at 2.27584 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 5 /GPIO06))
    (pad 19 smd rect (at 1.6256 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P1-Pad1)"))
    (pad 20 smd rect (at 0.97536 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P1-Pad3)"))
    (pad 21 smd rect (at 0.32512 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P1-Pad5)"))
    (pad 22 smd rect (at -0.32512 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P1-Pad7)"))
    (pad 23 smd rect (at -0.97536 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 11 smd rect (at 2.27584 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P1-Pad2)"))
    (pad 24 smd rect (at -1.6256 -2.794 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(P3-Pad3)"))
    (pad 3 smd rect (at -2.92608 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 2.92608 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 17 smd rect (at 2.92608 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 11 /GPIO19))
    (pad 26 smd rect (at -2.92608 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(P3-Pad7)"))
    (pad 2 smd rect (at -3.57378 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (pad 13 smd rect (at 3.57378 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 3.57378 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 12 /GPIO20))
    (pad 27 smd rect (at -3.57378 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 1 smd rect (at -4.22402 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 14 smd rect (at 4.22402 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 4.22402 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 13 /GPIO21))
    (pad 28 smd rect (at -4.22402 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (model smd/smd_dil/tssop-28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tssop-28 (layer F.Cu) (tedit 4E57952B)
    (at 112.522 112.776 180)
    (descr TSSOP-28)
    (attr smd)
    (fp_text reference U2 (at 0 0.508 180) (layer F.SilkS))
    (fp_text value ADG1607 (at 0 -1.143 180) (layer F.SilkS))
    (pad 7 smd rect (at -0.32512 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(P4-Pad2)"))
    (pad 8 smd rect (at 0.32512 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(P2-Pad8)"))
    (pad 9 smd rect (at 0.97536 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(P2-Pad6)"))
    (pad 10 smd rect (at 1.6256 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(P2-Pad4)"))
    (pad 25 smd rect (at -2.26568 -2.794 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(P4-Pad5)"))
    (pad 4 smd rect (at -2.27584 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(P4-Pad8)"))
    (pad 5 smd rect (at -1.6256 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(P4-Pad6)"))
    (pad 6 smd rect (at -0.97536 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(P4-Pad4)"))
    (pad 18 smd rect (at 2.27584 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 9 /GPIO12))
    (pad 19 smd rect (at 1.6256 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(P2-Pad1)"))
    (pad 20 smd rect (at 0.97536 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(P2-Pad3)"))
    (pad 21 smd rect (at 0.32512 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(P2-Pad5)"))
    (pad 22 smd rect (at -0.32512 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(P2-Pad7)"))
    (pad 23 smd rect (at -0.97536 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(P4-Pad1)"))
    (pad 11 smd rect (at 2.27584 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(P2-Pad2)"))
    (pad 24 smd rect (at -1.6256 -2.794 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(P4-Pad3)"))
    (pad 3 smd rect (at -2.92608 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 2.92608 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 17 smd rect (at 2.92608 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 11 /GPIO19))
    (pad 26 smd rect (at -2.92608 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(P4-Pad7)"))
    (pad 2 smd rect (at -3.57378 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (pad 13 smd rect (at 3.57378 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 3.57378 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 12 /GPIO20))
    (pad 27 smd rect (at -3.57378 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 1 smd rect (at -4.22402 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 14 smd rect (at 4.22402 2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 4.22402 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 13 /GPIO21))
    (pad 28 smd rect (at -4.22402 -2.79908 180) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (model smd/smd_dil/tssop-28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1812E (layer F.Cu) (tedit 5B8F83CA)
    (at 91.44 99.06)
    (attr smd)
    (fp_text reference C9 (at 0 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 -2.794 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.905 0) (size 1.778 3.556) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 2 smd rect (at 1.905 0) (size 1.778 3.556) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.2 0.25 0.25))
      (rotate (xyz 0 0 0))
    )
  )
  (module 8PIN_2.54_TERM. (layer F.Cu) (tedit 5BCAA6A3)
    (at 63.5 123.19)
    (fp_text reference P1 (at -1.397 7.366) (layer F.SilkS))
    (fp_text value CONN_8 (at 5.08 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -11.43 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -8.89 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at -6.35 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P1-Pad3)"))
    (pad 4 thru_hole circle (at -3.81 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P1-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P1-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P1-Pad6)"))
    (pad 7 thru_hole circle (at 3.81 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P1-Pad7)"))
    (pad 8 thru_hole circle (at 6.35 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P1-Pad8)"))
    (pad "" thru_hole circle (at -11.43 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -8.89 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -6.35 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -3.81 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -1.27 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 1.27 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 3.81 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 6.35 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  )
  (module 8PIN_2.54_TERM. (layer F.Cu) (tedit 5BD3AFD1)
    (at 84.328 123.19)
    (fp_text reference P3 (at -11.938 7.366) (layer F.SilkS))
    (fp_text value CONN_8 (at 5.08 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -11.43 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(P3-Pad1)"))
    (pad 2 thru_hole circle (at -8.89 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P3-Pad2)"))
    (pad 3 thru_hole circle (at -6.35 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(P3-Pad3)"))
    (pad 4 thru_hole circle (at -3.81 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(P3-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(P3-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P3-Pad6)"))
    (pad 7 thru_hole circle (at 3.81 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P3-Pad7)"))
    (pad 8 thru_hole circle (at 6.35 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(P3-Pad8)"))
    (pad "" thru_hole circle (at -11.43 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -8.89 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -6.35 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -3.81 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -1.27 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 1.27 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 3.81 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 6.35 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  )
  (module 8PIN_2.54_TERM. (layer F.Cu) (tedit 5BD3AFC0)
    (at 105.156 123.19)
    (fp_text reference P2 (at 0.508 7.112) (layer F.SilkS))
    (fp_text value CONN_8 (at 5.08 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -11.43 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(P2-Pad1)"))
    (pad 2 thru_hole circle (at -8.89 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P2-Pad2)"))
    (pad 3 thru_hole circle (at -6.35 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P2-Pad3)"))
    (pad 4 thru_hole circle (at -3.81 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P2-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P2-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P2-Pad6)"))
    (pad 7 thru_hole circle (at 3.81 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(P2-Pad7)"))
    (pad 8 thru_hole circle (at 6.35 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(P2-Pad8)"))
    (pad "" thru_hole circle (at -11.43 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -8.89 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -6.35 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -3.81 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -1.27 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 1.27 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 3.81 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 6.35 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  )
  (module 8PIN_2.54_TERM. (layer F.Cu) (tedit 5BCAA694)
    (at 125.984 123.19)
    (fp_text reference P4 (at -1.651 7.366) (layer F.SilkS))
    (fp_text value CONN_8 (at -0.635 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -11.43 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P4-Pad1)"))
    (pad 2 thru_hole circle (at -8.89 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P4-Pad2)"))
    (pad 3 thru_hole circle (at -6.35 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(P4-Pad3)"))
    (pad 4 thru_hole circle (at -3.81 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(P4-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(P4-Pad5)"))
    (pad 6 thru_hole circle (at 1.27 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(P4-Pad6)"))
    (pad 7 thru_hole circle (at 3.81 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(P4-Pad7)"))
    (pad 8 thru_hole circle (at 6.35 2.54) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(P4-Pad8)"))
    (pad "" thru_hole circle (at -11.43 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -8.89 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -6.35 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -3.81 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -1.27 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 1.27 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 3.81 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 6.35 5.08) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  )
  (module SM1206 (layer F.Cu) (tedit 5B8F8453)
    (at 119.38 113.03 270)
    (attr smd)
    (fp_text reference C5 (at 0 0 360) (layer F.SilkS))
    (fp_text value 100nF (at -2.032 -3.302 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer F.Cu) (tedit 5B8F83DC)
    (at 78.232 109.728)
    (attr smd)
    (fp_text reference C6 (at 0 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.778) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer F.Cu) (tedit 5B8F83F1)
    (at 92.71 113.538 90)
    (attr smd)
    (fp_text reference C7 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.778 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 90) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 2 smd rect (at 1.651 0 90) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer F.Cu) (tedit 5B8F83C2)
    (at 91.44 102.87)
    (attr smd)
    (fp_text reference C8 (at 0 0) (layer F.SilkS))
    (fp_text value 100nF (at 0.254 2.032) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer F.Cu) (tedit 5B8F83E9)
    (at 86.614 115.316 180)
    (attr smd)
    (fp_text reference C4 (at 0 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0.254 -1.778 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer F.Cu) (tedit 5B8F843C)
    (at 97.282 118.364 90)
    (attr smd)
    (fp_text reference C3 (at 0 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 3.302 -0.762 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 90) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 1.651 0 90) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer F.Cu) (tedit 5B8F8429)
    (at 101.6 119.38 180)
    (attr smd)
    (fp_text reference C1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 100nF (at -0.254 -1.778 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C1-Pad2)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer F.Cu) (tedit 5B8F83FC)
    (at 100.965 111.76)
    (attr smd)
    (fp_text reference C2 (at 0 0) (layer F.SilkS))
    (fp_text value 100nF (at 0.127 -1.778) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_20X2 (layer F.Cu) (tedit 5B935C17)
    (at 82.042 83.566)
    (descr "Double rangee de contacts 2 x 12 pins")
    (tags CONN)
    (fp_text reference P5 (at 7.112 3.81) (layer F.SilkS))
    (fp_text value CONN_20X2 (at 0 3.81) (layer F.SilkS))
    (pad 1 thru_hole rect (at -24.13 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at -24.13 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 11 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 "/GPIO17(GPIO_GEN0)"))
    (pad 4 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 13 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 "/GPIO27(GPIO_GEN2)"))
    (pad 6 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (pad 15 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "/GPIO22(GPIO_GEN3)"))
    (pad 8 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 "/(TXD0)GPIO14"))
    (pad 17 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 10 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 "/(RXD0)GPIO15"))
    (pad 19 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "/GPIO10(SPI_MOSI)"))
    (pad 12 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 "/(GPIO_GEN1)GPIO18"))
    (pad 21 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "/GPIO09(SPI_MISO)"))
    (pad 14 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (pad 23 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "/GPIO11(SPI_CLK)"))
    (pad 16 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 "/(GPIO_GEN4)GPIO23"))
    (pad 25 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (pad 18 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 "/(GPIO_GEN5)GPIO24"))
    (pad 27 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 "/ID_SD(I2CID EEPROM)"))
    (pad 20 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (pad 29 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /GPIO05))
    (pad 22 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 "/(GPIO_GEN6)GPIO25"))
    (pad 31 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /GPIO06))
    (pad 24 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "/(SPI_CE0_N)GPIO08"))
    (pad 26 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 "/(SPI_CE1_N)GPIO07"))
    (pad 33 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /GPIO13))
    (pad 28 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 "/(I2CID EEPROM)ID_SC"))
    (pad 32 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /GPIO12))
    (pad 34 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (pad 36 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 /GPIO16))
    (pad 38 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /GPIO20))
    (pad 35 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /GPIO19))
    (pad 37 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /GPIO26))
    (pad 3 thru_hole circle (at -21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 "/GPIO02(SDA1,I2C)"))
    (pad 5 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 "/GPIO03(SCL1,I2C)"))
    (pad 7 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 "/GPIO04(GPIO_GCLK)"))
    (pad 9 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (pad 39 thru_hole circle (at 24.13 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (pad 40 thru_hole circle (at 24.13 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /GPIO21))
    (pad 30 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (model pin_array/pins_array_20x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 5BCA9B9F)
    (at 128.524 84.328)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0 1.016) (layer F.Fab) hide)
  )
  (module Symbols:KiCad-Logo2_8mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 125.222 104.14)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo2_8mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Mounting_Holes:MountingHole_2.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 110.109 132.334)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 111.125 83.566)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 53.086 83.566)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mylib:Raspberry_logo (layer F.Cu) (tedit 0)
    (at 58.42 96.012)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text SPI_CLK (at 86.106 90.678 90) (layer B.SilkS))
  (gr_text MISO (at 83.312 88.9 90) (layer B.SilkS))
  (gr_text MOSI (at 80.772 88.9 90) (layer B.SilkS))
  (gr_text + (at 64.77 120.65) (layer F.SilkS))
  (gr_text - (at 62.23 120.65) (layer F.SilkS))
  (gr_text "Thermocouples supported:\nK, J, N, R, S, T, E & B" (at 89.154 132.334) (layer F.SilkS))
  (gr_text Ch.16 (at 131.064 117.856 90) (layer F.SilkS))
  (gr_text + (at 132.334 121.666) (layer F.SilkS))
  (gr_text "-\n" (at 129.54 121.666) (layer F.SilkS))
  (gr_text "Ch. 1" (at 53.086 116.84 90) (layer F.SilkS))
  (gr_text "..to Ch. 16--->" (at 75.692 120.65) (layer F.SilkS))
  (gr_text + (at 59.69 120.65) (layer F.SilkS))
  (gr_text - (at 57.15 120.65) (layer F.SilkS))
  (gr_text - (at 51.562 120.65) (layer F.SilkS))
  (gr_text + (at 54.102 120.65) (layer F.SilkS))
  (gr_text "PiPlay Ver 1.3" (at 114.808 89.408) (layer F.SilkS))
  (gr_text "16 Channel thermocouple multiplexer\nFor Raspberry Pi" (at 107.95 95.758) (layer F.SilkS))
  (gr_line (start 134.62 80.01) (end 49.53 80.01) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.62 135.89) (end 134.62 80.01) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.53 135.89) (end 134.62 135.89) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.53 80.01) (end 49.53 135.89) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 14) (net_name GND) (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 135.382) (xy 50.038 135.382) (xy 50.038 80.518) (xy 134.112 80.518)
      )
    )
  )
  (zone (net 14) (net_name GND) (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.112 135.382) (xy 50.038 135.382) (xy 50.038 80.518) (xy 134.112 80.518)
      )
    )
  )
)
