%CMF
# %PSECTS Section
# For each object file, details of its psects are enumerated here.
# The begining of the section is indicated by %PSECTS.  The first
# line indicates the name of the first object file, e.g.
#    $foo.obj
# Each line that follows describes a psect in that object file, until
# the next object file.  The lines that describe a psect have the
# format:
#    <psect name> <class name> <space> <link address> <load addresses> <length> <delta>
# All addresses and the length are given in unqualified hexadecimal
# in delta units.  Any other numeric values are decimal.
%PSECTS
$dist/default/production/ui_board.X.production.obj
cinit CODE 0 2E3 2E3 14 2
text1 CODE 0 114D 114D 4A 2
text2 CODE 0 1052 1052 2A 2
text3 CODE 0 1106 1106 47 2
text4 CODE 0 1326 1326 B1 2
text5 CODE 0 162D 162D 1D3 2
text6 CODE 0 1216 1216 87 2
text7 CODE 0 817 817 8A 2
text8 CODE 0 129D 129D 89 2
text9 CODE 0 2F7 2F7 389 2
text10 CODE 0 14A3 14A3 18A 2
text11 CODE 0 CB7 CB7 349 2
text12 CODE 0 10BF 10BF 47 2
text13 CODE 0 107C 107C 43 2
text14 CODE 0 7AD 7AD 53 2
text15 CODE 0 1197 1197 7F 2
text16 CODE 0 80D 80D A 2
text17 CODE 0 A8B A8B 22C 2
text18 CODE 0 1032 1032 20 2
text19 CODE 0 13D7 13D7 CC 2
text20 CODE 0 8A1 8A1 1EA 2
maintext CODE 0 680 680 12D 2
cstackCOMMON COMMON 1 70 70 6 1
cstackBANK0 BANK0 1 20 20 3F 1
cstackBANK1 BANK1 1 A0 A0 31 1
cstackBANK2 BANK2 1 120 120 29 1
cstackBANK3 BANK3 1 1A0 1A0 2E 1
stringtext1 STRCODE 0 180C 180C 1 2
stringtext2 STRCODE 0 180D 180D 1 2
stringtext3 STRCODE 0 180E 180E 1 2
stringtext4 STRCODE 0 180F 180F 1 2
stringtext5 STRCODE 0 1810 1810 1 2
stringtext6 STRCODE 0 1811 1811 1 2
stringtext7 STRCODE 0 1812 1812 1 2
stringtext8 STRCODE 0 1813 1813 1 2
stringtext9 STRCODE 0 1814 1814 1 2
intentry CODE 0 4 4 2DD 2
bssBANK1 BANK1 1 D1 D1 5 1
bssBANK3 BANK3 1 1CE 1CE 1B 1
swtext1 CONST 0 800 800 C 2
swtext2 CONST 0 1800 1800 C 2
swtext3 CONST 0 1000 1000 2A 2
clrtext CODE 0 102C 102C 6 2
bssCOMMON COMMON 1 76 76 3 1
$/tmp/xcX5Y7Rvk.obj
reset_vec CODE 0 0 0 2 2
end_init CODE 0 2E1 2E1 2 2
config CONFIG 0 8007 8007 2 2
# %UNUSED Section
# This section enumerates the unused ranges of each CLASS. Each entry
# is described on a single line as follows:
#    <class name> <range> <delta>
# Addresses given in the range are in hexadecimal and units of delta.
%UNUSED
RAM 5F-6F 1
RAM D6-EF 1
RAM 149-16F 1
RAM 1E9-1EF 1
RAM 220-26F 1
RAM 2A0-2EF 1
RAM 320-32F 1
BANK0 5F-6F 1
BANK1 D6-EF 1
BANK2 149-16F 1
BANK3 1E9-1EF 1
BANK4 220-26F 1
BANK5 2A0-2EF 1
BANK6 320-32F 1
CONST 2-3 2
CONST 80C-80C 2
CONST 102A-102B 2
CONST 1815-1FFF 2
ENTRY 2-3 2
ENTRY 80C-80C 2
ENTRY 102A-102B 2
ENTRY 1815-1FFF 2
IDLOC 8000-8003 2
SFR10 500-56F 1
SFR11 580-5EF 1
SFR12 600-66F 1
SFR13 680-6EF 1
SFR14 700-76F 1
SFR15 780-7EF 1
SFR16 800-86F 1
SFR17 880-8EF 1
SFR18 900-96F 1
SFR19 980-9EF 1
SFR20 A00-A6F 1
SFR21 A80-AEF 1
SFR22 B00-B6F 1
SFR23 B80-BEF 1
SFR24 C00-C6F 1
SFR25 C80-CEF 1
SFR26 D00-D6F 1
SFR27 D80-DEF 1
SFR28 E00-E6F 1
SFR29 E80-EEF 1
SFR30 F00-F6F 1
SFR31 F80-FEF 1
STACK 2139-21EF 1
CODE 2-3 2
CODE 80C-80C 2
CODE 102A-102B 2
CODE 1815-1FFF 2
SFR0 0-1F 1
SFR1 80-9F 1
SFR2 100-11F 1
SFR3 180-19F 1
SFR4 200-21F 1
SFR5 280-29F 1
SFR6 300-31F 1
SFR7 380-3EF 1
SFR8 400-46F 1
SFR9 480-4EF 1
BIGRAM 2000-21EF 1
COMMON 79-7D 1
STRCODE 2-3 2
STRCODE 80C-80C 2
STRCODE 102A-102B 2
STRCODE 1815-1FFF 2
STRING 2-3 2
STRING 80C-80C 2
STRING 102A-102B 2
STRING 1815-1FFF 2
# %LINETAB Section
# This section enumerates the file/line to address mappings.
# The beginning of the section is indicated by %LINETAB.
# The first line indicates the name of the first object file, e.g.
#   $foo.obj
# Each line that follows describes a single mapping until the next
# object file.  Mappings have the following format:
#    <address> <psect name> <class name> ><line number>:<file name>
# The address is absolute and given given in unqualified hex 
# in delta units of the psect. All mappings within an object file
# are in ascending order of addresses.
# All other numeric values are in decimal.
%LINETAB
$dist/default/production/ui_board.X.production.obj
2E3 cinit CODE >1340:/tmp/xcXhFngUs
2E3 cinit CODE >1343:/tmp/xcXhFngUs
2E3 cinit CODE >1394:/tmp/xcXhFngUs
2E4 cinit CODE >1395:/tmp/xcXhFngUs
2E5 cinit CODE >1396:/tmp/xcXhFngUs
2E6 cinit CODE >1400:/tmp/xcXhFngUs
2E7 cinit CODE >1401:/tmp/xcXhFngUs
2E8 cinit CODE >1402:/tmp/xcXhFngUs
2E9 cinit CODE >1403:/tmp/xcXhFngUs
2EA cinit CODE >1404:/tmp/xcXhFngUs
2EB cinit CODE >1405:/tmp/xcXhFngUs
2EC cinit CODE >1409:/tmp/xcXhFngUs
2ED cinit CODE >1410:/tmp/xcXhFngUs
2EE cinit CODE >1411:/tmp/xcXhFngUs
2EF cinit CODE >1412:/tmp/xcXhFngUs
2F0 cinit CODE >1413:/tmp/xcXhFngUs
2F1 cinit CODE >1414:/tmp/xcXhFngUs
2F3 cinit CODE >1420:/tmp/xcXhFngUs
2F3 cinit CODE >1422:/tmp/xcXhFngUs
2F4 cinit CODE >1423:/tmp/xcXhFngUs
2F5 cinit CODE >1424:/tmp/xcXhFngUs
4 intentry CODE >184:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
4 intentry CODE >10:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
9 intentry CODE >20:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11 intentry CODE >21:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
14 intentry CODE >22:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
5D intentry CODE >23:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
60 intentry CODE >24:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A9 intentry CODE >25:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
AD intentry CODE >26:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
F6 intentry CODE >27:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
FA intentry CODE >28:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
132 intentry CODE >29:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
136 intentry CODE >30:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
17F intentry CODE >31:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
183 intentry CODE >32:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1CC intentry CODE >33:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1D0 intentry CODE >34:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
219 intentry CODE >35:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
21D intentry CODE >36:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
25C intentry CODE >39:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
262 intentry CODE >41:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
280 intentry CODE >42:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
281 intentry CODE >43:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
282 intentry CODE >39:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
289 intentry CODE >45:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
28B intentry CODE >46:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
28C intentry CODE >49:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
291 intentry CODE >50:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
292 intentry CODE >52:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
294 intentry CODE >53:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
297 intentry CODE >54:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
299 intentry CODE >55:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
29B intentry CODE >56:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
29C intentry CODE >57:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
29E intentry CODE >59:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
29F intentry CODE >60:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2A2 intentry CODE >61:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2A4 intentry CODE >62:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2A6 intentry CODE >63:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2A7 intentry CODE >64:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2A9 intentry CODE >66:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2AA intentry CODE >67:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2AD intentry CODE >68:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2AF intentry CODE >69:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2B1 intentry CODE >70:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2B2 intentry CODE >71:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2B4 intentry CODE >73:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2B5 intentry CODE >74:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2B8 intentry CODE >75:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2BA intentry CODE >76:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2BC intentry CODE >77:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2BD intentry CODE >78:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2BF intentry CODE >81:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2C3 intentry CODE >82:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2C8 intentry CODE >83:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2CC intentry CODE >85:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2CD intentry CODE >86:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2D3 intentry CODE >90:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2D8 intentry CODE >91:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2DB intentry CODE >92:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2DC intentry CODE >94:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2DD intentry CODE >95:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
8A1 text20 CODE >8:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8A1 text20 CODE >26:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8A8 text20 CODE >27:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8AE text20 CODE >28:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8B1 text20 CODE >29:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8B3 text20 CODE >33:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8B7 text20 CODE >35:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8BA text20 CODE >37:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8C3 text20 CODE >40:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8C5 text20 CODE >42:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8C6 text20 CODE >43:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8C7 text20 CODE >46:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8D0 text20 CODE >49:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8D6 text20 CODE >50:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8DC text20 CODE >51:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8DF text20 CODE >52:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8E1 text20 CODE >56:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8E5 text20 CODE >58:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8E8 text20 CODE >60:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8F1 text20 CODE >63:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8F3 text20 CODE >65:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8F4 text20 CODE >66:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8F5 text20 CODE >69:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8FE text20 CODE >70:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
8FE text20 CODE >75:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
904 text20 CODE >76:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
90C text20 CODE >77:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
910 text20 CODE >78:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
919 text20 CODE >82:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
91D text20 CODE >83:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
926 text20 CODE >84:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
92F text20 CODE >88:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
945 text20 CODE >91:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
955 text20 CODE >92:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
95E text20 CODE >93:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
967 text20 CODE >95:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
968 text20 CODE >96:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
96C text20 CODE >99:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
96F text20 CODE >100:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
976 text20 CODE >101:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
97E text20 CODE >102:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
981 text20 CODE >103:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
983 text20 CODE >105:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
98B text20 CODE >111:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9A3 text20 CODE >114:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9A4 text20 CODE >115:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9B4 text20 CODE >117:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9B8 text20 CODE >96:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9B9 text20 CODE >121:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9BE text20 CODE >122:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9BF text20 CODE >126:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9C2 text20 CODE >127:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9CA text20 CODE >128:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9CD text20 CODE >129:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9CF text20 CODE >131:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9D7 text20 CODE >132:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9DB text20 CODE >126:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9DC text20 CODE >138:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9DE text20 CODE >139:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9E0 text20 CODE >140:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9F1 text20 CODE >141:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9F2 text20 CODE >144:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9F5 text20 CODE >145:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9F8 text20 CODE >149:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
9FC text20 CODE >150:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A05 text20 CODE >151:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A07 text20 CODE >152:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A2D text20 CODE >153:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A32 text20 CODE >158:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A3E text20 CODE >159:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A43 text20 CODE >160:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A4C text20 CODE >161:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A4C text20 CODE >164:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A58 text20 CODE >165:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A5B text20 CODE >166:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A64 text20 CODE >168:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A66 text20 CODE >169:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A66 text20 CODE >172:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A6B text20 CODE >174:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A6D text20 CODE >175:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A6F text20 CODE >176:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A70 text20 CODE >179:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A76 text20 CODE >180:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A76 text20 CODE >181:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A7C text20 CODE >182:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
A82 text20 CODE >183:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
13D7 text19 CODE >4:/opt/microchip/xc8/v1.45/sources/common/flge.c
13D7 text19 CODE >7:/opt/microchip/xc8/v1.45/sources/common/flge.c
13F1 text19 CODE >8:/opt/microchip/xc8/v1.45/sources/common/flge.c
13FA text19 CODE >9:/opt/microchip/xc8/v1.45/sources/common/flge.c
1414 text19 CODE >10:/opt/microchip/xc8/v1.45/sources/common/flge.c
141D text19 CODE >12:/opt/microchip/xc8/v1.45/sources/common/flge.c
1420 text19 CODE >13:/opt/microchip/xc8/v1.45/sources/common/flge.c
1457 text19 CODE >14:/opt/microchip/xc8/v1.45/sources/common/flge.c
1459 text19 CODE >15:/opt/microchip/xc8/v1.45/sources/common/flge.c
1490 text19 CODE >16:/opt/microchip/xc8/v1.45/sources/common/flge.c
1492 text19 CODE >17:/opt/microchip/xc8/v1.45/sources/common/flge.c
1494 text19 CODE >18:/opt/microchip/xc8/v1.45/sources/common/flge.c
1032 text18 CODE >4:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
1034 text18 CODE >5:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
1036 text18 CODE >6:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
103D text18 CODE >51:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
103F text18 CODE >52:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
1043 text18 CODE >53:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
1043 text18 CODE >54:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
1048 text18 CODE >55:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
104A text18 CODE >56:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
104D text18 CODE >59:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
A8B text17 CODE >8:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
A8B text17 CODE >17:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
A91 text17 CODE >18:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
A95 text17 CODE >19:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
A96 text17 CODE >20:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
A97 text17 CODE >24:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
A9A text17 CODE >26:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
A9D text17 CODE >28:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AA5 text17 CODE >31:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AA6 text17 CODE >33:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AA7 text17 CODE >36:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AAF text17 CODE >39:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AB4 text17 CODE >40:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AB8 text17 CODE >41:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AB9 text17 CODE >42:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
ABA text17 CODE >45:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
ABD text17 CODE >48:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AC0 text17 CODE >50:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AC8 text17 CODE >53:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AC9 text17 CODE >54:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
ACA text17 CODE >57:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AD2 text17 CODE >65:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AD7 text17 CODE >66:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AE0 text17 CODE >119:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AED text17 CODE >120:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AFA text17 CODE >121:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B07 text17 CODE >122:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B14 text17 CODE >123:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B21 text17 CODE >124:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B2E text17 CODE >125:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B3B text17 CODE >126:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B48 text17 CODE >127:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B55 text17 CODE >128:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B5C text17 CODE >129:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B69 text17 CODE >130:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B70 text17 CODE >131:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B7D text17 CODE >132:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B84 text17 CODE >133:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B8B text17 CODE >134:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B98 text17 CODE >135:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B9F text17 CODE >136:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BAC text17 CODE >137:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BB3 text17 CODE >138:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BC0 text17 CODE >139:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BC7 text17 CODE >140:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BD4 text17 CODE >141:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BE9 text17 CODE >145:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C00 text17 CODE >146:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C07 text17 CODE >149:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C12 text17 CODE >152:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C14 text17 CODE >153:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C1B text17 CODE >154:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C1C text17 CODE >155:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C1D text17 CODE >157:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C24 text17 CODE >158:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C28 text17 CODE >152:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C29 text17 CODE >163:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C2A text17 CODE >164:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C2C text17 CODE >165:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C3D text17 CODE >166:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C3E text17 CODE >169:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C40 text17 CODE >170:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C42 text17 CODE >174:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C45 text17 CODE >175:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C4D text17 CODE >176:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C4F text17 CODE >177:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C67 text17 CODE >178:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C6B text17 CODE >183:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C76 text17 CODE >184:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C7F text17 CODE >185:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C80 text17 CODE >187:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C8C text17 CODE >188:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C95 text17 CODE >190:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C96 text17 CODE >191:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C97 text17 CODE >194:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C9C text17 CODE >195:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CA4 text17 CODE >196:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CA5 text17 CODE >197:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CA6 text17 CODE >199:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CAA text17 CODE >200:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CAA text17 CODE >201:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CAE text17 CODE >203:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
80D text16 CODE >15:/opt/microchip/xc8/v1.45/sources/common/flneg.c
80D text16 CODE >17:/opt/microchip/xc8/v1.45/sources/common/flneg.c
814 text16 CODE >18:/opt/microchip/xc8/v1.45/sources/common/flneg.c
1197 text15 CODE >43:/opt/microchip/xc8/v1.45/sources/common/fltol.c
1197 text15 CODE >47:/opt/microchip/xc8/v1.45/sources/common/fltol.c
11A9 text15 CODE >48:/opt/microchip/xc8/v1.45/sources/common/fltol.c
11B2 text15 CODE >49:/opt/microchip/xc8/v1.45/sources/common/fltol.c
11C5 text15 CODE >50:/opt/microchip/xc8/v1.45/sources/common/fltol.c
11C6 text15 CODE >51:/opt/microchip/xc8/v1.45/sources/common/fltol.c
11CE text15 CODE >52:/opt/microchip/xc8/v1.45/sources/common/fltol.c
11D0 text15 CODE >53:/opt/microchip/xc8/v1.45/sources/common/fltol.c
11D2 text15 CODE >54:/opt/microchip/xc8/v1.45/sources/common/fltol.c
11D7 text15 CODE >55:/opt/microchip/xc8/v1.45/sources/common/fltol.c
11E0 text15 CODE >57:/opt/microchip/xc8/v1.45/sources/common/fltol.c
11E7 text15 CODE >58:/opt/microchip/xc8/v1.45/sources/common/fltol.c
11EE text15 CODE >60:/opt/microchip/xc8/v1.45/sources/common/fltol.c
11F2 text15 CODE >61:/opt/microchip/xc8/v1.45/sources/common/fltol.c
11FB text15 CODE >63:/opt/microchip/xc8/v1.45/sources/common/fltol.c
1202 text15 CODE >64:/opt/microchip/xc8/v1.45/sources/common/fltol.c
1204 text15 CODE >62:/opt/microchip/xc8/v1.45/sources/common/fltol.c
1204 text15 CODE >65:/opt/microchip/xc8/v1.45/sources/common/fltol.c
1207 text15 CODE >67:/opt/microchip/xc8/v1.45/sources/common/fltol.c
120A text15 CODE >68:/opt/microchip/xc8/v1.45/sources/common/fltol.c
1215 text15 CODE >70:/opt/microchip/xc8/v1.45/sources/common/fltol.c
7AD text14 CODE >6:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7AD text14 CODE >14:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7B6 text14 CODE >15:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7BC text14 CODE >16:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7BE text14 CODE >17:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7C0 text14 CODE >18:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7C7 text14 CODE >19:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7CB text14 CODE >17:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7CC text14 CODE >22:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7D3 text14 CODE >23:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7E3 text14 CODE >24:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7EB text14 CODE >25:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7EC text14 CODE >27:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7F3 text14 CODE >28:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
7F7 text14 CODE >30:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
107C text13 CODE >6:/opt/microchip/xc8/v1.45/sources/common/llmod.c
107C text13 CODE >13:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1083 text13 CODE >14:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1085 text13 CODE >15:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1087 text13 CODE >16:/opt/microchip/xc8/v1.45/sources/common/llmod.c
108E text13 CODE >17:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1092 text13 CODE >15:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1093 text13 CODE >20:/opt/microchip/xc8/v1.45/sources/common/llmod.c
10A3 text13 CODE >21:/opt/microchip/xc8/v1.45/sources/common/llmod.c
10AB text13 CODE >22:/opt/microchip/xc8/v1.45/sources/common/llmod.c
10B2 text13 CODE >23:/opt/microchip/xc8/v1.45/sources/common/llmod.c
10B6 text13 CODE >25:/opt/microchip/xc8/v1.45/sources/common/llmod.c
10BF text12 CODE >188:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10C1 text12 CODE >191:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10C2 text12 CODE >194:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10C4 text12 CODE >197:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10C5 text12 CODE >198:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10C6 text12 CODE >200:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10C7 text12 CODE >203:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10C9 text12 CODE >206:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10CB text12 CODE >209:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10CD text12 CODE >212:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10CF text12 CODE >215:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10D1 text12 CODE >218:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10D3 text12 CODE >221:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10D5 text12 CODE >224:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10D7 text12 CODE >227:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10D9 text12 CODE >230:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10DD text12 CODE >231:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
10DE text12 CODE >191:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1104 text12 CODE >232:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1000 swtext3 CONST >93:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
CB7 text11 CODE >51:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
CB7 text11 CODE >60:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
CD4 text11 CODE >62:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
CF7 text11 CODE >63:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
CF9 text11 CODE >67:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
CFE text11 CODE >71:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
D00 text11 CODE >72:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
D04 text11 CODE >71:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
D67 text11 CODE >73:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
D8A text11 CODE >76:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
DA1 text11 CODE >77:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
DA7 text11 CODE >78:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
DB6 text11 CODE >79:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
DBA text11 CODE >80:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
DC1 text11 CODE >81:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
DC7 text11 CODE >82:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
DC9 text11 CODE >83:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
DCD text11 CODE >86:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
E03 text11 CODE >87:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
E62 text11 CODE >88:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
EC1 text11 CODE >89:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F20 text11 CODE >90:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F7F text11 CODE >93:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F80 text11 CODE >96:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F82 text11 CODE >100:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F84 text11 CODE >104:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F88 text11 CODE >105:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F8A text11 CODE >108:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F8C text11 CODE >112:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F8E text11 CODE >116:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F92 text11 CODE >117:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F94 text11 CODE >120:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F96 text11 CODE >124:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F98 text11 CODE >128:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F9C text11 CODE >129:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F9E text11 CODE >132:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FA0 text11 CODE >136:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FA2 text11 CODE >140:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FA6 text11 CODE >141:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FA8 text11 CODE >144:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FAA text11 CODE >148:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FAC text11 CODE >152:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FB0 text11 CODE >153:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FB2 text11 CODE >156:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FB4 text11 CODE >160:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FB6 text11 CODE >164:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FBA text11 CODE >165:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FBC text11 CODE >168:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FBE text11 CODE >172:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FC0 text11 CODE >176:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FC4 text11 CODE >177:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FCC text11 CODE >179:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FCD text11 CODE >93:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FD7 text11 CODE >182:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FDC text11 CODE >183:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FEF text11 CODE >182:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FF7 text11 CODE >184:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FFF text11 CODE >185:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
14A3 text10 CODE >236:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
14A5 text10 CODE >238:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
14A6 text10 CODE >239:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
14A8 text10 CODE >241:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
14AB text10 CODE >243:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
14BA text10 CODE >244:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
14CA text10 CODE >245:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
14DA text10 CODE >246:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
14EA text10 CODE >247:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
14FA text10 CODE >248:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
150A text10 CODE >249:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
150B text10 CODE >252:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
151B text10 CODE >255:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1527 text10 CODE >258:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1537 text10 CODE >261:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1543 text10 CODE >264:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1553 text10 CODE >267:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1563 text10 CODE >269:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1564 text10 CODE >249:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1579 text10 CODE >271:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
157E text10 CODE >273:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1587 text10 CODE >274:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
158F text10 CODE >275:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1597 text10 CODE >276:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
159F text10 CODE >277:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
15A7 text10 CODE >278:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
15AF text10 CODE >279:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
15B0 text10 CODE >282:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
15C0 text10 CODE >283:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
15C1 text10 CODE >285:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
15D1 text10 CODE >286:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
15D2 text10 CODE >288:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
15E2 text10 CODE >289:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
15E3 text10 CODE >291:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
15F3 text10 CODE >292:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
15F4 text10 CODE >294:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1604 text10 CODE >295:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1605 text10 CODE >297:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1615 text10 CODE >299:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1616 text10 CODE >279:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
162B text10 CODE >299:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
162C text10 CODE >301:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1800 swtext2 CONST >17:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
2F7 text9 CODE >6:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
2F9 text9 CODE >12:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
2FF text9 CODE >13:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
303 text9 CODE >14:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
30A text9 CODE >17:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
30B text9 CODE >20:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
3E7 text9 CODE >21:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
447 text9 CODE >22:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
448 text9 CODE >24:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
4FA text9 CODE >25:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
53F text9 CODE >26:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
540 text9 CODE >28:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
563 text9 CODE >29:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
587 text9 CODE >30:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
588 text9 CODE >32:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5AC text9 CODE >33:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5D0 text9 CODE >34:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5D1 text9 CODE >36:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5F5 text9 CODE >37:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
619 text9 CODE >38:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
61A text9 CODE >40:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
63E text9 CODE >41:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
662 text9 CODE >43:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
663 text9 CODE >17:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
66E text9 CODE >46:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
676 text9 CODE >47:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
67F text9 CODE >48:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
129D text8 CODE >161:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
129D text8 CODE >167:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
12CE text8 CODE >168:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
12CE text8 CODE >169:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
12D0 text8 CODE >170:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
12D3 text8 CODE >171:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
12D5 text8 CODE >172:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
12F4 text8 CODE >173:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
12F5 text8 CODE >167:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
131D text8 CODE >176:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
817 text7 CODE >147:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
819 text7 CODE >149:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
81A text7 CODE >150:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
82A text7 CODE >151:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
83B text7 CODE >152:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
84C text7 CODE >153:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
85D text7 CODE >154:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
86E text7 CODE >155:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
87F text7 CODE >156:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
890 text7 CODE >157:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
8A0 text7 CODE >158:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1216 text6 CODE >260:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1218 text6 CODE >265:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
122C text6 CODE >266:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
123E text6 CODE >267:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1250 text6 CODE >268:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1251 text6 CODE >271:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1265 text6 CODE >272:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1266 text6 CODE >274:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
127A text6 CODE >275:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
127B text6 CODE >277:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
128F text6 CODE >279:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1290 text6 CODE >268:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
129C text6 CODE >280:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
800 swtext1 CONST >205:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
162D text5 CODE >188:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
162F text5 CODE >193:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1643 text5 CODE >194:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1655 text5 CODE >195:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1667 text5 CODE >196:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1679 text5 CODE >197:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
168B text5 CODE >198:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
169D text5 CODE >199:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
16AF text5 CODE >200:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
16C1 text5 CODE >201:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
16D3 text5 CODE >202:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
16E5 text5 CODE >203:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
16F7 text5 CODE >204:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1709 text5 CODE >205:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
170A text5 CODE >208:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
171E text5 CODE >209:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1730 text5 CODE >210:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1731 text5 CODE >212:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1745 text5 CODE >213:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1757 text5 CODE >214:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1758 text5 CODE >216:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
176C text5 CODE >217:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
177E text5 CODE >218:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
177F text5 CODE >220:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1793 text5 CODE >221:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
17A5 text5 CODE >222:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
17A6 text5 CODE >224:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
17BA text5 CODE >225:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
17CC text5 CODE >226:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
17CD text5 CODE >228:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
17E1 text5 CODE >229:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
17F3 text5 CODE >231:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
17F4 text5 CODE >205:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
17FF text5 CODE >232:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1326 text4 CODE >234:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1328 text4 CODE >239:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
133C text4 CODE >240:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
134E text4 CODE >241:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1360 text4 CODE >242:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1372 text4 CODE >243:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1373 text4 CODE >246:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1387 text4 CODE >247:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1388 text4 CODE >249:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
139C text4 CODE >250:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
139D text4 CODE >252:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13B1 text4 CODE >253:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13B2 text4 CODE >255:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13C6 text4 CODE >257:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13C7 text4 CODE >243:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13D6 text4 CODE >258:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1106 text3 CODE >98:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1108 text3 CODE >100:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
110B text3 CODE >101:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
110F text3 CODE >103:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1111 text3 CODE >104:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1112 text3 CODE >105:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1113 text3 CODE >107:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1115 text3 CODE >108:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1116 text3 CODE >109:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1117 text3 CODE >110:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1118 text3 CODE >111:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1119 text3 CODE >112:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
111A text3 CODE >113:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
111B text3 CODE >114:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
111C text3 CODE >115:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
111D text3 CODE >116:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
111E text3 CODE >117:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1120 text3 CODE >118:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1122 text3 CODE >121:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1123 text3 CODE >122:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1124 text3 CODE >123:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1125 text3 CODE >125:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1127 text3 CODE >126:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1128 text3 CODE >127:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
112C text3 CODE >128:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
112D text3 CODE >130:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
112E text3 CODE >131:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
112F text3 CODE >133:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1133 text3 CODE >134:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
113C text3 CODE >135:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1144 text3 CODE >137:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1146 text3 CODE >138:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1147 text3 CODE >139:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1149 text3 CODE >140:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
114A text3 CODE >141:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
114B text3 CODE >142:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
114C text3 CODE >144:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1052 text2 CODE >282:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1052 text2 CODE >287:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1056 text2 CODE >288:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1069 text2 CODE >290:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
114D text1 CODE >180:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
114F text1 CODE >182:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1152 text1 CODE >183:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1196 text1 CODE >184:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
680 maintext CODE >40:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
680 maintext CODE >43:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
68F maintext CODE >44:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
691 maintext CODE >45:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
692 maintext CODE >47:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
694 maintext CODE >48:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
698 maintext CODE >49:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6A9 maintext CODE >50:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6BB maintext CODE >51:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6CD maintext CODE >52:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6CF maintext CODE >54:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6CF maintext CODE >56:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6D1 maintext CODE >57:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6D4 maintext CODE >59:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6D8 maintext CODE >60:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6DC maintext CODE >62:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6E5 maintext CODE >64:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6E7 maintext CODE >65:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6E8 maintext CODE >66:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6E9 maintext CODE >67:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6EB maintext CODE >68:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6EC maintext CODE >69:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6F0 maintext CODE >70:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6F2 maintext CODE >73:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6F4 maintext CODE >74:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6F5 maintext CODE >76:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6FD maintext CODE >78:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
6FF maintext CODE >79:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
705 maintext CODE >80:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
709 maintext CODE >81:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
70A maintext CODE >82:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
70E maintext CODE >85:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
717 maintext CODE >87:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
719 maintext CODE >88:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
71F maintext CODE >89:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
721 maintext CODE >90:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
727 maintext CODE >91:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
72B maintext CODE >94:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
734 maintext CODE >96:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
736 maintext CODE >97:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
73C maintext CODE >98:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
73F maintext CODE >99:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
740 maintext CODE >100:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
744 maintext CODE >103:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
74D maintext CODE >105:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
74F maintext CODE >106:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
755 maintext CODE >107:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
758 maintext CODE >108:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
759 maintext CODE >109:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
75D maintext CODE >112:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
766 maintext CODE >114:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
768 maintext CODE >115:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
76A maintext CODE >116:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
76B maintext CODE >117:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
76E maintext CODE >120:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
777 maintext CODE >122:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
779 maintext CODE >123:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
77B maintext CODE >124:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
77C maintext CODE >125:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
77F maintext CODE >128:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
788 maintext CODE >130:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
78A maintext CODE >131:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
78C maintext CODE >132:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
78D maintext CODE >133:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
790 maintext CODE >136:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
796 maintext CODE >138:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
798 maintext CODE >139:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
79B maintext CODE >140:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
79E maintext CODE >142:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
79F maintext CODE >143:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
7A2 maintext CODE >146:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
7A8 maintext CODE >148:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
7AA maintext CODE >149:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
7AC maintext CODE >54:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
102C clrtext CODE >1383:/tmp/xcXhFngUs
102C clrtext CODE >1384:/tmp/xcXhFngUs
102D clrtext CODE >1385:/tmp/xcXhFngUs
102D clrtext CODE >1386:/tmp/xcXhFngUs
102E clrtext CODE >1387:/tmp/xcXhFngUs
102F clrtext CODE >1388:/tmp/xcXhFngUs
1030 clrtext CODE >1389:/tmp/xcXhFngUs
1031 clrtext CODE >1390:/tmp/xcXhFngUs
# %SYMTAB Section
# An enumeration of all symbols in the program.
# The beginning of the section is indicated by %SYMTAB.
# Each line describes a single symbol as follows:
#    <label> <value> [-]<load-adj> <class> <space> <psect> <file-name>
# The value and load-adj are both in unqualified hexadecimal.
# All other numeric values are in decimal.  The load-adj is the
# quantity one needs to add to the symbol value in order to obtain the load
# address of the symbol.  This value may be signed. If the symbol
# was defined in a psect then <psect> will be "-". File-name
# is the name of the object file in which the symbol was defined.
%SYMTAB
___latbits 2 0 ABS 0 - dist/default/production/ui_board.X.production.obj
tc_int@multiplex_sel 78 0 COMMON 1 bssCOMMON dist/default/production/ui_board.X.production.obj
__end_ofleds_shift@off 301A 0 STRCODE 0 stringtext1 dist/default/production/ui_board.X.production.obj
__Hspace_0 8009 0 ABS 0 - -
__Hspace_1 1E9 0 ABS 0 - -
__Hspace_2 0 0 ABS 0 - -
__Hspace_3 0 0 ABS 0 - -
__CFG_IESO$OFF 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__size_of_leds_amp_sel 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_g_shift 1D4 0 BANK3 1 bssBANK3 dist/default/production/ui_board.X.production.obj
__Heeprom_data 0 0 EEDATA 3 eeprom_data -
__CFG_MCLRE$ON 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__Hstrings 0 0 ABS 0 strings -
float_to_bcd@i_7s C8 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
___sp 0 0 STACK 2 stack /tmp/xcX5Y7Rvk.obj
_init 220C 0 CODE 0 text3 dist/default/production/ui_board.X.production.obj
_main D00 0 CODE 0 maintext dist/default/production/ui_board.X.production.obj
btemp 7E 0 ABS 0 - dist/default/production/ui_board.X.production.obj
start 5C2 0 CODE 0 init /tmp/xcX5Y7Rvk.obj
___flmul@aexp 48 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
___flmul@bexp 4D 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
___flmul@prod 4E 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
___flmul@sign 47 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
___flmul@temp 52 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__size_of___fldiv 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__size_of___flmul 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__size_of___flneg 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__size_of___fltol 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__size_of_init 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__size_of_main 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__size_of___lldiv 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__size_of___llmod 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__HbssCOMMON 0 0 ABS 0 bssCOMMON -
display@hys_buf D2 0 BANK1 1 bssBANK1 dist/default/production/ui_board.X.production.obj
__end_of_leds_amp_sel 253A 0 CODE 0 text6 dist/default/production/ui_board.X.production.obj
__size_of_char_to_7seg 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_OPTION_REGbits 95 0 ABS 0 - dist/default/production/ui_board.X.production.obj
suffix_to_leds@on 34 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__Hpowerup 0 0 CODE 0 powerup -
suffix_to_leds@disp_nr 31 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
send_config@config 36 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__size_of_get_result 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__size_of_suffix_to_leds 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
float_to_bcd@dp_pos CE 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
intlevel0 0 0 ENTRY 0 functab /tmp/xcX5Y7Rvk.obj
intlevel1 0 0 ENTRY 0 functab /tmp/xcX5Y7Rvk.obj
intlevel2 0 0 ENTRY 0 functab /tmp/xcX5Y7Rvk.obj
intlevel3 0 0 ENTRY 0 functab /tmp/xcX5Y7Rvk.obj
intlevel4 0 0 ENTRY 0 functab /tmp/xcX5Y7Rvk.obj
intlevel5 0 0 ENTRY 0 functab /tmp/xcX5Y7Rvk.obj
__LbssCOMMON 0 0 ABS 0 bssCOMMON -
__end_of_char_to_7seg 220C 0 CODE 0 text12 dist/default/production/ui_board.X.production.obj
_OSCCONbits 99 0 ABS 0 - dist/default/production/ui_board.X.production.obj
wtemp0 7E 0 ABS 0 - dist/default/production/ui_board.X.production.obj
___llmod@divisor 31 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__Hfunctab 0 0 ENTRY 0 functab -
__Hclrtext 0 0 ABS 0 clrtext -
_ANSELA 18C 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_ANSELB 18D 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_ANSELC 18E 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__end_of__Umul8_16 20A4 0 CODE 0 text18 dist/default/production/ui_board.X.production.obj
__size_of_leds_fq_sel 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
suffix_to_leds@suffix 32 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__size_of__Umul8_16 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
float_to_bcd@float_num B2 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
_display 5EE 0 CODE 0 text9 dist/default/production/ui_board.X.production.obj
__end_of___flge 2946 0 CODE 0 text19 dist/default/production/ui_board.X.production.obj
leds_fq_sel@fq_sel 32 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
leds_fq_sel@on 3022 0 STRCODE 0 stringtext6 dist/default/production/ui_board.X.production.obj
main@del 1C2 0 BANK3 1 cstackBANK3 dist/default/production/ui_board.X.production.obj
__Lmaintext 0 0 ABS 0 maintext -
___fldiv@aexp B1 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
___fldiv@bexp B0 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
___fldiv@sign A5 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
_float_to_bcd 196E 0 CODE 0 text11 dist/default/production/ui_board.X.production.obj
__Umul8_16 2064 0 CODE 0 text18 dist/default/production/ui_board.X.production.obj
__end_of_send_config 232E 0 CODE 0 text1 dist/default/production/ui_board.X.production.obj
__end_of___fldiv 1516 0 CODE 0 text20 dist/default/production/ui_board.X.production.obj
__end_of___flmul 196E 0 CODE 0 text17 dist/default/production/ui_board.X.production.obj
__end_of___flneg 102E 0 CODE 0 text16 dist/default/production/ui_board.X.production.obj
__end_of___fltol 242C 0 CODE 0 text15 dist/default/production/ui_board.X.production.obj
__end_of___lldiv 1000 0 CODE 0 text14 dist/default/production/ui_board.X.production.obj
__end_of___llmod 217E 0 CODE 0 text13 dist/default/production/ui_board.X.production.obj
get_res_double@var_size 3028 0 STRCODE 0 stringtext9 dist/default/production/ui_board.X.production.obj
float_to_bcd@disp_pt B6 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
float_to_bcd@suffix B7 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
__Umul8_16@multiplicand 31 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__size_of_leds_shift 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
___fldiv@a 54 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
___fldiv@b 58 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
___flmul@a 3E 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
___flmul@b 3A 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
___lldiv@counter 48 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__CFG_FCMEN$OFF 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
start_initialization 5C6 0 CODE 0 cinit dist/default/production/ui_board.X.production.obj
_TRISAbits 8C 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_TRISBbits 8D 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_TRISCbits 8E 0 ABS 0 - dist/default/production/ui_board.X.production.obj
float_to_bcd@ext C9 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
___lldiv@dividend 3F 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__size_of_float_to_bcd 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_display$661 130 0 BANK2 1 cstackBANK2 dist/default/production/ui_board.X.production.obj
_display$662 134 0 BANK2 1 cstackBANK2 dist/default/production/ui_board.X.production.obj
_display$663 138 0 BANK2 1 cstackBANK2 dist/default/production/ui_board.X.production.obj
_display$664 13C 0 BANK2 1 cstackBANK2 dist/default/production/ui_board.X.production.obj
_display$665 140 0 BANK2 1 cstackBANK2 dist/default/production/ui_board.X.production.obj
_display$666 144 0 BANK2 1 cstackBANK2 dist/default/production/ui_board.X.production.obj
clear_ram0 2058 0 CODE 0 clrtext dist/default/production/ui_board.X.production.obj
__pcstackBANK0 20 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__pcstackBANK1 A0 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
__pcstackBANK2 120 0 BANK2 1 cstackBANK2 dist/default/production/ui_board.X.production.obj
__pcstackBANK3 1A0 0 BANK3 1 cstackBANK3 dist/default/production/ui_board.X.production.obj
init@config 33 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
char_to_7seg@seg_char 32 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
display@last_disp_format D1 0 BANK1 1 bssBANK1 dist/default/production/ui_board.X.production.obj
___int_sp 0 0 STACK 2 stack /tmp/xcX5Y7Rvk.obj
__end_of_float_to_bcd 2000 0 CODE 0 text11 dist/default/production/ui_board.X.production.obj
__Hbank0 0 0 ABS 0 bank0 -
__Hbank1 0 0 ABS 0 bank1 -
__Hbank2 0 0 ABS 0 bank2 -
__Hbank3 0 0 ABS 0 bank3 -
__Hbank4 0 0 ABS 0 bank4 -
__Hbank5 0 0 ABS 0 bank5 -
__Hbank6 0 0 ABS 0 bank6 -
__Hbank7 0 0 BANK7 1 bank7 -
__Hbank8 0 0 BANK8 1 bank8 -
__Hbank9 0 0 BANK9 1 bank9 -
__Hcinit 5EE 0 CODE 0 cinit -
get_res_double@temp_int32 3A 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__Hidloc 0 0 IDLOC 0 idloc -
_get_res_double 253A 0 CODE 0 text8 dist/default/production/ui_board.X.production.obj
__Hsfr10 0 0 ABS 0 sfr10 -
__Hsfr11 0 0 ABS 0 sfr11 -
__Hsfr12 0 0 ABS 0 sfr12 -
__Hsfr13 0 0 ABS 0 sfr13 -
__Hsfr14 0 0 ABS 0 sfr14 -
__Hsfr15 0 0 ABS 0 sfr15 -
__Hsfr16 0 0 ABS 0 sfr16 -
__Hsfr17 0 0 ABS 0 sfr17 -
__Hsfr18 0 0 ABS 0 sfr18 -
__Hsfr19 0 0 ABS 0 sfr19 -
__Hsfr20 0 0 ABS 0 sfr20 -
__Hsfr21 0 0 ABS 0 sfr21 -
__Hsfr22 0 0 ABS 0 sfr22 -
__Hsfr23 0 0 ABS 0 sfr23 -
__Hsfr24 0 0 ABS 0 sfr24 -
__Hsfr25 0 0 ABS 0 sfr25 -
__Hsfr26 0 0 ABS 0 sfr26 -
__Hsfr27 0 0 ABS 0 sfr27 -
__Hsfr28 0 0 ABS 0 sfr28 -
__Hsfr29 0 0 ABS 0 sfr29 -
__Hsfr30 0 0 ABS 0 sfr30 -
__Hsfr31 0 0 ABS 0 sfr31 -
__Hstack 0 0 STACK 2 stack -
__end_of_tc_int 5C2 0 CODE 0 intentry dist/default/production/ui_board.X.production.obj
__Hbank10 0 0 BANK10 1 bank10 -
__Hbank11 0 0 BANK11 1 bank11 -
__Hbank12 0 0 BANK12 1 bank12 -
__Hbank13 0 0 BANK13 1 bank13 -
__Hbank14 0 0 BANK14 1 bank14 -
__Hbank15 0 0 BANK15 1 bank15 -
__Hbank16 0 0 BANK16 1 bank16 -
__Hbank17 0 0 BANK17 1 bank17 -
__Hbank18 0 0 BANK18 1 bank18 -
__Hbank19 0 0 BANK19 1 bank19 -
__Hbank20 0 0 BANK20 1 bank20 -
__Hbank21 0 0 BANK21 1 bank21 -
__Hbank22 0 0 BANK22 1 bank22 -
__Hbank23 0 0 BANK23 1 bank23 -
__Hbank24 0 0 BANK24 1 bank24 -
__Hbank25 0 0 BANK25 1 bank25 -
__Hbank26 0 0 BANK26 1 bank26 -
__Hbank27 0 0 BANK27 1 bank27 -
__Hbank28 0 0 BANK28 1 bank28 -
__Hbank29 0 0 BANK29 1 bank29 -
__Hbank30 0 0 BANK30 1 bank30 -
__Hbank31 0 0 BANK31 1 bank31 -
__Hbigram 0 0 ABS 0 bigram -
__Hmaintext 0 0 ABS 0 maintext -
suffix_to_leds@off 33 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
_display$1030 120 0 BANK2 1 cstackBANK2 dist/default/production/ui_board.X.production.obj
_display$1031 124 0 BANK2 1 cstackBANK2 dist/default/production/ui_board.X.production.obj
_display$1032 128 0 BANK2 1 cstackBANK2 dist/default/production/ui_board.X.production.obj
_display$1033 12C 0 BANK2 1 cstackBANK2 dist/default/production/ui_board.X.production.obj
__CFG_FOSC$INTOSC 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__Hcommon 0 0 ABS 0 common -
__Hconfig 10012 0 CONFIG 0 config -
__Lbank0 0 0 ABS 0 bank0 -
__Lbank1 0 0 ABS 0 bank1 -
__Lbank2 0 0 ABS 0 bank2 -
__Lbank3 0 0 ABS 0 bank3 -
__Lbank4 0 0 ABS 0 bank4 -
__Lbank5 0 0 ABS 0 bank5 -
__Lbank6 0 0 ABS 0 bank6 -
__Lbank7 0 0 BANK7 1 bank7 -
__Lbank8 0 0 BANK8 1 bank8 -
__Lbank9 0 0 BANK9 1 bank9 -
__Lcinit 5C6 0 CODE 0 cinit -
__Lidloc 0 0 IDLOC 0 idloc -
__Lsfr10 0 0 ABS 0 sfr10 -
__Lsfr11 0 0 ABS 0 sfr11 -
__Lsfr12 0 0 ABS 0 sfr12 -
__Lsfr13 0 0 ABS 0 sfr13 -
__Lsfr14 0 0 ABS 0 sfr14 -
__Lsfr15 0 0 ABS 0 sfr15 -
__Lsfr16 0 0 ABS 0 sfr16 -
__Lsfr17 0 0 ABS 0 sfr17 -
__Lsfr18 0 0 ABS 0 sfr18 -
__Lsfr19 0 0 ABS 0 sfr19 -
__Lsfr20 0 0 ABS 0 sfr20 -
__Lsfr21 0 0 ABS 0 sfr21 -
__Lsfr22 0 0 ABS 0 sfr22 -
__Lsfr23 0 0 ABS 0 sfr23 -
__Lsfr24 0 0 ABS 0 sfr24 -
__Lsfr25 0 0 ABS 0 sfr25 -
__Lsfr26 0 0 ABS 0 sfr26 -
__Lsfr27 0 0 ABS 0 sfr27 -
__Lsfr28 0 0 ABS 0 sfr28 -
__Lsfr29 0 0 ABS 0 sfr29 -
__Lsfr30 0 0 ABS 0 sfr30 -
__Lsfr31 0 0 ABS 0 sfr31 -
__Lstack 0 0 STACK 2 stack -
___flmul@grs 49 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
char_to_7seg@seg_decoded 33 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
_PORTCbits E 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_INTCONbits B 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_leds_disp_format 2C5A 0 CODE 0 text5 dist/default/production/ui_board.X.production.obj
__Habs1 0 0 ABS 0 abs1 -
__Hcode 0 0 ABS 0 code -
__Hinit 5C2 0 CODE 0 init -
__Hsfr0 0 0 ABS 0 sfr0 -
__Hsfr1 0 0 ABS 0 sfr1 -
__Hsfr2 0 0 ABS 0 sfr2 -
__Hsfr3 0 0 ABS 0 sfr3 -
__Hsfr4 0 0 ABS 0 sfr4 -
__Hsfr5 0 0 ABS 0 sfr5 -
__Hsfr6 0 0 ABS 0 sfr6 -
__Hsfr7 0 0 ABS 0 sfr7 -
__Hsfr8 0 0 ABS 0 sfr8 -
__Hsfr9 0 0 ABS 0 sfr9 -
__Htext 0 0 ABS 0 text -
__Labs1 0 0 ABS 0 abs1 -
__Lcode 0 0 ABS 0 code -
__Linit 5C2 0 CODE 0 init -
__Lsfr0 0 0 ABS 0 sfr0 -
__Lsfr1 0 0 ABS 0 sfr1 -
__Lsfr2 0 0 ABS 0 sfr2 -
__Lsfr3 0 0 ABS 0 sfr3 -
__Lsfr4 0 0 ABS 0 sfr4 -
__Lsfr5 0 0 ABS 0 sfr5 -
__Lsfr6 0 0 ABS 0 sfr6 -
__Lsfr7 0 0 ABS 0 sfr7 -
__Lsfr8 0 0 ABS 0 sfr8 -
__Lsfr9 0 0 ABS 0 sfr9 -
__Ltext 0 0 ABS 0 text -
__pstringtext1 3018 0 STRCODE 0 stringtext1 dist/default/production/ui_board.X.production.obj
__pstringtext2 301A 0 STRCODE 0 stringtext2 dist/default/production/ui_board.X.production.obj
__pstringtext3 301C 0 STRCODE 0 stringtext3 dist/default/production/ui_board.X.production.obj
__pstringtext4 301E 0 STRCODE 0 stringtext4 dist/default/production/ui_board.X.production.obj
__pstringtext5 3020 0 STRCODE 0 stringtext5 dist/default/production/ui_board.X.production.obj
__pstringtext6 3022 0 STRCODE 0 stringtext6 dist/default/production/ui_board.X.production.obj
__pstringtext7 3024 0 STRCODE 0 stringtext7 dist/default/production/ui_board.X.production.obj
__pstringtext8 3026 0 STRCODE 0 stringtext8 dist/default/production/ui_board.X.production.obj
__pstringtext9 3028 0 STRCODE 0 stringtext9 dist/default/production/ui_board.X.production.obj
leds_disp_format@disp_format 32 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
___flge 27AE 0 CODE 0 text19 dist/default/production/ui_board.X.production.obj
leds_amp_sel@on 301E 0 STRCODE 0 stringtext4 dist/default/production/ui_board.X.production.obj
__LcstackBANK0 0 0 ABS 0 cstackBANK0 -
__LcstackBANK1 0 0 ABS 0 cstackBANK1 -
__LcstackBANK2 0 0 ABS 0 cstackBANK2 -
__LcstackBANK3 0 0 ABS 0 cstackBANK3 -
int$flags 7E 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__HcstackCOMMON 0 0 ABS 0 cstackCOMMON -
__S0 8009 0 ABS 0 - -
__S1 1E9 0 ABS 0 - -
__S2 0 0 ABS 0 - -
__end_ofleds_fq_sel@on 3024 0 STRCODE 0 stringtext6 dist/default/production/ui_board.X.production.obj
tc_int@i_shift 74 0 COMMON 1 cstackCOMMON dist/default/production/ui_board.X.production.obj
main@del_168 1C4 0 BANK3 1 cstackBANK3 dist/default/production/ui_board.X.production.obj
main@del_169 1C6 0 BANK3 1 cstackBANK3 dist/default/production/ui_board.X.production.obj
__size_of_send_config 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_leds_fq_sel 264C 0 CODE 0 text4 dist/default/production/ui_board.X.production.obj
__end_of_get_res_double 264C 0 CODE 0 text8 dist/default/production/ui_board.X.production.obj
tc_int@keys_tmp 75 0 COMMON 1 cstackCOMMON dist/default/production/ui_board.X.production.obj
__CFG_BOREN$ON 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__Lintentry 8 0 CODE 0 intentry -
___lldiv@divisor 3B 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
?_get_res_double 31 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__end_ofget_res_double@var_size 302A 0 STRCODE 0 stringtext9 dist/default/production/ui_board.X.production.obj
reset_vec 0 0 CODE 0 reset_vec /tmp/xcX5Y7Rvk.obj
leds_fq_sel@off 3020 0 STRCODE 0 stringtext5 dist/default/production/ui_board.X.production.obj
_suffix_to_leds 2946 0 CODE 0 text10 dist/default/production/ui_board.X.production.obj
__size_of___flge 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__end_ofleds_amp_sel@off 301E 0 STRCODE 0 stringtext3 dist/default/production/ui_board.X.production.obj
__LbssBANK1 0 0 ABS 0 bssBANK1 -
__LbssBANK3 0 0 ABS 0 bssBANK3 -
__Lstringtext1 0 0 ABS 0 stringtext1 -
__Lstringtext2 0 0 ABS 0 stringtext2 -
__Lstringtext3 0 0 ABS 0 stringtext3 -
__Lstringtext4 0 0 ABS 0 stringtext4 -
__Lstringtext5 0 0 ABS 0 stringtext5 -
__Lstringtext6 0 0 ABS 0 stringtext6 -
__Lstringtext7 0 0 ABS 0 stringtext7 -
__Lstringtext8 0 0 ABS 0 stringtext8 -
__Lstringtext9 0 0 ABS 0 stringtext9 -
__end_ofleds_amp_sel@on 3020 0 STRCODE 0 stringtext4 dist/default/production/ui_board.X.production.obj
_RCSTAbits 19D 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__ptext10 2946 0 CODE 0 text10 dist/default/production/ui_board.X.production.obj
__ptext11 196E 0 CODE 0 text11 dist/default/production/ui_board.X.production.obj
__ptext12 217E 0 CODE 0 text12 dist/default/production/ui_board.X.production.obj
__ptext13 20F8 0 CODE 0 text13 dist/default/production/ui_board.X.production.obj
__ptext14 F5A 0 CODE 0 text14 dist/default/production/ui_board.X.production.obj
__ptext15 232E 0 CODE 0 text15 dist/default/production/ui_board.X.production.obj
__ptext16 101A 0 CODE 0 text16 dist/default/production/ui_board.X.production.obj
__ptext17 1516 0 CODE 0 text17 dist/default/production/ui_board.X.production.obj
__ptext18 2064 0 CODE 0 text18 dist/default/production/ui_board.X.production.obj
__ptext19 27AE 0 CODE 0 text19 dist/default/production/ui_board.X.production.obj
__ptext20 1142 0 CODE 0 text20 dist/default/production/ui_board.X.production.obj
float_to_bcd@hys_buf B8 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
___fldiv 1142 0 CODE 0 text20 dist/default/production/ui_board.X.production.obj
___flmul 1516 0 CODE 0 text17 dist/default/production/ui_board.X.production.obj
___flneg 101A 0 CODE 0 text16 dist/default/production/ui_board.X.production.obj
___fltol 232E 0 CODE 0 text15 dist/default/production/ui_board.X.production.obj
___lldiv F5A 0 CODE 0 text14 dist/default/production/ui_board.X.production.obj
___llmod 20F8 0 CODE 0 text13 dist/default/production/ui_board.X.production.obj
__Lbank10 0 0 BANK10 1 bank10 -
__Lbank11 0 0 BANK11 1 bank11 -
__Lbank12 0 0 BANK12 1 bank12 -
__Lbank13 0 0 BANK13 1 bank13 -
__Lbank14 0 0 BANK14 1 bank14 -
__Lbank15 0 0 BANK15 1 bank15 -
__Lbank16 0 0 BANK16 1 bank16 -
__Lbank17 0 0 BANK17 1 bank17 -
__Lbank18 0 0 BANK18 1 bank18 -
__Lbank19 0 0 BANK19 1 bank19 -
__Lbank20 0 0 BANK20 1 bank20 -
__Lbank21 0 0 BANK21 1 bank21 -
__Lbank22 0 0 BANK22 1 bank22 -
__Lbank23 0 0 BANK23 1 bank23 -
__Lbank24 0 0 BANK24 1 bank24 -
__Lbank25 0 0 BANK25 1 bank25 -
__Lbank26 0 0 BANK26 1 bank26 -
__Lbank27 0 0 BANK27 1 bank27 -
__Lbank28 0 0 BANK28 1 bank28 -
__Lbank29 0 0 BANK29 1 bank29 -
__Lbank30 0 0 BANK30 1 bank30 -
__Lbank31 0 0 BANK31 1 bank31 -
__pmaintext D00 0 CODE 0 maintext dist/default/production/ui_board.X.production.obj
_ui_state 1D5 0 BANK3 1 bssBANK3 dist/default/production/ui_board.X.production.obj
__Lbigram 0 0 ABS 0 bigram -
__CFG_BORV$LO 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__Umul8_16@multiplier 39 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__Lcommon 0 0 ABS 0 common -
__Lconfig 1000E 0 CONFIG 0 config -
__CFG_CP$OFF 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__CFG_WDTE$OFF 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__end_of_leds_disp_format 3000 0 CODE 0 text5 dist/default/production/ui_board.X.production.obj
_LATAbits 10C 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_LATCbits 10E 0 ABS 0 - dist/default/production/ui_board.X.production.obj
___fldiv@grs AC 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
___fldiv@rem A6 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
get_result@results 42 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
main@F4144 1CE 0 BANK3 1 bssBANK3 dist/default/production/ui_board.X.production.obj
tc_int@keys_tmp_bck 77 0 COMMON 1 bssCOMMON dist/default/production/ui_board.X.production.obj
__size_of_leds_disp_format 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_tc_int 8 0 CODE 0 intentry dist/default/production/ui_board.X.production.obj
___fldiv@new_exp AA 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
__size_of_display 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
stackhi 21EF 0 ABS 0 - /tmp/xcX5Y7Rvk.obj
stacklo 2139 0 ABS 0 - /tmp/xcX5Y7Rvk.obj
_get_result 102E 0 CODE 0 text7 dist/default/production/ui_board.X.production.obj
__end_ofleds_fq_sel@off 3022 0 STRCODE 0 stringtext5 dist/default/production/ui_board.X.production.obj
__end_of_suffix_to_leds 2C5A 0 CODE 0 text10 dist/default/production/ui_board.X.production.obj
leds_amp_sel@off 301C 0 STRCODE 0 stringtext3 dist/default/production/ui_board.X.production.obj
__Lspace_0 0 0 ABS 0 - -
__Lspace_1 0 0 ABS 0 - -
__Lspace_2 0 0 ABS 0 - -
__Lspace_3 0 0 ABS 0 - -
__pbssCOMMON 76 0 COMMON 1 bssCOMMON dist/default/production/ui_board.X.production.obj
main@config 1C8 0 BANK3 1 cstackBANK3 dist/default/production/ui_board.X.production.obj
tc_int@disp_register 70 0 COMMON 1 cstackCOMMON dist/default/production/ui_board.X.production.obj
__HcstackBANK0 0 0 ABS 0 cstackBANK0 -
__HcstackBANK1 0 0 ABS 0 cstackBANK1 -
__HcstackBANK2 0 0 ABS 0 cstackBANK2 -
__HcstackBANK3 0 0 ABS 0 cstackBANK3 -
__Umul8_16@product 35 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
leds_disp_format@off 3024 0 STRCODE 0 stringtext7 dist/default/production/ui_board.X.production.obj
___flge@ff1 54 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
___flge@ff2 58 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
_PIR1bits 11 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__Lend_init 5C2 0 CODE 0 end_init -
__CFG_LVP$ON 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__LcstackCOMMON 0 0 ABS 0 cstackCOMMON -
___fltol@exp1 3B 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
main@results 1A1 0 BANK3 1 cstackBANK3 dist/default/production/ui_board.X.production.obj
end_of_initialization 5E6 0 CODE 0 cinit dist/default/production/ui_board.X.production.obj
leds_shift@off 3018 0 STRCODE 0 stringtext1 dist/default/production/ui_board.X.production.obj
__Hintentry 5C2 0 CODE 0 intentry -
__CFG_STVREN$ON 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__Lstrings 0 0 ABS 0 strings -
?___fldiv 54 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
?___flmul 3A 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
?___flneg 31 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
?___fltol 31 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
?___lldiv 3B 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
?___llmod 31 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
leds_shift@on 301A 0 STRCODE 0 stringtext2 dist/default/production/ui_board.X.production.obj
__Hreset_vec 4 0 CODE 0 reset_vec -
__HbssBANK1 0 0 ABS 0 bssBANK1 -
__HbssBANK3 0 0 ABS 0 bssBANK3 -
__size_of_tc_int 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
display@config CF 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
___flneg@f1 31 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__ptext1 229A 0 CODE 0 text1 dist/default/production/ui_board.X.production.obj
__ptext2 20A4 0 CODE 0 text2 dist/default/production/ui_board.X.production.obj
__ptext3 220C 0 CODE 0 text3 dist/default/production/ui_board.X.production.obj
__ptext4 264C 0 CODE 0 text4 dist/default/production/ui_board.X.production.obj
__ptext5 2C5A 0 CODE 0 text5 dist/default/production/ui_board.X.production.obj
__ptext6 242C 0 CODE 0 text6 dist/default/production/ui_board.X.production.obj
__ptext7 102E 0 CODE 0 text7 dist/default/production/ui_board.X.production.obj
__ptext8 253A 0 CODE 0 text8 dist/default/production/ui_board.X.production.obj
__ptext9 5EE 0 CODE 0 text9 dist/default/production/ui_board.X.production.obj
get_res_double@i_shift 3E 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
?__Umul8_16 31 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__end_ofleds_disp_format@on 3028 0 STRCODE 0 stringtext8 dist/default/production/ui_board.X.production.obj
main@locked 1C1 0 BANK3 1 cstackBANK3 dist/default/production/ui_board.X.production.obj
__Lpowerup 0 0 CODE 0 powerup -
__Leeprom_data 0 0 EEDATA 3 eeprom_data -
__Umul8_16@word_mpld 37 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
___fltol@sign1 3A 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__end_of_get_result 1142 0 CODE 0 text7 dist/default/production/ui_board.X.production.obj
float_to_bcd@int_num CA 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
__Lreset_vec 0 0 CODE 0 reset_vec -
__Hstringtext1 0 0 ABS 0 stringtext1 -
__Hstringtext2 0 0 ABS 0 stringtext2 -
__Hstringtext3 0 0 ABS 0 stringtext3 -
__Hstringtext4 0 0 ABS 0 stringtext4 -
__Hstringtext5 0 0 ABS 0 stringtext5 -
__Hstringtext6 0 0 ABS 0 stringtext6 -
__Hstringtext7 0 0 ABS 0 stringtext7 -
__Hstringtext8 0 0 ABS 0 stringtext8 -
__Hstringtext9 0 0 ABS 0 stringtext9 -
__CFG_LPBOR$OFF 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
___fltol@f1 31 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__CFG_CLKOUTEN$OFF 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_leds_shift 20A4 0 CODE 0 text2 dist/default/production/ui_board.X.production.obj
__end_of__initialization 5E6 0 CODE 0 cinit dist/default/production/ui_board.X.production.obj
__Lfunctab 0 0 ENTRY 0 functab -
float_to_bcd@disp_arr C2 0 BANK1 1 cstackBANK1 dist/default/production/ui_board.X.production.obj
__end_of_display D00 0 CODE 0 text9 dist/default/production/ui_board.X.production.obj
_send_config 229A 0 CODE 0 text1 dist/default/production/ui_board.X.production.obj
__Lclrtext 0 0 ABS 0 clrtext -
tc_int@debounce 76 0 COMMON 1 bssCOMMON dist/default/production/ui_board.X.production.obj
leds_disp_format@on 3026 0 STRCODE 0 stringtext8 dist/default/production/ui_board.X.production.obj
___lldiv@quotient 44 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__pcstackCOMMON 70 0 COMMON 1 cstackCOMMON dist/default/production/ui_board.X.production.obj
_TXSTAbits 19E 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__Hend_init 5C6 0 CODE 0 end_init -
___llmod@dividend 35 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
display@results 148 0 BANK2 1 cstackBANK2 dist/default/production/ui_board.X.production.obj
___llmod@counter 3A 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__end_of_init 229A 0 CODE 0 text3 dist/default/production/ui_board.X.production.obj
__end_of_main F5A 0 CODE 0 maintext dist/default/production/ui_board.X.production.obj
__end_ofleds_shift@on 301C 0 STRCODE 0 stringtext2 dist/default/production/ui_board.X.production.obj
__end_ofleds_disp_format@off 3026 0 STRCODE 0 stringtext7 dist/default/production/ui_board.X.production.obj
_leds_amp_sel 242C 0 CODE 0 text6 dist/default/production/ui_board.X.production.obj
_RCREG 199 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_SPBRG 19B 0 ABS 0 - dist/default/production/ui_board.X.production.obj
_TXREG 19A 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__Hram 0 0 ABS 0 ram -
__Lram 0 0 ABS 0 ram -
__end_of_leds_fq_sel 27AE 0 CODE 0 text4 dist/default/production/ui_board.X.production.obj
__pintentry 8 0 CODE 0 intentry dist/default/production/ui_board.X.production.obj
leds_amp_sel@amp_sel 32 0 BANK0 1 cstackBANK0 dist/default/production/ui_board.X.production.obj
__initialization 5C6 0 CODE 0 cinit dist/default/production/ui_board.X.production.obj
__CFG_PWRTE$OFF 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__pbssBANK1 D1 0 BANK1 1 bssBANK1 dist/default/production/ui_board.X.production.obj
__pbssBANK3 1CE 0 BANK3 1 bssBANK3 dist/default/production/ui_board.X.production.obj
__size_of_get_res_double 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__CFG_WRT$OFF 0 0 ABS 0 - dist/default/production/ui_board.X.production.obj
__end_of_leds_shift 20F8 0 CODE 0 text2 dist/default/production/ui_board.X.production.obj
main@tmp_resetnextcycle 1A0 0 BANK3 1 cstackBANK3 dist/default/production/ui_board.X.production.obj
_char_to_7seg 217E 0 CODE 0 text12 dist/default/production/ui_board.X.production.obj
__pswtext1 1000 0 CONST 0 swtext1 dist/default/production/ui_board.X.production.obj
__pswtext2 3000 0 CONST 0 swtext2 dist/default/production/ui_board.X.production.obj
__pswtext3 2000 0 CONST 0 swtext3 dist/default/production/ui_board.X.production.obj
# %SPLITSTAB Section
# This section enumerates all the psect splits performed by the assembler.
# The beginning of the section is indicated by %SPLITSTAB.
# Each line is a record a particular split, where the parent psect is on
# the left and the child on the right.  Note that a child psect is always
# split form the top of the parent psect. All splits from a given parent
# are listed in the order in which they occurred.
%SPLITSTAB
# %DABS Section
# This section contains a table of all usuage of the assember
# directive DABS in the program. Each line has the following format:
#   <name> <space> <address> <size>
# If the DABS was originally labelled then that shall be <name>,
# otherwise name will be "-".  The <space> number is in decimal.
# <address> and <size> are in byte units as unqaulified hexadecimal
%DABS
- 1 7E 2
# %SEGMENTS Section
# This sections enumerates the segments of the program.  Each segment
# is described on a single line as follows:
#    <name> <space> <link address> <file address> <size> <delta>
# Addresses and size are in unqualified hexadecimal.  The link address
# and size are in units of delta. The file address is in units of bytes.
# All other numeric quantities are in decimal.
%SEGMENTS
text1 0 114D 229A 4A 2
text2 0 1052 20A4 2A 2
text3 0 1106 220C 47 2
text4 0 1326 264C B1 2
text5 0 162D 2C5A 1D3 2
text6 0 1216 242C 87 2
text7 0 817 102E 8A 2
text8 0 129D 253A 89 2
text10 0 14A3 2946 18A 2
text11 0 CB7 196E 349 2
text12 0 10BF 217E 47 2
text13 0 107C 20F8 43 2
text15 0 1197 232E 7F 2
text16 0 80D 101A A 2
text17 0 A8B 1516 22C 2
text18 0 1032 2064 20 2
text19 0 13D7 27AE CC 2
text20 0 8A1 1142 1EA 2
cstackCOMMON 1 70 70 9 1
cstackBANK0 1 20 20 3F 1
cstackBANK1 1 A0 A0 36 1
cstackBANK2 1 120 120 29 1
cstackBANK3 1 1A0 1A0 49 1
stringtext1 0 180C 3018 9 2
intentry 0 4 8 7FC 2
reset_vec 0 0 0 2 2
swtext1 0 800 1000 C 2
swtext2 0 1800 3000 C 2
swtext3 0 1000 2000 2A 2
clrtext 0 102C 2058 6 2
config 0 8007 1000E 2 2
