%CMF
# %PSECTS Section
# For each object file, details of its psects are enumerated here.
# The begining of the section is indicated by %PSECTS.  The first
# line indicates the name of the first object file, e.g.
#    $foo.obj
# Each line that follows describes a psect in that object file, until
# the next object file.  The lines that describe a psect have the
# format:
#    <psect name> <class name> <space> <link address> <load addresses> <length> <delta>
# All addresses and the length are given in unqualified hexadecimal
# in delta units.  Any other numeric values are decimal.
%PSECTS
$/tmp/xcXwsrphy.obj
reset_vec CODE 0 0 0 3 2
end_init CODE 0 2E1 2E1 2 2
config CONFIG 0 8007 8007 2 2
$dist/default/debug/ui_board.X.debug.obj
cinit CODE 0 2E3 2E3 17 2
text1 CODE 0 1188 1188 4A 2
text2 CODE 0 7CA 7CA 2E 2
text3 CODE 0 11D2 11D2 4B 2
text4 CODE 0 82E 82E B1 2
text5 CODE 0 8DF 8DF 1D3 2
text6 CODE 0 12EF 12EF 87 2
text7 CODE 0 13FF 13FF 8A 2
text8 CODE 0 1376 1376 89 2
text9 CODE 0 CDE CDE 322 2
text10 CODE 0 640 640 18A 2
text11 CODE 0 2FA 2FA 346 2
text12 CODE 0 1141 1141 47 2
text13 CODE 0 10FE 10FE 43 2
text14 CODE 0 121D 121D 53 2
text15 CODE 0 1270 1270 7F 2
text16 CODE 0 10D4 10D4 A 2
text17 CODE 0 AB2 AB2 22C 2
text18 CODE 0 10DE 10DE 20 2
text19 CODE 0 1489 1489 9A 2
text20 CODE 0 163D 163D 1C3 2
maintext CODE 0 1523 1523 11A 2
cstackCOMMON COMMON 1 70 70 6 1
cstackBANK0 BANK0 1 20 20 39 1
cstackBANK1 BANK1 1 A0 A0 37 1
cstackBANK2 BANK2 1 120 120 4E 1
stringtext1 STRCODE 0 1800 1800 1 2
stringtext2 STRCODE 0 1801 1801 1 2
stringtext3 STRCODE 0 1802 1802 1 2
stringtext4 STRCODE 0 1803 1803 1 2
stringtext5 STRCODE 0 1804 1804 1 2
stringtext6 STRCODE 0 1805 1805 1 2
stringtext7 STRCODE 0 1806 1806 1 2
stringtext8 STRCODE 0 1807 1807 1 2
stringtext9 STRCODE 0 1808 1808 1 2
intentry CODE 0 4 4 2DD 2
bssBANK0 BANK0 1 59 59 6 1
bssBANK1 BANK1 1 D7 D7 19 1
bssBANK2 BANK2 1 16E 16E 1 1
swtext1 CONST 0 1000 1000 C 2
swtext2 CONST 0 100C 100C C 2
swtext3 CONST 0 800 800 2A 2
clrtext CODE 0 7F8 7F8 6 2
bssCOMMON COMMON 1 76 76 3 1
# %UNUSED Section
# This section enumerates the unused ranges of each CLASS. Each entry
# is described on a single line as follows:
#    <class name> <range> <delta>
# Addresses given in the range are in hexadecimal and units of delta.
%UNUSED
RAM 5F-6F 1
RAM 16F-16F 1
RAM 1A0-1EF 1
RAM 220-26F 1
RAM 2A0-2EF 1
BANK0 5F-6F 1
BANK2 16F-16F 1
BANK3 1A0-1EF 1
BANK4 220-26F 1
BANK5 2A0-2EF 1
CONST 3-3 2
CONST 7FE-7FF 2
CONST 82A-82D 2
CONST 1018-10D3 2
CONST 1809-1FFF 2
ENTRY 3-3 2
ENTRY 7FE-7FF 2
ENTRY 82A-82D 2
ENTRY 1018-10D3 2
ENTRY 1809-1FFF 2
IDLOC 8000-8003 2
SFR10 500-56F 1
SFR11 580-5EF 1
SFR12 600-66F 1
SFR13 680-6EF 1
SFR14 700-76F 1
SFR15 780-7EF 1
SFR16 800-86F 1
SFR17 880-8EF 1
SFR18 900-96F 1
SFR19 980-9EF 1
SFR20 A00-A6F 1
SFR21 A80-AEF 1
SFR22 B00-B6F 1
SFR23 B80-BEF 1
SFR24 C00-C6F 1
SFR25 C80-CEF 1
SFR26 D00-D6F 1
SFR27 D80-DEF 1
SFR28 E00-E6F 1
SFR29 E80-EEF 1
SFR30 F00-F6F 1
SFR31 F80-FEF 1
STACK 20EF-21DF 1
CODE 3-3 2
CODE 7FE-7FF 2
CODE 82A-82D 2
CODE 1018-10D3 2
CODE 1809-1FFF 2
SFR0 0-1F 1
SFR1 80-9F 1
SFR2 100-11F 1
SFR3 180-19F 1
SFR4 200-21F 1
SFR5 280-29F 1
SFR6 300-36F 1
SFR7 380-3EF 1
SFR8 400-46F 1
SFR9 480-4EF 1
BIGRAM 2000-21DF 1
COMMON 79-7D 1
STRCODE 3-3 2
STRCODE 7FE-7FF 2
STRCODE 82A-82D 2
STRCODE 1018-10D3 2
STRCODE 1809-1FFF 2
STRING 3-3 2
STRING 7FE-7FF 2
STRING 82A-82D 2
STRING 1018-10D3 2
STRING 1809-1FFF 2
# %LINETAB Section
# This section enumerates the file/line to address mappings.
# The beginning of the section is indicated by %LINETAB.
# The first line indicates the name of the first object file, e.g.
#   $foo.obj
# Each line that follows describes a single mapping until the next
# object file.  Mappings have the following format:
#    <address> <psect name> <class name> ><line number>:<file name>
# The address is absolute and given given in unqualified hex 
# in delta units of the psect. All mappings within an object file
# are in ascending order of addresses.
# All other numeric values are in decimal.
%LINETAB
$dist/default/debug/ui_board.X.debug.obj
2E3 cinit CODE >1339:/tmp/xcXzfBX4R
2E3 cinit CODE >1342:/tmp/xcXzfBX4R
2E3 cinit CODE >1396:/tmp/xcXzfBX4R
2E4 cinit CODE >1397:/tmp/xcXzfBX4R
2E5 cinit CODE >1398:/tmp/xcXzfBX4R
2E6 cinit CODE >1402:/tmp/xcXzfBX4R
2E7 cinit CODE >1403:/tmp/xcXzfBX4R
2E8 cinit CODE >1404:/tmp/xcXzfBX4R
2E9 cinit CODE >1405:/tmp/xcXzfBX4R
2EA cinit CODE >1406:/tmp/xcXzfBX4R
2EB cinit CODE >1407:/tmp/xcXzfBX4R
2EC cinit CODE >1408:/tmp/xcXzfBX4R
2ED cinit CODE >1412:/tmp/xcXzfBX4R
2EE cinit CODE >1413:/tmp/xcXzfBX4R
2EF cinit CODE >1414:/tmp/xcXzfBX4R
2F0 cinit CODE >1415:/tmp/xcXzfBX4R
2F1 cinit CODE >1416:/tmp/xcXzfBX4R
2F2 cinit CODE >1417:/tmp/xcXzfBX4R
2F4 cinit CODE >1421:/tmp/xcXzfBX4R
2F5 cinit CODE >1422:/tmp/xcXzfBX4R
2F6 cinit CODE >1428:/tmp/xcXzfBX4R
2F6 cinit CODE >1430:/tmp/xcXzfBX4R
2F7 cinit CODE >1431:/tmp/xcXzfBX4R
2F8 cinit CODE >1432:/tmp/xcXzfBX4R
4 intentry CODE >184:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
4 intentry CODE >10:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
9 intentry CODE >20:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11 intentry CODE >21:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
14 intentry CODE >22:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
5D intentry CODE >23:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
60 intentry CODE >24:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A9 intentry CODE >25:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
AD intentry CODE >26:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
F6 intentry CODE >27:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
FA intentry CODE >28:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
132 intentry CODE >29:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
136 intentry CODE >30:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
17F intentry CODE >31:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
183 intentry CODE >32:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1CC intentry CODE >33:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1D0 intentry CODE >34:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
219 intentry CODE >35:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
21D intentry CODE >36:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
25C intentry CODE >39:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
262 intentry CODE >41:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
280 intentry CODE >42:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
281 intentry CODE >43:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
282 intentry CODE >39:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
289 intentry CODE >45:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
28B intentry CODE >46:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
28C intentry CODE >49:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
291 intentry CODE >50:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
292 intentry CODE >52:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
294 intentry CODE >53:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
297 intentry CODE >54:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
299 intentry CODE >55:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
29B intentry CODE >56:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
29C intentry CODE >57:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
29E intentry CODE >59:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
29F intentry CODE >60:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2A2 intentry CODE >61:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2A4 intentry CODE >62:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2A6 intentry CODE >63:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2A7 intentry CODE >64:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2A9 intentry CODE >66:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2AA intentry CODE >67:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2AD intentry CODE >68:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2AF intentry CODE >69:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2B1 intentry CODE >70:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2B2 intentry CODE >71:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2B4 intentry CODE >73:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2B5 intentry CODE >74:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2B8 intentry CODE >75:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2BA intentry CODE >76:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2BC intentry CODE >77:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2BD intentry CODE >78:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2BF intentry CODE >81:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2C3 intentry CODE >82:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2C8 intentry CODE >83:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2CC intentry CODE >85:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2CD intentry CODE >86:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2D3 intentry CODE >90:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2D8 intentry CODE >91:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2DB intentry CODE >92:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2DC intentry CODE >94:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
2DD intentry CODE >95:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
163D text20 CODE >8:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
163D text20 CODE >26:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1645 text20 CODE >27:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
164B text20 CODE >28:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
164C text20 CODE >29:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
164D text20 CODE >33:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1650 text20 CODE >35:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1653 text20 CODE >37:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
165B text20 CODE >40:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
165C text20 CODE >42:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
165D text20 CODE >43:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
165E text20 CODE >46:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1666 text20 CODE >49:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
166D text20 CODE >50:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1673 text20 CODE >51:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1674 text20 CODE >52:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1675 text20 CODE >56:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1678 text20 CODE >58:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
167B text20 CODE >60:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1683 text20 CODE >63:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1684 text20 CODE >65:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1685 text20 CODE >66:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1686 text20 CODE >69:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
168E text20 CODE >70:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
168E text20 CODE >75:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1694 text20 CODE >76:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
169C text20 CODE >77:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
16A0 text20 CODE >78:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
16A9 text20 CODE >82:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
16AC text20 CODE >83:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
16B4 text20 CODE >84:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
16BD text20 CODE >88:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
16D8 text20 CODE >91:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
16E0 text20 CODE >92:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
16E8 text20 CODE >93:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
16F0 text20 CODE >95:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
16F1 text20 CODE >96:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
16F5 text20 CODE >99:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
16F8 text20 CODE >100:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
16FF text20 CODE >101:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1706 text20 CODE >102:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1707 text20 CODE >103:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1708 text20 CODE >105:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
170F text20 CODE >111:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
171F text20 CODE >114:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1720 text20 CODE >115:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1728 text20 CODE >117:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
172E text20 CODE >96:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
172F text20 CODE >121:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1734 text20 CODE >122:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1735 text20 CODE >126:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1737 text20 CODE >127:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
173E text20 CODE >128:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
173F text20 CODE >129:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1740 text20 CODE >131:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1747 text20 CODE >132:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
174B text20 CODE >126:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
174C text20 CODE >138:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
174D text20 CODE >139:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
174F text20 CODE >140:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1768 text20 CODE >141:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
176A text20 CODE >143:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
176A text20 CODE >144:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
176D text20 CODE >145:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
176F text20 CODE >149:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1772 text20 CODE >150:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
177A text20 CODE >151:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
177C text20 CODE >152:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17A2 text20 CODE >153:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17A6 text20 CODE >158:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17B3 text20 CODE >159:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17B8 text20 CODE >160:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17C0 text20 CODE >161:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17C0 text20 CODE >164:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17CE text20 CODE >165:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17D1 text20 CODE >166:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17D9 text20 CODE >168:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17DA text20 CODE >169:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17DA text20 CODE >172:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17E1 text20 CODE >174:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17E3 text20 CODE >175:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17E4 text20 CODE >176:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17E5 text20 CODE >179:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17EB text20 CODE >180:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17EB text20 CODE >181:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17F1 text20 CODE >182:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
17F7 text20 CODE >183:/opt/microchip/xc8/v1.45/sources/common/sprcdiv.c
1489 text19 CODE >4:/opt/microchip/xc8/v1.45/sources/common/flge.c
1489 text19 CODE >7:/opt/microchip/xc8/v1.45/sources/common/flge.c
149C text19 CODE >8:/opt/microchip/xc8/v1.45/sources/common/flge.c
14A4 text19 CODE >9:/opt/microchip/xc8/v1.45/sources/common/flge.c
14B6 text19 CODE >10:/opt/microchip/xc8/v1.45/sources/common/flge.c
14BE text19 CODE >12:/opt/microchip/xc8/v1.45/sources/common/flge.c
14C0 text19 CODE >13:/opt/microchip/xc8/v1.45/sources/common/flge.c
14E7 text19 CODE >14:/opt/microchip/xc8/v1.45/sources/common/flge.c
14E9 text19 CODE >15:/opt/microchip/xc8/v1.45/sources/common/flge.c
1510 text19 CODE >16:/opt/microchip/xc8/v1.45/sources/common/flge.c
1512 text19 CODE >17:/opt/microchip/xc8/v1.45/sources/common/flge.c
1514 text19 CODE >18:/opt/microchip/xc8/v1.45/sources/common/flge.c
10DE text18 CODE >4:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
10E0 text18 CODE >5:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
10E2 text18 CODE >6:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
10E9 text18 CODE >51:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
10EB text18 CODE >52:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
10EF text18 CODE >53:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
10EF text18 CODE >54:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
10F4 text18 CODE >55:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
10F6 text18 CODE >56:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
10F9 text18 CODE >59:/opt/microchip/xc8/v1.45/sources/common/Umul8_16.c
AB2 text17 CODE >8:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AB2 text17 CODE >17:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AB8 text17 CODE >18:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
ABC text17 CODE >19:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
ABD text17 CODE >20:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
ABE text17 CODE >24:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AC1 text17 CODE >26:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AC4 text17 CODE >28:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
ACC text17 CODE >31:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
ACD text17 CODE >33:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
ACE text17 CODE >36:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AD6 text17 CODE >39:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
ADB text17 CODE >40:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
ADF text17 CODE >41:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AE0 text17 CODE >42:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AE1 text17 CODE >45:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AE4 text17 CODE >48:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AE7 text17 CODE >50:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AEF text17 CODE >53:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AF0 text17 CODE >54:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AF1 text17 CODE >57:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AF9 text17 CODE >65:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
AFE text17 CODE >66:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B07 text17 CODE >119:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B14 text17 CODE >120:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B21 text17 CODE >121:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B2E text17 CODE >122:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B3B text17 CODE >123:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B48 text17 CODE >124:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B55 text17 CODE >125:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B62 text17 CODE >126:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B6F text17 CODE >127:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B7C text17 CODE >128:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B83 text17 CODE >129:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B90 text17 CODE >130:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
B97 text17 CODE >131:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BA4 text17 CODE >132:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BAB text17 CODE >133:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BB2 text17 CODE >134:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BBF text17 CODE >135:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BC6 text17 CODE >136:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BD3 text17 CODE >137:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BDA text17 CODE >138:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BE7 text17 CODE >139:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BEE text17 CODE >140:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
BFB text17 CODE >141:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C10 text17 CODE >145:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C27 text17 CODE >146:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C2E text17 CODE >149:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C39 text17 CODE >152:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C3B text17 CODE >153:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C42 text17 CODE >154:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C43 text17 CODE >155:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C44 text17 CODE >157:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C4B text17 CODE >158:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C4F text17 CODE >152:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C50 text17 CODE >163:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C51 text17 CODE >164:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C53 text17 CODE >165:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C64 text17 CODE >166:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C65 text17 CODE >169:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C67 text17 CODE >170:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C69 text17 CODE >174:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C6C text17 CODE >175:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C74 text17 CODE >176:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C76 text17 CODE >177:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C8E text17 CODE >178:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C92 text17 CODE >183:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
C9D text17 CODE >184:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CA6 text17 CODE >185:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CA7 text17 CODE >187:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CB3 text17 CODE >188:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CBC text17 CODE >190:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CBD text17 CODE >191:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CBE text17 CODE >194:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CC3 text17 CODE >195:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CCB text17 CODE >196:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CCC text17 CODE >197:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CCD text17 CODE >199:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CD1 text17 CODE >200:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CD1 text17 CODE >201:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
CD5 text17 CODE >203:/opt/microchip/xc8/v1.45/sources/common/sprcmul.c
10D4 text16 CODE >15:/opt/microchip/xc8/v1.45/sources/common/flneg.c
10D4 text16 CODE >17:/opt/microchip/xc8/v1.45/sources/common/flneg.c
10DB text16 CODE >18:/opt/microchip/xc8/v1.45/sources/common/flneg.c
1270 text15 CODE >43:/opt/microchip/xc8/v1.45/sources/common/fltol.c
1270 text15 CODE >47:/opt/microchip/xc8/v1.45/sources/common/fltol.c
1282 text15 CODE >48:/opt/microchip/xc8/v1.45/sources/common/fltol.c
128B text15 CODE >49:/opt/microchip/xc8/v1.45/sources/common/fltol.c
129E text15 CODE >50:/opt/microchip/xc8/v1.45/sources/common/fltol.c
129F text15 CODE >51:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12A7 text15 CODE >52:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12A9 text15 CODE >53:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12AB text15 CODE >54:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12B0 text15 CODE >55:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12B9 text15 CODE >57:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12C0 text15 CODE >58:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12C7 text15 CODE >60:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12CB text15 CODE >61:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12D4 text15 CODE >63:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12DB text15 CODE >64:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12DD text15 CODE >62:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12DD text15 CODE >65:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12E0 text15 CODE >67:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12E3 text15 CODE >68:/opt/microchip/xc8/v1.45/sources/common/fltol.c
12EE text15 CODE >70:/opt/microchip/xc8/v1.45/sources/common/fltol.c
121D text14 CODE >6:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
121D text14 CODE >14:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
1226 text14 CODE >15:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
122C text14 CODE >16:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
122E text14 CODE >17:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
1230 text14 CODE >18:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
1237 text14 CODE >19:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
123B text14 CODE >17:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
123C text14 CODE >22:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
1243 text14 CODE >23:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
1253 text14 CODE >24:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
125B text14 CODE >25:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
125C text14 CODE >27:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
1263 text14 CODE >28:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
1267 text14 CODE >30:/opt/microchip/xc8/v1.45/sources/common/lldiv.c
10FE text13 CODE >6:/opt/microchip/xc8/v1.45/sources/common/llmod.c
10FE text13 CODE >13:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1105 text13 CODE >14:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1107 text13 CODE >15:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1109 text13 CODE >16:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1110 text13 CODE >17:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1114 text13 CODE >15:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1115 text13 CODE >20:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1125 text13 CODE >21:/opt/microchip/xc8/v1.45/sources/common/llmod.c
112D text13 CODE >22:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1134 text13 CODE >23:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1138 text13 CODE >25:/opt/microchip/xc8/v1.45/sources/common/llmod.c
1141 text12 CODE >188:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1143 text12 CODE >191:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1144 text12 CODE >194:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1146 text12 CODE >197:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1147 text12 CODE >198:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1148 text12 CODE >200:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1149 text12 CODE >203:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
114B text12 CODE >206:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
114D text12 CODE >209:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
114F text12 CODE >212:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1151 text12 CODE >215:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1153 text12 CODE >218:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1155 text12 CODE >221:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1157 text12 CODE >224:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1159 text12 CODE >227:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
115B text12 CODE >230:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
115F text12 CODE >231:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1160 text12 CODE >191:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1186 text12 CODE >232:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
800 swtext3 CONST >93:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
2FA text11 CODE >51:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
2FA text11 CODE >60:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
310 text11 CODE >62:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
333 text11 CODE >63:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
335 text11 CODE >67:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
33A text11 CODE >71:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
33C text11 CODE >72:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
340 text11 CODE >71:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
3AA text11 CODE >73:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
3CD text11 CODE >76:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
3E4 text11 CODE >77:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
3EA text11 CODE >78:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
3F9 text11 CODE >79:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
3FD text11 CODE >80:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
404 text11 CODE >81:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
40A text11 CODE >82:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
40C text11 CODE >83:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
410 text11 CODE >86:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
446 text11 CODE >87:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
4A5 text11 CODE >88:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
504 text11 CODE >89:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
563 text11 CODE >90:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5C2 text11 CODE >93:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5C3 text11 CODE >96:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5C5 text11 CODE >100:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5C7 text11 CODE >104:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5CB text11 CODE >105:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5CD text11 CODE >108:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5CF text11 CODE >112:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5D1 text11 CODE >116:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5D5 text11 CODE >117:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5D7 text11 CODE >120:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5D9 text11 CODE >124:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5DB text11 CODE >128:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5DF text11 CODE >129:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5E1 text11 CODE >132:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5E3 text11 CODE >136:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5E5 text11 CODE >140:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5E9 text11 CODE >141:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5EB text11 CODE >144:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5ED text11 CODE >148:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5EF text11 CODE >152:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5F3 text11 CODE >153:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5F5 text11 CODE >156:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5F7 text11 CODE >160:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5F9 text11 CODE >164:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5FD text11 CODE >165:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
5FF text11 CODE >168:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
601 text11 CODE >172:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
603 text11 CODE >176:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
607 text11 CODE >177:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
60E text11 CODE >179:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
60F text11 CODE >93:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
619 text11 CODE >182:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
61E text11 CODE >183:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
630 text11 CODE >182:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
638 text11 CODE >184:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
63F text11 CODE >185:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
640 text10 CODE >236:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
642 text10 CODE >238:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
643 text10 CODE >239:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
645 text10 CODE >241:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
648 text10 CODE >243:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
657 text10 CODE >244:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
667 text10 CODE >245:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
677 text10 CODE >246:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
687 text10 CODE >247:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
697 text10 CODE >248:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
6A7 text10 CODE >249:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
6A8 text10 CODE >252:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
6B8 text10 CODE >255:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
6C4 text10 CODE >258:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
6D4 text10 CODE >261:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
6E0 text10 CODE >264:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
6F0 text10 CODE >267:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
700 text10 CODE >269:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
701 text10 CODE >249:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
716 text10 CODE >271:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
71B text10 CODE >273:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
724 text10 CODE >274:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
72C text10 CODE >275:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
734 text10 CODE >276:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
73C text10 CODE >277:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
744 text10 CODE >278:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
74C text10 CODE >279:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
74D text10 CODE >282:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
75D text10 CODE >283:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
75E text10 CODE >285:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
76E text10 CODE >286:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
76F text10 CODE >288:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
77F text10 CODE >289:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
780 text10 CODE >291:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
790 text10 CODE >292:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
791 text10 CODE >294:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
7A1 text10 CODE >295:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
7A2 text10 CODE >297:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
7B2 text10 CODE >299:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
7B3 text10 CODE >279:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
7C8 text10 CODE >299:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
7C9 text10 CODE >301:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
100C swtext2 CONST >17:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
CDE text9 CODE >6:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
CE0 text9 CODE >12:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
CE5 text9 CODE >13:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
CE9 text9 CODE >14:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
CED text9 CODE >17:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
CEE text9 CODE >20:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
DCA text9 CODE >21:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
E02 text9 CODE >22:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
E03 text9 CODE >24:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
EB6 text9 CODE >25:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
EEE text9 CODE >26:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
EEF text9 CODE >28:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F0C text9 CODE >29:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F2A text9 CODE >30:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F2B text9 CODE >32:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F49 text9 CODE >33:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F67 text9 CODE >34:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F68 text9 CODE >36:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
F86 text9 CODE >37:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FA4 text9 CODE >38:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FA5 text9 CODE >40:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FC3 text9 CODE >41:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FE1 text9 CODE >43:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FE2 text9 CODE >17:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FED text9 CODE >46:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FF5 text9 CODE >47:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
FFF text9 CODE >48:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/processing.c
1376 text8 CODE >161:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1376 text8 CODE >167:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13A7 text8 CODE >168:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13A7 text8 CODE >169:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13A9 text8 CODE >170:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13AC text8 CODE >171:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13AE text8 CODE >172:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13CD text8 CODE >173:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13CE text8 CODE >167:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13F6 text8 CODE >176:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
13FF text7 CODE >147:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1401 text7 CODE >149:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1402 text7 CODE >150:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1412 text7 CODE >151:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1423 text7 CODE >152:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1434 text7 CODE >153:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1445 text7 CODE >154:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1456 text7 CODE >155:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1467 text7 CODE >156:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1478 text7 CODE >157:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1488 text7 CODE >158:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
12EF text6 CODE >260:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
12F1 text6 CODE >265:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1305 text6 CODE >266:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1317 text6 CODE >267:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1329 text6 CODE >268:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
132A text6 CODE >271:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
133E text6 CODE >272:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
133F text6 CODE >274:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1353 text6 CODE >275:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1354 text6 CODE >277:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1368 text6 CODE >279:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1369 text6 CODE >268:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1375 text6 CODE >280:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1000 swtext1 CONST >205:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
8DF text5 CODE >188:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
8E1 text5 CODE >193:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
8F5 text5 CODE >194:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
907 text5 CODE >195:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
919 text5 CODE >196:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
92B text5 CODE >197:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
93D text5 CODE >198:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
94F text5 CODE >199:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
961 text5 CODE >200:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
973 text5 CODE >201:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
985 text5 CODE >202:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
997 text5 CODE >203:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
9A9 text5 CODE >204:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
9BB text5 CODE >205:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
9BC text5 CODE >208:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
9D0 text5 CODE >209:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
9E2 text5 CODE >210:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
9E3 text5 CODE >212:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
9F7 text5 CODE >213:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A09 text5 CODE >214:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A0A text5 CODE >216:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A1E text5 CODE >217:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A30 text5 CODE >218:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A31 text5 CODE >220:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A45 text5 CODE >221:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A57 text5 CODE >222:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A58 text5 CODE >224:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A6C text5 CODE >225:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A7E text5 CODE >226:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A7F text5 CODE >228:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
A93 text5 CODE >229:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
AA5 text5 CODE >231:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
AA6 text5 CODE >205:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
AB1 text5 CODE >232:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
82E text4 CODE >234:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
830 text4 CODE >239:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
844 text4 CODE >240:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
856 text4 CODE >241:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
868 text4 CODE >242:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
87A text4 CODE >243:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
87B text4 CODE >246:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
88F text4 CODE >247:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
890 text4 CODE >249:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
8A4 text4 CODE >250:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
8A5 text4 CODE >252:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
8B9 text4 CODE >253:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
8BA text4 CODE >255:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
8CE text4 CODE >257:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
8CF text4 CODE >243:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
8DE text4 CODE >258:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11D2 text3 CODE >98:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11D4 text3 CODE >100:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11D7 text3 CODE >101:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11DB text3 CODE >103:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11DD text3 CODE >104:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11DE text3 CODE >105:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11DF text3 CODE >107:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11E1 text3 CODE >108:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11E2 text3 CODE >109:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11E3 text3 CODE >110:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11E4 text3 CODE >111:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11E5 text3 CODE >112:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11E6 text3 CODE >113:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11E7 text3 CODE >114:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11E8 text3 CODE >115:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11E9 text3 CODE >116:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11EA text3 CODE >117:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11EC text3 CODE >118:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11EE text3 CODE >119:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11F0 text3 CODE >121:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11F2 text3 CODE >122:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11F3 text3 CODE >123:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11F4 text3 CODE >125:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11F6 text3 CODE >126:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11F7 text3 CODE >127:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11FB text3 CODE >128:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11FC text3 CODE >130:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11FD text3 CODE >131:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11FE text3 CODE >133:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1203 text3 CODE >134:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
120C text3 CODE >135:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1214 text3 CODE >137:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1216 text3 CODE >138:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1217 text3 CODE >139:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1219 text3 CODE >140:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
121A text3 CODE >141:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
121B text3 CODE >142:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
121C text3 CODE >144:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
7CA text2 CODE >282:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
7CA text2 CODE >287:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
7CE text2 CODE >288:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
7E3 text2 CODE >290:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1188 text1 CODE >180:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
118A text1 CODE >182:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
118D text1 CODE >183:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
11D1 text1 CODE >184:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/hardware.c
1523 maintext CODE >40:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1523 maintext CODE >43:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1532 maintext CODE >44:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1534 maintext CODE >46:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1535 maintext CODE >47:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1558 maintext CODE >48:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
155C maintext CODE >52:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
155E maintext CODE >53:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1561 maintext CODE >55:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1565 maintext CODE >56:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1569 maintext CODE >58:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1572 maintext CODE >60:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1574 maintext CODE >61:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1575 maintext CODE >62:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1576 maintext CODE >63:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1578 maintext CODE >64:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1579 maintext CODE >67:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
157D maintext CODE >68:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
157F maintext CODE >70:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1589 maintext CODE >72:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
158B maintext CODE >73:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1590 maintext CODE >74:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1594 maintext CODE >75:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1595 maintext CODE >76:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1599 maintext CODE >79:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15A3 maintext CODE >81:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15A5 maintext CODE >82:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15AA maintext CODE >83:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15AC maintext CODE >84:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15B0 maintext CODE >85:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15B4 maintext CODE >88:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15BE maintext CODE >90:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15C0 maintext CODE >91:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15C6 maintext CODE >92:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15C9 maintext CODE >93:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15CA maintext CODE >94:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15CE maintext CODE >97:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15D8 maintext CODE >99:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15DA maintext CODE >100:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15E0 maintext CODE >101:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15E3 maintext CODE >102:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15E4 maintext CODE >103:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15E8 maintext CODE >106:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15F2 maintext CODE >108:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15F4 maintext CODE >109:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15F6 maintext CODE >110:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15F7 maintext CODE >111:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
15FA maintext CODE >114:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1604 maintext CODE >116:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1606 maintext CODE >117:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1608 maintext CODE >118:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1609 maintext CODE >119:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
160C maintext CODE >122:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1616 maintext CODE >124:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1618 maintext CODE >125:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
161A maintext CODE >126:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
161B maintext CODE >127:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
161E maintext CODE >130:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1625 maintext CODE >132:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1627 maintext CODE >133:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
162A maintext CODE >134:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
162D maintext CODE >136:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
162E maintext CODE >137:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1631 maintext CODE >140:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
1638 maintext CODE >142:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
163A maintext CODE >143:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
163C maintext CODE >50:/home/michal/ELEKTRONIKA/asdf_lcr1/firmware/ui_board.X/main.c
7F8 clrtext CODE >1385:/tmp/xcXzfBX4R
7F8 clrtext CODE >1386:/tmp/xcXzfBX4R
7F9 clrtext CODE >1387:/tmp/xcXzfBX4R
7F9 clrtext CODE >1388:/tmp/xcXzfBX4R
7FA clrtext CODE >1389:/tmp/xcXzfBX4R
7FB clrtext CODE >1390:/tmp/xcXzfBX4R
7FC clrtext CODE >1391:/tmp/xcXzfBX4R
7FD clrtext CODE >1392:/tmp/xcXzfBX4R
# %SYMTAB Section
# An enumeration of all symbols in the program.
# The beginning of the section is indicated by %SYMTAB.
# Each line describes a single symbol as follows:
#    <label> <value> [-]<load-adj> <class> <space> <psect> <file-name>
# The value and load-adj are both in unqualified hexadecimal.
# All other numeric values are in decimal.  The load-adj is the
# quantity one needs to add to the symbol value in order to obtain the load
# address of the symbol.  This value may be signed. If the symbol
# was defined in a psect then <psect> will be "-". File-name
# is the name of the object file in which the symbol was defined.
%SYMTAB
___latbits 2 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
tc_int@multiplex_sel 78 0 COMMON 1 bssCOMMON dist/default/debug/ui_board.X.debug.obj
__end_ofleds_shift@off 3002 0 STRCODE 0 stringtext1 dist/default/debug/ui_board.X.debug.obj
__Hspace_0 8009 0 ABS 0 - -
__Hspace_1 16F 0 ABS 0 - -
__Hspace_2 0 0 ABS 0 - -
__Hspace_3 0 0 ABS 0 - -
__CFG_IESO$OFF 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__size_of_leds_amp_sel 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_g_shift 16E 0 BANK2 1 bssBANK2 dist/default/debug/ui_board.X.debug.obj
__Heeprom_data 0 0 EEDATA 3 eeprom_data -
__CFG_MCLRE$ON 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__Hstrings 0 0 ABS 0 strings -
float_to_bcd@i_7s CB 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
___sp 0 0 STACK 2 stack /tmp/xcXwsrphy.obj
_init 23A4 0 CODE 0 text3 dist/default/debug/ui_board.X.debug.obj
_main 2A46 0 CODE 0 maintext dist/default/debug/ui_board.X.debug.obj
btemp 7E 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
start 5C2 0 CODE 0 init /tmp/xcXwsrphy.obj
___flmul@aexp 48 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
___flmul@bexp 4D 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
___flmul@prod 4E 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
___flmul@sign 47 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
___flmul@temp 52 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__size_of___fldiv 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__size_of___flmul 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__size_of___flneg 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__size_of___fltol 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__size_of_init 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__size_of_main 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__size_of___lldiv 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__size_of___llmod 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__HbssCOMMON 0 0 ABS 0 bssCOMMON -
display@hys_buf EC 0 BANK1 1 bssBANK1 dist/default/debug/ui_board.X.debug.obj
__end_of_leds_amp_sel 26EC 0 CODE 0 text6 dist/default/debug/ui_board.X.debug.obj
__size_of_char_to_7seg 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_OPTION_REGbits 95 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
suffix_to_leds@on 34 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__Hpowerup 0 0 CODE 0 powerup -
suffix_to_leds@disp_nr 31 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
send_config@config 36 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__size_of_get_result 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__size_of_suffix_to_leds 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
float_to_bcd@dp_pos D1 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
intlevel0 0 0 ENTRY 0 functab /tmp/xcXwsrphy.obj
intlevel1 0 0 ENTRY 0 functab /tmp/xcXwsrphy.obj
intlevel2 0 0 ENTRY 0 functab /tmp/xcXwsrphy.obj
intlevel3 0 0 ENTRY 0 functab /tmp/xcXwsrphy.obj
intlevel4 0 0 ENTRY 0 functab /tmp/xcXwsrphy.obj
intlevel5 0 0 ENTRY 0 functab /tmp/xcXwsrphy.obj
__LbssCOMMON 0 0 ABS 0 bssCOMMON -
__end_of_char_to_7seg 2310 0 CODE 0 text12 dist/default/debug/ui_board.X.debug.obj
_OSCCONbits 99 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
wtemp0 7E 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
___llmod@divisor 31 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__Hfunctab 0 0 ENTRY 0 functab -
__Hclrtext 0 0 ABS 0 clrtext -
_ANSELA 18C 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_ANSELB 18D 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_ANSELC 18E 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__end_of__Umul8_16 21FC 0 CODE 0 text18 dist/default/debug/ui_board.X.debug.obj
__size_of_leds_fq_sel 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
suffix_to_leds@suffix 32 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__size_of__Umul8_16 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
float_to_bcd@float_num B5 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
_display 19BC 0 CODE 0 text9 dist/default/debug/ui_board.X.debug.obj
__end_of___flge 2A46 0 CODE 0 text19 dist/default/debug/ui_board.X.debug.obj
leds_fq_sel@fq_sel 32 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
leds_fq_sel@on 300A 0 STRCODE 0 stringtext6 dist/default/debug/ui_board.X.debug.obj
main@del 166 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
__Lmaintext 0 0 ABS 0 maintext -
___fldiv@aexp B4 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
___fldiv@bexp B3 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
___fldiv@sign A8 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
_float_to_bcd 5F4 0 CODE 0 text11 dist/default/debug/ui_board.X.debug.obj
__Umul8_16 21BC 0 CODE 0 text18 dist/default/debug/ui_board.X.debug.obj
__end_of_send_config 23A4 0 CODE 0 text1 dist/default/debug/ui_board.X.debug.obj
__end_of___fldiv 3000 0 CODE 0 text20 dist/default/debug/ui_board.X.debug.obj
__end_of___flmul 19BC 0 CODE 0 text17 dist/default/debug/ui_board.X.debug.obj
__end_of___flneg 21BC 0 CODE 0 text16 dist/default/debug/ui_board.X.debug.obj
__end_of___fltol 25DE 0 CODE 0 text15 dist/default/debug/ui_board.X.debug.obj
__end_of___lldiv 24E0 0 CODE 0 text14 dist/default/debug/ui_board.X.debug.obj
__end_of___llmod 2282 0 CODE 0 text13 dist/default/debug/ui_board.X.debug.obj
get_res_double@var_size 3010 0 STRCODE 0 stringtext9 dist/default/debug/ui_board.X.debug.obj
float_to_bcd@disp_pt B9 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
float_to_bcd@suffix BA 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
__Umul8_16@multiplicand 31 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__size_of_leds_shift 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
___fldiv@a A0 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
___fldiv@b A4 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
___flmul@a 3E 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
___flmul@b 3A 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
___lldiv@counter 48 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__CFG_FCMEN$OFF 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
start_initialization 5C6 0 CODE 0 cinit dist/default/debug/ui_board.X.debug.obj
_TRISAbits 8C 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_TRISBbits 8D 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_TRISCbits 8E 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
float_to_bcd@ext CC 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
___lldiv@dividend 3F 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__size_of_float_to_bcd 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_display$658 12C 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
_display$659 130 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
_display$660 134 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
_display$661 138 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
_display$662 13C 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
_display$663 140 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
clear_ram0 FF0 0 CODE 0 clrtext dist/default/debug/ui_board.X.debug.obj
__pcstackBANK0 20 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__pcstackBANK1 A0 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
__pcstackBANK2 120 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
init@config 33 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
char_to_7seg@seg_char 32 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
display@last_disp_format D7 0 BANK1 1 bssBANK1 dist/default/debug/ui_board.X.debug.obj
___int_sp 0 0 STACK 2 stack /tmp/xcXwsrphy.obj
__end_of_float_to_bcd C80 0 CODE 0 text11 dist/default/debug/ui_board.X.debug.obj
__Hbank0 0 0 ABS 0 bank0 -
__Hbank1 0 0 ABS 0 bank1 -
__Hbank2 0 0 ABS 0 bank2 -
__Hbank3 0 0 ABS 0 bank3 -
__Hbank4 0 0 ABS 0 bank4 -
__Hbank5 0 0 ABS 0 bank5 -
__Hbank6 0 0 BANK6 1 bank6 -
__Hbank7 0 0 BANK7 1 bank7 -
__Hbank8 0 0 BANK8 1 bank8 -
__Hbank9 0 0 BANK9 1 bank9 -
__Hcinit 5F4 0 CODE 0 cinit -
get_res_double@temp_int32 3A 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__Hidloc 0 0 IDLOC 0 idloc -
_get_res_double 26EC 0 CODE 0 text8 dist/default/debug/ui_board.X.debug.obj
__Hsfr10 0 0 ABS 0 sfr10 -
__Hsfr11 0 0 ABS 0 sfr11 -
__Hsfr12 0 0 ABS 0 sfr12 -
__Hsfr13 0 0 ABS 0 sfr13 -
__Hsfr14 0 0 ABS 0 sfr14 -
__Hsfr15 0 0 ABS 0 sfr15 -
__Hsfr16 0 0 ABS 0 sfr16 -
__Hsfr17 0 0 ABS 0 sfr17 -
__Hsfr18 0 0 ABS 0 sfr18 -
__Hsfr19 0 0 ABS 0 sfr19 -
__Hsfr20 0 0 ABS 0 sfr20 -
__Hsfr21 0 0 ABS 0 sfr21 -
__Hsfr22 0 0 ABS 0 sfr22 -
__Hsfr23 0 0 ABS 0 sfr23 -
__Hsfr24 0 0 ABS 0 sfr24 -
__Hsfr25 0 0 ABS 0 sfr25 -
__Hsfr26 0 0 ABS 0 sfr26 -
__Hsfr27 0 0 ABS 0 sfr27 -
__Hsfr28 0 0 ABS 0 sfr28 -
__Hsfr29 0 0 ABS 0 sfr29 -
__Hsfr30 0 0 ABS 0 sfr30 -
__Hsfr31 0 0 ABS 0 sfr31 -
__Hstack 0 0 STACK 2 stack -
__end_of_tc_int 5C2 0 CODE 0 intentry dist/default/debug/ui_board.X.debug.obj
__Hbank10 0 0 BANK10 1 bank10 -
__Hbank11 0 0 BANK11 1 bank11 -
__Hbank12 0 0 BANK12 1 bank12 -
__Hbank13 0 0 BANK13 1 bank13 -
__Hbank14 0 0 BANK14 1 bank14 -
__Hbank15 0 0 BANK15 1 bank15 -
__Hbank16 0 0 BANK16 1 bank16 -
__Hbank17 0 0 BANK17 1 bank17 -
__Hbank18 0 0 BANK18 1 bank18 -
__Hbank19 0 0 BANK19 1 bank19 -
__Hbank20 0 0 BANK20 1 bank20 -
__Hbank21 0 0 BANK21 1 bank21 -
__Hbank22 0 0 BANK22 1 bank22 -
__Hbank23 0 0 BANK23 1 bank23 -
__Hbank24 0 0 BANK24 1 bank24 -
__Hbank25 0 0 BANK25 1 bank25 -
__Hbank26 0 0 BANK26 1 bank26 -
__Hbank27 0 0 BANK27 1 bank27 -
__Hbank28 0 0 BANK28 1 bank28 -
__Hbank29 0 0 BANK29 1 bank29 -
__Hbank30 0 0 BANK30 1 bank30 -
__Hbank31 0 0 BANK31 1 bank31 -
__Hbigram 0 0 ABS 0 bigram -
__Hmaintext 0 0 ABS 0 maintext -
suffix_to_leds@off 33 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
_display$1027 120 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
_display$1028 124 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
_display$1029 128 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
__CFG_FOSC$INTOSC 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__Hcommon 0 0 ABS 0 common -
__Hconfig 10012 0 CONFIG 0 config -
__Lbank0 0 0 ABS 0 bank0 -
__Lbank1 0 0 ABS 0 bank1 -
__Lbank2 0 0 ABS 0 bank2 -
__Lbank3 0 0 ABS 0 bank3 -
__Lbank4 0 0 ABS 0 bank4 -
__Lbank5 0 0 ABS 0 bank5 -
__Lbank6 0 0 BANK6 1 bank6 -
__Lbank7 0 0 BANK7 1 bank7 -
__Lbank8 0 0 BANK8 1 bank8 -
__Lbank9 0 0 BANK9 1 bank9 -
__Lcinit 5C6 0 CODE 0 cinit -
__Lidloc 0 0 IDLOC 0 idloc -
__Lsfr10 0 0 ABS 0 sfr10 -
__Lsfr11 0 0 ABS 0 sfr11 -
__Lsfr12 0 0 ABS 0 sfr12 -
__Lsfr13 0 0 ABS 0 sfr13 -
__Lsfr14 0 0 ABS 0 sfr14 -
__Lsfr15 0 0 ABS 0 sfr15 -
__Lsfr16 0 0 ABS 0 sfr16 -
__Lsfr17 0 0 ABS 0 sfr17 -
__Lsfr18 0 0 ABS 0 sfr18 -
__Lsfr19 0 0 ABS 0 sfr19 -
__Lsfr20 0 0 ABS 0 sfr20 -
__Lsfr21 0 0 ABS 0 sfr21 -
__Lsfr22 0 0 ABS 0 sfr22 -
__Lsfr23 0 0 ABS 0 sfr23 -
__Lsfr24 0 0 ABS 0 sfr24 -
__Lsfr25 0 0 ABS 0 sfr25 -
__Lsfr26 0 0 ABS 0 sfr26 -
__Lsfr27 0 0 ABS 0 sfr27 -
__Lsfr28 0 0 ABS 0 sfr28 -
__Lsfr29 0 0 ABS 0 sfr29 -
__Lsfr30 0 0 ABS 0 sfr30 -
__Lsfr31 0 0 ABS 0 sfr31 -
__Lstack 0 0 STACK 2 stack -
___flmul@grs 49 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
char_to_7seg@seg_decoded 33 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
_PORTCbits E 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_INTCONbits B 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_leds_disp_format 11BE 0 CODE 0 text5 dist/default/debug/ui_board.X.debug.obj
__Habs1 0 0 ABS 0 abs1 -
__Hcode 0 0 ABS 0 code -
__Hinit 5C2 0 CODE 0 init -
__Hsfr0 0 0 ABS 0 sfr0 -
__Hsfr1 0 0 ABS 0 sfr1 -
__Hsfr2 0 0 ABS 0 sfr2 -
__Hsfr3 0 0 ABS 0 sfr3 -
__Hsfr4 0 0 ABS 0 sfr4 -
__Hsfr5 0 0 ABS 0 sfr5 -
__Hsfr6 0 0 ABS 0 sfr6 -
__Hsfr7 0 0 ABS 0 sfr7 -
__Hsfr8 0 0 ABS 0 sfr8 -
__Hsfr9 0 0 ABS 0 sfr9 -
__Htext 0 0 ABS 0 text -
__Labs1 0 0 ABS 0 abs1 -
__Lcode 0 0 ABS 0 code -
__Linit 5C2 0 CODE 0 init -
__Lsfr0 0 0 ABS 0 sfr0 -
__Lsfr1 0 0 ABS 0 sfr1 -
__Lsfr2 0 0 ABS 0 sfr2 -
__Lsfr3 0 0 ABS 0 sfr3 -
__Lsfr4 0 0 ABS 0 sfr4 -
__Lsfr5 0 0 ABS 0 sfr5 -
__Lsfr6 0 0 ABS 0 sfr6 -
__Lsfr7 0 0 ABS 0 sfr7 -
__Lsfr8 0 0 ABS 0 sfr8 -
__Lsfr9 0 0 ABS 0 sfr9 -
__Ltext 0 0 ABS 0 text -
__pstringtext1 3000 0 STRCODE 0 stringtext1 dist/default/debug/ui_board.X.debug.obj
__pstringtext2 3002 0 STRCODE 0 stringtext2 dist/default/debug/ui_board.X.debug.obj
__pstringtext3 3004 0 STRCODE 0 stringtext3 dist/default/debug/ui_board.X.debug.obj
__pstringtext4 3006 0 STRCODE 0 stringtext4 dist/default/debug/ui_board.X.debug.obj
__pstringtext5 3008 0 STRCODE 0 stringtext5 dist/default/debug/ui_board.X.debug.obj
__pstringtext6 300A 0 STRCODE 0 stringtext6 dist/default/debug/ui_board.X.debug.obj
__pstringtext7 300C 0 STRCODE 0 stringtext7 dist/default/debug/ui_board.X.debug.obj
__pstringtext8 300E 0 STRCODE 0 stringtext8 dist/default/debug/ui_board.X.debug.obj
__pstringtext9 3010 0 STRCODE 0 stringtext9 dist/default/debug/ui_board.X.debug.obj
leds_disp_format@disp_format 32 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
___flge 2912 0 CODE 0 text19 dist/default/debug/ui_board.X.debug.obj
leds_amp_sel@on 3006 0 STRCODE 0 stringtext4 dist/default/debug/ui_board.X.debug.obj
__LcstackBANK0 0 0 ABS 0 cstackBANK0 -
__LcstackBANK1 0 0 ABS 0 cstackBANK1 -
__LcstackBANK2 0 0 ABS 0 cstackBANK2 -
int$flags 7E 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__HcstackCOMMON 0 0 ABS 0 cstackCOMMON -
__S0 8009 0 ABS 0 - -
__S1 16F 0 ABS 0 - -
__S2 0 0 ABS 0 - -
__end_ofleds_fq_sel@on 300C 0 STRCODE 0 stringtext6 dist/default/debug/ui_board.X.debug.obj
tc_int@i_shift 74 0 COMMON 1 cstackCOMMON dist/default/debug/ui_board.X.debug.obj
__size_of_send_config 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_leds_fq_sel 105C 0 CODE 0 text4 dist/default/debug/ui_board.X.debug.obj
__end_of_get_res_double 27FE 0 CODE 0 text8 dist/default/debug/ui_board.X.debug.obj
tc_int@keys_tmp 75 0 COMMON 1 cstackCOMMON dist/default/debug/ui_board.X.debug.obj
__CFG_BOREN$ON 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__Lintentry 8 0 CODE 0 intentry -
___lldiv@divisor 3B 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
?_get_res_double 31 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__end_ofget_res_double@var_size 3012 0 STRCODE 0 stringtext9 dist/default/debug/ui_board.X.debug.obj
reset_vec 0 0 CODE 0 reset_vec /tmp/xcXwsrphy.obj
leds_fq_sel@off 3008 0 STRCODE 0 stringtext5 dist/default/debug/ui_board.X.debug.obj
_suffix_to_leds C80 0 CODE 0 text10 dist/default/debug/ui_board.X.debug.obj
__size_of___flge 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__end_ofleds_amp_sel@off 3006 0 STRCODE 0 stringtext3 dist/default/debug/ui_board.X.debug.obj
__LbssBANK0 0 0 ABS 0 bssBANK0 -
__LbssBANK1 0 0 ABS 0 bssBANK1 -
__LbssBANK2 0 0 ABS 0 bssBANK2 -
__Lstringtext1 0 0 ABS 0 stringtext1 -
__Lstringtext2 0 0 ABS 0 stringtext2 -
__Lstringtext3 0 0 ABS 0 stringtext3 -
__Lstringtext4 0 0 ABS 0 stringtext4 -
__Lstringtext5 0 0 ABS 0 stringtext5 -
__Lstringtext6 0 0 ABS 0 stringtext6 -
__Lstringtext7 0 0 ABS 0 stringtext7 -
__Lstringtext8 0 0 ABS 0 stringtext8 -
__Lstringtext9 0 0 ABS 0 stringtext9 -
__end_ofleds_amp_sel@on 3008 0 STRCODE 0 stringtext4 dist/default/debug/ui_board.X.debug.obj
_RCSTAbits 19D 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__ptext10 C80 0 CODE 0 text10 dist/default/debug/ui_board.X.debug.obj
__ptext11 5F4 0 CODE 0 text11 dist/default/debug/ui_board.X.debug.obj
__ptext12 2282 0 CODE 0 text12 dist/default/debug/ui_board.X.debug.obj
__ptext13 21FC 0 CODE 0 text13 dist/default/debug/ui_board.X.debug.obj
__ptext14 243A 0 CODE 0 text14 dist/default/debug/ui_board.X.debug.obj
__ptext15 24E0 0 CODE 0 text15 dist/default/debug/ui_board.X.debug.obj
__ptext16 21A8 0 CODE 0 text16 dist/default/debug/ui_board.X.debug.obj
__ptext17 1564 0 CODE 0 text17 dist/default/debug/ui_board.X.debug.obj
__ptext18 21BC 0 CODE 0 text18 dist/default/debug/ui_board.X.debug.obj
__ptext19 2912 0 CODE 0 text19 dist/default/debug/ui_board.X.debug.obj
__ptext20 2C7A 0 CODE 0 text20 dist/default/debug/ui_board.X.debug.obj
float_to_bcd@hys_buf BB 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
___fldiv 2C7A 0 CODE 0 text20 dist/default/debug/ui_board.X.debug.obj
___flmul 1564 0 CODE 0 text17 dist/default/debug/ui_board.X.debug.obj
___flneg 21A8 0 CODE 0 text16 dist/default/debug/ui_board.X.debug.obj
___fltol 24E0 0 CODE 0 text15 dist/default/debug/ui_board.X.debug.obj
___lldiv 243A 0 CODE 0 text14 dist/default/debug/ui_board.X.debug.obj
___llmod 21FC 0 CODE 0 text13 dist/default/debug/ui_board.X.debug.obj
__Lbank10 0 0 BANK10 1 bank10 -
__Lbank11 0 0 BANK11 1 bank11 -
__Lbank12 0 0 BANK12 1 bank12 -
__Lbank13 0 0 BANK13 1 bank13 -
__Lbank14 0 0 BANK14 1 bank14 -
__Lbank15 0 0 BANK15 1 bank15 -
__Lbank16 0 0 BANK16 1 bank16 -
__Lbank17 0 0 BANK17 1 bank17 -
__Lbank18 0 0 BANK18 1 bank18 -
__Lbank19 0 0 BANK19 1 bank19 -
__Lbank20 0 0 BANK20 1 bank20 -
__Lbank21 0 0 BANK21 1 bank21 -
__Lbank22 0 0 BANK22 1 bank22 -
__Lbank23 0 0 BANK23 1 bank23 -
__Lbank24 0 0 BANK24 1 bank24 -
__Lbank25 0 0 BANK25 1 bank25 -
__Lbank26 0 0 BANK26 1 bank26 -
__Lbank27 0 0 BANK27 1 bank27 -
__Lbank28 0 0 BANK28 1 bank28 -
__Lbank29 0 0 BANK29 1 bank29 -
__Lbank30 0 0 BANK30 1 bank30 -
__Lbank31 0 0 BANK31 1 bank31 -
__pmaintext 2A46 0 CODE 0 maintext dist/default/debug/ui_board.X.debug.obj
_ui_state D8 0 BANK1 1 bssBANK1 dist/default/debug/ui_board.X.debug.obj
__Lbigram 0 0 ABS 0 bigram -
__CFG_BORV$LO 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__Umul8_16@multiplier 39 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__Lcommon 0 0 ABS 0 common -
__Lconfig 1000E 0 CONFIG 0 config -
__CFG_CP$OFF 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__CFG_WDTE$OFF 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__end_of_leds_disp_format 1564 0 CODE 0 text5 dist/default/debug/ui_board.X.debug.obj
_LATAbits 10C 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_LATCbits 10E 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
___fldiv@grs AF 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
___fldiv@rem A9 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
get_result@results 42 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
main@F4144 59 0 BANK0 1 bssBANK0 dist/default/debug/ui_board.X.debug.obj
tc_int@keys_tmp_bck 77 0 COMMON 1 bssCOMMON dist/default/debug/ui_board.X.debug.obj
__size_of_leds_disp_format 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_tc_int 8 0 CODE 0 intentry dist/default/debug/ui_board.X.debug.obj
___fldiv@new_exp AD 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
__size_of_display 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
stackhi 21DF 0 ABS 0 - /tmp/xcXwsrphy.obj
stacklo 20EF 0 ABS 0 - /tmp/xcXwsrphy.obj
_get_result 27FE 0 CODE 0 text7 dist/default/debug/ui_board.X.debug.obj
__end_ofleds_fq_sel@off 300A 0 STRCODE 0 stringtext5 dist/default/debug/ui_board.X.debug.obj
__end_of_suffix_to_leds F94 0 CODE 0 text10 dist/default/debug/ui_board.X.debug.obj
leds_amp_sel@off 3004 0 STRCODE 0 stringtext3 dist/default/debug/ui_board.X.debug.obj
__Lspace_0 0 0 ABS 0 - -
__Lspace_1 0 0 ABS 0 - -
__Lspace_2 0 0 ABS 0 - -
__Lspace_3 0 0 ABS 0 - -
__pbssCOMMON 76 0 COMMON 1 bssCOMMON dist/default/debug/ui_board.X.debug.obj
main@config 168 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
tc_int@disp_register 70 0 COMMON 1 cstackCOMMON dist/default/debug/ui_board.X.debug.obj
__HcstackBANK0 0 0 ABS 0 cstackBANK0 -
__HcstackBANK1 0 0 ABS 0 cstackBANK1 -
__HcstackBANK2 0 0 ABS 0 cstackBANK2 -
__Umul8_16@product 35 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
leds_disp_format@off 300C 0 STRCODE 0 stringtext7 dist/default/debug/ui_board.X.debug.obj
___flge@ff1 A0 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
___flge@ff2 A4 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
_PIR1bits 11 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__Lend_init 5C2 0 CODE 0 end_init -
__CFG_LVP$ON 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__LcstackCOMMON 0 0 ABS 0 cstackCOMMON -
___fltol@exp1 3B 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
main@results 145 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
end_of_initialization 5EC 0 CODE 0 cinit dist/default/debug/ui_board.X.debug.obj
leds_shift@off 3000 0 STRCODE 0 stringtext1 dist/default/debug/ui_board.X.debug.obj
__Hintentry 5C2 0 CODE 0 intentry -
__CFG_STVREN$ON 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__Lstrings 0 0 ABS 0 strings -
?___fldiv A0 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
?___flmul 3A 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
?___flneg 31 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
?___fltol 31 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
?___lldiv 3B 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
?___llmod 31 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
leds_shift@on 3002 0 STRCODE 0 stringtext2 dist/default/debug/ui_board.X.debug.obj
__Hreset_vec 6 0 CODE 0 reset_vec -
__HbssBANK0 0 0 ABS 0 bssBANK0 -
__HbssBANK1 0 0 ABS 0 bssBANK1 -
__HbssBANK2 0 0 ABS 0 bssBANK2 -
__size_of_tc_int 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
display@config D2 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
___flneg@f1 31 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__ptext1 2310 0 CODE 0 text1 dist/default/debug/ui_board.X.debug.obj
__ptext2 F94 0 CODE 0 text2 dist/default/debug/ui_board.X.debug.obj
__ptext3 23A4 0 CODE 0 text3 dist/default/debug/ui_board.X.debug.obj
__ptext4 105C 0 CODE 0 text4 dist/default/debug/ui_board.X.debug.obj
__ptext5 11BE 0 CODE 0 text5 dist/default/debug/ui_board.X.debug.obj
__ptext6 25DE 0 CODE 0 text6 dist/default/debug/ui_board.X.debug.obj
__ptext7 27FE 0 CODE 0 text7 dist/default/debug/ui_board.X.debug.obj
__ptext8 26EC 0 CODE 0 text8 dist/default/debug/ui_board.X.debug.obj
__ptext9 19BC 0 CODE 0 text9 dist/default/debug/ui_board.X.debug.obj
get_res_double@i_shift 3E 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
?__Umul8_16 31 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__end_ofleds_disp_format@on 3010 0 STRCODE 0 stringtext8 dist/default/debug/ui_board.X.debug.obj
main@locked 165 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
__Lpowerup 0 0 CODE 0 powerup -
__Leeprom_data 0 0 EEDATA 3 eeprom_data -
__Umul8_16@word_mpld 37 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
___fltol@sign1 3A 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__end_of_get_result 2912 0 CODE 0 text7 dist/default/debug/ui_board.X.debug.obj
float_to_bcd@int_num CD 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
__Lreset_vec 0 0 CODE 0 reset_vec -
__Hstringtext1 0 0 ABS 0 stringtext1 -
__Hstringtext2 0 0 ABS 0 stringtext2 -
__Hstringtext3 0 0 ABS 0 stringtext3 -
__Hstringtext4 0 0 ABS 0 stringtext4 -
__Hstringtext5 0 0 ABS 0 stringtext5 -
__Hstringtext6 0 0 ABS 0 stringtext6 -
__Hstringtext7 0 0 ABS 0 stringtext7 -
__Hstringtext8 0 0 ABS 0 stringtext8 -
__Hstringtext9 0 0 ABS 0 stringtext9 -
__CFG_LPBOR$OFF 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
___fltol@f1 31 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__CFG_CLKOUTEN$OFF 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_leds_shift F94 0 CODE 0 text2 dist/default/debug/ui_board.X.debug.obj
__end_of__initialization 5EC 0 CODE 0 cinit dist/default/debug/ui_board.X.debug.obj
__Lfunctab 0 0 ENTRY 0 functab -
float_to_bcd@disp_arr C5 0 BANK1 1 cstackBANK1 dist/default/debug/ui_board.X.debug.obj
__end_of_display 2000 0 CODE 0 text9 dist/default/debug/ui_board.X.debug.obj
_send_config 2310 0 CODE 0 text1 dist/default/debug/ui_board.X.debug.obj
__Lclrtext 0 0 ABS 0 clrtext -
tc_int@debounce 76 0 COMMON 1 bssCOMMON dist/default/debug/ui_board.X.debug.obj
leds_disp_format@on 300E 0 STRCODE 0 stringtext8 dist/default/debug/ui_board.X.debug.obj
___lldiv@quotient 44 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__pcstackCOMMON 70 0 COMMON 1 cstackCOMMON dist/default/debug/ui_board.X.debug.obj
_TXSTAbits 19E 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__Hend_init 5C6 0 CODE 0 end_init -
___llmod@dividend 35 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
display@results 144 0 BANK2 1 cstackBANK2 dist/default/debug/ui_board.X.debug.obj
___llmod@counter 3A 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__end_of_init 243A 0 CODE 0 text3 dist/default/debug/ui_board.X.debug.obj
__end_of_main 2C7A 0 CODE 0 maintext dist/default/debug/ui_board.X.debug.obj
__end_ofleds_shift@on 3004 0 STRCODE 0 stringtext2 dist/default/debug/ui_board.X.debug.obj
__end_ofleds_disp_format@off 300E 0 STRCODE 0 stringtext7 dist/default/debug/ui_board.X.debug.obj
_leds_amp_sel 25DE 0 CODE 0 text6 dist/default/debug/ui_board.X.debug.obj
_RCREG 199 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_SPBRG 19B 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
_TXREG 19A 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__Hram 0 0 ABS 0 ram -
__Lram 0 0 ABS 0 ram -
__end_of_leds_fq_sel 11BE 0 CODE 0 text4 dist/default/debug/ui_board.X.debug.obj
__pintentry 8 0 CODE 0 intentry dist/default/debug/ui_board.X.debug.obj
leds_amp_sel@amp_sel 32 0 BANK0 1 cstackBANK0 dist/default/debug/ui_board.X.debug.obj
__initialization 5C6 0 CODE 0 cinit dist/default/debug/ui_board.X.debug.obj
__CFG_PWRTE$OFF 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__pbssBANK0 59 0 BANK0 1 bssBANK0 dist/default/debug/ui_board.X.debug.obj
__pbssBANK1 D7 0 BANK1 1 bssBANK1 dist/default/debug/ui_board.X.debug.obj
__pbssBANK2 16E 0 BANK2 1 bssBANK2 dist/default/debug/ui_board.X.debug.obj
__size_of_get_res_double 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__CFG_WRT$OFF 0 0 ABS 0 - dist/default/debug/ui_board.X.debug.obj
__end_of_leds_shift FF0 0 CODE 0 text2 dist/default/debug/ui_board.X.debug.obj
_char_to_7seg 2282 0 CODE 0 text12 dist/default/debug/ui_board.X.debug.obj
__pswtext1 2000 0 CONST 0 swtext1 dist/default/debug/ui_board.X.debug.obj
__pswtext2 2018 0 CONST 0 swtext2 dist/default/debug/ui_board.X.debug.obj
__pswtext3 1000 0 CONST 0 swtext3 dist/default/debug/ui_board.X.debug.obj
# %SPLITSTAB Section
# This section enumerates all the psect splits performed by the assembler.
# The beginning of the section is indicated by %SPLITSTAB.
# Each line is a record a particular split, where the parent psect is on
# the left and the child on the right.  Note that a child psect is always
# split form the top of the parent psect. All splits from a given parent
# are listed in the order in which they occurred.
%SPLITSTAB
# %DABS Section
# This section contains a table of all usuage of the assember
# directive DABS in the program. Each line has the following format:
#   <name> <space> <address> <size>
# If the DABS was originally labelled then that shall be <name>,
# otherwise name will be "-".  The <space> number is in decimal.
# <address> and <size> are in byte units as unqaulified hexadecimal
%DABS
- 1 7E 2
# %SEGMENTS Section
# This sections enumerates the segments of the program.  Each segment
# is described on a single line as follows:
#    <name> <space> <link address> <file address> <size> <delta>
# Addresses and size are in unqualified hexadecimal.  The link address
# and size are in units of delta. The file address is in units of bytes.
# All other numeric quantities are in decimal.
%SEGMENTS
text1 0 1188 2310 4A 2
text3 0 11D2 23A4 4B 2
text4 0 82E 105C B1 2
text5 0 8DF 11BE 1D3 2
text6 0 12EF 25DE 87 2
text7 0 13FF 27FE 8A 2
text8 0 1376 26EC 89 2
text9 0 CDE 19BC 322 2
text12 0 1141 2282 47 2
text13 0 10FE 21FC 43 2
text14 0 121D 243A 53 2
text15 0 1270 24E0 7F 2
text16 0 10D4 21A8 A 2
text17 0 AB2 1564 22C 2
text18 0 10DE 21BC 20 2
text19 0 1489 2912 9A 2
text20 0 163D 2C7A 1C3 2
maintext 0 1523 2A46 11A 2
cstackCOMMON 1 70 70 9 1
cstackBANK0 1 20 20 3F 1
cstackBANK1 1 A0 A0 50 1
cstackBANK2 1 120 120 4F 1
stringtext1 0 1800 3000 9 2
intentry 0 4 8 7FA 2
reset_vec 0 0 0 3 2
swtext1 0 1000 2000 18 2
swtext3 0 800 1000 2A 2
config 0 8007 1000E 2 2
