<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.0">
<drawing>
<library>
<packages>
<package name="SHITTYADDON">
</package>
<package name="2X3-SHROUDED-MALE">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3-SHROUDED-FEMALE">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="SHITTYADDON">
<pin name="$SDA"/>
<pin name="$SCL"/>
<pin name="$VCC"/>
<pin name="$GND"/>
</symbol>
<symbol name="SHITTYADDON-1.69">
<pin name="$SDA"/>
<pin name="$SCL"/>
<pin name="$VCC"/>
<pin name="$GND"/>
<pin name="$GPIO1"/>
<pin name="$GPIO2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SHITTYADDON">
<description>It's a shitty DEFCON26 Add-on Connector!

it's a shitty little library for the shitty DEFCON add-on connector, originally from Brian B. link below. simple 3.3volt I2C connecto in a 2x2 .1inch 2.54mm spacing.

align VCC to the target. can you hit a target?

https://hackaday.io/benchoff</description>
<gates>
<gate name="G$1" symbol="SHITTYADDON"/>
</gates>
<devices>
<device name="" package="SHITTYADDON">
<connects>
<connect gate="G$1" pin="$GND" pad="$GND"/>
<connect gate="G$1" pin="$SCL" pad="$SCL"/>
<connect gate="G$1" pin="$SDA" pad="$SDA"/>
<connect gate="G$1" pin="$VCC" pad="$VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAO-1.69">
<gates>
<gate name="G$1" symbol="SHITTYADDON-1.69"/>
</gates>
<devices>
<device name="" package="2X3-SHROUDED-FEMALE">
<connects>
<connect gate="G$1" pin="$GND" pad="$GND"/>
<connect gate="G$1" pin="$GPIO1" pad="$GPIO1"/>
<connect gate="G$1" pin="$GPIO2" pad="$GPIO2"/>
<connect gate="G$1" pin="$SCL" pad="$SCL"/>
<connect gate="G$1" pin="$SDA" pad="$SDA"/>
<connect gate="G$1" pin="$VCC" pad="$VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAOBADGE-1.69">
<gates>
<gate name="G$1" symbol="SHITTYADDON-1.69"/>
</gates>
<devices>
<device name="" package="2X3-SHROUDED-MALE">
<connects>
<connect gate="G$1" pin="$GND" pad="GND"/>
<connect gate="G$1" pin="$GPIO1" pad="GPIO1"/>
<connect gate="G$1" pin="$GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="$SCL" pad="SCL"/>
<connect gate="G$1" pin="$SDA" pad="SDA"/>
<connect gate="G$1" pin="$VCC" pad="3V3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
