<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.0">
<drawing>
<library>
<description>Generated from &lt;b&gt;ts350r1-190404.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name=".1/.041">
</package>
<package name=".1/.052">
</package>
<package name=".06/.040">
</package>
<package name=".15/.0635">
</package>
<package name=".16/.120">
</package>
<package name="0476SERIES">
</package>
<package name="0476SERIES-L">
</package>
<package name="0476SERIES-M">
</package>
<package name="1206">
</package>
<package name="D2PAK">
</package>
<package name="DIP24">
</package>
<package name="DPAK">
</package>
<package name="DPAK-3">
</package>
<package name="FUSE-HOLDER-MINI">
<description>For Littelfuse Mini 297 or 997 series/Bussmann ATM or equivalents.</description>
</package>
<package name="FUSE-HOLDER-MINI-H">
<description>Mini use holder, PCB horizontal mount.</description>
</package>
<package name="HDR02">
<description>2-pin header, 100mil pitch.</description>
</package>
<package name="HS-C220-050">
<description>Ohmite C series 50mm dual TO220 heatsink with TO220 pad placements for high or low switches.
For use with full bridge gate driver card.</description>
</package>
<package name="HS-CSM222-30-L">
</package>
<package name="HS-CSM222-30-R">
</package>
<package name="JACK-PP-45-PCB-2V">
<description>Anderson 45A Power Pole PCB, 2-vertical stack.</description>
</package>
<package name="L5-11">
</package>
<package name="L1210">
<description>Chip inductor 1210 package.</description>
</package>
<package name="LED-BD">
<description>3mm bidirectional LED (2 with opposing polarity).</description>
</package>
<package name="MCR25">
<description>Rohm MCR25, .5W, SMD resistor</description>
</package>
<package name="MCR50">
<description>Rohm MCR50, .5W, SMD resistor</description>
</package>
<package name="MCR50B">
<description>Rohm MCR50, .5W, SMD resistor

For mounting on bottom layer.</description>
</package>
<package name="MOD-CTRL-SINE-190226R1">
<description>Sine full bridge gate driver and controller card.</description>
</package>
<package name="MOD-GD-FB-190131">
<description>Full bridge gate driver module with current sense, rev 190131.</description>
</package>
<package name="MOV-CH8">
<description>Littelfuse CH-8 series chip varistor.</description>
</package>
<package name="P0613/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 15 mm</description>
</package>
<package name="PAD-8X8-3_25-M">
</package>
<package name="PAD-8X10-3_25-M">
</package>
<package name="PAD-OCT-120-/067">
</package>
<package name="PAD-RND-AUTO/.65-M">
</package>
<package name="PAD-RND-AUTO/032">
</package>
<package name="PAD-RND-AUTO/040">
</package>
<package name="PAD-RT-5_2.5-M">
</package>
<package name="PAD-SQ-5_5-M">
</package>
<package name="R0805">
</package>
<package name="R2512-CS">
<description>Current sense resistor in larger version of 2512 pad dimensions.</description>
</package>
<package name="RES_WSC_2515">
</package>
<package name="RES_WSC_2515-L">
</package>
<package name="RES_WSC_2515-M">
</package>
<package name="RM14-SCR">
</package>
<package name="SMA">
</package>
<package name="SMB">
</package>
<package name="SMBJ">
</package>
<package name="SMC">
</package>
<package name="SO-28W">
</package>
<package name="SO08">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AA</description>
</package>
<package name="SOD123">
<description>SOD123 package</description>
</package>
<package name="SOT-223">
</package>
<package name="SOT23">
<description>SOT23</description>
</package>
<package name="SPST-200AWMSP1T1A1M7QE">
<description>Eswitch Toggle Switch SPDT Through Hole, Right Angle, Vertical.  Second tap (pin 3) removed to function as SPST.
Part #200AWMSP1T1A1M7QE</description>
</package>
<package name="SSOP-28">
</package>
<package name="TO-252-3">
<description>Used for Infineon TO-252-3 DPAK</description>
</package>
<package name="TO-263-7106">
</package>
<package name="TO-263AB">
<description>TO-263AB package drawn to International Rectifier specifications.</description>
</package>
<package name="TO92-SGD">
</package>
<package name="TO220H">
</package>
<package name="TO220H-2">
</package>
<package name="TO220V">
<description>TO220 vertical mount.</description>
</package>
<package name="TOROID-FLYBACK-B64290L0038X087-H">
</package>
<package name="TOROID-FLYBACK-B64290L0045X087-H">
</package>
<package name="TOROID-FLYBACK-B64290L0045X087-VM">
</package>
<package name="TOROID-FLYBACK-B64290P0037X087-H">
</package>
<package name="TOROID-FLYBACK-B64290P0037X087-V">
</package>
<package name="TOROID-MAGNETICS-55894A2-90">
<description>Core manufacturer = Magnetics Core part # = 55894A2 Core OD, cm = 2.69000 Core ID, cm = 1.47000 Core height, cm = 1.12000 Core material = MPP Core permeability, µi = 60 Tolerance, % = 8% Core mh/1K turn, AL = 75.00</description>
</package>
<package name="TOROID-MAGNETICS-55894A2-180">
<description>Core manufacturer =  Magnetics
Core part # =  55894A2
Core OD, cm =  2.69000
Core ID, cm =  1.47000
Core height, cm =  1.12000
Core material =  MPP
Core permeability, µi  =  60
Tolerance, % =  8%
Core mh/1K turn, AL =  75.00</description>
</package>
<package name="TOROID-MAGNETICS-58109A2-180">
<description>Core manufacturer =  Magnetics
Core part # =  58109A2
Core OD, cm =  5.804
Core ID, cm =  3.474
Core height, cm =  1.49
Core material =  High Flux
Core permeability, µi  =  125
Tolerance, % =  8%
Core AL =   156.00</description>
</package>
<package name="TOROID-MAGNETICS-58109A2-V">
</package>
<package name="T_1W_11.9_4.6_V">
<description>Toroid 11.9 OD x 4.6 H, single winding, vertical mount, no bobbin.</description>
</package>
<package name="T_1W_33.6_11.5_VB">
<description>Toroid 33.6 OD x 11.5 H, single winding, vertical mount, in mag-inc bobbin TVH38134A.</description>
</package>
<package name="WE-IND-7447075">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-IND-768772821">
<description>WE-TI HV Radial Leaded Wire Wound Inductor (High Voltage)</description>
</package>
<package name="ZX62-AB">
<description>Hirose Micro AB - Standard (Bottom mount), Shell SMT

Note:  extended pads to support hand soldering.</description>
</package>
<package name="SO14">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AA</description>
</package>
<package name="TO92-EBC">
<description>&lt;b&gt;TO-92&lt;/b&gt; Pads In Line E B C from top&lt;p&gt;</description>
</package>
<package name="SOT23-5">
</package>
<package name="J1-1,27">
<description>Jumper with 50mil (1.27mm) pitch pins.</description>
</package>
<package name="J1">
</package>
<package name="DIL14">
</package>
</packages>
<symbols>
<symbol name="FAN">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="FLYBACK-SL">
<pin name="P1" direction="pas"/>
<pin name="P2" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
</symbol>
<symbol name="FUSE3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="GNDS">
<description>Transformer isolated secondary common (ground) return.</description>
<pin name="GNDS" direction="sup"/>
</symbol>
<symbol name="HDR02">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="HDRF02">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="HS-C220-050-HH">
<description>Schematic for dual TO220 mounted to Ohmite C series 50mm heatsink with faraday screens for heatsink shields.
For use with full bridge gate driver card driving two high or low switches on heatsink.</description>
<pin name="DL" direction="pas"/>
<pin name="DR" direction="pas"/>
<pin name="GL" direction="pas"/>
<pin name="GR" direction="pas"/>
<pin name="HSGL" direction="pwr"/>
<pin name="HSGR" direction="pwr"/>
<pin name="SGL" direction="pwr"/>
<pin name="SGR" direction="pwr"/>
<pin name="SL" direction="pas"/>
<pin name="SR" direction="pas"/>
</symbol>
<symbol name="HS-C220-050-HL">
<description>Schematic for dual TO220 mounted to Ohmite C series 50mm heatsink with faraday screens for heatsink shields.
For use with full bridge gate driver card driving half-bridge (high/low pair) on heatsink.</description>
<pin name="DH" direction="pas"/>
<pin name="DL" direction="pas"/>
<pin name="GH" direction="pas"/>
<pin name="GL" direction="pas"/>
<pin name="HSGH" direction="pwr"/>
<pin name="HSGL" direction="pwr"/>
<pin name="SGH" direction="pwr"/>
<pin name="SGL" direction="pwr"/>
<pin name="SH" direction="pas"/>
<pin name="SL" direction="pas"/>
</symbol>
<symbol name="HS-DIODE-FB">
<description>Full bridge rectifier with heatsink attachment and faraday screens.  For use with common cathode / common anode diode pairs.</description>
<pin name="1B" direction="pas"/>
<pin name="1F" direction="pas"/>
<pin name="2B" direction="pas"/>
<pin name="2F" direction="pas"/>
<pin name="3B" direction="pas"/>
<pin name="3F" direction="pas"/>
<pin name="HSGL" direction="pwr"/>
<pin name="HSGR" direction="pwr"/>
<pin name="SGB" direction="pwr"/>
<pin name="SGF" direction="pwr"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="JACK-2S">
<description>Two-node jack with ground / mechanical strength pad.</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="LDO-3PIN">
<pin name="ADJ" direction="pwr"/>
<pin name="IN" direction="pwr"/>
<pin name="OUT" direction="pwr"/>
</symbol>
<symbol name="LED-BD">
<description>Bidirectional LED</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="MOD-CTRL-SINE-190226R1">
<description>Full bridge gate drive &amp; controller for true-sine power applications.</description>
<pin name="ACK" direction="out"/>
<pin name="CA"/>
<pin name="CB"/>
<pin name="CMD" direction="in"/>
<pin name="HA"/>
<pin name="HB"/>
<pin name="LA"/>
<pin name="LB"/>
<pin name="SA"/>
<pin name="SB"/>
<pin name="TMP" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="MOD-GD-FB-190131">
<description>Full bridge gate driver module with current sense, rev 190131.</description>
<pin name="AC"/>
<pin name="AH"/>
<pin name="AL"/>
<pin name="AS"/>
<pin name="BC"/>
<pin name="BH"/>
<pin name="BL"/>
<pin name="BS"/>
<pin name="CS" direction="out"/>
<pin name="HIA" direction="in"/>
<pin name="HIB" direction="in"/>
<pin name="INV+" direction="pwr"/>
<pin name="INV-" direction="pwr"/>
<pin name="LIA" direction="in"/>
<pin name="LIB" direction="in"/>
<pin name="R+"/>
<pin name="R-"/>
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS1" direction="pwr"/>
<pin name="VSS2" direction="pwr"/>
</symbol>
<symbol name="MOV">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="N-MOSFET">
<description>N channel MOSFET</description>
<pin name="D" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="P-MOSFET">
<pin name="D" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="PAD">
<pin name="P" direction="pas"/>
</symbol>
<symbol name="PIC16F1776">
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RA4"/>
<pin name="RA5"/>
<pin name="RA6"/>
<pin name="RA7"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="RC6"/>
<pin name="RC7"/>
<pin name="VDD" direction="pwr"/>
<pin name="VPP" direction="in"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
</symbol>
<symbol name="R-AC-DUPLEX">
<description>NEMA 120VAC duplex receptacle.</description>
<pin name="B" direction="pas"/>
<pin name="W" direction="pas"/>
</symbol>
<symbol name="RESISTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SI8621">
<pin name="A1" direction="in"/>
<pin name="A2" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="in"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2"/>
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
</symbol>
<symbol name="SMPS-DC-DC">
<description>SMPS DC-DC converter</description>
<pin name="+VIN" direction="in"/>
<pin name="+VOUT"/>
<pin name="-VIN"/>
<pin name="-VOUT"/>
</symbol>
<symbol name="SPST-M">
<description>SPST switch with mount / ground shield connection.</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="G" direction="pwr"/>
</symbol>
<symbol name="T_P1_S1_S2_SCR">
<description>Boost transformer with primary &amp; secondary faraday screens and low voltage auxillary secondary.
Pins at ends of core are grounds for core clips.</description>
<pin name="G1" direction="pwr"/>
<pin name="G2" direction="pwr"/>
<pin name="G3" direction="pwr"/>
<pin name="G4" direction="pwr"/>
<pin name="P1" direction="pas"/>
<pin name="P2" direction="pas"/>
<pin name="PG" direction="pwr"/>
<pin name="S1A" direction="pas"/>
<pin name="S1B" direction="pas"/>
<pin name="S2A" direction="pas"/>
<pin name="S2B" direction="pas"/>
<pin name="SG" direction="pwr"/>
</symbol>
<symbol name="USB">
<description>Generic USB receptacle</description>
<pin name="D+" direction="in"/>
<pin name="D-" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="ID" direction="in"/>
<pin name="VBUS" direction="pwr"/>
</symbol>
<symbol name="ZENER">
<description>Zener diode.</description>
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="IRS21864S">
<description>International Rectifier 600V high / low bootstrap gate driver.</description>
<pin name="COM" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="HO" direction="out"/>
<pin name="LIN" direction="in"/>
<pin name="LO" direction="out"/>
<pin name="VB" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="in"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
</symbol>
<symbol name="OPAMP">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="J1">
<description>Jumper - 1</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="PIC16F18324">
<description>PIC16F18324</description>
<pin name="GND" direction="pwr"/>
<pin name="ICSPCLK"/>
<pin name="ICSPDAT"/>
<pin name="RA2"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="SOSCI"/>
<pin name="SOSCO"/>
<pin name="VDD" direction="pwr"/>
<pin name="VPP"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BSN20" prefix="Q">
<description>Diodes Inc.
N-CHANNEL ENHANCEMENT MODE FIELD MOSFET

Product Summary
Description
This new generation MOSFET has been designed to minimize the on- state resistance (RDS(ON)) and yet maintain superior switching performance, making it ideal for high efficiency power management applications.
BSN20
N-CHANNEL ENHANCEMENT MODE FIELD MOSFET Features and Benefits
 Low On-Resistance
 Low Input Capacitance
 Fast Switching Speed
 Low Input/Output Leakage
 Totally Lead-Free &amp; Fully RoHS Compliant (Notes 1 &amp; 2)
 Halogen and Antimony Free. “Green” Device (Note 3)
 Qualified to AEC-Q101 Standards for High Reliability
 PPAP Capable (Note 4)
Mechanical Data
 Case: SOT23
 Case Material: Molded Plastic “Green” Molding Compound.
UL Flammability Classification Rating 94V-0
 Moisture Sensitivity: Level 1 per J-STD-020
 Terminals: Matte Tin Finish annealed over Alloy 42 leadframe
(Lead Free Plating). Solderable per MIL-STD-202, Method 208 e3
 Terminal Connections: See Diagram
 Weight: 0.008 grams (approximate)
V(BR)DSS</description>
<gates>
<gate name="G$1" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FAN" prefix="M" uservalue="yes">
<gates>
<gate name="G$1" symbol="FAN"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="_EXTERNAL_" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FB_P1_S1" prefix="L" uservalue="yes">
<gates>
<gate name="G$1" symbol="FLYBACK-SL"/>
</gates>
<devices>
<device name="H" package="TOROID-FLYBACK-B64290L0045X087-H">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HS" package="TOROID-FLYBACK-B64290L0038X087-H">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HT" package="TOROID-FLYBACK-B64290P0037X087-H">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="TOROID-FLYBACK-B64290L0045X087-VM">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VT" package="TOROID-FLYBACK-B64290P0037X087-V">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FUSE" prefix="F" uservalue="yes">
<gates>
<gate name="G$1" symbol="FUSE3"/>
</gates>
<devices>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2410" package="0476SERIES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2410L" package="0476SERIES-L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2410M" package="0476SERIES-M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MINI-H" package="FUSE-HOLDER-MINI-H">
<connects>
<connect gate="G$1" pin="1" pad="1A 1B"/>
<connect gate="G$1" pin="2" pad="2A 2B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MINI-V" package="FUSE-HOLDER-MINI">
<connects>
<connect gate="G$1" pin="1" pad="1A 1B"/>
<connect gate="G$1" pin="2" pad="2A 2B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GNDS" prefix="GNDS">
<gates>
<gate name="G$1" symbol="GNDS"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HDR" prefix="J" uservalue="yes">
<description>100mil pitch header.</description>
<gates>
<gate name="G$1" symbol="HDR02"/>
</gates>
<devices>
<device name="02" package="HDR02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HDRF02_E" prefix="P" uservalue="yes">
<description>Non-PCB 2-pin 100mill (2.54mm) female header.</description>
<gates>
<gate name="G$1" symbol="HDRF02"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="_EXTERNAL_" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HS-C220-050-HH" prefix="Q" uservalue="yes">
<description>Ohmite C series 50mm dual TO220 heatsink with TO220 pad placements for high or low switches.
Includes ground pads for swtich-heatsink mounting faraday screens.  For use with full bridge gate driver card.</description>
<gates>
<gate name="G$1" symbol="HS-C220-050-HH"/>
</gates>
<devices>
<device name="" package="HS-C220-050">
<connects>
<connect gate="G$1" pin="DL" pad="2"/>
<connect gate="G$1" pin="DR" pad="5"/>
<connect gate="G$1" pin="GL" pad="1"/>
<connect gate="G$1" pin="GR" pad="4"/>
<connect gate="G$1" pin="HSGL" pad="HSGL1 HSGL2"/>
<connect gate="G$1" pin="HSGR" pad="HSGR1 HSGR2"/>
<connect gate="G$1" pin="SGL" pad="SGL"/>
<connect gate="G$1" pin="SGR" pad="SGR"/>
<connect gate="G$1" pin="SL" pad="3"/>
<connect gate="G$1" pin="SR" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HS-C220-050-HL" prefix="Q" uservalue="yes">
<description>For dual TO220 mounted to Ohmite C series 50mm heatsink with faraday screens for heatsink sheilds.
For use with full bridge gate driver card driving half-bridge (high/low pair) on heatsink.</description>
<gates>
<gate name="G$1" symbol="HS-C220-050-HL"/>
</gates>
<devices>
<device name="LEFT" package="HS-C220-050">
<connects>
<connect gate="G$1" pin="DH" pad="5"/>
<connect gate="G$1" pin="DL" pad="2"/>
<connect gate="G$1" pin="GH" pad="4"/>
<connect gate="G$1" pin="GL" pad="1"/>
<connect gate="G$1" pin="HSGH" pad="HSGR1 HSGR2"/>
<connect gate="G$1" pin="HSGL" pad="HSGL1 HSGL2"/>
<connect gate="G$1" pin="SGH" pad="SGR"/>
<connect gate="G$1" pin="SGL" pad="SGL"/>
<connect gate="G$1" pin="SH" pad="6"/>
<connect gate="G$1" pin="SL" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RIGHT" package="HS-C220-050">
<connects>
<connect gate="G$1" pin="DH" pad="2"/>
<connect gate="G$1" pin="DL" pad="5"/>
<connect gate="G$1" pin="GH" pad="1"/>
<connect gate="G$1" pin="GL" pad="4"/>
<connect gate="G$1" pin="HSGH" pad="HSGL1 HSGL2"/>
<connect gate="G$1" pin="HSGL" pad="HSGR1 HSGR2"/>
<connect gate="G$1" pin="SGH" pad="SGL"/>
<connect gate="G$1" pin="SGL" pad="SGR"/>
<connect gate="G$1" pin="SH" pad="3"/>
<connect gate="G$1" pin="SL" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HS-CSM222-30-FB" prefix="D" uservalue="yes">
<description>Full bridge rectifier consisting of a discrete pair of common anode / cathode rectifiers in TO220 package attached to Ohmite CSM222-30 heatsink.</description>
<gates>
<gate name="G$1" symbol="HS-DIODE-FB"/>
</gates>
<devices>
<device name="LEFT" package="HS-CSM222-30-L">
<connects>
<connect gate="G$1" pin="1B" pad="1B"/>
<connect gate="G$1" pin="1F" pad="1F"/>
<connect gate="G$1" pin="2B" pad="2B"/>
<connect gate="G$1" pin="2F" pad="2F"/>
<connect gate="G$1" pin="3B" pad="3B"/>
<connect gate="G$1" pin="3F" pad="3F"/>
<connect gate="G$1" pin="HSGL" pad="HSGL"/>
<connect gate="G$1" pin="HSGR" pad="HSGR"/>
<connect gate="G$1" pin="SGB" pad="SGB"/>
<connect gate="G$1" pin="SGF" pad="SGF"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RIGHT" package="HS-CSM222-30-R">
<connects>
<connect gate="G$1" pin="1B" pad="1B"/>
<connect gate="G$1" pin="1F" pad="1F"/>
<connect gate="G$1" pin="2B" pad="2B"/>
<connect gate="G$1" pin="2F" pad="2F"/>
<connect gate="G$1" pin="3B" pad="3B"/>
<connect gate="G$1" pin="3F" pad="3F"/>
<connect gate="G$1" pin="HSGL" pad="HSGL"/>
<connect gate="G$1" pin="HSGR" pad="HSGR"/>
<connect gate="G$1" pin="SGB" pad="SGB"/>
<connect gate="G$1" pin="SGF" pad="SGF"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" prefix="L" uservalue="yes">
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="5-11" package="L5-11">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="L1210">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="55894" package="TOROID-MAGNETICS-55894A2-180">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="58109-180" package="TOROID-MAGNETICS-58109A2-180">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="58109-V" package="TOROID-MAGNETICS-58109A2-V">
<connects>
<connect gate="G$1" pin="+" pad="1 3"/>
<connect gate="G$1" pin="-" pad="2 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FI" package="WE-IND-7447075">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TI" package="WE-IND-768772821">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TOROID-MAGNETICS-55894A2-90" package="TOROID-MAGNETICS-55894A2-90">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T_1W_11.9_4.6_V" package="T_1W_11.9_4.6_V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T_1W_33.6_11.5_VB" package="T_1W_33.6_11.5_VB">
<connects>
<connect gate="G$1" pin="+" pad="1 3"/>
<connect gate="G$1" pin="-" pad="2 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JACK-2S" prefix="J" uservalue="yes">
<description>Two-node jack with ground / mechanical strength pad.</description>
<gates>
<gate name="G$1" symbol="JACK-2S"/>
</gates>
<devices>
<device name="" package="JACK-PP-45-PCB-2V">
<connects>
<connect gate="G$1" pin="1" pad="J1A J1B"/>
<connect gate="G$1" pin="2" pad="J2A J2B"/>
<connect gate="G$1" pin="G" pad="CLAMP1 CLAMP2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LDO-3PIN" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="LDO-3PIN"/>
</gates>
<devices>
<device name="DPAK" package="DPAK">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DPAK-3" package="DPAK-3">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-BD" prefix="D" uservalue="yes">
<description>Bi-directional LED.</description>
<gates>
<gate name="G$1" symbol="LED-BD"/>
</gates>
<devices>
<device name="T-1" package="LED-BD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOD-CTRL-SINE-190226R1" prefix="U" uservalue="yes">
<description>True sine controller &amp; gate driver card for power applications.</description>
<gates>
<gate name="G$1" symbol="MOD-CTRL-SINE-190226R1"/>
</gates>
<devices>
<device name="" package="MOD-CTRL-SINE-190226R1">
<connects>
<connect gate="G$1" pin="ACK" pad="ACK"/>
<connect gate="G$1" pin="CA" pad="CA"/>
<connect gate="G$1" pin="CB" pad="CB"/>
<connect gate="G$1" pin="CMD" pad="CMD"/>
<connect gate="G$1" pin="HA" pad="HA"/>
<connect gate="G$1" pin="HB" pad="HB"/>
<connect gate="G$1" pin="LA" pad="LA"/>
<connect gate="G$1" pin="LB" pad="LB"/>
<connect gate="G$1" pin="SA" pad="SA"/>
<connect gate="G$1" pin="SB" pad="SB"/>
<connect gate="G$1" pin="TMP" pad="TMP"/>
<connect gate="G$1" pin="V+" pad="V+"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
<connect gate="G$1" pin="VSS" pad="VSS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOD-GD-FB-190131" prefix="U" uservalue="yes">
<description>Full bridge gate driver module with current sense, rev 190131.</description>
<gates>
<gate name="G$1" symbol="MOD-GD-FB-190131"/>
</gates>
<devices>
<device name="" package="MOD-GD-FB-190131">
<connects>
<connect gate="G$1" pin="AC" pad="AC"/>
<connect gate="G$1" pin="AH" pad="AH"/>
<connect gate="G$1" pin="AL" pad="AL"/>
<connect gate="G$1" pin="AS" pad="AS"/>
<connect gate="G$1" pin="BC" pad="BC"/>
<connect gate="G$1" pin="BH" pad="BH"/>
<connect gate="G$1" pin="BL" pad="BL"/>
<connect gate="G$1" pin="BS" pad="BS"/>
<connect gate="G$1" pin="CS" pad="CS"/>
<connect gate="G$1" pin="HIA" pad="HIA"/>
<connect gate="G$1" pin="HIB" pad="HIB"/>
<connect gate="G$1" pin="INV+" pad="INV+"/>
<connect gate="G$1" pin="INV-" pad="INV-"/>
<connect gate="G$1" pin="LIA" pad="LIA"/>
<connect gate="G$1" pin="LIB" pad="LIB"/>
<connect gate="G$1" pin="R+" pad="R+"/>
<connect gate="G$1" pin="R-" pad="R-"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VS" pad="VS"/>
<connect gate="G$1" pin="VSS" pad="VSS"/>
<connect gate="G$1" pin="VSS1" pad="VSS1"/>
<connect gate="G$1" pin="VSS2" pad="VSS2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOV" prefix="MOV" uservalue="yes">
<gates>
<gate name="G$1" symbol="MOV"/>
</gates>
<devices>
<device name="CH8" package="MOV-CH8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NFET" prefix="Q" uservalue="yes">
<gates>
<gate name="G$1" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="D2PAK" package="D2PAK">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO220H" package="TO220H">
<connects>
<connect gate="G$1" pin="D" pad="2 T"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO220H-2" package="TO220H-2">
<connects>
<connect gate="G$1" pin="D" pad="T"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO220V" package="TO220V">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO252-3" package="TO-252-3">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO263-7106" package="TO-263-7106">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO263AB" package="TO-263AB">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NTC" prefix="RT" uservalue="yes">
<description>NTC Thermistor</description>
<gates>
<gate name="G$1" symbol="MOV"/>
</gates>
<devices>
<device name="805" package="R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PAD" prefix="P" uservalue="yes">
<gates>
<gate name="G$1" symbol="PAD"/>
</gates>
<devices>
<device name=".032" package="PAD-RND-AUTO/032">
<connects>
<connect gate="G$1" pin="P" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".040" package=".06/.040">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".041" package=".1/.041">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".052" package=".1/.052">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".65M" package="PAD-RND-AUTO/.65-M">
<connects>
<connect gate="G$1" pin="P" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".120" package=".16/.120">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".0635" package=".15/.0635">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.5SMD" package="PAD-RT-5_2.5-M">
<connects>
<connect gate="G$1" pin="P" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5SMD" package="PAD-SQ-5_5-M">
<connects>
<connect gate="G$1" pin="P" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="8X8" package="PAD-8X8-3_25-M">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="8X10" package="PAD-8X10-3_25-M">
<connects>
<connect gate="G$1" pin="P" pad="B1 P1 T1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O067" package="PAD-OCT-120-/067">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R040" package="PAD-RND-AUTO/040">
<connects>
<connect gate="G$1" pin="P" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PFET" prefix="Q" uservalue="yes">
<gates>
<gate name="G$1" symbol="P-MOSFET"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT223" package="SOT-223">
<connects>
<connect gate="G$1" pin="D" pad="2 4"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92" package="TO92-SGD">
<connects>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F1776" prefix="U" uservalue="yes">
<description>PIC16f1776</description>
<gates>
<gate name="G$1" symbol="PIC16F1776"/>
</gates>
<devices>
<device name="SO" package="SO-28W">
<connects>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RA6" pad="10"/>
<connect gate="G$1" pin="RA7" pad="9"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6" pad="27"/>
<connect gate="G$1" pin="RB7" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VPP" pad="1"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SS" package="SSOP-28">
<connects>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="4"/>
<connect gate="G$1" pin="RA3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5" pad="7"/>
<connect gate="G$1" pin="RA6" pad="10"/>
<connect gate="G$1" pin="RA7" pad="9"/>
<connect gate="G$1" pin="RB0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6" pad="27"/>
<connect gate="G$1" pin="RB7" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RC6" pad="17"/>
<connect gate="G$1" pin="RC7" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VPP" pad="1"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R-AC-DUPLEX" prefix="J" uservalue="yes">
<description>NEMA 120VAC duplex receptacle.</description>
<gates>
<gate name="G$1" symbol="R-AC-DUPLEX"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="_EXTERNAL_" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<description>Resistor</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="2512" package="R2512-CS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2515" package="RES_WSC_2515">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2515L" package="RES_WSC_2515-L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2515M" package="RES_WSC_2515-M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DPAK" package="DPAK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MCR25" package="MCR25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MCR50" package="MCR50">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MCR50B" package="MCR50B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P0613/15" package="P0613/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO252" package="TO-252-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO263" package="TO-263AB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCHOTTKY" prefix="D" uservalue="yes">
<gates>
<gate name="G$1" symbol="SCHOTTKY"/>
</gates>
<devices>
<device name="SMA" package="SMA">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMB" package="SMB">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMBJ" package="SMBJ">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMC" package="SMC">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD123" package="SOD123">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI8621" prefix="U" uservalue="yes">
<description>Silicon Labs 1x1 1 Mbps, 2.5 kVRMS Digital Isolator</description>
<gates>
<gate name="G$1" symbol="SI8621"/>
</gates>
<devices>
<device name="SOIC" package="SO08">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="B1" pad="7"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMPS-DC-DC" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="SMPS-DC-DC"/>
</gates>
<devices>
<device name="SCWN06" package="DIP24">
<connects>
<connect gate="G$1" pin="+VIN" pad="22 23"/>
<connect gate="G$1" pin="+VOUT" pad="14"/>
<connect gate="G$1" pin="-VIN" pad="2 3"/>
<connect gate="G$1" pin="-VOUT" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPST-M" prefix="S" uservalue="yes">
<description>SPST switch with mount / ground shield connection.</description>
<gates>
<gate name="G$1" symbol="SPST-M"/>
</gates>
<devices>
<device name="VERT" package="SPST-200AWMSP1T1A1M7QE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="G" pad="G"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="T_P1_S1_S2_SCR" prefix="T" uservalue="yes">
<gates>
<gate name="G$1" symbol="T_P1_S1_S2_SCR"/>
</gates>
<devices>
<device name="RM14" package="RM14-SCR">
<connects>
<connect gate="G$1" pin="G1" pad="G1"/>
<connect gate="G$1" pin="G2" pad="G2"/>
<connect gate="G$1" pin="G3" pad="G3"/>
<connect gate="G$1" pin="G4" pad="G4"/>
<connect gate="G$1" pin="P1" pad="1 2 3"/>
<connect gate="G$1" pin="P2" pad="4 5 6"/>
<connect gate="G$1" pin="PG" pad="PG"/>
<connect gate="G$1" pin="S1A" pad="8"/>
<connect gate="G$1" pin="S1B" pad="7"/>
<connect gate="G$1" pin="S2A" pad="11"/>
<connect gate="G$1" pin="S2B" pad="10"/>
<connect gate="G$1" pin="SG" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-MICRO" prefix="X" uservalue="yes">
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="AB" package="ZX62-AB">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="GND@3" pad="GND@3"/>
<connect gate="G$1" pin="GND@4" pad="GND@4"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZENER" prefix="D" uservalue="yes">
<gates>
<gate name="G$1" symbol="ZENER"/>
</gates>
<devices>
<device name="SMA" package="SMA">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMB" package="SMB">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMBJ" package="SMBJ">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMC" package="SMC">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD123" package="SOD123">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS21864S" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="IRS21864S"/>
</gates>
<devices>
<device name="SOIC" package="SO14">
<connects>
<connect gate="G$1" pin="COM" pad="5"/>
<connect gate="G$1" pin="HIN" pad="1"/>
<connect gate="G$1" pin="HO" pad="12"/>
<connect gate="G$1" pin="LIN" pad="2"/>
<connect gate="G$1" pin="LO" pad="6"/>
<connect gate="G$1" pin="VB" pad="13"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VS" pad="11"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NPN" prefix="Q" uservalue="yes">
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92" package="TO92-EBC">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPAMP-S" prefix="U" uservalue="yes">
<description>Generic device for single op-amps.  Variant indicates model.</description>
<gates>
<gate name="G$1" symbol="OPAMP"/>
</gates>
<devices>
<device name="OPA197_SOO8" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OPA197_SOT23-5" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="J1"/>
</gates>
<devices>
<device name="J1-1,27" package="J1-1,27">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J1-68" package="J1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F18324" prefix="U" uservalue="yes">
<description>PIC16(L)F18324/18344 microcontrollers feature Analog, Core Independent Peripherals
and Communication Peripherals, combined with eXtreme Low Power (XLP) for a wide
 range of general purpose and low-power applications. The Peripheral Pin Select (PPS)
 functionality enables pin mapping when using the digital peripherals (CLC, CWG, CCP,
 PWM and communications) to add flexibility to the application design. 

http://ww1.microchip.com/downloads/en/DeviceDoc/40001800A.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16F18324"/>
</gates>
<devices>
<device name="DIL" package="DIL14">
<connects>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="ICSPCLK" pad="12"/>
<connect gate="G$1" pin="ICSPDAT" pad="13"/>
<connect gate="G$1" pin="RA2" pad="11"/>
<connect gate="G$1" pin="RC0" pad="10"/>
<connect gate="G$1" pin="RC1" pad="9"/>
<connect gate="G$1" pin="RC2" pad="8"/>
<connect gate="G$1" pin="RC3" pad="7"/>
<connect gate="G$1" pin="RC4" pad="6"/>
<connect gate="G$1" pin="RC5" pad="5"/>
<connect gate="G$1" pin="SOSCI" pad="2"/>
<connect gate="G$1" pin="SOSCO" pad="3"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VPP" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO08" package="SO14">
<connects>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="ICSPCLK" pad="12"/>
<connect gate="G$1" pin="ICSPDAT" pad="13"/>
<connect gate="G$1" pin="RA2" pad="11"/>
<connect gate="G$1" pin="RC0" pad="10"/>
<connect gate="G$1" pin="RC1" pad="9"/>
<connect gate="G$1" pin="RC2" pad="8"/>
<connect gate="G$1" pin="RC3" pad="7"/>
<connect gate="G$1" pin="RC4" pad="6"/>
<connect gate="G$1" pin="RC5" pad="5"/>
<connect gate="G$1" pin="SOSCI" pad="2"/>
<connect gate="G$1" pin="SOSCO" pad="3"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VPP" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
