(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1ubuntu2)
  (general
    (links 17)
    (no_connects 0)
    (area 121.944143 65.264 184.252858 108.191)
    (thickness 1.6)
    (drawings 9)
    (tracks 458)
    (zones 0)
    (modules 5)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.00254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 7 7)
    (pad_drill 4.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4_ISO14580_Pad (layer F.Cu) (tedit 5CEDBA1D)
    (at 168.91 102.362)
    (descr "Mounting Hole 4.3mm, M4, ISO14580")
    (tags "mounting hole 4.3mm m4 iso14580")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_4.3mm_M4_ISO14580_Pad (at 0 4.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0.254 -0.508) (size 7 7) (drill 4.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4_ISO14580_Pad (layer F.Cu) (tedit 5CEDBA05)
    (at 168.91 70.739)
    (descr "Mounting Hole 4.3mm, M4, ISO14580")
    (tags "mounting hole 4.3mm m4 iso14580")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_4.3mm_M4_ISO14580_Pad (at 0 4.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0.254 0.127) (size 7 7) (drill 4.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4_ISO14580_Pad (layer F.Cu) (tedit 5CEDB9FD)
    (at 137.287 71.247)
    (descr "Mounting Hole 4.3mm, M4, ISO14580")
    (tags "mounting hole 4.3mm m4 iso14580")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_4.3mm_M4_ISO14580_Pad (at 0 4.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0.889 -0.381) (size 7 7) (drill 4.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4_ISO14580_Pad (layer F.Cu) (tedit 5CEDBA15)
    (at 138.43 102.616)
    (descr "Mounting Hole 4.3mm, M4, ISO14580")
    (tags "mounting hole 4.3mm m4 iso14580")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_4.3mm_M4_ISO14580_Pad (at 0 4.5) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.254 -0.762) (size 7 7) (drill 4.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connectors:SMA_SMD_Jack_Straight (layer F.Cu) (tedit 58C35474)
    (at 153.67 98.21 90)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference J1 (at 0 -5 90) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 5 90) (layer F.Fab))
    (fp_text user %R (at 0 -5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.85 2.38 110) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.85 2.38 70) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.85 -2.38 70) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.85 -2.38 110) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.515 1.749 140) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.515 1.749 40) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.515 -1.749 40) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.515 -1.749 140) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.6 2.38 180) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 2.8 180) (size 1.51 7.11) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.6 2.38 180) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.6 -2.38 180) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd circle (at 0 0 180) (size 1.73 1.73) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0 -2.8 180) (size 1.51 7.11) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.6 -2.38 180) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (gr_text "KF5COQ\n\nWR90 to MSL adapter" (at 153.67 74.93) (layer F.SilkS))
  (gr_line (start 132.969 107.061) (end 132.969 65.659) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.371 65.659) (end 174.371 107.061) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.371 107.188) (end 132.969 107.188) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.969 65.659) (end 174.371 65.659) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch none 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.00254))
    (min_thickness 0.0254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 154.942344 86.992656) (xy 153.672344 88.262656) (xy 152.402344 86.992656) (xy 153.037344 86.357656) (xy 154.307344 86.357656)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch none 0.508)
    (connect_pads yes (clearance 0.00254))
    (min_thickness 0.0254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 174.371 107.188) (xy 132.969 107.188) (xy 132.969 65.659) (xy 174.371 65.659)
      )
    )
    (polygon
      (pts        (xy 142.24 81.28) (xy 142.24 91.44) (xy 152.908 91.44) (xy 152.908 96.52) (xy 142.24 96.52)
        (xy 142.24 101.6) (xy 165.1 101.6) (xy 165.1 81.28)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch none 0.508)
    (connect_pads yes (clearance 0.00254))
    (min_thickness 0.0254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 165.1 96.52) (xy 165.061804 91.44) (xy 154.432 91.44) (xy 154.432 96.52)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch none 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.00254))
    (min_thickness 0.0254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 142.24 96.52) (xy 151.384 96.52) (xy 151.384 101.6) (xy 142.24 101.6)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch none 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.00254))
    (min_thickness 0.0254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 155.956 96.52) (xy 165.1 96.52) (xy 165.1 101.6) (xy 155.956 101.6)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch none 0.508)
    (connect_pads yes (clearance 0.00254))
    (min_thickness 0.0254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 174.371 107.188) (xy 132.969 107.188) (xy 132.969 65.659) (xy 174.371 65.659)
      )
    )
    (polygon
      (pts        (xy 142.24 81.28) (xy 142.24 91.44) (xy 152.908 91.44) (xy 142.24 91.44) (xy 165.1 91.44)
        (xy 165.1 81.28)
      )
    )
  )
)
