<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<library>
<description>Generated from &lt;b&gt;GabozeExpress.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="-503182-1852_MOLEX_503182-1852">
</package>
<package name="2.6&quot;-TFT-51P_TFT-DISPLAY-2.6-51PIN">
</package>
<package name="CONDUCTIVE-BUTTONS_CONDUCTIVE_BUTTON_DIRECTIONAL_THICK">
</package>
<package name="CONDUCTIVE-BUTTONS_CONDUCTIVE_BUTTON_THICK">
</package>
<package name="CONDUCTIVE-BUTTONS_CONDUCTIVE_BUTTON_THICK_STARTSELECT">
</package>
<package name="ESP32-WROVER_ESP32-WROVER">
</package>
<package name="GBA_VOLUME">
</package>
<package name="LED_DUOLED-A-3MM">
<description>&lt;b&gt;T-1(3mm) BI-COLOR INDICATOR LAMP&lt;/b&gt;&lt;p&gt;
Source: Kingbright .. 2_colour_led_.pdf</description>
</package>
<package name="MICROBUILDER_0603-MINI">
<description>0603-Mini
&lt;p&gt;Mini footprint for dense boards&lt;/p&gt;</description>
</package>
<package name="MICROBUILDER_EIA3216-18/A-W">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="MICROBUILDER_SOD-123">
<description>&lt;b&gt;SOD-123&lt;/b&gt;
&lt;p&gt;Source: http://www.diodes.com/datasheets/ds30139.pdf&lt;/p&gt;</description>
</package>
<package name="MICROBUILDER_SOT23-5$1">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
<package name="MICROBUILDER_SOT23-R">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Reflow soldering</description>
</package>
<package name="SEEED-CONNECTOR_MICRO-USB5+6P-SMD-0.65-AB">
</package>
<package name="SPARKFUN-CONNECTORS_1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-CONNECTORS_AUDIO-JACK-KIT">
<description>&lt;h3&gt;3.5mm Stereo Audio Jack -Kit Version&lt;/h3&gt;
Reduced openings in tStop, pins spread a tiny bit out to hold part on PCB during assembly
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Audio-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-CONNECTORS_JST-2-SMD">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-RETIRED_KPS-1290">
</package>
<package name="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_4.6X2.8MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 4.6 x 2.8mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ck-components.com/media/1479/kmr2.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN_SOT23-3">
</package>
<package name="TESTPAD_TP18R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TEXAS_SOIC8">
</package>
<package name="GABOZEPOCAIOGO_MICROBUILDER_0603-MINI">
<description>0603-Mini
&lt;p&gt;Mini footprint for dense boards&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-IC-COMMS_SSOP28DB">
<description>&lt;h3&gt;Small Shrink Outline Package - 28 DB&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 28&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;FT232RL&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MICROBUILDER_CHIPLED_0603">
<description>&lt;b&gt;CHIPLED 0603&lt;/b&gt;</description>
</package>
<package name="MICROBUILDER_SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
<package name="_EXPRESS">
</package>
<package name="_GITHUB">
</package>
</packages>
<symbols>
<symbol name="503182-1852_503182-1852">
<pin name="CD/DAT3"/>
<pin name="CLK" function="clk"/>
<pin name="CMD"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="DATA2"/>
<pin name="DETECT"/>
<pin name="SHIELD" direction="pas"/>
<pin name="SWITCH"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="2.6&quot;-TFT-51P_TFT-DISPLAY-2.6-51PIN">
<pin name="BS0"/>
<pin name="BS1"/>
<pin name="BS2"/>
<pin name="BS3"/>
<pin name="CSX"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="DB8"/>
<pin name="DB9"/>
<pin name="DB10"/>
<pin name="DB11"/>
<pin name="DB12"/>
<pin name="DB13"/>
<pin name="DB14"/>
<pin name="DB15"/>
<pin name="DB16"/>
<pin name="DB17"/>
<pin name="DE"/>
<pin name="DSI_CLKN"/>
<pin name="DSI_CLKP"/>
<pin name="DSI_DON"/>
<pin name="DSI_DOP"/>
<pin name="DSI_VCC"/>
<pin name="FMARK"/>
<pin name="GND"/>
<pin name="HSYNC"/>
<pin name="IOVCC"/>
<pin name="LEDA"/>
<pin name="LEDK1"/>
<pin name="LEDK2"/>
<pin name="LEDK3"/>
<pin name="LEDK4"/>
<pin name="PCLK"/>
<pin name="PWM_OUT"/>
<pin name="RDX"/>
<pin name="RESET"/>
<pin name="RSX"/>
<pin name="SDI"/>
<pin name="VCC"/>
<pin name="VSYNC"/>
<pin name="WRX"/>
<pin name="XL"/>
<pin name="XR"/>
<pin name="YD"/>
<pin name="YU"/>
</symbol>
<symbol name="CONDUCTIVE-BUTTONS_CONDUCTIVE_BUTTON">
<pin name="P$ACTIVE"/>
<pin name="P$GND"/>
</symbol>
<symbol name="CONDUCTIVE-BUTTONS_CONDUCTIVE_BUTTON_STARTSELECT">
<pin name="P$ACTIVE"/>
<pin name="P$GND"/>
</symbol>
<symbol name="ESP32-WROVER_ESP32-WROVER">
<pin name="3V3"/>
<pin name="CLK"/>
<pin name="CMD"/>
<pin name="EN"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="IO0"/>
<pin name="IO2"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO15"/>
<pin name="IO18"/>
<pin name="IO19"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="NC"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="P_GND"/>
<pin name="RXD0"/>
<pin name="SD0"/>
<pin name="SD1"/>
<pin name="SD2"/>
<pin name="SD3"/>
<pin name="SENSR_VN"/>
<pin name="SENSR_VP"/>
<pin name="TXD0"/>
</symbol>
<symbol name="GBA_VOLUME">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="LED_DUOLED-RG-A">
<pin name="A" direction="pas"/>
<pin name="CG" direction="pas"/>
<pin name="CR" direction="pas"/>
</symbol>
<symbol name="MICROBUILDER_CAPACITOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="MICROBUILDER_CAPACITOR_POL">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="MICROBUILDER_DIODE-SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="MICROBUILDER_MCP73831/2">
<pin name="PROG" direction="in"/>
<pin name="STAT" direction="out"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="MICROBUILDER_MOSFET-P">
<pin name="D" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="MICROBUILDER_RESISTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SEEED-CONNECTOR_ZX62D-B-5P8(30)(11)">
<description>&lt;b&gt;ZX62D-B-5P8(30)(11)&lt;/b&gt;&lt;br&gt;
Hirose Micro-USB B connector&lt;br&gt;
SMD type&lt;br&gt;</description>
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND" direction="sup"/>
<pin name="ID"/>
<pin name="SHIELD" direction="sup"/>
<pin name="VBUS" direction="sup"/>
</symbol>
<symbol name="SPARKFUN-CONNECTORS_AUDIO-JACK2">
<description>&lt;h3&gt; Audio Jack &lt;/h3&gt;
&lt;p&gt;  Basic Audio Jack with bypass switches&lt;/p&gt;</description>
<pin name="RING"/>
<pin name="RSH"/>
<pin name="SLEEVE"/>
<pin name="TIP"/>
<pin name="TSH"/>
</symbol>
<symbol name="SPARKFUN-CONNECTORS_CONN_02">
<description>&lt;h3&gt;2 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SPARKFUN-CONNECTORS_JST_2MM_MALE">
<pin name="+"/>
<pin name="-"/>
<pin name="PAD1"/>
<pin name="PAD2"/>
</symbol>
<symbol name="SPARKFUN-RETIRED_SW_SPDT">
<pin name="O" direction="pas"/>
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="SPARKFUN-SWITCHES_SWITCH-MOMENTARY-2">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SPARKFUN_NPN">
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
</symbol>
<symbol name="SUPPLY1_GND:1">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="TESTPAD_PS">
<pin name="TP" direction="in"/>
</symbol>
<symbol name="TEXAS_LM4875">
<pin name="BYP"/>
<pin name="DC_VOL" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="HPHONE" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="VOUT1" direction="out"/>
<pin name="VOUT2" direction="out"/>
</symbol>
<symbol name="GABOZEPOCAIOGO_MICROBUILDER_CAPACITOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SPARKFUN-IC-COMMS_FT232R">
<pin name="3V3OUT" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="CTS" direction="in" function="dot"/>
<pin name="DCD" direction="in" function="dot"/>
<pin name="DSR" direction="in" function="dot"/>
<pin name="DTR" direction="out" function="dot"/>
<pin name="GND7" direction="pwr"/>
<pin name="GND18" direction="pwr"/>
<pin name="GND21" direction="pwr"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="PWREN" direction="in" function="dot"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="RI" direction="in" function="dot"/>
<pin name="RTS" direction="out" function="dot"/>
<pin name="RXD" direction="in"/>
<pin name="RXLED" direction="in" function="dot"/>
<pin name="SLEEP" direction="in" function="dot"/>
<pin name="TEST" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="TXDEN" direction="in"/>
<pin name="TXLED" direction="in" function="dot"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
</symbol>
<symbol name="MICROBUILDER_LED">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="MICROBUILDER_VREG_SOT23-5">
<pin name="EN"/>
<pin name="GND"/>
<pin name="IN"/>
<pin name="OUT"/>
<pin name="P4"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="503182-1852_503182-1852" prefix="J">
<description>Conn Micro SD Card M 8 POS 1.09mm Solder RA SMD Embossed T/R 0.5A/Contact</description>
<gates>
<gate name="G$1" symbol="503182-1852_503182-1852"/>
</gates>
<devices>
<device name="" package="-503182-1852_MOLEX_503182-1852">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="2"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="3"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DATA2" pad="1"/>
<connect gate="G$1" pin="DETECT" pad="DT"/>
<connect gate="G$1" pin="SHIELD" pad="P1 P2 P3 P4 P5"/>
<connect gate="G$1" pin="SWITCH" pad="SW"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value=" MICRO SD NORMAL ULTRALOWPRO8CKTE "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="WM12834CT-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.ca/product-detail/en/molex/5031821852/WM12834CT-ND/5823232?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Molex"/>
<attribute name="MP" value="5031821852"/>
<attribute name="PACKAGE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.6&quot;-TFT-51P_TFT-DISPLAY-2.6-51PIN">
<description>ILI9342 51P 2.6" TFT LCD</description>
<gates>
<gate name="G$1" symbol="2.6&quot;-TFT-51P_TFT-DISPLAY-2.6-51PIN"/>
</gates>
<devices>
<device name="" package="2.6&quot;-TFT-51P_TFT-DISPLAY-2.6-51PIN">
<connects>
<connect gate="G$1" pin="BS0" pad="P$43"/>
<connect gate="G$1" pin="BS1" pad="P$44"/>
<connect gate="G$1" pin="BS2" pad="P$45"/>
<connect gate="G$1" pin="BS3" pad="P$46"/>
<connect gate="G$1" pin="CSX" pad="P$29"/>
<connect gate="G$1" pin="DB0" pad="P$11"/>
<connect gate="G$1" pin="DB1" pad="P$12"/>
<connect gate="G$1" pin="DB10" pad="P$21"/>
<connect gate="G$1" pin="DB11" pad="P$22"/>
<connect gate="G$1" pin="DB12" pad="P$23"/>
<connect gate="G$1" pin="DB13" pad="P$24"/>
<connect gate="G$1" pin="DB14" pad="P$25"/>
<connect gate="G$1" pin="DB15" pad="P$26"/>
<connect gate="G$1" pin="DB16" pad="P$27"/>
<connect gate="G$1" pin="DB17" pad="P$28"/>
<connect gate="G$1" pin="DB2" pad="P$13"/>
<connect gate="G$1" pin="DB3" pad="P$14"/>
<connect gate="G$1" pin="DB4" pad="P$15"/>
<connect gate="G$1" pin="DB5" pad="P$16"/>
<connect gate="G$1" pin="DB6" pad="P$17"/>
<connect gate="G$1" pin="DB7" pad="P$18"/>
<connect gate="G$1" pin="DB8" pad="P$19"/>
<connect gate="G$1" pin="DB9" pad="P$20"/>
<connect gate="G$1" pin="DE" pad="P$38"/>
<connect gate="G$1" pin="DSI_CLKN" pad="P$36"/>
<connect gate="G$1" pin="DSI_CLKP" pad="P$37"/>
<connect gate="G$1" pin="DSI_DON" pad="P$34"/>
<connect gate="G$1" pin="DSI_DOP" pad="P$35"/>
<connect gate="G$1" pin="DSI_VCC" pad="P$33"/>
<connect gate="G$1" pin="FMARK" pad="P$9"/>
<connect gate="G$1" pin="GND" pad="P$5"/>
<connect gate="G$1" pin="HSYNC" pad="P$40"/>
<connect gate="G$1" pin="IOVCC" pad="P$6"/>
<connect gate="G$1" pin="LEDA" pad="P$47"/>
<connect gate="G$1" pin="LEDK1" pad="P$48"/>
<connect gate="G$1" pin="LEDK2" pad="P$49"/>
<connect gate="G$1" pin="LEDK3" pad="P$50"/>
<connect gate="G$1" pin="LEDK4" pad="P$51"/>
<connect gate="G$1" pin="PCLK" pad="P$39"/>
<connect gate="G$1" pin="PWM_OUT" pad="P$8"/>
<connect gate="G$1" pin="RDX" pad="P$32"/>
<connect gate="G$1" pin="RESET" pad="P$10"/>
<connect gate="G$1" pin="RSX" pad="P$30"/>
<connect gate="G$1" pin="SDI" pad="P$42"/>
<connect gate="G$1" pin="VCC" pad="P$7"/>
<connect gate="G$1" pin="VSYNC" pad="P$41"/>
<connect gate="G$1" pin="WRX" pad="P$31"/>
<connect gate="G$1" pin="XL" pad="P$2"/>
<connect gate="G$1" pin="XR" pad="P$4"/>
<connect gate="G$1" pin="YD" pad="P$3"/>
<connect gate="G$1" pin="YU" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONDUCTIVE-BUTTONS_CONDUCTIVE_BUTTON">
<gates>
<gate name="G$1" symbol="CONDUCTIVE-BUTTONS_CONDUCTIVE_BUTTON"/>
</gates>
<devices>
<device name="CONDUCTIVE_BUTTON_DIRECTIONAL_THICK" package="CONDUCTIVE-BUTTONS_CONDUCTIVE_BUTTON_DIRECTIONAL_THICK">
<connects>
<connect gate="G$1" pin="P$ACTIVE" pad="P$ACTIVE"/>
<connect gate="G$1" pin="P$GND" pad="P$GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CONDUCTIVE_BUTTON_THICK" package="CONDUCTIVE-BUTTONS_CONDUCTIVE_BUTTON_THICK">
<connects>
<connect gate="G$1" pin="P$ACTIVE" pad="P$ACTIVE"/>
<connect gate="G$1" pin="P$GND" pad="P$GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONDUCTIVE-BUTTONS_CONDUCTIVE_BUTTON_STARTSELECT">
<gates>
<gate name="G$1" symbol="CONDUCTIVE-BUTTONS_CONDUCTIVE_BUTTON_STARTSELECT"/>
</gates>
<devices>
<device name="CONDUCTIVE_BUTTON_THICK_STARTSELECT" package="CONDUCTIVE-BUTTONS_CONDUCTIVE_BUTTON_THICK_STARTSELECT">
<connects>
<connect gate="G$1" pin="P$ACTIVE" pad="P$ACTIVE P$ACTIVE1 P$ACTIVE2 P$ACTIVE3 P$ACTIVE4 P$ACTIVE5 P$ACTIVE6"/>
<connect gate="G$1" pin="P$GND" pad="P$GND P$GND1 P$GND2 P$GND3" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP32-WROVER_ESP32-WROVER">
<gates>
<gate name="G$1" symbol="ESP32-WROVER_ESP32-WROVER"/>
</gates>
<devices>
<device name="" package="ESP32-WROVER_ESP32-WROVER">
<connects>
<connect gate="G$1" pin="3V3" pad="VDD33"/>
<connect gate="G$1" pin="CLK" pad="CLK"/>
<connect gate="G$1" pin="CMD" pad="CMD"/>
<connect gate="G$1" pin="EN" pad="EN"/>
<connect gate="G$1" pin="GND1" pad="GND"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND_2"/>
<connect gate="G$1" pin="IO0" pad="IO0"/>
<connect gate="G$1" pin="IO12" pad="IO12"/>
<connect gate="G$1" pin="IO13" pad="IO13"/>
<connect gate="G$1" pin="IO14" pad="IO14"/>
<connect gate="G$1" pin="IO15" pad="IO15"/>
<connect gate="G$1" pin="IO18" pad="IO18"/>
<connect gate="G$1" pin="IO19" pad="IO19"/>
<connect gate="G$1" pin="IO2" pad="IO2"/>
<connect gate="G$1" pin="IO21" pad="IO21"/>
<connect gate="G$1" pin="IO22" pad="IO22"/>
<connect gate="G$1" pin="IO23" pad="IO23"/>
<connect gate="G$1" pin="IO25" pad="IO25"/>
<connect gate="G$1" pin="IO26" pad="IO26"/>
<connect gate="G$1" pin="IO27" pad="IO27"/>
<connect gate="G$1" pin="IO32" pad="IO32"/>
<connect gate="G$1" pin="IO33" pad="IO33"/>
<connect gate="G$1" pin="IO34" pad="IO34"/>
<connect gate="G$1" pin="IO35" pad="IO35"/>
<connect gate="G$1" pin="IO4" pad="IO4"/>
<connect gate="G$1" pin="IO5" pad="IO5"/>
<connect gate="G$1" pin="NC" pad="NC0"/>
<connect gate="G$1" pin="NC1" pad="NC1"/>
<connect gate="G$1" pin="NC2" pad="NC2"/>
<connect gate="G$1" pin="P_GND" pad="GND3"/>
<connect gate="G$1" pin="RXD0" pad="RXD0"/>
<connect gate="G$1" pin="SD0" pad="SD0"/>
<connect gate="G$1" pin="SD1" pad="SD1"/>
<connect gate="G$1" pin="SD2" pad="SD2"/>
<connect gate="G$1" pin="SD3" pad="SD3"/>
<connect gate="G$1" pin="SENSR_VN" pad="SENSOR_VN"/>
<connect gate="G$1" pin="SENSR_VP" pad="SENSOR_VP"/>
<connect gate="G$1" pin="TXD0" pad="TXD0"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GBA_VOLUME" prefix="R" uservalue="yes">
<gates>
<gate name="R$1" symbol="GBA_VOLUME"/>
</gates>
<devices>
<device name="" package="GBA_VOLUME">
<connects>
<connect gate="R$1" pin="A" pad="1"/>
<connect gate="R$1" pin="E" pad="5"/>
<connect gate="R$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_L-115WEGW-CA" prefix="LED">
<description>&lt;b&gt;T-1(3mm) BI-COLOR INDICATOR LAMP&lt;/b&gt;&lt;p&gt;
Source: Kingbright .. 2_colour_led_.pdf</description>
<gates>
<gate name="G$1" symbol="LED_DUOLED-RG-A"/>
</gates>
<devices>
<device name="" package="LED_DUOLED-A-3MM">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="CG" pad="1"/>
<connect gate="G$1" pin="CR" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROBUILDER_CAP_CERAMIC" prefix="C" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Ceramic Capacitors&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;For new designs, use the packages preceded by an '_' character since they are more reliable:&lt;/p&gt;
&lt;p&gt;The following footprints should be used on most boards:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;_0402&lt;/b&gt; - Standard footprint for regular board layouts&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_0603&lt;/b&gt; - Standard footprint for regular board layouts&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_0805&lt;/b&gt; - Standard footprint for regular board layouts&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_1206&lt;/b&gt; - Standard footprint for regular board layouts&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;For extremely tight-pitch boards where space is at a premium, the following 'micro-pitch' footprints can be used (smaller pads, no silkscreen outline, etc.):&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;_0402MP&lt;/b&gt; - Micro-pitch footprint for very dense/compact boards&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_0603MP&lt;/b&gt; - Micro-pitch footprint for very dense/compact boards&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_0805MP&lt;/b&gt; - Micro-pitch footprint for very dense/compact boards&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_1206MP&lt;/b&gt; - Micro-pitch footprint for very dense/compact boards&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MICROBUILDER_CAPACITOR"/>
</gates>
<devices>
<device name="0603MINI" package="MICROBUILDER_0603-MINI">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROBUILDER_CAP_TANTALUM" prefix="C" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Tantalum Capacitors&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Wave&lt;/b&gt; footprints have larger pads and are meant to be used for hand soldering.&lt;br/&gt;
&lt;b&gt;Reflow&lt;/b&gt; footprints are optimised for solder paste and a reflow oven.&lt;/p&gt;
&lt;b&gt;EIA3216-18/A-[R/W]&lt;/b&gt; - Size A / 3216-18 / 1206 footprint
&lt;ul&gt;
&lt;li&gt;4.7µF 25V 10% Tantalum Capacitor&lt;/li&gt;
&lt;li&gt;10µF 16V 10% Tantalum Capacitor [Digikey: 495-2236-2-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;EIA3528-21/B-[R/W]&lt;/b&gt; - Size B / 3528-21
&lt;ul&gt;
&lt;li&gt;47µF 10V 10% Tantalum Capactior [Digikey: 495-2216-1-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;EIA6032-28/C-[R/W]&lt;/b&gt; - Size C / 6032-28
&lt;ul&gt;
&lt;li&gt;10µF 35V 20% Tantalum Capacitor [Digikey: 495-2285-1-ND]&lt;/li&gt;
&lt;li&gt;100µF 16V 10% Tantalum Capactior [Digikey: 399-5214-1-ND]&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MICROBUILDER_CAPACITOR_POL"/>
</gates>
<devices>
<device name="A/3216_WAVE" package="MICROBUILDER_EIA3216-18/A-W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROBUILDER_DIODE-SCHOTTKY" prefix="D" uservalue="yes">
<gates>
<gate name="G$1" symbol="MICROBUILDER_DIODE-SCHOTTKY"/>
</gates>
<devices>
<device name="SOD-123" package="MICROBUILDER_SOD-123">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23_REFLOW" package="MICROBUILDER_SOT23-R">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROBUILDER_MCP73831/2" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;MCP73831/2 LIPO Charger&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;VDD: 3.75 - 6V&lt;/li&gt;
&lt;li&gt;Temp -40 - 85°C&lt;/li&gt;
&lt;li&gt;Programmable Charge Rate: 15-500mA&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;
&lt;p&gt;&lt;b&gt;NOTE:&lt;/b&gt; STAT is a tri-state logic output on the MCP73831 and an open-drain output on the MCP73832.&lt;/p&gt;
&lt;p&gt;SOT23-5 with 4.2V output and tri-state logic on STAT = MCP73831T-2ACI/OT&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MICROBUILDER_MCP73831/2"/>
</gates>
<devices>
<device name="" package="MICROBUILDER_SOT23-5$1">
<connects>
<connect gate="G$1" pin="PROG" pad="5"/>
<connect gate="G$1" pin="STAT" pad="1"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROBUILDER_MOSFET-P" prefix="Q" uservalue="yes">
<description>&lt;b&gt;P-Channel Mosfet&lt;/b&gt;
&lt;p&gt;&lt;b&gt;LEGEND&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;
&lt;b&gt;VDS&lt;/b&gt;: Voltage Drain-Source&lt;br/&gt;
&lt;b&gt;ID&lt;/b&gt;: Drain Current&lt;br/&gt;
&lt;b&gt;RDS(ON)&lt;/b&gt;: Drain-Source On-State Resistance&lt;br/&gt;
&lt;b&gt;VGS(TH)&lt;/b&gt;: Gate-Source Threshold Voltage&lt;br/&gt;
&lt;b&gt;CISS&lt;/b&gt;: Drain-Source Input Capacitance
&lt;/p&gt;
&lt;p&gt;
&lt;b&gt;SOT-23&lt;/b&gt;
&lt;table border="0" width="90%" cellspacing="0" cellpadding="5"&gt;
&lt;tr bgcolor="#DDDDDD"&gt;
&lt;td&gt;Name&lt;/td&gt;
&lt;td&gt;VDS&lt;/td&gt;
&lt;td&gt;ID&lt;/td&gt;
&lt;td&gt;RDS(ON)&lt;/td&gt;
&lt;td&gt;VGS(TH)&lt;/td&gt;
&lt;td&gt;CISS&lt;/td&gt;
&lt;td&gt;Order Number&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;IRLML5103&lt;/td&gt;
&lt;td&gt;30V&lt;/td&gt;
&lt;td&gt;760mA&lt;/td&gt;
&lt;td&gt;600 mOhm&lt;/td&gt;
&lt;td&gt;--&lt;/td&gt;
&lt;td&gt;75pF @ 25V&lt;/td&gt;
&lt;td&gt;Digikey: IRLML5103PBFCT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;IRLML6401&lt;/td&gt;
&lt;td&gt;12V&lt;/td&gt;
&lt;td&gt;4.3A&lt;/td&gt;
&lt;td&gt;50 mOhm&lt;/td&gt;
&lt;td&gt;950mV @ 250µA&lt;/td&gt;
&lt;td&gt;830pF @ 10V&lt;/td&gt;
&lt;td&gt;Digikey: IRLML6401PBFTR-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;NTR0202PL&lt;/td&gt;
&lt;td&gt;20V&lt;/td&gt;
&lt;td&gt;400mA&lt;/td&gt;
&lt;td&gt;800 mOhm&lt;/td&gt;
&lt;td&gt;2.3V @ 250uA&lt;/td&gt;
&lt;td&gt;70pF @ 5V&lt;/td&gt;
&lt;td&gt;Digikey: NTR0202PLT1GOSTR-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;NTR4101PT1G&lt;/td&gt;
&lt;td&gt;20V&lt;/td&gt;
&lt;td&gt;1.8A&lt;/td&gt;
&lt;td&gt;85 mOhm&lt;/td&gt;
&lt;td&gt;1.2V @ 250uA&lt;/td&gt;
&lt;td&gt;675pF @ 10V&lt;/td&gt;
&lt;td&gt;Digikey: NTR4101PT1GOSCT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;DMP2004K&lt;/td&gt;
&lt;td&gt;20V&lt;/td&gt;
&lt;td&gt;600mA&lt;/td&gt;
&lt;td&gt;900 mOhm&lt;/td&gt;
&lt;td&gt;1V @ 250uA&lt;/td&gt;
&lt;td&gt;175pF @ 16V&lt;/td&gt;
&lt;td&gt;Digikey: DMP2004KDICT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;PMV65XP&lt;/td&gt;
&lt;td&gt;20V&lt;/td&gt;
&lt;td&gt;3.9A&lt;/td&gt;
&lt;td&gt;76 mOhm&lt;/td&gt;
&lt;td&gt;950mV @ 1mA&lt;/td&gt;
&lt;td&gt;725pF @ 20V&lt;/td&gt;
&lt;td&gt;Digikey: 568-2358-2-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt; 
&lt;b&gt;TO-252&lt;/b&gt;
&lt;table border="0" width="90%" cellspacing="0" cellpadding="5"&gt;
&lt;tr bgcolor="#DDDDDD"&gt;
&lt;td&gt;Name&lt;/td&gt;
&lt;td&gt;VDS&lt;/td&gt;
&lt;td&gt;ID&lt;/td&gt;
&lt;td&gt;RDS(ON)&lt;/td&gt;
&lt;td&gt;VGS(TH)&lt;/td&gt;
&lt;td&gt;CISS&lt;/td&gt;
&lt;td&gt;Order Number&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;AOD417&lt;/td&gt;
&lt;td&gt;30V&lt;/td&gt;
&lt;td&gt;25A&lt;/td&gt;
&lt;td&gt;34 mOhm&lt;/td&gt;
&lt;td&gt;3V @ 250µA&lt;/td&gt;
&lt;td&gt;920pF @ 15V&lt;/td&gt;
&lt;td&gt;Digikey: 785-1106-2-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MICROBUILDER_MOSFET-P"/>
</gates>
<devices>
<device name="" package="MICROBUILDER_SOT23-R">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROBUILDER_RESISTOR" prefix="R" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Resistors&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;For new designs, use the packages preceded by an '_' character since they are more reliable:&lt;/p&gt;
&lt;p&gt;The following footprints should be used on most boards:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;_0402&lt;/b&gt; - Standard footprint for regular board layouts&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_0603&lt;/b&gt; - Standard footprint for regular board layouts&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_0805&lt;/b&gt; - Standard footprint for regular board layouts&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_1206&lt;/b&gt; - Standard footprint for regular board layouts&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;For extremely tight-pitch boards where space is at a premium, the following 'micro-pitch' footprints can be used (smaller pads, no silkscreen outline, etc.):&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;_0402MP&lt;/b&gt; - Micro-pitch footprint for very dense/compact boards&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_0603MP&lt;/b&gt; - Micro-pitch footprint for very dense/compact boards&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_0805MP&lt;/b&gt; - Micro-pitch footprint for very dense/compact boards&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_1206MP&lt;/b&gt; - Micro-pitch footprint for very dense/compact boards&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MICROBUILDER_RESISTOR"/>
</gates>
<devices>
<device name="0603MINI" package="MICROBUILDER_0603-MINI">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CONNECTOR_MICRO-USB-SMD(ZX62D-B-5P8(30))" prefix="USB" uservalue="yes">
<description>320010005</description>
<gates>
<gate name="G$1" symbol="SEEED-CONNECTOR_ZX62D-B-5P8(30)(11)"/>
</gates>
<devices>
<device name="" package="SEEED-CONNECTOR_MICRO-USB5+6P-SMD-0.65-AB">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="P1 P2 P3 P4 P5 P6"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ZX62D-B-5P8(30)"/>
<attribute name="VALUE" value="ZX62D-B-5P8(30)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-CONNECTORS_AUDIO_JACK_3.5MM" prefix="J">
<description>&lt;h3&gt;Audio Jack&lt;/h3&gt;
&lt;p&gt; 3.5mm variants of PTH and SMT stereo audio jack with bypass switches.&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/11177]”&gt;SparkFun SparkPunk Sound Kit &lt;/a&gt; - PTH&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13720”&gt;MP3 Trigger&lt;/a&gt; -3.5mm SMD&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11888”&gt;SparkFun PicoBoard&lt;/a&gt;- 2.5mm SMD&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-CONNECTORS_AUDIO-JACK2"/>
</gates>
<devices>
<device name="_KIT" package="SPARKFUN-CONNECTORS_AUDIO-JACK-KIT">
<connects>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RSH" pad="RSH"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TSH" pad="TSH"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10353"/>
<attribute name="SF_ID" value="PRT-08032"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-CONNECTORS_CONN_02" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;

 Molex polarized connector foot print use with: PRT-08233 with associated crimp pins and housings.&lt;br&gt;&lt;br&gt;

2.54_SCREWTERM for use with  PRT-10571.&lt;br&gt;&lt;br&gt;

3.5mm Screw Terminal footprints for  PRT-08084&lt;br&gt;&lt;br&gt;

5mm Screw Terminal footprints for use with PRT-08432</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-CONNECTORS_CONN_02"/>
</gates>
<devices>
<device name="" package="SPARKFUN-CONNECTORS_1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13512"/>
<attribute name="SF_ID" value="PRT-09918"/>
<attribute name="SF_SKU" value="PRT-08432"/>
<attribute name="SKU" value="PRT-09914"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-CONNECTORS_JST_2MM_MALE" prefix="J" uservalue="yes">
<description>&lt;h3&gt;JST 2MM MALE RA CONNECTOR&lt;/h3&gt;
Two pin, compact surface mount connector. Commonly used as a battery input connection point. We really like the solid locking feeling and high current rating on these small connectors. We use these all the time as battery connectors. Mates to single-cell LiPo batteries.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8612"&gt;JST Right Angle Connector - White&lt;/a&gt; (PRT-08612)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/Connectors/JST-Horizontal.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It was used on these SparkFun products:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11214"&gt;SparkFun MOSFET Power Controller&lt;/a&gt; (PRT-11214)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13777"&gt;SparkFun Battery Babysitter - LiPo Battery Manager&lt;/a&gt; (PRT-13777)&lt;/li&gt;
&lt;li&gt;And many, many others that required a lipo battery connection.&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-CONNECTORS_JST_2MM_MALE"/>
</gates>
<devices>
<device name="" package="SPARKFUN-CONNECTORS_JST-2-SMD">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
<connect gate="G$1" pin="PAD1" pad="NC1"/>
<connect gate="G$1" pin="PAD2" pad="NC2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="SF_ID" value="PRT-08612"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-RETIRED_SWITCH_SPDT">
<description>SWCH-10651

Side-actuated SPDT slide switch, as used on the Arduino Pro</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-RETIRED_SW_SPDT"/>
</gates>
<devices>
<device name="" package="SPARKFUN-RETIRED_KPS-1290">
<connects>
<connect gate="G$1" pin="O" pad="O"/>
<connect gate="G$1" pin="P" pad="P"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-10651"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-SWITCHES_MOMENTARY-SWITCH-SPST" prefix="S">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;h4&gt;Variants&lt;/h4&gt;
&lt;h5&gt;PTH-12MM - 12mm square, through-hole&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9190"&gt;Momentary Pushbutton Switch - 12mm Square&lt;/a&gt; (COM-09190)&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;PTH-6.0MM, PTH-6.0MM-KIT - 6.0mm square, through-hole&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/97"&gt;Mini Pushbutton Switch&lt;/a&gt; (COM-00097)&lt;/li&gt;
&lt;li&gt;KIT package intended for soldering kit's - only one side of pads' copper is exposed.&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;PTH-RIGHT-ANGLE-KIT - Right-angle, through-hole&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10791"&gt;Right Angle Tactile Button&lt;/a&gt; - Used on &lt;a href="https://www.sparkfun.com/products/11734"&gt;
SparkFun BigTime Watch Kit&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-12MM - 12mm square, surface-mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12993"&gt;Tactile Button - SMD (12mm)&lt;/a&gt; (COM-12993)&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/11888"&gt;SparkFun PicoBoard&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-4.5MM - 4.5mm Square Trackball Switch&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13169"&gt;SparkFun Blackberry Trackballer Breakout&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-4.6MMX2.8MM -  4.60mm x 2.80mm, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13664"&gt;SparkFun SAMD21 Mini Breakout&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-5.2MM, SMD-5.2-REDUNDANT - 5.2mm square, surface-mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8720"&gt;Mini Pushbutton Switch - SMD&lt;/a&gt; (COM-08720)&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/11114"&gt;Arduino Pro Mini&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;REDUNDANT package connects both switch circuits together&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-6.0X3.5MM - 6.0 x 3.5mm, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8229"&gt;Momentary Reset Switch SMD&lt;/a&gt; (COM-08229)&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-6.2MM-TALL - 6.2mm square, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12992"&gt;Tactile Button - SMD (6mm)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/12651"&gt;SparkFun Digital Sandbox&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-RIGHT-ANGLE - Right-angle, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13036"&gt;SparkFun Block for Intel® Edison - Arduino&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-SWITCHES_SWITCH-MOMENTARY-2"/>
</gates>
<devices>
<device name="-SMD-4.6X2.8MM" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_4.6X2.8MM">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="3 4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-12265"/>
<attribute name="SF_SKU" value="COM-12993"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN_TRANSISTOR_NPN" prefix="Q" uservalue="yes">
<description>&lt;b&gt;Transistor NPN&lt;/b&gt;
BJT configuration in SOT23 package. MMBT2222 is the common NPN we use. Double check BCE configuration again layout.</description>
<gates>
<gate name="G$1" symbol="SPARKFUN_NPN"/>
</gates>
<devices>
<device name="SOT23-3" package="SPARKFUN_SOT23-3">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY1_GND*?:1" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="SUPPLY1_GND:1"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TESTPAD_PTR1" prefix="TP">
<description>&lt;b&gt;TEST PIN&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TESTPAD_PS"/>
</gates>
<devices>
<device name="TP18R" package="TESTPAD_TP18R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEXAS_LM4875" prefix="U">
<gates>
<gate name="U$1" symbol="TEXAS_LM4875"/>
</gates>
<devices>
<device name="" package="TEXAS_SOIC8">
<connects>
<connect gate="U$1" pin="BYP" pad="7"/>
<connect gate="U$1" pin="DC_VOL" pad="4"/>
<connect gate="U$1" pin="GND" pad="6"/>
<connect gate="U$1" pin="HPHONE" pad="3"/>
<connect gate="U$1" pin="VDD" pad="1"/>
<connect gate="U$1" pin="VIN" pad="2"/>
<connect gate="U$1" pin="VOUT1" pad="5"/>
<connect gate="U$1" pin="VOUT2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GABOZEPOCAIOGO_MICROBUILDER_CAP_CERAMIC" prefix="C" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Ceramic Capacitors&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;For new designs, use the packages preceded by an '_' character since they are more reliable:&lt;/p&gt;
&lt;p&gt;The following footprints should be used on most boards:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;_0402&lt;/b&gt; - Standard footprint for regular board layouts&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_0603&lt;/b&gt; - Standard footprint for regular board layouts&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_0805&lt;/b&gt; - Standard footprint for regular board layouts&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_1206&lt;/b&gt; - Standard footprint for regular board layouts&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;For extremely tight-pitch boards where space is at a premium, the following 'micro-pitch' footprints can be used (smaller pads, no silkscreen outline, etc.):&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;_0402MP&lt;/b&gt; - Micro-pitch footprint for very dense/compact boards&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_0603MP&lt;/b&gt; - Micro-pitch footprint for very dense/compact boards&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_0805MP&lt;/b&gt; - Micro-pitch footprint for very dense/compact boards&lt;/li&gt;
&lt;li&gt;&lt;b&gt;_1206MP&lt;/b&gt; - Micro-pitch footprint for very dense/compact boards&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="GABOZEPOCAIOGO_MICROBUILDER_CAPACITOR"/>
</gates>
<devices>
<device name="0603MINI" package="GABOZEPOCAIOGO_MICROBUILDER_0603-MINI">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-IC-COMMS_FT232RL" prefix="U">
<description>&lt;h3&gt;FT232RL USB UART&lt;/h3&gt;
&lt;p&gt;FT232RL 4&lt;sup&gt;th&lt;/sup&gt; Generation USB UART (USB &amp;lt;-&amp;gt; Serial) Controller.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/IC/FT232R_v104.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/650"&gt;Component&lt;/a&gt; (COM-00650)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12097"&gt;SparkFun RedBot Mainboard&lt;/a&gt; (ROB-12097)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9716"&gt;SparkFun FTDI Basic Breakout - 5V&lt;/a&gt; (DEV-09716)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9873"&gt;SparkFun FTDI Basic Breakout - 3.3V&lt;/a&gt; (DEV-09873)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12942"&gt;Bus Pirate - v3.6a&lt;/a&gt; (TOL-12942)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12731"&gt;SparkFun USB to Serial Breakout - FT232RL&lt;/a&gt; (BOB-12731)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11888"&gt;SparkFun PicoBoard&lt;/a&gt; (WIG-11888)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9963"&gt;SparkFun RFID USB Reader&lt;/a&gt; (SEN-09963)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10275"&gt;LilyPad FTDI Basic Breakout - 5V&lt;/a&gt; (DEV-10275)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13899"&gt;SparkFun Stepoko&lt;/a&gt; (ROB-13899)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-IC-COMMS_FT232R"/>
</gates>
<devices>
<device name="SSOP" package="SPARKFUN-IC-COMMS_SSOP28DB">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="CTS" pad="11"/>
<connect gate="G$1" pin="DCD" pad="10"/>
<connect gate="G$1" pin="DSR" pad="9"/>
<connect gate="G$1" pin="DTR" pad="2"/>
<connect gate="G$1" pin="GND18" pad="18"/>
<connect gate="G$1" pin="GND21" pad="21"/>
<connect gate="G$1" pin="GND7" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="PWREN" pad="14"/>
<connect gate="G$1" pin="RESET" pad="19"/>
<connect gate="G$1" pin="RI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="RXLED" pad="22"/>
<connect gate="G$1" pin="SLEEP" pad="12"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="TXDEN" pad="13"/>
<connect gate="G$1" pin="TXLED" pad="23"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-00870"/>
<attribute name="VALUE" value="FT232RL"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROBUILDER_LED" prefix="LED" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;LED&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;0603&lt;/b&gt; - 0603 Surface Mount Package
&lt;hr&gt;
&lt;p&gt;&lt;b&gt;&lt;u&gt;2mA:&lt;/u&gt;&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Green LED - Low Power (3.9mcd, 2ma, 1.7Vf) - Digikey: 475-2709-2-ND&lt;/li&gt;
&lt;li&gt;Orange LED - Low Power (9.8mcd, 2ma, 1.8Vf) - Digikey: 475-1194-2-ND&lt;/li&gt;
&lt;li&gt;Red LED - Low Power (5mcd, 2ma, 1.8Vf) - Digikey: 475-1195-2-ND&lt;/li&gt;
&lt;li&gt;Yellow LED - Low Power (7mcd, 2ma, 1.8Vf) - Digikey: 475-1196-2-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;b&gt;&lt;u&gt;5mA:&lt;/u&gt;&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Blue LED - Low Power (17mcd, 5ma, 2.9Vf) - Digikey: LNJ937W8CRACT-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0805&lt;/b&gt; - 0805 Surface Mount Package
&lt;hr&gt;
&lt;p&gt;&lt;b&gt;&lt;u&gt;2mA:&lt;/u&gt;&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Red LED (8.8mcd, 2mA, 1.8Vf, Clear) - Low Power [Digikey: 475-2510-1-ND]&lt;/li&gt;
&lt;li&gt;Green LED (5mcd, 2mA, 1.8Vf, Clear) - Low Power [Digikey: 475-2730-1-ND]&lt;/li&gt;
&lt;li&gt;Yellow LED (11.3mcd, 2mA, 1.8Vf, Clear) - Low Power [Digikey: 475-2555-1-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;b&gt;&lt;u&gt;20mA:&lt;/u&gt;&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Red LED (104mcd, 20mA, Diffused) - LS R976 [Digikey: 475-1278-6-ND]&lt;/li&gt;
&lt;li&gt;Red LED (12mcd, 20mA, 2.0Vf, Clear) - APT2012EC [Digikey: 754-1128-1-ND]&lt;/li&gt;
&lt;li&gt;Green LED (15mcd, 20mA, 2.2Vf, Clear) - APT2012GC [Digikey: 754-1131-1-ND]&lt;/li&gt;
&lt;li&gt;Orange LED (160mcd, 20mA, 2.1Vf, Clear) - APT2012SECK [Digikey: 754-1130-1-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;li&gt;&lt;b&gt;1206&lt;/b&gt; - 1206 Surface Mount Package
&lt;hr&gt;
&lt;ul&gt;
&lt;li&gt;Green LED (26mcd, 20mA, Diffused) - LG N971  [Digikey: 475-1407-6-ND]&lt;/li&gt;
&lt;li&gt;Red LED (15mcd, 20mA, Diffused) - LH N974 [Digikey: 475-1416-6-ND]&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MICROBUILDER_LED"/>
</gates>
<devices>
<device name="0603" package="MICROBUILDER_CHIPLED_0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROBUILDER_VREG_SOT23-5" prefix="U" uservalue="yes">
<description>&lt;b&gt;SOT23-5 Fixed Voltage Regulators&lt;/b&gt;
&lt;p&gt;To better organise some of the SOT23-5 fixed voltage regulators in this library, this new part was created.&lt;br/&gt;&lt;/p&gt;
&lt;table width="550"&gt;
&lt;tr bgcolor="#EEEEEE" &gt;
&lt;td&gt;&lt;b&gt;Part&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;Current Out&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V Out&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V In&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V Dropout&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;Digikey Part No.&lt;/b&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;ADP121&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.4-5.5V&lt;/td&gt;
  &lt;td&gt;0.09V @ 150mA&lt;/td&gt;
  &lt;td&gt;ADP121-AUJZ33R7CT-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;ADP121&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.0V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.1-5.5V&lt;/td&gt;
  &lt;td&gt;0.09V @ 150mA&lt;/td&gt;
  &lt;td&gt;ADP121-AUJZ30R7CT-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;ADP122&lt;/td&gt;
  &lt;td&gt;&lt;strong&gt;300mA&lt;/strong&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.4-5.5V&lt;/td&gt;
  &lt;td&gt;0.085V @ 300mA&lt;/td&gt;
  &lt;td&gt;ADP122AUJZ-3.3-R7CT-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;ADP1712&lt;/td&gt;
  &lt;td&gt;&lt;strong&gt;300mA&lt;/strong&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5-5.5V&lt;/td&gt;
  &lt;td&gt;0.17V @ 300mA&lt;/td&gt;
  &lt;td&gt;ADP1712AUJZ-3.3-R7TR-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;AP7311 (&lt;b&gt;Low Cost&lt;/b&gt;)&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5-6V&lt;/td&gt;
  &lt;td&gt;0.15V @ 150mA&lt;/td&gt;
  &lt;td&gt;AP7311-33WG-7DICT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
  &lt;td&gt;LD39015M18R&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;1.8V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;1.9V-5.5V&lt;/td&gt;
  &lt;td&gt;0.08V @ 100mA&lt;/td&gt;
  &lt;td&gt;497-6977-1-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
  &lt;td&gt;MCP1824T-3302E/OT&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;300mA&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5V-6V&lt;/td&gt;
  &lt;td&gt;0.2V @ 300mA&lt;/td&gt;
  &lt;td&gt;MCP1824T-3302E/OTCT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
  &lt;td&gt;MIC5205-2.5YM5 TR&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;2.5V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;2.7-16V&lt;/td&gt;
  &lt;td&gt;0.165V @ 150mA&lt;/td&gt;
  &lt;td&gt;576-1257-2-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;MIC5205-3.0YM5 TR&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.0V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.2V-16V&lt;/td&gt;
  &lt;td&gt;0.165V @ 150mA&lt;/td&gt;
  &lt;td&gt;576-1258-2-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;MIC5205-3.3YM5 TR&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5V-16V&lt;/td&gt;
  &lt;td&gt;0.165V @ 150mA&lt;/td&gt;
  &lt;td&gt;576-1259-2-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;TPS780330220&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V+2.2V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.6-5.5V&lt;/td&gt;
  &lt;td&gt;250mV Max&lt;/td&gt;
  &lt;td&gt;296-23332-1-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;TDA3663/N1,135&lt;/td&gt;
  &lt;td&gt;100mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5-&lt;b&gt;45V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;0.18V @ 50mA&lt;/td&gt;
  &lt;td&gt;568-5343-1-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;

&lt;/table&gt;</description>
<gates>
<gate name="G$1" symbol="MICROBUILDER_VREG_SOT23-5"/>
</gates>
<devices>
<device name="" package="MICROBUILDER_SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="P4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
