(kicad_pcb (version 20171130) (host pcbnew 5.1.4-1.fc30)
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 797)
    (zones 0)
    (modules 25)
    (nets 86)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/tmp/uart4"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 A15)
  (net 4 A14)
  (net 5 A13)
  (net 6 A12)
  (net 7 A11)
  (net 8 A7)
  (net 9 A6)
  (net 10 A5)
  (net 11 A4)
  (net 12 A3)
  (net 13 A2)
  (net 14 A1)
  (net 15 A0)
  (net 16 M1)
  (net 17 RESET)
  (net 18 CLK)
  (net 19 INT)
  (net 20 WR)
  (net 21 RD)
  (net 22 IORQ)
  (net 23 D0)
  (net 24 D1)
  (net 25 D2)
  (net 26 D3)
  (net 27 D4)
  (net 28 D5)
  (net 29 D6)
  (net 30 D7)
  (net 31 "Net-(J1-Pad35)")
  (net 32 "Net-(J1-Pad36)")
  (net 33 IEO)
  (net 34 IEI)
  (net 35 "Net-(J2-Pad1)")
  (net 36 "Net-(J2-Pad3)")
  (net 37 "Net-(J2-Pad5)")
  (net 38 "Net-(J2-Pad7)")
  (net 39 "Net-(J2-Pad9)")
  (net 40 "Net-(J2-Pad11)")
  (net 41 "Net-(J2-Pad13)")
  (net 42 "Net-(J3-Pad6)")
  (net 43 "Net-(J3-Pad5)")
  (net 44 "Net-(J3-Pad4)")
  (net 45 "Net-(J3-Pad2)")
  (net 46 "Net-(J4-Pad2)")
  (net 47 "Net-(J4-Pad4)")
  (net 48 "Net-(J4-Pad5)")
  (net 49 "Net-(J4-Pad6)")
  (net 50 "Net-(J5-Pad6)")
  (net 51 "Net-(J5-Pad5)")
  (net 52 "Net-(J5-Pad4)")
  (net 53 "Net-(J5-Pad2)")
  (net 54 "Net-(J6-Pad2)")
  (net 55 "Net-(J6-Pad4)")
  (net 56 "Net-(J6-Pad5)")
  (net 57 "Net-(J6-Pad6)")
  (net 58 GPO0)
  (net 59 GPO1)
  (net 60 "Net-(JP1-Pad2)")
  (net 61 "Net-(JP1-Pad1)")
  (net 62 "Net-(JP2-Pad2)")
  (net 63 COM1_TX)
  (net 64 COM1_RX)
  (net 65 COM1_RTS)
  (net 66 COM1_CTS)
  (net 67 COM2_RTS)
  (net 68 COM2_RX)
  (net 69 COM2_TX)
  (net 70 COM2_CTS)
  (net 71 COM3_RTS)
  (net 72 COM3_RX)
  (net 73 COM3_TX)
  (net 74 COM3_CTS)
  (net 75 COM4_RTS)
  (net 76 COM4_RX)
  (net 77 COM4_TX)
  (net 78 COM4_CTS)
  (net 79 "Net-(RN1-Pad2)")
  (net 80 "Net-(U1-Pad43)")
  (net 81 IOCS)
  (net 82 "Net-(U1-Pad15)")
  (net 83 "Net-(U1-Pad20)")
  (net 84 "Net-(U1-Pad38)")
  (net 85 "Net-(U2-Pad13)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A11)
    (add_net A12)
    (add_net A13)
    (add_net A14)
    (add_net A15)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net CLK)
    (add_net COM1_CTS)
    (add_net COM1_RTS)
    (add_net COM1_RX)
    (add_net COM1_TX)
    (add_net COM2_CTS)
    (add_net COM2_RTS)
    (add_net COM2_RX)
    (add_net COM2_TX)
    (add_net COM3_CTS)
    (add_net COM3_RTS)
    (add_net COM3_RX)
    (add_net COM3_TX)
    (add_net COM4_CTS)
    (add_net COM4_RTS)
    (add_net COM4_RX)
    (add_net COM4_TX)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net GPO0)
    (add_net GPO1)
    (add_net IEI)
    (add_net IEO)
    (add_net INT)
    (add_net IOCS)
    (add_net IORQ)
    (add_net M1)
    (add_net "Net-(J1-Pad35)")
    (add_net "Net-(J1-Pad36)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(J6-Pad5)")
    (add_net "Net-(J6-Pad6)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(RN1-Pad2)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U2-Pad13)")
    (add_net RD)
    (add_net RESET)
    (add_net WR)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 250.7615 197.358 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at 0 -2.794) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 IEO))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(JP2-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 180.5305 169.799)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C1 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 190.754 193.548 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C2 (at 4.572 -0.0635 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer B.Cu) (tedit 5AE50EF0)
    (at 227.076 186.3725 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C3 (at 4.445 -0.127 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 1.25 -2.25 270) (layer B.Fab))
    (fp_text user %R (at 1.25 0 270) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 190.5 177.6095 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C4 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.678499 -0.965001 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x40_P2.54mm_Horizontal (layer B.Cu) (tedit 59FED5CB)
    (at 161.163 202.8825 270)
    (descr "Through hole angled pin header, 1x40, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x40 2.54mm single row")
    (fp_text reference J1 (at 4.385 2.27 270) (layer B.SilkS))
    (fp_text value Conn_01x40 (at 4.385 -101.33 270) (layer B.Fab))
    (fp_text user %R (at 2.77 -49.53) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 A15))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 A14))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 A13))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 A12))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 A11))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 A7))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 A6))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 A5))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 A4))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 A3))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 A2))
    (pad 15 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 A1))
    (pad 16 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 A0))
    (pad 17 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 19 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 M1))
    (pad 20 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 RESET))
    (pad 21 thru_hole oval (at 0 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 CLK))
    (pad 22 thru_hole oval (at 0 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 INT))
    (pad 23 thru_hole oval (at 0 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 0 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 WR))
    (pad 25 thru_hole oval (at 0 -60.96 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 RD))
    (pad 26 thru_hole oval (at 0 -63.5 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 IORQ))
    (pad 27 thru_hole oval (at 0 -66.04 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 D0))
    (pad 28 thru_hole oval (at 0 -68.58 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 D1))
    (pad 29 thru_hole oval (at 0 -71.12 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 D2))
    (pad 30 thru_hole oval (at 0 -73.66 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 D3))
    (pad 31 thru_hole oval (at 0 -76.2 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 D4))
    (pad 32 thru_hole oval (at 0 -78.74 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 D5))
    (pad 33 thru_hole oval (at 0 -81.28 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 D6))
    (pad 34 thru_hole oval (at 0 -83.82 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 D7))
    (pad 35 thru_hole oval (at 0 -86.36 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad35)"))
    (pad 36 thru_hole oval (at 0 -88.9 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J1-Pad36)"))
    (pad 37 thru_hole oval (at 0 -91.44 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 0 -93.98 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 IEO))
    (pad 39 thru_hole oval (at 0 -96.52 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 IEI))
    (pad 40 thru_hole oval (at 0 -99.06 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x40_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x07_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 166.243 196.6595 180)
    (descr "Through hole straight pin header, 2x07, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x07 2.54mm double row")
    (fp_text reference J2 (at 1.3335 -2.6035) (layer F.SilkS))
    (fp_text value Conn_02x07_Odd_Even (at 1.27 17.57) (layer F.Fab))
    (fp_text user %R (at 1.27 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 218.2495 164.719 90)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 0 -2.921 180) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 4.385 14.97 90) (layer F.Fab))
    (fp_text user %R (at 2.77 6.35) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J3-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J3-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J3-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 194.437 164.719 90)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J4 (at 0.0635 -2.9845 180) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 4.385 14.97 90) (layer F.Fab))
    (fp_text user %R (at 2.77 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J4-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 241.808 164.719 90)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J5 (at -0.635 -3.048 180) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 4.385 14.97 90) (layer F.Fab))
    (fp_text user %R (at 2.77 6.35) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J5-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J5-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J5-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 259.3975 174.3075)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J6 (at -0.0635 -2.7305) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 4.385 14.97) (layer F.Fab))
    (fp_text user %R (at 2.77 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(J6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J6-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(J6-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(J6-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 246.5705 192.2145)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at -0.0635 -2.794) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 GPO0))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 GPO1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 254.9525 192.913)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 0.0635 7.5565) (layer F.SilkS))
    (fp_text value Jumper_3_Open (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 IEI))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(JP1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(JP1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 242.2525 197.612 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at 0.254 -2.6035) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 COM1_TX))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad35)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 242.697 190.8175 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP4 (at 0 4.953) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at -1.397 1.0795 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J1-Pad36)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 COM1_RX))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 258.6355 191.0715 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 9.398 0 180) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(JP1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP9 (layer F.Cu) (tedit 5A14249F)
    (at 171.323 177.038 270)
    (descr "9-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 22.86 -0.127 180) (layer F.SilkS))
    (fp_text value 10K (at 11.43 2.4 90) (layer F.Fab))
    (fp_text user %R (at 10.16 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(RN1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(J2-Pad13)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad11)"))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad9)"))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad7)"))
    (pad 7 thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad5)"))
    (pad 8 thru_hole oval (at 17.78 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad3)"))
    (pad 9 thru_hole oval (at 20.32 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LCC:PLCC-44_THT-Socket (layer F.Cu) (tedit 5A02ECC8)
    (at 221.1705 184.3405 90)
    (descr "PLCC, 44 pins, through hole")
    (tags "plcc leaded")
    (fp_text reference U1 (at -2.794 -7.366 180) (layer F.SilkS))
    (fp_text value XR82C684-44 (at -1.27 19.1 90) (layer F.Fab))
    (fp_text user %R (at -1.27 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -2.54 0 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 COM2_TX))
    (pad 5 thru_hole circle (at -5.08 0 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 CLK))
    (pad 43 thru_hole circle (at 2.54 0 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(U1-Pad43)"))
    (pad 41 thru_hole circle (at 5.08 0 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 COM1_RTS))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 GPO0))
    (pad 4 thru_hole circle (at -5.08 -2.54 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 COM2_RX))
    (pad 6 thru_hole circle (at -7.62 -2.54 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask))
    (pad 44 thru_hole circle (at 0 -2.54 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 42 thru_hole circle (at 2.54 -2.54 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 COM2_RTS))
    (pad 8 thru_hole circle (at -7.62 0 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 D1))
    (pad 10 thru_hole circle (at -7.62 2.54 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 D3))
    (pad 12 thru_hole circle (at -7.62 5.08 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 D5))
    (pad 14 thru_hole circle (at -7.62 7.62 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 D7))
    (pad 16 thru_hole circle (at -7.62 10.16 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 IOCS))
    (pad 7 thru_hole circle (at -10.16 0 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 D0))
    (pad 9 thru_hole circle (at -10.16 2.54 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 D2))
    (pad 11 thru_hole circle (at -10.16 5.08 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 D4))
    (pad 13 thru_hole circle (at -10.16 7.62 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 D6))
    (pad 15 thru_hole circle (at -10.16 10.16 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(U1-Pad15)"))
    (pad 17 thru_hole circle (at -10.16 12.7 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 COM4_RX))
    (pad 19 thru_hole circle (at -7.62 12.7 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(JP2-Pad2)"))
    (pad 21 thru_hole circle (at -5.08 12.7 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 INT))
    (pad 23 thru_hole circle (at -2.54 12.7 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 12.7 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 COM3_RTS))
    (pad 27 thru_hole circle (at 2.54 12.7 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 COM3_RX))
    (pad 29 thru_hole circle (at 7.62 12.7 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 COM4_CTS))
    (pad 18 thru_hole circle (at -7.62 15.24 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 COM4_TX))
    (pad 20 thru_hole circle (at -5.08 15.24 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(U1-Pad20)"))
    (pad 22 thru_hole circle (at -2.54 15.24 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 GPO1))
    (pad 24 thru_hole circle (at 0 15.24 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 COM4_RTS))
    (pad 26 thru_hole circle (at 2.54 15.24 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 COM3_TX))
    (pad 28 thru_hole circle (at 5.08 15.24 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(JP1-Pad2)"))
    (pad 30 thru_hole circle (at 5.08 12.7 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 COM3_CTS))
    (pad 32 thru_hole circle (at 5.08 10.16 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 A14))
    (pad 34 thru_hole circle (at 5.08 7.62 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 A12))
    (pad 36 thru_hole circle (at 5.08 5.08 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 COM1_CTS))
    (pad 38 thru_hole circle (at 5.08 2.54 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(U1-Pad38)"))
    (pad 40 thru_hole circle (at 5.08 -2.54 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 COM1_TX))
    (pad 31 thru_hole circle (at 7.62 10.16 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 A15))
    (pad 33 thru_hole circle (at 7.62 7.62 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 A13))
    (pad 35 thru_hole circle (at 7.62 5.08 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 A11))
    (pad 37 thru_hole circle (at 7.62 2.54 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 COM2_CTS))
    (pad 39 thru_hole circle (at 7.62 0 90) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 COM1_RX))
    (model ${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-44_THT-Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 193.9925 195.8975 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at -0.127 -2.9845 180) (layer F.SilkS))
    (fp_text value 74HCT32 (at 3.81 17.57 90) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 M1))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(U1-Pad38)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 IORQ))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 IOCS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(U1-Pad20)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 RD))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 WR))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 IOCS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 IOCS))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 A0))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(U1-Pad15)"))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(U2-Pad13)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 193.6115 182.499 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 0.127 -3.1115 180) (layer F.SilkS))
    (fp_text value 74HCT00 (at 3.81 17.57 90) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(U1-Pad43)"))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 RESET))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 RESET))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 185.674 197.9295 180)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U4 (at 3.8735 -2.6035) (layer F.SilkS))
    (fp_text value 74HCT688 (at 3.81 25.19) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 IORQ))
    (pad 11 thru_hole oval (at 7.62 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 A3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 A7))
    (pad 12 thru_hole oval (at 7.62 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad9)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 A2))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 A6))
    (pad 14 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad11)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad3)"))
    (pad 15 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 A1))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 A5))
    (pad 16 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(J2-Pad13)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad5)"))
    (pad 17 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 M1))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 A4))
    (pad 18 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(RN1-Pad2)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad7)"))
    (pad 19 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(U2-Pad13)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP8 (layer F.Cu) (tedit 5A14249F)
    (at 211.2645 168.7195)
    (descr "8-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN2 (at 11.8745 2.8575) (layer F.SilkS))
    (fp_text value R_Pack04_SIP (at 10.16 2.4) (layer F.Fab))
    (fp_text user %R (at 8.89 0) (layer F.Fab))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 COM1_CTS))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(J3-Pad6)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 COM1_TX))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(J3-Pad5)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 COM1_RX))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(J3-Pad4)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 COM1_RTS))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP8 (layer F.Cu) (tedit 5A14249F)
    (at 189.4205 168.656)
    (descr "8-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN3 (at 9.271 2.54) (layer F.SilkS))
    (fp_text value R_Pack04_SIP (at 10.16 2.4) (layer F.Fab))
    (fp_text user %R (at 8.89 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(J4-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 COM2_RTS))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(J4-Pad4)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 COM2_RX))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 COM2_TX))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(J4-Pad6)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 COM2_CTS))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP8 (layer F.Cu) (tedit 5A14249F)
    (at 232.8545 168.7195)
    (descr "8-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN4 (at 9.0805 2.921) (layer F.SilkS))
    (fp_text value R_Pack04_SIP (at 10.16 2.4) (layer F.Fab))
    (fp_text user %R (at 8.89 0) (layer F.Fab))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 COM3_CTS))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(J5-Pad6)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 COM3_TX))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(J5-Pad5)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 COM3_RX))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(J5-Pad4)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 COM3_RTS))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP8 (layer F.Cu) (tedit 5A14249F)
    (at 255.016 171.2595 270)
    (descr "8-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN5 (at 9.3345 3.1115 180) (layer F.SilkS))
    (fp_text value R_Pack04_SIP (at 10.16 2.4 90) (layer F.Fab))
    (fp_text user %R (at 8.89 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(J6-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 COM4_RTS))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(J6-Pad4)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 COM4_RX))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(J6-Pad5)"))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 COM4_TX))
    (pad 7 thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(J6-Pad6)"))
    (pad 8 thru_hole oval (at 17.78 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 COM4_CTS))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text EPSER4 (at 246.507 182.753 90) (layer F.SilkS))
  (gr_text "Pint Pot 0.1\nEtched Pixels (C) 2019\n" (at 172.1485 170.561 45) (layer F.SilkS))
  (gr_text 4 (at 260.2865 169.926) (layer F.SilkS))
  (gr_text 3 (at 237.109 164.1475) (layer F.SilkS))
  (gr_text 1 (at 213.868 164.211) (layer F.SilkS))
  (gr_text 2 (at 189.611 164.338) (layer F.SilkS))
  (gr_text "Port: " (at 185.674 164.4015) (layer F.SilkS))
  (gr_text Address (at 161.163 188.9125 90) (layer F.SilkS))
  (gr_line (start 261.493 204.2795) (end 261.493 162.56) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.3215 204.2795) (end 159.3215 180.1495) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.3215 204.2795) (end 261.493 204.2795) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 176.911 162.56) (end 159.3215 180.1495) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.816 162.56) (end 176.911 162.56) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 261.493 162.56) (end 178.816 162.56) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.3215 204.2795) (xy 159.3215 180.086) (xy 176.9745 162.56) (xy 261.493 162.56) (xy 261.493 204.2795)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.3215 204.2795) (xy 159.3215 180.1495) (xy 177.038 162.4965) (xy 261.493 162.56) (xy 261.493 204.2795)
      )
    )
  )
)
