<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="41.97703125" y1="72.06" x2="21.5352" y2="72.06" width="0" layer="20"/>
<wire x1="21.5352" y1="72.06" x2="17.78" y2="68.3048" width="0" layer="20" curve="90"/>
<wire x1="17.78" y1="68.3048" x2="17.78" y2="27.94" width="0" layer="20"/>
<wire x1="17.78" y1="27.94" x2="21.59" y2="24.13" width="0" layer="20"/>
<wire x1="21.59" y1="24.13" x2="21.59" y2="2.54" width="0" layer="20"/>
<wire x1="21.59" y1="2.54" x2="24.13" y2="0" width="0" layer="20"/>
<wire x1="30.734" y1="2.54" x2="30.734" y2="21.463" width="0" layer="20"/>
<wire x1="30.734" y1="21.463" x2="34.036" y2="21.463" width="0" layer="20"/>
<wire x1="34.036" y1="21.463" x2="34.036" y2="2.54" width="0" layer="20"/>
<wire x1="34.036" y1="2.54" x2="36.195" y2="0" width="0" layer="20"/>
<wire x1="36.195" y1="0" x2="40.005" y2="0" width="0" layer="20"/>
<wire x1="40.005" y1="0" x2="42.164" y2="2.159" width="0" layer="20"/>
<wire x1="42.164" y1="2.159" x2="42.164" y2="24.13" width="0" layer="20"/>
<wire x1="42.164" y1="24.13" x2="45.7" y2="27.94" width="0" layer="20"/>
<wire x1="45.7" y1="27.94" x2="45.7" y2="68.33703125" width="0" layer="20"/>
<wire x1="45.7" y1="68.33703125" x2="41.97703125" y2="72.06" width="0" layer="20" curve="90"/>
<wire x1="24.13" y1="0" x2="28.448" y2="0" width="0" layer="20"/>
<wire x1="28.448" y1="0" x2="30.734" y2="2.54" width="0" layer="20"/>
<text>GearsNGenes</text>
<text>EMFMeter FeatherWing</text>
<text>May 2019 001</text>
</plain>
<libraries>
<library name="MG-Eagle_v1">
<packages>
<package name="1X02">
</package>
<package name="1X12">
</package>
<package name="1X16">
</package>
</packages>
</library>
<library name="SidV parts">
<packages>
<package name="1UF_CAP_SV">
</package>
<package name="INDUCT_1.5KOHM">
</package>
<package name="ADS1115_SV">
</package>
<package name="10K_RESARR_SV">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CH1A" library="MG-Eagle_v1" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CH1B" library="MG-Eagle_v1" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CH2A" library="MG-Eagle_v1" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CH2B" library="MG-Eagle_v1" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="MG-Eagle_v1" package="1X12" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="MG-Eagle_v1" package="1X16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SidV parts" package="1UF_CAP_SV" value="1UF_CAP_SV">
<attribute name="NAME"/>
</element>
<element name="U$2" library="SidV parts" package="1UF_CAP_SV" value="1UF_CAP_SV">
<attribute name="NAME"/>
</element>
<element name="U$3" library="SidV parts" package="INDUCT_1.5KOHM" value="INDUCT_1.5KOHM">
<attribute name="NAME"/>
</element>
<element name="U$4" library="SidV parts" package="INDUCT_1.5KOHM" value="INDUCT_1.5KOHM">
<attribute name="NAME"/>
</element>
<element name="U1" library="SidV parts" package="ADS1115_SV" value="ADS1115_SV">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SidV parts" package="10K_RESARR_SV" value="10K_RESARR_SV">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="P$3"/>
<contactref element="U2" pad="R2B"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="U$4" pad="P$2"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="P$8"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="U2" pad="R3B"/>
<contactref element="U2" pad="R4B"/>
<contactref element="U2" pad="R1B"/>
<contactref element="U$3" pad="P$2"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="P$10"/>
<contactref element="U2" pad="R3A"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="P$9"/>
<contactref element="U2" pad="R4A"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="P$2"/>
<contactref element="U2" pad="R1A"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="P$1"/>
<contactref element="U2" pad="R2A"/>
</signal>
<signal name="N$5">
<contactref element="J2" pad="15"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="U$4" pad="P$1"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="J2" pad="13"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="P$4"/>
<contactref element="CH1A" pad="2"/>
<contactref element="CH1A" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="CH1B" pad="2"/>
<contactref element="U1" pad="P$5"/>
<contactref element="CH1B" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="CH2B" pad="2"/>
<contactref element="CH2B" pad="1"/>
<contactref element="U1" pad="P$7"/>
</signal>
<signal name="N$10">
<contactref element="CH2A" pad="2"/>
<contactref element="CH2A" pad="1"/>
<contactref element="U1" pad="P$6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
