(kicad_pcb (version 20171130) (host pcbnew 5.1.5-1.fc31)
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 835)
    (zones 0)
    (modules 29)
    (nets 57)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/tmp/kicad/ps2"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 RD)
  (net 3 A7)
  (net 4 A6)
  (net 5 A5)
  (net 6 A4)
  (net 7 A3)
  (net 8 IORQ)
  (net 9 D1)
  (net 10 D2)
  (net 11 D3)
  (net 12 D4)
  (net 13 D5)
  (net 14 D6)
  (net 15 D7)
  (net 16 A2)
  (net 17 A1)
  (net 18 A0)
  (net 19 RESET)
  (net 20 WR)
  (net 21 "Net-(J2-Pad8)")
  (net 22 "Net-(J2-Pad10)")
  (net 23 "Net-(J2-Pad12)")
  (net 24 "Net-(J2-Pad14)")
  (net 25 "Net-(U1-Pad2)")
  (net 26 IORD)
  (net 27 IOWR)
  (net 28 "Net-(J2-Pad2)")
  (net 29 "Net-(J2-Pad4)")
  (net 30 "Net-(J2-Pad6)")
  (net 31 VCC)
  (net 32 D0)
  (net 33 "Net-(J2-Pad16)")
  (net 34 "Net-(J3-Pad7)")
  (net 35 "Net-(J4-Pad7)")
  (net 36 "Net-(U3-Pad2)")
  (net 37 MOUSECLK)
  (net 38 "Net-(U3-Pad5)")
  (net 39 MOUSEDATA)
  (net 40 "Net-(J5-Pad1)")
  (net 41 "Net-(J5-Pad2)")
  (net 42 "Net-(C8-Pad1)")
  (net 43 "Net-(C9-Pad1)")
  (net 44 KCLKIN)
  (net 45 KDATAIN)
  (net 46 MDATAIN)
  (net 47 MCLKIN)
  (net 48 JSC)
  (net 49 JSD)
  (net 50 "Net-(J5-Pad6)")
  (net 51 "Net-(RN2-Pad4)")
  (net 52 "Net-(RN2-Pad5)")
  (net 53 "Net-(RN2-Pad6)")
  (net 54 "Net-(RN2-Pad7)")
  (net 55 JSB)
  (net 56 JSA)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net IORD)
    (add_net IORQ)
    (add_net IOWR)
    (add_net JSA)
    (add_net JSB)
    (add_net JSC)
    (add_net JSD)
    (add_net KCLKIN)
    (add_net KDATAIN)
    (add_net MCLKIN)
    (add_net MDATAIN)
    (add_net MOUSECLK)
    (add_net MOUSEDATA)
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(RN2-Pad4)")
    (add_net "Net-(RN2-Pad5)")
    (add_net "Net-(RN2-Pad6)")
    (add_net "Net-(RN2-Pad7)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad5)")
    (add_net RD)
    (add_net RESET)
    (add_net VCC)
    (add_net WR)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module Package_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 242 124.55)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U5 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74HCT245 (at 3.81 25.19) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 JSD))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 D0))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 JSC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 D1))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 JSB))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 D2))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 JSA))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 D3))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 KDATAIN))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 D4))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 KCLKIN))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 D5))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 MDATAIN))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 D6))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 MCLKIN))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 D7))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 IORD))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP9 (layer F.Cu) (tedit 5A14249F)
    (at 184.912 118.364 180)
    (descr "9-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at -3.308 -0.036) (layer F.SilkS))
    (fp_text value 10K (at 11.43 2.4) (layer F.Fab))
    (fp_text user %R (at 10.16 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 VCC))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad4)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad8)"))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad10)"))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad12)"))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad14)"))
    (pad 9 thru_hole oval (at 20.32 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad16)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP10 (layer F.Cu) (tedit 5A14249F)
    (at 230.7 105.35 180)
    (descr "10-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN2 (at 12.7 -2.4) (layer F.SilkS))
    (fp_text value R2SIP10 (at 12.7 2.4) (layer F.Fab))
    (fp_text user %R (at 11.43 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(C8-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(RN2-Pad4)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(RN2-Pad5)"))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(RN2-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(RN2-Pad7)"))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 20.32 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 22.86 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 161.671 133.477 90)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 7.527 -2.871 180) (layer F.SilkS))
    (fp_text value 74HCT688 (at 3.81 25.19 90) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 IORQ))
    (pad 11 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad8)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad16)"))
    (pad 12 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 A3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 A7))
    (pad 13 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad6)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad14)"))
    (pad 14 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 A2))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 A6))
    (pad 15 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad4)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad12)"))
    (pad 16 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 A1))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 A5))
    (pad 17 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad2)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad10)"))
    (pad 18 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 A0))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 A4))
    (pad 19 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad2)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x40_P2.54mm_Horizontal (layer B.Cu) (tedit 59FED5CB)
    (at 155.702 152.4 270)
    (descr "Through hole angled pin header, 1x40, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x40 2.54mm single row")
    (fp_text reference J1 (at 4.385 2.27 270) (layer B.SilkS))
    (fp_text value Conn_01x40 (at 4.385 -101.33 270) (layer B.Fab))
    (fp_text user %R (at 2.77 -49.53) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 A7))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 A6))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 A5))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 A4))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 A3))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 A2))
    (pad 15 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 A1))
    (pad 16 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 A0))
    (pad 17 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 VCC))
    (pad 19 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 RESET))
    (pad 21 thru_hole oval (at 0 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 0 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 0 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 WR))
    (pad 25 thru_hole oval (at 0 -60.96 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 RD))
    (pad 26 thru_hole oval (at 0 -63.5 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 IORQ))
    (pad 27 thru_hole oval (at 0 -66.04 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 D0))
    (pad 28 thru_hole oval (at 0 -68.58 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 D1))
    (pad 29 thru_hole oval (at 0 -71.12 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 D2))
    (pad 30 thru_hole oval (at 0 -73.66 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 D3))
    (pad 31 thru_hole oval (at 0 -76.2 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 D4))
    (pad 32 thru_hole oval (at 0 -78.74 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 D5))
    (pad 33 thru_hole oval (at 0 -81.28 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 D6))
    (pad 34 thru_hole oval (at 0 -83.82 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 D7))
    (pad 35 thru_hole oval (at 0 -86.36 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at 0 -88.9 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 0 -91.44 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 0 -93.98 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 -96.52 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 40 thru_hole oval (at 0 -99.06 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x40_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 583F5ADB)
    (at 158.9278 120.2436)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 26.6446 -55.0545) (layer F.SilkS) hide)
    (fp_text value "" (at 2.3368 -73.0631 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Package_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 161.798 145.923 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 7.553 -2.738 180) (layer F.SilkS))
    (fp_text value 74HCT32 (at 3.81 17.57 90) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 RD))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 JSB))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 IORD))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(J5-Pad6)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 JSA))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 WR))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(J5-Pad6)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 IOWR))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(J5-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 158.496 128.397 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C1 (at 0.953 2.671 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 158.623 142.748 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C2 (at 1.548 -2.463 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 186.69 109.601 270)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference J2 (at 1.579 -3.37 180) (layer F.SilkS))
    (fp_text value Conn_02x08_Top_Bottom (at 1.27 20.11 90) (layer F.Fab))
    (fp_text user %R (at 1.27 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad16)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ps2:MINI-DIN-6-FULL-SHIELD (layer F.Cu) (tedit 5D93B244)
    (at 268.05 137.9 270)
    (fp_text reference J3 (at -6.76 14.46 180) (layer F.SilkS))
    (fp_text value PS2-MINIDIN6-FEMALE (at 0.15 1.325 90) (layer F.Fab) hide)
    (pad 7 thru_hole circle (at -6.75 5.5 270) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 34 "Net-(J3-Pad7)"))
    (pad 7 thru_hole circle (at 6.75 5.5 270) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 34 "Net-(J3-Pad7)"))
    (pad 4 thru_hole circle (at 3.4 8.5 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 VCC))
    (pad 6 thru_hole circle (at 3.4 11 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -3.4 8.5 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -3.4 11 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 KCLKIN))
    (pad 2 thru_hole circle (at 1.3 8.5 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.3 8.5 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 45 KDATAIN))
    (pad 7 thru_hole circle (at 0 4.7 270) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 34 "Net-(J3-Pad7)"))
  )
  (module ps2:MINI-DIN-6-FULL-SHIELD (layer F.Cu) (tedit 5D93B244)
    (at 268.1 118.05 270)
    (fp_text reference J4 (at -6.83 14.64 180) (layer F.SilkS))
    (fp_text value PS2-MINIDIN6-FEMALE (at 0.15 1.325 90) (layer F.Fab) hide)
    (pad 7 thru_hole circle (at 0 4.7 270) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad7)"))
    (pad 1 thru_hole circle (at -1.3 8.5 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 46 MDATAIN))
    (pad 2 thru_hole circle (at 1.3 8.5 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -3.4 11 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 47 MCLKIN))
    (pad 3 thru_hole circle (at -3.4 8.5 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 3.4 11 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 3.4 8.5 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 VCC))
    (pad 7 thru_hole circle (at 6.75 5.5 270) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad7)"))
    (pad 7 thru_hole circle (at -6.75 5.5 270) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad7)"))
  )
  (module Package_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 204.65 122.6)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74HCT273 (at 3.81 25.19) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 RESET))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 IOWR))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U3-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(RN2-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 D0))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 D4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 D1))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 D5))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(U3-Pad5)"))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(RN2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 MOUSECLK))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(RN2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 D2))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 D6))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 D3))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 D7))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 MOUSEDATA))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(RN2-Pad7)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 191.35 123.9)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U4 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74HCT125 (at 3.81 17.57) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 MOUSECLK))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 KDATAIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 MCLKIN))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(U3-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 MOUSEDATA))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 KCLKIN))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 MDATAIN))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U3-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 246.65 120.6 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C3 (at 1.13 2.42) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 246.5 109.65 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C4 (at 1.25 2.37) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 196.5 119.45 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C5 (at 1.15 2.25) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 209.45 118.9 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C6 (at 1.45 2.025) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P3.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 199.25 145.5 180)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C7 (at 7.53 1.61) (layer F.SilkS))
    (fp_text value 10uF (at 1.75 5.25) (layer F.Fab))
    (fp_text user %R (at 1.75 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 VCC))
    (pad 2 thru_hole circle (at 3.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 234.7 109.35)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C8 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 236.95 102 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C9 (at 1.3 2.13) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(C8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Dsub:DSUB-9_Male_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm (layer F.Cu) (tedit 59FEDEE2)
    (at 204.4 108.2 180)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.54mm pin-PCB-offset 9.4mm")
    (fp_text reference J5 (at 5.54 -1.8) (layer F.SilkS))
    (fp_text value DB9_Male (at 5.54 19.84) (layer F.Fab))
    (fp_text user %R (at 5.54 15.34) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J5-Pad1)"))
    (pad 2 thru_hole circle (at 2.77 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J5-Pad2)"))
    (pad 3 thru_hole circle (at 5.54 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 48 JSC))
    (pad 4 thru_hole circle (at 8.31 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 49 JSD))
    (pad 5 thru_hole circle (at 11.08 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 1.385 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J5-Pad6)"))
    (pad 7 thru_hole circle (at 4.155 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 6.925 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 31 VCC))
    (pad 9 thru_hole circle (at 9.695 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-9_Male_Horizontal_P2.77x2.54mm_EdgePinOffset9.40mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Audio:Jack_3.5mm_CUI_SJ1-3533NG_Horizontal (layer F.Cu) (tedit 5BAD3514)
    (at 266.82 103.6 270)
    (descr "TRS 3.5mm, horizontal, through-hole, https://www.cui.com/product/resource/sj1-353xng.pdf")
    (tags "TRS audio jack stereo horizontal")
    (fp_text reference J6 (at 3.99 -6.97 180) (layer F.SilkS))
    (fp_text value AudioJack3 (at 0.1 14.05 90) (layer F.Fab))
    (fp_text user %R (at 0.1 3.8 90) (layer F.Fab))
    (pad S thru_hole oval (at 0 0 270) (size 2.8 1.8) (drill oval 2 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad T thru_hole oval (at 2 2.4 270) (size 2.8 1.8) (drill oval 2 1) (layers *.Cu *.Mask)
      (net 43 "Net-(C9-Pad1)"))
    (pad R thru_hole oval (at 2 7.9 270) (size 2.8 1.8) (drill oval 2 1) (layers *.Cu *.Mask)
      (net 43 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3533NG_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 240.35 101.8 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.64 -0.14 180) (layer F.SilkS))
    (fp_text value 2.2K (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(C9-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 217.9 98.95)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.79 -0.02) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 217.9 102.15)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3.88 -0.03) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(J5-Pad6)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 179.15 105.05)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 3.87 -0.15) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 JSB))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 179.2 101.6)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.86 -0.02) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 JSA))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 213.75 117.69)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 3.81 -2.37) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(J5-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 74HCT245 (at 246.04 135.83 90) (layer F.SilkS))
  (gr_text 74HCT273 (at 208.48 134.16 90) (layer F.SilkS))
  (gr_text 74HCT125 (at 195.13 130.99 90) (layer F.SilkS))
  (gr_text 74HCT32 (at 170.73 142.16) (layer F.SilkS))
  (gr_text 74HCT688 (at 172.43 129.26) (layer F.SilkS))
  (gr_text "“If Pac-Man had affected us as kids, \nwe'd all be running around in dark rooms, munching pills\nand listening to repetitive electronic music.”\n― Marcus Brigstocke" (at 227.02 132.5) (layer F.SilkS))
  (gr_text EPPS2JDSP (at 225.24 142.85) (layer F.SilkS))
  (gr_text "PS/2 Keyboard,  Mouse, Joystick, Sound v0.3\n(C) 2019 Etched Pixels CC-NC" (at 218.67 112.03) (layer F.SilkS))
  (gr_text Keyboard (at 261.04 148.55) (layer F.SilkS))
  (gr_text "80 40 20 10 08 04 02 01" (at 177.86 115.08) (layer F.SilkS))
  (gr_line (start 266.15 96.85) (end 268.1 98.5) (layer Edge.Cuts) (width 0.15))
  (gr_text "Pin 1" (at 155.68168 146.60118 90) (layer F.SilkS))
  (gr_text "A15\nA14\nA13\nA12\nA11\nA10\nA9\nA8\nA7\nA6\nA5\nA4\nA3\nA2\nA1\nA0\nGnd\n5v\nM1\nReset\nClock\nINT\nMreq\nWr\nRo\nIORQ\nD0\nD1\nD2\nD3\nD4\nD5\nD6\nD7\nTx\nRx\nUSR1\nUSR2\nUSR3" (at 203.9112 153.6573 90) (layer F.SilkS))
  (gr_line (start 268.1 98.5) (end 268.1 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 266.15 96.85) (end 175.65 96.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.8986 118.5164) (end 153.8986 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.65 96.85) (end 153.8986 118.5164) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.8986 153.3652) (end 268.1 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.924 153.416) (xy 153.924 118.618) (xy 175.65 96.65) (xy 266.1 96.8) (xy 268 98.6)
        (xy 268.15 153.383)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.924 153.416) (xy 153.924 118.364) (xy 175.85 96.7) (xy 266.05 96.8) (xy 268.1 98.6)
        (xy 268.15 153.365)
      )
    )
  )
)
