<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<text>16-&gt;RST</text>
<text>Batt-&gt;A0</text>
<text>FeatherWing Adapter v1.0</text>
<text>by Kritch</text>
<text>Designed by</text>
<text>Kritch 2019</text>
<hole x="27.94" y="63.5" drill="3.556"/>
<hole x="78.74" y="48.26" drill="3.556"/>
<hole x="78.74" y="20.32" drill="3.556"/>
<hole x="26.67" y="15.24" drill="3.556"/>
</plain>
<libraries>
<library name="adafruit3">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="FEATHERWING">
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="EVQ-Q2">
</package>
<package name="JST-PH-2-SMT-RA">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
</packages>
</library>
<library name="switch-dil">
<description>&lt;b&gt;DIL Switches and Code Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DP-02">
<description>&lt;b&gt;DIL/CODE SWITCH&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="ARDUINOR3">
<description>The new Arduino R3 'classic' adds duplicate I2C pins and an IORef pin (and an unused pin</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="adafruit3" package="LED3MM" value="PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MS1" library="adafruit3" package="FEATHERWING" value="FEATHERWING"/>
<element name="R1" library="adafruit3" package="0207/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit3" package="0207/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit3" package="0207/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch-dil" package="DP-02" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCDP02"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1255233"/>
<attribute name="OC_NEWARK" value="26M1095"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="adafruit3" package="EVQ-Q2" value="SPST_TACT-EVQQ2">
<attribute name="NAME"/>
</element>
<element name="U1" library="adafruit" package="ARDUINOR3" value="ARDUINOR3-DIMENSION"/>
<element name="CN1" library="adafruit3" package="JST-PH-2-SMT-RA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VIN">
<contactref element="U1" pad="VIN"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="SCL"/>
<contactref element="MS1" pad="18"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="SDA"/>
<contactref element="MS1" pad="17"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="AREF"/>
<contactref element="MS1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="GND"/>
<contactref element="U1" pad="GND1"/>
<contactref element="U1" pad="GND2"/>
<contactref element="MS1" pad="4"/>
<contactref element="RESET" pad="A"/>
<contactref element="LED1" pad="K"/>
<contactref element="R3" pad="1"/>
<contactref element="CN1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="D0"/>
<contactref element="MS1" pad="14"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="D1"/>
<contactref element="MS1" pad="15"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="D13"/>
<contactref element="MS1" pad="11"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="D12"/>
<contactref element="MS1" pad="13"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="D11"/>
<contactref element="MS1" pad="12"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="A0"/>
<contactref element="MS1" pad="5"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="A1"/>
<contactref element="MS1" pad="6"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="A2"/>
<contactref element="MS1" pad="7"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="A3"/>
<contactref element="MS1" pad="8"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="A4"/>
<contactref element="MS1" pad="9"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="A5"/>
<contactref element="MS1" pad="10"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="RESET"/>
<contactref element="MS1" pad="1"/>
<contactref element="RESET" pad="B"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="D2"/>
<contactref element="MS1" pad="22"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="D3"/>
<contactref element="MS1" pad="21"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="D4"/>
<contactref element="MS1" pad="20"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="D5"/>
<contactref element="MS1" pad="19"/>
</signal>
<signal name="N$21">
<contactref element="U1" pad="D6"/>
<contactref element="MS1" pad="23"/>
</signal>
<signal name="N$22">
<contactref element="U1" pad="D7"/>
<contactref element="MS1" pad="24"/>
</signal>
<signal name="N$23">
<contactref element="U1" pad="D8"/>
<contactref element="MS1" pad="25"/>
</signal>
<signal name="3V">
<contactref element="U1" pad="3V"/>
<contactref element="MS1" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="USB">
<contactref element="U1" pad="5V"/>
<contactref element="MS1" pad="26"/>
</signal>
<signal name="N$24">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="VBAT">
<contactref element="MS1" pad="28"/>
<contactref element="CN1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="GND">
</signal>
</signals>
</board>
</drawing>
</eagle>
