<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="72.39" y2="0" width="0" layer="20"/>
<wire x1="72.39" y1="0" x2="72.39" y2="49.276" width="0" layer="20"/>
<wire x1="72.39" y1="49.276" x2="0" y2="49.276" width="0" layer="20"/>
<wire x1="0" y1="49.276" x2="0" y2="0" width="0" layer="20"/>
<text>ICSP</text>
<text>GO!</text>
<hole x="69.596" y="46.482" drill="3.1"/>
<hole x="2.794" y="9.652" drill="3.1"/>
<hole x="69.596" y="2.794" drill="3.1"/>
<hole x="32.258" y="46.482" drill="3.1"/>
<text>sjm4306</text>
<text>HV Rescue</text>
<hole x="2.794" y="33.782" drill="3.1"/>
<hole x="40.894" y="2.794" drill="3.1"/>
<text>USB PWR</text>
<text>010920</text>
<text>JLCJLCJLCJLC</text>
<text>+12Vdc</text>
<text>c.pos.</text>
<text>+12V</text>
<text>+5V</text>
<text>+</text>
<text>+</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1X03-CLEANBIG">
</package>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="1X14-CB">
</package>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="DIP28">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MINIB">
<description>&lt;h3&gt;USB Type Mini-B Surface Mounted&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5 main, 4 shield pins&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/miniUSB-Dimensional.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_Mini-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="sjm4306_LOGO">
<packages>
<package name="SJM4306_LOGO_LARGE">
</package>
<package name="SJM4306_MEDIUM_NO_MASK">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92-EZ">
</package>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C4" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="adafruit" package="1X03-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="adafruit" package="1X03-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="PWR" library="adafruit" package="CHIP-LED0603" value="Red">
<attribute name="NAME"/>
</element>
<element name="BURN" library="adafruit" package="CHIP-LED0603" value="Green">
<attribute name="NAME"/>
</element>
<element name="Q1" library="adafruit" package="HC49U-V" value="16MHz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1666969"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-IC-Microcontroller" package="TQFP32-08" value="ATMEGA328P_TQFP">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09069"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="M0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0805" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0805" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PGM_ST" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="USB-MINIB" value="USB_MINI-B_SMT">
<attribute name="PROD_ID" value="CONN-08193"/>
<attribute name="SF_ID" value="PRT-00587"/>
</element>
<element name="U2" library="SparkFun-IC-Microcontroller" package="DIP28" value="ATMEGA328P_PDIP">
<attribute name="PROD_ID" value="IC-09136"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SparkFun-IC-Microcontroller" package="TQFP32-08" value="ATMEGA328P_TQFP">
<attribute name="PROD_ID" value="IC-09069"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="sjm4306_LOGO" package="SJM4306_LOGO_LARGE" value=""/>
<element name="JP6" library="adafruit" package="1X14-CB" value=""/>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92-EZ" value="200mA/40V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08447"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT23-3" value="500mA/300V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-09116"/>
</element>
<element name="R4" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R6" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R7" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R8" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R9" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R10" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R11" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R12" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R13" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R14" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R15" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R16" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R17" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R18" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R19" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R20" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R21" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R22" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="CN1" library="adafruit" package="DCJACK_2MM_PTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="linear" package="TO252" value="7805DT">
<attribute name="POPULARITY" value="0"/>
</element>
<element name="U$3" library="sjm4306_LOGO" package="SJM4306_MEDIUM_NO_MASK" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C4" pad="2"/>
<contactref element="PWR" pad="C"/>
<contactref element="JP2" pad="1"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="BURN" pad="C"/>
<contactref element="J1" pad="S2"/>
<contactref element="J1" pad="S1"/>
<contactref element="J1" pad="S3"/>
<contactref element="J1" pad="S4"/>
<contactref element="J1" pad="GND"/>
<contactref element="PGM_ST" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="22"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="21"/>
<contactref element="JP6" pad="7"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="CN1" pad="GND"/>
<contactref element="CN1" pad="GNDBREAK"/>
<contactref element="J3" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="C4" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="JP2" pad="3"/>
<contactref element="J1" pad="VBUS"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="20"/>
<contactref element="J3" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="PWR" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="BURN" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RST">
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="29"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="17"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="JP2" pad="2"/>
<contactref element="U1" pad="15"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="8"/>
<contactref element="C2" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="7"/>
<contactref element="C3" pad="1"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="25"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="27"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="28"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="A6">
<contactref element="U1" pad="19"/>
</signal>
<signal name="A7">
<contactref element="U1" pad="22"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="32"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="2"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="9"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="10"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="11"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="S_RST">
<contactref element="U2" pad="1"/>
<contactref element="U3" pad="29"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="PGM_ST">
<contactref element="PGM_ST" pad="3"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="N$14">
<contactref element="U2" pad="21"/>
<contactref element="JP6" pad="8"/>
</signal>
<signal name="N$18">
<contactref element="U2" pad="26"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="U2" pad="27"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="U2" pad="28"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="D+">
<contactref element="J1" pad="D+"/>
</signal>
<signal name="D-">
<contactref element="J1" pad="D-"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="31"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="D0">
<contactref element="U1" pad="30"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="S_PWR">
<contactref element="U1" pad="12"/>
<contactref element="U2" pad="7"/>
<contactref element="U2" pad="20"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="18"/>
<contactref element="JP6" pad="9"/>
</signal>
<signal name="D9">
<contactref element="U1" pad="13"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="D10">
<contactref element="U1" pad="14"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="A3">
<contactref element="U1" pad="26"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="PGM_LED">
<contactref element="U1" pad="23"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="Q3" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="12V">
<contactref element="R5" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="CN1" pad="PWR"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="PC2">
<contactref element="R6" pad="1"/>
<contactref element="U2" pad="25"/>
<contactref element="JP6" pad="4"/>
<contactref element="U3" pad="25"/>
</signal>
<signal name="PD6">
<contactref element="R8" pad="1"/>
<contactref element="U2" pad="12"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="PD7">
<contactref element="U2" pad="13"/>
<contactref element="U3" pad="11"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="S_OSC">
<contactref element="U2" pad="9"/>
<contactref element="U3" pad="7"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="PB0">
<contactref element="R10" pad="1"/>
<contactref element="U2" pad="14"/>
<contactref element="U3" pad="12"/>
</signal>
<signal name="PB1">
<contactref element="R11" pad="1"/>
<contactref element="U2" pad="15"/>
<contactref element="JP6" pad="14"/>
<contactref element="U3" pad="13"/>
</signal>
<signal name="PB2">
<contactref element="R12" pad="1"/>
<contactref element="U2" pad="16"/>
<contactref element="JP6" pad="13"/>
<contactref element="U3" pad="14"/>
</signal>
<signal name="PB3">
<contactref element="R13" pad="1"/>
<contactref element="U2" pad="17"/>
<contactref element="JP6" pad="12"/>
<contactref element="U3" pad="15"/>
</signal>
<signal name="PB4">
<contactref element="R14" pad="1"/>
<contactref element="U2" pad="18"/>
<contactref element="JP6" pad="11"/>
<contactref element="U3" pad="16"/>
</signal>
<signal name="PB5">
<contactref element="R15" pad="1"/>
<contactref element="U2" pad="19"/>
<contactref element="JP6" pad="10"/>
<contactref element="U3" pad="17"/>
</signal>
<signal name="PC0">
<contactref element="R16" pad="1"/>
<contactref element="U2" pad="23"/>
<contactref element="JP6" pad="6"/>
<contactref element="U3" pad="23"/>
</signal>
<signal name="PC1">
<contactref element="R17" pad="1"/>
<contactref element="U2" pad="24"/>
<contactref element="JP6" pad="5"/>
<contactref element="U3" pad="24"/>
</signal>
<signal name="PD4">
<contactref element="R18" pad="1"/>
<contactref element="U2" pad="6"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="PD3">
<contactref element="R19" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="PD2">
<contactref element="R20" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="U3" pad="32"/>
</signal>
<signal name="PD1">
<contactref element="R21" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="U3" pad="31"/>
</signal>
<signal name="PD5">
<contactref element="R22" pad="1"/>
<contactref element="U2" pad="11"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="U3" pad="30"/>
</signal>
<signal name="N$16">
<contactref element="U3" pad="22"/>
</signal>
<signal name="N$17">
<contactref element="U3" pad="19"/>
</signal>
<signal name="N$21">
<contactref element="U3" pad="28"/>
</signal>
<signal name="N$22">
<contactref element="U3" pad="27"/>
</signal>
<signal name="N$24">
<contactref element="U3" pad="26"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
