<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="2.8575" y1="0" x2="43.16" y2="0" width="0" layer="20"/>
<wire x1="43.16" y1="0" x2="43.16" y2="18.0975" width="0" layer="20"/>
<wire x1="43.16" y1="18.0975" x2="3.175" y2="18.0975" width="0" layer="20"/>
<wire x1="0" y1="14.9225" x2="0" y2="2.8575" width="0" layer="20"/>
<wire x1="0" y1="14.9225" x2="3.175" y2="18.0975" width="0.1524" layer="20"/>
<wire x1="0" y1="2.8575" x2="2.8575" y2="0" width="0.1524" layer="20"/>
<text>sjm4306</text>
<text>ArduinoISP</text>
<text>021920</text>
<text>JLCJLCJLCJLC</text>
<text>USB</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-MICROB-PTH">
</package>
<package name="USB-A-H">
<description>&lt;h3&gt;USB Type 'A' Male Connector - PTH&lt;/h3&gt;
Shield pins may be grounded.
&lt;br&gt; tDocu shows plug end. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/10016.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_A&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="sjm4306-custom">
<packages>
<package name="SO16">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AC</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-SMD-5X3.2-2PAD">
<description>&lt;h3&gt;5x3.2mm 2-pad SMD Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.txccrystal.com/images/pdf/7a.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_2_NC_TRACE_NO-SILK">
</package>
</packages>
</library>
<library name="SOICbite_Eagle">
<description>&lt;b&gt;SOICbite footprint&lt;/b&gt; &lt;br&gt;
Allows for direct clipping of a SOIC-8 Testclip onto a PCB edge for Programming/Debugging purposes without extra components.
&lt;br&gt;
&lt;br&gt;
Original footprint created by: Simon Merrit &lt;br&gt;
Adapted to Eagle by: Chiel Voswijk (Foxhood)
&lt;br&gt;
&lt;br&gt;
NOTE: Footprint is to be used on the edge of a PCB and may require the use of thin traces for accessing the inner pads. This may violate some Design Rules! One can often ignore these, but understand working is NOT guaranteed.</description>
<packages>
<package name="SOICBITE">
</package>
</packages>
</library>
<library name="sjm4306_LOGO">
<packages>
<package name="SJM4306_LOGO_SMALL">
</package>
<package name="SJM4306_LOGO_MEDIUM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="USB" library="SparkFun-Connectors" package="USB-MICROB-PTH" value="AMP FCI 10103594-0001LF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-13711"/>
</element>
<element name="HB" library="adafruit" package="CHIP-LED0805" value="Green">
<attribute name="NAME"/>
</element>
<element name="R3" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="ER" library="adafruit" package="CHIP-LED0805" value="Red">
<attribute name="NAME"/>
</element>
<element name="R6" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="PR" library="adafruit" package="CHIP-LED0805" value="Orange">
<attribute name="NAME"/>
</element>
<element name="R7" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="J19" library="SparkFun-Connectors" package="USB-A-H" value="USB_A_PTH_MALE">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08367"/>
<attribute name="SF_ID" value="PRT-00437"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="sjm4306-custom" package="SO16" value="CH340G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-Clocks" package="CRYSTAL-SMD-5X3.2-2PAD" value="12MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="adafruit" package="C0805" value="22pF">
<attribute name="NAME"/>
</element>
<element name="C6" library="adafruit" package="C0805" value="22pF">
<attribute name="NAME"/>
</element>
<element name="C7" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R5" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="C8" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="Q1" library="SparkFun-Clocks" package="CRYSTAL-SMD-5X3.2-2PAD" value="16MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-IC-Microcontroller" package="TQFP32-08" value="ATMEGA328P_TQFP">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09069"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="M0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0805" value="22pF">
<attribute name="NAME"/>
</element>
<element name="C3" library="adafruit" package="C0805" value="22pF">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_TRACE_NO-SILK" value="JUMPER-SMT_2_NC_TRACE_NO-SILK">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X3" value="ICSP">
<attribute name="PROD_ID" value="CONN-09701"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SOICbite_Eagle" package="SOICBITE" value="SOICBITE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="sjm4306_LOGO" package="SJM4306_LOGO_SMALL" value=""/>
<element name="U$2" library="sjm4306_LOGO" package="SJM4306_LOGO_MEDIUM" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="USB" pad="GND"/>
<contactref element="R3" pad="1"/>
<contactref element="USB" pad="P$2"/>
<contactref element="USB" pad="SHIELD4"/>
<contactref element="USB" pad="P$3"/>
<contactref element="USB" pad="SHEILD2"/>
<contactref element="USB" pad="P$4"/>
<contactref element="USB" pad="SHIELD"/>
<contactref element="USB" pad="P$6"/>
<contactref element="USB" pad="P$10"/>
<contactref element="USB" pad="SHIELD3"/>
<contactref element="USB" pad="P$8"/>
<contactref element="USB" pad="P$12"/>
<contactref element="USB" pad="P$1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="J19" pad="GND"/>
<contactref element="J19" pad="SHLD1"/>
<contactref element="J19" pad="SHLD2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="RST">
<contactref element="C7" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="15"/>
<contactref element="J1" pad="4"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="16"/>
<contactref element="J1" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="17"/>
<contactref element="J1" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="HB" pad="C"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="USB" pad="VBUS"/>
<contactref element="U2" pad="16"/>
<contactref element="C9" pad="1"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="20"/>
<contactref element="J1" pad="2"/>
<contactref element="JP2" pad="6"/>
<contactref element="J19" pad="VBUS"/>
</signal>
<signal name="D+">
<contactref element="USB" pad="D+"/>
<contactref element="J19" pad="D+"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="D-">
<contactref element="USB" pad="D-"/>
<contactref element="J19" pad="D-"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="ER" pad="C"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="PR" pad="C"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="Q2" pad="P$1"/>
<contactref element="C5" pad="1"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="N$10">
<contactref element="U2" pad="7"/>
<contactref element="Q2" pad="P$2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="U2" pad="4"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="RX">
<contactref element="U2" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="TX">
<contactref element="U2" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U2" pad="13"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="RX_O">
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="30"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="TX_O">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="31"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="PGM">
<contactref element="U1" pad="23"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="8"/>
<contactref element="C2" pad="1"/>
<contactref element="Q1" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="7"/>
<contactref element="C3" pad="1"/>
<contactref element="Q1" pad="P$2"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="25"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="27"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="28"/>
</signal>
<signal name="A6">
<contactref element="U1" pad="19"/>
</signal>
<signal name="A7">
<contactref element="U1" pad="22"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="32"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="1"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="2"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="9"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="10"/>
</signal>
<signal name="SRST">
<contactref element="U1" pad="14"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="PGM_ST">
<contactref element="U1" pad="24"/>
</signal>
<signal name="SPK">
<contactref element="U1" pad="26"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="29"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="ER">
<contactref element="ER" pad="A"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="PR">
<contactref element="PR" pad="A"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="HB">
<contactref element="HB" pad="A"/>
<contactref element="U1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
