(kicad_pcb (version 20171130) (host pcbnew 5.1.6)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 40)
    (zones 0)
    (modules 12)
    (nets 38)
  )
  (page User 200 150.012)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.8)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 0.7)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 66.04 99.06)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01000_fffffffe)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAMOutputs/"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 +3V3)
  (net 4 "Net-(E1-Pad3)")
  (net 5 "Net-(E1-Pad4)")
  (net 6 "Net-(E1-Pad5)")
  (net 7 "Net-(E1-Pad6)")
  (net 8 "Net-(E1-Pad7)")
  (net 9 "Net-(E1-Pad8)")
  (net 10 "Net-(E1-Pad9)")
  (net 11 "Net-(E1-Pad10)")
  (net 12 "Net-(E1-Pad11)")
  (net 13 "Net-(E1-Pad12)")
  (net 14 "Net-(E1-Pad13)")
  (net 15 "Net-(E1-Pad14)")
  (net 16 "Net-(E1-Pad15)")
  (net 17 "Net-(E1-Pad16)")
  (net 18 "Net-(E1-Pad17)")
  (net 19 "Net-(E1-Pad18)")
  (net 20 "Net-(E1-Pad19)")
  (net 21 "Net-(E1-Pad21)")
  (net 22 "Net-(E1-Pad22)")
  (net 23 "Net-(E1-Pad23)")
  (net 24 "Net-(E1-Pad24)")
  (net 25 "Net-(E1-Pad25)")
  (net 26 "Net-(E1-Pad26)")
  (net 27 "Net-(E1-Pad27)")
  (net 28 "Net-(E1-Pad28)")
  (net 29 "Net-(E1-Pad29)")
  (net 30 "Net-(E1-Pad30)")
  (net 31 /SOLAR-)
  (net 32 /SOLAR+)
  (net 33 BATT+)
  (net 34 "Net-(R1-Pad2)")
  (net 35 "Net-(R2-Pad2)")
  (net 36 ANE_OUT)
  (net 37 "Net-(U4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /SOLAR+)
    (add_net /SOLAR-)
    (add_net ANE_OUT)
    (add_net BATT+)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(E1-Pad10)")
    (add_net "Net-(E1-Pad11)")
    (add_net "Net-(E1-Pad12)")
    (add_net "Net-(E1-Pad13)")
    (add_net "Net-(E1-Pad14)")
    (add_net "Net-(E1-Pad15)")
    (add_net "Net-(E1-Pad16)")
    (add_net "Net-(E1-Pad17)")
    (add_net "Net-(E1-Pad18)")
    (add_net "Net-(E1-Pad19)")
    (add_net "Net-(E1-Pad21)")
    (add_net "Net-(E1-Pad22)")
    (add_net "Net-(E1-Pad23)")
    (add_net "Net-(E1-Pad24)")
    (add_net "Net-(E1-Pad25)")
    (add_net "Net-(E1-Pad26)")
    (add_net "Net-(E1-Pad27)")
    (add_net "Net-(E1-Pad28)")
    (add_net "Net-(E1-Pad29)")
    (add_net "Net-(E1-Pad3)")
    (add_net "Net-(E1-Pad30)")
    (add_net "Net-(E1-Pad4)")
    (add_net "Net-(E1-Pad5)")
    (add_net "Net-(E1-Pad6)")
    (add_net "Net-(E1-Pad7)")
    (add_net "Net-(E1-Pad8)")
    (add_net "Net-(E1-Pad9)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(U4-Pad1)")
  )
  (module Package_DIP:DIP-8_W7.62mm_Socket (layer F.Cu) (tedit 5F066761)
    (at 91.44 92.71 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U3 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value LM393 (at 3.81 5.08 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R2-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 ANE_OUT))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 86.36 83.82 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 3.81 1.65 270) (layer B.SilkS))
    (fp_text value 10K (at 3.81 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 ANE_OUT))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 76.2 83.82 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 3.81 1.65 270) (layer B.SilkS))
    (fp_text value 10K (at 3.81 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 35 "Net-(R2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5AE5139B)
    (at 81.28 83.82 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 3.81 1.65 270) (layer B.SilkS))
    (fp_text value 47R (at 3.81 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 34 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module misc:TC4056A_BREAKOUT (layer F.Cu) (tedit 5F06B17F)
    (at 115.57 54.61 90)
    (fp_text reference U2 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value TC4056A_BREAKOUT (at -0.635 -1.77 90) (layer F.Fab))
    (fp_text user OUTPUT (at 0 -8.89 90) (layer F.SilkS))
    (fp_text user INPUT (at 0 8.89 90) (layer F.SilkS))
    (pad 3 thru_hole circle (at 6.35 -8.89 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 6.35 8.89 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /SOLAR-))
    (pad 4 thru_hole circle (at -7.62 -8.89 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 BATT+))
    (pad 1 thru_hole rect (at -7.62 8.89 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /SOLAR+))
  )
  (module headers:2_double_spaced (layer F.Cu) (tedit 5F0667CC)
    (at 107.95 36.83 180)
    (fp_text reference J2 (at 0 -3.31) (layer F.SilkS))
    (fp_text value BATT (at 0 -5.08) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 BATT+))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module headers:2_double_spaced (layer F.Cu) (tedit 5F0667CC)
    (at 118.11 36.83 180)
    (fp_text reference J1 (at 0 -2.04) (layer F.SilkS))
    (fp_text value SOLAR (at 0 -3.81) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /SOLAR+))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /SOLAR-))
  )
  (module headers:4x1 (layer F.Cu) (tedit 5F0667B9)
    (at 80.01 93.98 180)
    (fp_text reference U1 (at 1.27 3.81) (layer F.SilkS))
    (fp_text value TCRT5000 (at 0 -2.54) (layer F.Fab))
    (pad 4 thru_hole circle (at 3.81 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R2-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.27 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R1-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module headers:4x1 (layer F.Cu) (tedit 5F0667B9)
    (at 106.68 69.85 270)
    (fp_text reference U4 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value REGULATOR (at 0 -5.08 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 3.81 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 3 thru_hole circle (at 1.27 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.27 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 BATT+))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U4-Pad1)"))
  )
  (module headers:3_double_spaced (layer F.Cu) (tedit 5F0667BF)
    (at 111.76 81.28)
    (fp_text reference RV1 (at 0 -3.31) (layer F.SilkS))
    (fp_text value R_POT (at 0 -5.08) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at -5.08 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module microcontroller:ESP31-DEVKIT (layer F.Cu) (tedit 5F066798)
    (at 87.63 57.15)
    (fp_text reference E1 (at 0 2.54) (layer F.SilkS))
    (fp_text value ESP32-DEVKIT (at 0 0) (layer F.Fab))
    (pad 30 thru_hole circle (at -12.7 -19.05) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(E1-Pad30)"))
    (pad 29 thru_hole circle (at -12.7 -16.51) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(E1-Pad29)"))
    (pad 28 thru_hole circle (at -12.7 -13.97) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(E1-Pad28)"))
    (pad 27 thru_hole circle (at -12.7 -11.43) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(E1-Pad27)"))
    (pad 26 thru_hole circle (at -12.7 -8.89) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(E1-Pad26)"))
    (pad 25 thru_hole circle (at -12.7 -6.35) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(E1-Pad25)"))
    (pad 24 thru_hole circle (at -12.7 -3.81) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(E1-Pad24)"))
    (pad 23 thru_hole circle (at -12.7 -1.27) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(E1-Pad23)"))
    (pad 22 thru_hole circle (at -12.7 1.27) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(E1-Pad22)"))
    (pad 21 thru_hole circle (at -12.7 3.81) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(E1-Pad21)"))
    (pad 20 thru_hole circle (at -12.7 6.35) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 ANE_OUT))
    (pad 19 thru_hole circle (at -12.7 8.89) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(E1-Pad19)"))
    (pad 18 thru_hole circle (at -12.7 11.43) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(E1-Pad18)"))
    (pad 17 thru_hole circle (at -12.7 13.97) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(E1-Pad17)"))
    (pad 16 thru_hole circle (at -12.7 16.51) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(E1-Pad16)"))
    (pad 15 thru_hole circle (at 12.7 -19.05) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(E1-Pad15)"))
    (pad 14 thru_hole circle (at 12.7 -16.51) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(E1-Pad14)"))
    (pad 13 thru_hole circle (at 12.7 -13.97) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(E1-Pad13)"))
    (pad 12 thru_hole circle (at 12.7 -11.43) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(E1-Pad12)"))
    (pad 11 thru_hole circle (at 12.7 -8.89) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(E1-Pad11)"))
    (pad 10 thru_hole circle (at 12.7 -6.35) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(E1-Pad10)"))
    (pad 9 thru_hole circle (at 12.7 -3.81) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(E1-Pad9)"))
    (pad 8 thru_hole circle (at 12.7 -1.27) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(E1-Pad8)"))
    (pad 7 thru_hole circle (at 12.7 1.27) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(E1-Pad7)"))
    (pad 6 thru_hole circle (at 12.7 3.81) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(E1-Pad6)"))
    (pad 5 thru_hole circle (at 12.7 6.35) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(E1-Pad5)"))
    (pad 4 thru_hole circle (at 12.7 8.89) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(E1-Pad4)"))
    (pad 3 thru_hole circle (at 12.7 11.43) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(E1-Pad3)"))
    (pad 2 thru_hole circle (at 12.7 13.97) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 12.7 16.51) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +3V3))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 101.6 88.9 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 2.54 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 128.27 36.83) (end 132.08 36.83) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "ANEMOMETER BOARD\nV1.0" (at 87.63 57.15 90) (layer B.Cu))
  (gr_line (start 69.85 99.06) (end 128.27 99.06) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.04 36.83) (end 66.04 95.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.27 33.02) (end 69.85 33.02) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 132.08 95.25) (end 132.08 36.83) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 69.85 95.25) (end 66.04 95.25) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 69.85 36.83) (end 69.85 33.02) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 128.27 33.02) (end 133.35 33.02) (angle 0) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 128.27 95.25) (end 128.27 99.06) (angle -90) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1.4) (smoothing fillet))
    (polygon
      (pts
        (xy 132.08 99.06) (xy 66.04 99.06) (xy 66.04 33.02) (xy 132.08 33.02)
      )
    )
  )
)
