(kicad_pcb (version 20171130) (host pcbnew 5.1.5-1.fc31)
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 597)
    (zones 0)
    (modules 23)
    (nets 52)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/tmp/kicad/65c816mini"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 M1)
  (net 3 RD)
  (net 4 A15)
  (net 5 A14)
  (net 6 A13)
  (net 7 A12)
  (net 8 A11)
  (net 9 A10)
  (net 10 A9)
  (net 11 A8)
  (net 12 A7)
  (net 13 A6)
  (net 14 A5)
  (net 15 A4)
  (net 16 A3)
  (net 17 IORQ)
  (net 18 D1)
  (net 19 D2)
  (net 20 D3)
  (net 21 D4)
  (net 22 D5)
  (net 23 D6)
  (net 24 D7)
  (net 25 A2)
  (net 26 A1)
  (net 27 A0)
  (net 28 RESET)
  (net 29 CLK)
  (net 30 MREQ)
  (net 31 WR)
  (net 32 VCC)
  (net 33 IRQ)
  (net 34 D0)
  (net 35 "Net-(R2-Pad1)")
  (net 36 "Net-(R3-Pad1)")
  (net 37 "Net-(R4-Pad1)")
  (net 38 RW)
  (net 39 "Net-(U3-Pad5)")
  (net 40 "Net-(J1-Pad39)")
  (net 41 VP)
  (net 42 VDA)
  (net 43 VPA)
  (net 44 "Net-(R7-Pad1)")
  (net 45 CLK0)
  (net 46 "Net-(U4-Pad1)")
  (net 47 "Net-(U4-Pad4)")
  (net 48 "Net-(U4-Pad12)")
  (net 49 "Net-(J1-Pad38)")
  (net 50 NMI)
  (net 51 "Net-(JP3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A10)
    (add_net A11)
    (add_net A12)
    (add_net A13)
    (add_net A14)
    (add_net A15)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net A8)
    (add_net A9)
    (add_net CLK)
    (add_net CLK0)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net IORQ)
    (add_net IRQ)
    (add_net M1)
    (add_net MREQ)
    (add_net NMI)
    (add_net "Net-(J1-Pad38)")
    (add_net "Net-(J1-Pad39)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad4)")
    (add_net RD)
    (add_net RESET)
    (add_net RW)
    (add_net VCC)
    (add_net VDA)
    (add_net VP)
    (add_net VPA)
    (add_net WR)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 249.682 117.856 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 1.016 10.414) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 VP))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 VDA))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 VPA))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 NMI))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 177.575001 132.314999 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U4 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value 74AHC00 (at 3.81 17.57 90) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(U4-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U4-Pad4)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(U4-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 CLK0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(U4-Pad12)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 CLK0))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U4-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 CLK))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U4-Pad4)"))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(U4-Pad12)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(U4-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(U4-Pad12)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-40_W15.24mm (layer F.Cu) (tedit 5A02E8C5)
    (at 250.952 123.19 270)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U1 (at -2.52984 0.08636 180) (layer F.SilkS))
    (fp_text value W65C816SxP (at 7.62 50.59 90) (layer F.Fab))
    (fp_text user %R (at 7.62 24.13 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 VP))
    (pad 21 thru_hole oval (at 15.24 48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R4-Pad1)"))
    (pad 22 thru_hole oval (at 15.24 45.72 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 A12))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(R7-Pad1)"))
    (pad 23 thru_hole oval (at 15.24 43.18 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 A13))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 IRQ))
    (pad 24 thru_hole oval (at 15.24 40.64 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 A14))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 15.24 38.1 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 A15))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 NMI))
    (pad 26 thru_hole oval (at 15.24 35.56 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 D7))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 VPA))
    (pad 27 thru_hole oval (at 15.24 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 D6))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 28 thru_hole oval (at 15.24 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 D5))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 A0))
    (pad 29 thru_hole oval (at 15.24 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 D4))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 A1))
    (pad 30 thru_hole oval (at 15.24 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 D3))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 A2))
    (pad 31 thru_hole oval (at 15.24 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 D2))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 A3))
    (pad 32 thru_hole oval (at 15.24 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 D1))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 A4))
    (pad 33 thru_hole oval (at 15.24 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 D0))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 A5))
    (pad 34 thru_hole oval (at 15.24 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 RW))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 A6))
    (pad 35 thru_hole oval (at 15.24 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 A7))
    (pad 36 thru_hole oval (at 15.24 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R3-Pad1)"))
    (pad 17 thru_hole oval (at 0 40.64 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 A8))
    (pad 37 thru_hole oval (at 15.24 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 CLK))
    (pad 18 thru_hole oval (at 0 43.18 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 A9))
    (pad 38 thru_hole oval (at 15.24 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R2-Pad1)"))
    (pad 19 thru_hole oval (at 0 45.72 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 A10))
    (pad 39 thru_hole oval (at 15.24 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 VDA))
    (pad 20 thru_hole oval (at 0 48.26 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 A11))
    (pad 40 thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 RESET))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 242.951 115.189 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 3.859 0.059 90) (layer F.SilkS))
    (fp_text value 3K3 (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 37 "Net-(R4-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 245.65 115.15 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R7 (at 3.8 0.05 90) (layer F.SilkS))
    (fp_text value 3K3 (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 44 "Net-(R7-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x40_P2.54mm_Horizontal (layer B.Cu) (tedit 59FED5CB)
    (at 155.702 152.4 270)
    (descr "Through hole angled pin header, 1x40, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x40 2.54mm single row")
    (fp_text reference J1 (at 4.385 2.27 270) (layer B.SilkS))
    (fp_text value Conn_01x40 (at 4.385 -101.33 270) (layer B.Fab))
    (fp_text user %R (at 2.77 -49.53) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 A15))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 A14))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 A13))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 A12))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 A11))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 A10))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 A9))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 A8))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 A7))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 A6))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 A5))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 A4))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 A3))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 A2))
    (pad 15 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 A1))
    (pad 16 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 A0))
    (pad 17 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 19 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 M1))
    (pad 20 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 RESET))
    (pad 21 thru_hole oval (at 0 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 CLK))
    (pad 22 thru_hole oval (at 0 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 IRQ))
    (pad 23 thru_hole oval (at 0 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 MREQ))
    (pad 24 thru_hole oval (at 0 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 WR))
    (pad 25 thru_hole oval (at 0 -60.96 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 RD))
    (pad 26 thru_hole oval (at 0 -63.5 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 IORQ))
    (pad 27 thru_hole oval (at 0 -66.04 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 D0))
    (pad 28 thru_hole oval (at 0 -68.58 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 D1))
    (pad 29 thru_hole oval (at 0 -71.12 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 D2))
    (pad 30 thru_hole oval (at 0 -73.66 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 D3))
    (pad 31 thru_hole oval (at 0 -76.2 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 D4))
    (pad 32 thru_hole oval (at 0 -78.74 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 D5))
    (pad 33 thru_hole oval (at 0 -81.28 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 D6))
    (pad 34 thru_hole oval (at 0 -83.82 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 D7))
    (pad 35 thru_hole oval (at 0 -86.36 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at 0 -88.9 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 0 -91.44 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 0 -93.98 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J1-Pad38)"))
    (pad 39 thru_hole oval (at 0 -96.52 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad39)"))
    (pad 40 thru_hole oval (at 0 -99.06 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x40_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 174.752 113.284 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 3.81 -2.33 180) (layer F.SilkS))
    (fp_text value 74AHC00 (at 3.81 17.57 90) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 RW))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U3-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 CLK0))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 RW))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 RD))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 RW))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 CLK0))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 MREQ))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U3-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(JP3-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 WR))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(JP3-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Oscillator:Oscillator_DIP-8 (layer F.Cu) (tedit 58CD3344)
    (at 213.65 115.2)
    (descr "Oscillator, DIP8,http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf")
    (tags oscillator)
    (fp_text reference X1 (at -1.45 3.55) (layer F.SilkS))
    (fp_text value CXO_DIP8 (at 3.81 3.74) (layer F.Fab))
    (fp_text user %R (at 3.81 -3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 CLK0))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_DIP-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 163.068 125.603)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74HCT688 (at 3.81 25.19) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 A11))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 A15))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 A10))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 A14))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 A9))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 A13))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 A8))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 A12))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(JP3-Pad1)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 583F5ADB)
    (at 158.9278 120.2436)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 26.6446 -55.0545) (layer F.SilkS) hide)
    (fp_text value "" (at 2.3368 -73.0631 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 169.799 108.966 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C1 (at 1.25984 2.02692 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 167.854 120.396 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C2 (at 1.42812 2.09296) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 229.87 119.38 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C3 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 201.422 149.606 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 4.064 -0.08636 90) (layer F.SilkS))
    (fp_text value 10K (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 M1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 240.792 115.189 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 3.849 0.108 90) (layer F.SilkS))
    (fp_text value 3K3 (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 35 "Net-(R2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 238.633 115.189 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 3.84048 0.17272 90) (layer F.SilkS))
    (fp_text value 3K3 (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 236.093 115.189 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 3.84048 0.0762 90) (layer F.SilkS))
    (fp_text value 3K3 (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 50 NMI))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 208.915 149.479 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at 3.80492 -0.02032 90) (layer F.SilkS))
    (fp_text value 3K3 (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 33 IRQ))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 250.444 145.288)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 RW))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad39)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 195.86 126.88 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C4 (at 1.25 -2.25 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 198.91 148.12 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C5 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 246.634 145.288)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 CLK))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J1-Pad38)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 203.708 106.68)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(JP3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 IORQ))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text IORQ (at 199.644 107.696) (layer F.SilkS))
  (gr_text "65C816 Mini CPU for RC2014 v0.1\n(C) 2019 Etched Pixels CC-NC\nI/O at $FExx" (at 187.19 119.17) (layer F.SilkS))
  (gr_text "JP1: Connect RW to Pin 39\nJP2: Connect E Clock to Pin 38" (at 219.71 147.32) (layer F.SilkS))
  (gr_text "“I’m in empowerment technology. \n I want to empower people to do their idea.\"\n-- Bill Mensch" (at 188.19 141.42) (layer F.SilkS))
  (gr_text 74HCT688 (at 166.57828 136.017 270) (layer F.SilkS))
  (gr_text 74AHC00 (at 182.99684 109.73308) (layer F.SilkS))
  (gr_text 65C816 (at 221.95 126.5) (layer F.SilkS))
  (gr_text "Pin 1" (at 155.68168 146.60118 90) (layer F.SilkS))
  (gr_text "A15\nA14\nA13\nA12\nA11\nA10\nA9\nA8\nA7\nA6\nA5\nA4\nA3\nA2\nA1\nA0\nGnd\n5v\nM1\nReset\nClock\nINT\nMreq\nWr\nRo\nIORQ\nD0\nD1\nD2\nD3\nD4\nD5\nD6\nD7\nTx\nRx\nUSR1\nUSR2\nUSR3" (at 203.9112 153.6573 90) (layer F.SilkS))
  (gr_line (start 253 108.685) (end 253 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 247.8184 103.505) (end 168.91 103.505) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 247.8184 108.685) (end 247.8184 103.505) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.8986 118.5164) (end 153.8986 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.91 103.505) (end 153.8986 118.5164) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.8986 153.3652) (end 253 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.924 153.416) (xy 153.924 118.618) (xy 168.91 103.378) (xy 247.904 103.378) (xy 252.984 107.95)
        (xy 252.984 153.416)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.924 153.416) (xy 153.924 118.364) (xy 168.91 103.378) (xy 248.158 103.378) (xy 252.984 107.95)
        (xy 252.984 153.416)
      )
    )
  )
)
