(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 166)
    (zones 0)
    (modules 34)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J2-Pad1)")
  (net 5 "Net-(J2-Pad2)")
  (net 6 "Net-(J2-Pad3)")
  (net 7 "Net-(J2-Pad4)")
  (net 8 "Net-(J2-Pad6)")
  (net 9 "Net-(J2-Pad7)")
  (net 10 "Net-(J2-Pad8)")
  (net 11 "Net-(J2-Pad9)")
  (net 12 "Net-(J2-Pad10)")
  (net 13 "Net-(J2-Pad11)")
  (net 14 "Net-(J2-Pad12)")
  (net 15 "Net-(J2-Pad13)")
  (net 16 "Net-(J2-Pad14)")
  (net 17 "Net-(J2-Pad15)")
  (net 18 "Net-(J2-Pad16)")
  (net 19 "Net-(J2-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Horizontal (layer F.Cu) (tedit 59FED737)
    (at 195 58)
    (descr "Through hole angled pin header, 1x02, 1.00mm pitch, 2.0mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 1.00mm single row")
    (fp_text reference J1 (at 0.5 -1.56) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0.5 1.56) (layer F.Fab))
    (fp_text user %R (at 0.5 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 1) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x16_P1.00mm_Horizontal (layer F.Cu) (tedit 59FED737)
    (at 196 86)
    (descr "Through hole angled pin header, 1x16, 1.00mm pitch, 2.0mm pin length, single row")
    (tags "Through hole angled pin header THT 1x16 1.00mm single row")
    (fp_text reference J2 (at 0 -1.56) (layer F.SilkS))
    (fp_text value Conn_01x16 (at 0 16.56) (layer F.Fab))
    (fp_text user %R (at 0 7.5 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 0 15) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad16)"))
    (pad 15 thru_hole oval (at 0 14) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad15)"))
    (pad 14 thru_hole oval (at 0 13) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad14)"))
    (pad 13 thru_hole oval (at 0 12) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad13)"))
    (pad 12 thru_hole oval (at 0 11) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 10) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 0 9) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 8) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 0 7) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 6) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 0 5) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 4) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 0 3) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 2) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 1) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x16_P1.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 114 65)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R1 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 111 55)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 134 65)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R4 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 131 55)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 154 65)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R6 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 151 55)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 174 65)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R8 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 171 55)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 114 85)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R10 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad8)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 111 75)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad8)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 134 85)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R12 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad7)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 131 75)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad7)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 154 85)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R14 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad6)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 151 75)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R15 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad6)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 174 85)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R16 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad5)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 171 75)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R17 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad5)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 114 105)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R18 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad9)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 110.84 95)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R19 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad9)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 134 105)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R20 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad10)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 131 95)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R21 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad10)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 154 105)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R22 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad11)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 151 95)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R23 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad11)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 174 105)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R24 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad12)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 171 95)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R25 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad12)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 114 125)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R26 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad13)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 111 115)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R27 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad13)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 134 125)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R28 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad14)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 130.84 115)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R29 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad14)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 154 125)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R30 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad15)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 151 115)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R31 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad15)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical (layer F.Cu) (tedit 5B860497)
    (at 174 125)
    (descr "Resistor, LDR D=6.4mm, see http://yourduino.com/docs/Photoresistor-5516-datasheet.pdf")
    (tags "Resistor LDRD=6.4mm")
    (fp_text reference R32 (at 1.7 -4) (layer F.SilkS))
    (fp_text value A1060 (at 1.7 4.1) (layer F.Fab))
    (fp_text user %R (at 1.7 -4) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad16)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_D6.4mm_P3.4mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 171 115)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R33 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad16)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 105 145) (end 105 147.5) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 195 145) (end 195 147.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100 50) (end 200 50) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200 150) (end 100 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200 50) (end 200 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100 150) (end 100 50) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200 150) (xy 100 150) (xy 100 50) (xy 200 50)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200 150) (xy 100 150) (xy 100 50) (xy 200 50)
      )
    )
  )
)
