(kicad_pcb (version 20171130) (host pcbnew 5.1.5-1.fc31)
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 646)
    (zones 0)
    (modules 21)
    (nets 79)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/tmp/kicad/multi-io"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 RD)
  (net 3 A7)
  (net 4 A6)
  (net 5 A5)
  (net 6 A4)
  (net 7 A3)
  (net 8 IORQ)
  (net 9 D1)
  (net 10 D2)
  (net 11 D3)
  (net 12 D4)
  (net 13 D5)
  (net 14 D6)
  (net 15 D7)
  (net 16 A2)
  (net 17 A1)
  (net 18 A0)
  (net 19 RESET)
  (net 20 CLK)
  (net 21 INT)
  (net 22 WR)
  (net 23 "Net-(J2-Pad10)")
  (net 24 D0)
  (net 25 VCC)
  (net 26 "Net-(D1-Pad1)")
  (net 27 "Net-(J1-Pad35)")
  (net 28 "Net-(J1-Pad36)")
  (net 29 "Net-(J2-Pad1)")
  (net 30 "Net-(J2-Pad3)")
  (net 31 "Net-(J2-Pad5)")
  (net 32 "Net-(J2-Pad7)")
  (net 33 "Net-(J2-Pad9)")
  (net 34 "Net-(J2-Pad11)")
  (net 35 "Net-(J2-Pad13)")
  (net 36 "Net-(J2-Pad15)")
  (net 37 TXRDYA)
  (net 38 "Net-(J3-Pad11)")
  (net 39 "Net-(J3-Pad10)")
  (net 40 "Net-(J3-Pad9)")
  (net 41 "Net-(J3-Pad8)")
  (net 42 "Net-(J3-Pad7)")
  (net 43 "Net-(J3-Pad6)")
  (net 44 "Net-(J3-Pad5)")
  (net 45 "Net-(J3-Pad4)")
  (net 46 "Net-(J3-Pad2)")
  (net 47 "Net-(J4-Pad2)")
  (net 48 "Net-(J4-Pad4)")
  (net 49 "Net-(J4-Pad5)")
  (net 50 "Net-(J4-Pad6)")
  (net 51 "Net-(J4-Pad7)")
  (net 52 "Net-(J4-Pad8)")
  (net 53 "Net-(J4-Pad9)")
  (net 54 "Net-(J4-Pad10)")
  (net 55 "Net-(J4-Pad11)")
  (net 56 TXRDYB)
  (net 57 TXA)
  (net 58 RXA)
  (net 59 DTRA)
  (net 60 CTSA)
  (net 61 RTSA)
  (net 62 RIA)
  (net 63 CDA)
  (net 64 MFA)
  (net 65 DSRA)
  (net 66 RTSB)
  (net 67 RXB)
  (net 68 TXB)
  (net 69 CTSB)
  (net 70 DTRB)
  (net 71 DSRB)
  (net 72 MFB)
  (net 73 CDB)
  (net 74 RIB)
  (net 75 "Net-(U1-Pad17)")
  (net 76 "Net-(U1-Pad21)")
  (net 77 "Net-(U1-Pad34)")
  (net 78 "Net-(JP3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net CDA)
    (add_net CDB)
    (add_net CLK)
    (add_net CTSA)
    (add_net CTSB)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net DSRA)
    (add_net DSRB)
    (add_net DTRA)
    (add_net DTRB)
    (add_net INT)
    (add_net IORQ)
    (add_net MFA)
    (add_net MFB)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J1-Pad35)")
    (add_net "Net-(J1-Pad36)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J4-Pad10)")
    (add_net "Net-(J4-Pad11)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(J4-Pad9)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad34)")
    (add_net RD)
    (add_net RESET)
    (add_net RIA)
    (add_net RIB)
    (add_net RTSA)
    (add_net RTSB)
    (add_net RXA)
    (add_net RXB)
    (add_net TXA)
    (add_net TXB)
    (add_net TXRDYA)
    (add_net TXRDYB)
    (add_net VCC)
    (add_net WR)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x40_P2.54mm_Horizontal (layer B.Cu) (tedit 59FED5CB)
    (at 155.702 152.4 270)
    (descr "Through hole angled pin header, 1x40, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x40 2.54mm single row")
    (fp_text reference J1 (at 4.385 2.27 270) (layer B.SilkS))
    (fp_text value Conn_01x40 (at 4.385 -101.33 270) (layer B.Fab))
    (fp_text user %R (at 2.77 -49.53) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 A7))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 A6))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 A5))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 A4))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 A3))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 A2))
    (pad 15 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 A1))
    (pad 16 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 A0))
    (pad 17 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 19 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 RESET))
    (pad 21 thru_hole oval (at 0 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 CLK))
    (pad 22 thru_hole oval (at 0 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 INT))
    (pad 23 thru_hole oval (at 0 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 0 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 WR))
    (pad 25 thru_hole oval (at 0 -60.96 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 RD))
    (pad 26 thru_hole oval (at 0 -63.5 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 IORQ))
    (pad 27 thru_hole oval (at 0 -66.04 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 D0))
    (pad 28 thru_hole oval (at 0 -68.58 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 D1))
    (pad 29 thru_hole oval (at 0 -71.12 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 D2))
    (pad 30 thru_hole oval (at 0 -73.66 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 D3))
    (pad 31 thru_hole oval (at 0 -76.2 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 D4))
    (pad 32 thru_hole oval (at 0 -78.74 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 D5))
    (pad 33 thru_hole oval (at 0 -81.28 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 D6))
    (pad 34 thru_hole oval (at 0 -83.82 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 D7))
    (pad 35 thru_hole oval (at 0 -86.36 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad35)"))
    (pad 36 thru_hole oval (at 0 -88.9 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad36)"))
    (pad 37 thru_hole oval (at 0 -91.44 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 0 -93.98 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 -96.52 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 40 thru_hole oval (at 0 -99.06 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x40_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 583F5ADB)
    (at 158.9278 120.2436)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 26.6446 -55.0545) (layer F.SilkS) hide)
    (fp_text value "" (at 2.3368 -73.0631 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 244.348 124.714 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C1 (at 1.25 2.032) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 165.862 126.746)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C2 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 183.896 126.492)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C3 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 216.662 121.92)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C4 (at 1.25 -2.25) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 208.788 141.478 270)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 4.064 -0.254 180) (layer F.SilkS))
    (fp_text value 1N517 (at 3.81 2.47 90) (layer F.Fab))
    (fp_text user %R (at 4.2 0 90) (layer F.Fab))
    (fp_text user K (at 0 -1.9 90) (layer F.Fab))
    (fp_text user K (at 0 -1.9 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 INT))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 159.512 147.574 180)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value Conn_02x08_Odd_Even (at 1.27 20.11) (layer F.Fab))
    (fp_text user %R (at 1.27 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad10)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad10)"))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad10)"))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad10)"))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad10)"))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad10)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 171.45 105.918 90)
    (descr "Through hole angled pin header, 1x12, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x12 2.54mm single row")
    (fp_text reference J3 (at 0.508 -2.27 180) (layer F.SilkS))
    (fp_text value Conn_01x12 (at 4.385 30.21 90) (layer F.Fab))
    (fp_text user %R (at 2.77 13.97) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 TXRDYA))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J3-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J3-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J3-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J3-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J3-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J3-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J3-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 218.44 107.188 90)
    (descr "Through hole angled pin header, 1x12, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x12 2.54mm single row")
    (fp_text reference J4 (at 2.54 -2.794 180) (layer F.SilkS))
    (fp_text value Conn_01x12 (at 4.385 30.21 90) (layer F.Fab))
    (fp_text user %R (at 2.77 13.97) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J4-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J4-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J4-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J4-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(J4-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J4-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 TXRDYB))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 242.57 131.318 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 0 4.572) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad35)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 TXA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 246.634 131.318 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at 0 4.826) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 RXA))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad36)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP10 (layer F.Cu) (tedit 5A14249F)
    (at 167.64 109.728)
    (descr "10-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 0.254 -2.286) (layer F.SilkS))
    (fp_text value R_Pack05_SIP (at 12.7 2.4) (layer F.Fab))
    (fp_text user %R (at 11.43 0) (layer F.Fab))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(J3-Pad7)"))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 DTRA))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(J3-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 CTSA))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(J3-Pad5)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 TXA))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(J3-Pad4)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 RXA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 RTSA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP8 (layer F.Cu) (tedit 5A14249F)
    (at 194.31 109.728)
    (descr "8-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN2 (at 10.16 -2.4) (layer F.SilkS))
    (fp_text value R_Pack04_SIP (at 10.16 2.4) (layer F.Fab))
    (fp_text user %R (at 8.89 0) (layer F.Fab))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(J3-Pad11)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 RIA))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad10)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 CDA))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(J3-Pad9)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 MFA))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(J3-Pad8)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 DSRA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP10 (layer F.Cu) (tedit 5A14249F)
    (at 223.774 110.998)
    (descr "10-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN3 (at 26.416 0.254) (layer F.SilkS))
    (fp_text value R_Pack05_SIP (at 12.7 2.4) (layer F.Fab))
    (fp_text user %R (at 11.43 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 RTSB))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 RXB))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 TXB))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(J4-Pad5)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 CTSB))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(J4-Pad6)"))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 DTRB))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(J4-Pad7)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP8 (layer F.Cu) (tedit 5A14249F)
    (at 228.854 114.554)
    (descr "8-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN4 (at 21.336 0.254) (layer F.SilkS))
    (fp_text value R_Pack04_SIP (at 10.16 2.4) (layer F.Fab))
    (fp_text user %R (at 8.89 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 DSRB))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(J4-Pad8)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 MFB))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(J4-Pad9)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 CDB))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(J4-Pad10)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 RIB))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(J4-Pad11)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LCC:PLCC-44_THT-Socket (layer F.Cu) (tedit 5A02ECC8)
    (at 226.568 142.24 180)
    (descr "PLCC, 44 pins, through hole")
    (tags "plcc leaded")
    (fp_text reference U1 (at -1.27 -6.4) (layer F.SilkS))
    (fp_text value 16C2552 (at -1.27 19.1) (layer F.Fab))
    (fp_text user %R (at -1.27 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 TXRDYA))
    (pad 3 thru_hole circle (at -2.54 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 D1))
    (pad 5 thru_hole circle (at -5.08 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 D3))
    (pad 43 thru_hole circle (at 2.54 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 RIA))
    (pad 41 thru_hole circle (at 5.08 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 DSRA))
    (pad 2 thru_hole circle (at -2.54 -2.54 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 D0))
    (pad 4 thru_hole circle (at -5.08 -2.54 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 D2))
    (pad 6 thru_hole circle (at -7.62 -2.54 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 D4))
    (pad 44 thru_hole circle (at 0 -2.54 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 42 thru_hole circle (at 2.54 -2.54 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 CDA))
    (pad 8 thru_hole circle (at -7.62 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 D6))
    (pad 10 thru_hole circle (at -7.62 2.54 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 A0))
    (pad 12 thru_hole circle (at -7.62 5.08 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole circle (at -7.62 7.62 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 A1))
    (pad 16 thru_hole circle (at -7.62 10.16 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 A3))
    (pad 7 thru_hole circle (at -10.16 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 D5))
    (pad 9 thru_hole circle (at -10.16 2.54 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 D7))
    (pad 11 thru_hole circle (at -10.16 5.08 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(JP3-Pad1)"))
    (pad 13 thru_hole circle (at -10.16 7.62 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at -10.16 10.16 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 A2))
    (pad 17 thru_hole circle (at -10.16 12.7 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(U1-Pad17)"))
    (pad 19 thru_hole circle (at -7.62 12.7 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 MFB))
    (pad 21 thru_hole circle (at -5.08 12.7 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(U1-Pad21)"))
    (pad 23 thru_hole circle (at -2.54 12.7 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 RTSB))
    (pad 25 thru_hole circle (at 0 12.7 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 RXB))
    (pad 27 thru_hole circle (at 2.54 12.7 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 DTRB))
    (pad 29 thru_hole circle (at 7.62 12.7 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 DSRB))
    (pad 18 thru_hole circle (at -7.62 15.24 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad10)"))
    (pad 20 thru_hole circle (at -5.08 15.24 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 WR))
    (pad 22 thru_hole circle (at -2.54 15.24 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole circle (at 0 15.24 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 RD))
    (pad 26 thru_hole circle (at 2.54 15.24 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 TXB))
    (pad 28 thru_hole circle (at 5.08 15.24 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 CTSB))
    (pad 30 thru_hole circle (at 5.08 12.7 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 CDB))
    (pad 32 thru_hole circle (at 5.08 10.16 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 TXRDYB))
    (pad 34 thru_hole circle (at 5.08 7.62 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(U1-Pad34)"))
    (pad 36 thru_hole circle (at 5.08 5.08 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 RTSA))
    (pad 38 thru_hole circle (at 5.08 2.54 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 TXA))
    (pad 40 thru_hole circle (at 5.08 -2.54 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 CTSA))
    (pad 31 thru_hole circle (at 7.62 10.16 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 RIB))
    (pad 33 thru_hole circle (at 7.62 7.62 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 35 thru_hole circle (at 7.62 5.08 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 MFA))
    (pad 37 thru_hole circle (at 7.62 2.54 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 DTRA))
    (pad 39 thru_hole circle (at 7.62 0 180) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 RXA))
    (model ${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-44_THT-Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm_Socket (layer F.Cu) (tedit 5A02E8C5)
    (at 170.942 147.828 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U2 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74HCT138 (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 A7))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad13)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 A5))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad11)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 A6))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad9)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 A4))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad7)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 IORQ))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad3)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad15)"))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-14_W7.62mm_Socket (layer F.Cu) (tedit 5A02E8C5)
    (at 189.23 145.542 180)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U3 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74HC02 (at 3.81 17.57) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(U1-Pad21)"))
    (pad 8 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 RESET))
    (pad 9 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 RESET))
    (pad 10 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(D1-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(U1-Pad34)"))
    (pad 12 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(U1-Pad17)"))
    (pad 13 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Oscillator:Oscillator_DIP-8 (layer F.Cu) (tedit 58CD3344)
    (at 243.332 145.288)
    (descr "Oscillator, DIP8,http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf")
    (tags oscillator)
    (fp_text reference X1 (at 3.81 -11.26) (layer F.SilkS))
    (fp_text value CXO_DIP8 (at 3.81 3.74) (layer F.Fab))
    (fp_text user %R (at 3.81 -3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 VCC))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(JP3-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_DIP-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 203.454 144.018)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(JP3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 CLK))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "“The single biggest problem in communication is the illusion that it has taken place.”\n― George Bernard Shaw " (at 194.818 122.174) (layer F.SilkS))
  (gr_text EPDSER (at 164.592 116.078) (layer F.SilkS))
  (gr_text "Dual 16C550 UART\n(C) 2020 Etched Pixels CC-NC" (at 195.326 118.11) (layer F.SilkS))
  (gr_text 16C2552 (at 228.092 133.858) (layer F.SilkS))
  (gr_text "Serial Port 2" (at 235.458 117.856) (layer F.SilkS))
  (gr_text "Serial Port 1" (at 186.436 112.776) (layer F.SilkS))
  (gr_text 74HC02 (at 185.166 137.922 270) (layer F.SilkS))
  (gr_text I/O (at 158.242 127) (layer F.SilkS))
  (gr_text 74HCT138 (at 167.132 138.938 270) (layer F.SilkS))
  (gr_text "Pin 1" (at 155.68168 146.60118 90) (layer F.SilkS))
  (gr_text "A15\nA14\nA13\nA12\nA11\nA10\nA9\nA8\nA7\nA6\nA5\nA4\nA3\nA2\nA1\nA0\nGnd\n5v\nM1\nReset\nClock\nINT\nMreq\nWr\nRo\nIORQ\nD0\nD1\nD2\nD3\nD4\nD5\nD6\nD7\nTx\nRx\nUSR1\nUSR2\nUSR3" (at 203.9112 153.6573 90) (layer F.SilkS))
  (gr_line (start 253 108.685) (end 253 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 247.8184 103.505) (end 168.91 103.505) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 247.8184 108.685) (end 247.8184 103.505) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.8986 118.5164) (end 153.8986 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.91 103.505) (end 153.8986 118.5164) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.8986 153.3652) (end 253 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.924 153.416) (xy 153.924 118.618) (xy 168.91 103.378) (xy 247.904 103.378) (xy 252.984 107.95)
        (xy 252.984 153.416)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.924 153.416) (xy 153.924 118.364) (xy 168.91 103.378) (xy 248.158 103.378) (xy 252.984 107.95)
        (xy 252.984 153.416)
      )
    )
  )
)
