(kicad_pcb (version 20171130) (host pcbnew 5.1.5-1.fc31)
  (general
    (thickness 1.6)
    (drawings 31)
    (tracks 793)
    (zones 0)
    (modules 26)
    (nets 70)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/tmp/kicad/uart2"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 RD)
  (net 3 A7)
  (net 4 A6)
  (net 5 A5)
  (net 6 A4)
  (net 7 A3)
  (net 8 IORQ)
  (net 9 WR)
  (net 10 "Net-(J2-Pad10)")
  (net 11 VCC)
  (net 12 A2)
  (net 13 A1)
  (net 14 A0)
  (net 15 RESET)
  (net 16 CLK)
  (net 17 INT)
  (net 18 D0)
  (net 19 D1)
  (net 20 D2)
  (net 21 D3)
  (net 22 D4)
  (net 23 D5)
  (net 24 D6)
  (net 25 D7)
  (net 26 TXDA)
  (net 27 RXDA)
  (net 28 "Net-(J2-Pad1)")
  (net 29 "Net-(J2-Pad3)")
  (net 30 "Net-(J2-Pad5)")
  (net 31 "Net-(J2-Pad7)")
  (net 32 "Net-(J2-Pad9)")
  (net 33 "Net-(J2-Pad11)")
  (net 34 "Net-(J2-Pad13)")
  (net 35 "Net-(J2-Pad15)")
  (net 36 SPI0_CS)
  (net 37 SPICLK)
  (net 38 SPIDATA)
  (net 39 SPI0_RX)
  (net 40 SPI0_IN)
  (net 41 SPI0_OUT)
  (net 42 SPI1_OUT)
  (net 43 SPI1_IN)
  (net 44 SPI1_RX)
  (net 45 SPI1_CS)
  (net 46 SPI2_CS)
  (net 47 SPI2_RX)
  (net 48 SPI2_IN)
  (net 49 "Net-(J7-Pad2)")
  (net 50 "Net-(J7-Pad4)")
  (net 51 "Net-(J7-Pad5)")
  (net 52 "Net-(J7-Pad6)")
  (net 53 "Net-(J8-Pad6)")
  (net 54 "Net-(J8-Pad5)")
  (net 55 "Net-(J8-Pad4)")
  (net 56 "Net-(J8-Pad2)")
  (net 57 "Net-(JP1-Pad1)")
  (net 58 CTSA)
  (net 59 RTSA)
  (net 60 RTSB)
  (net 61 RXDB)
  (net 62 TXDB)
  (net 63 CTSB)
  (net 64 SPI_RX)
  (net 65 MUX1)
  (net 66 NRESET)
  (net 67 MUX0)
  (net 68 "Net-(J1-Pad35)")
  (net 69 "Net-(J1-Pad36)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net CLK)
    (add_net CTSA)
    (add_net CTSB)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net INT)
    (add_net IORQ)
    (add_net MUX0)
    (add_net MUX1)
    (add_net NRESET)
    (add_net "Net-(J1-Pad35)")
    (add_net "Net-(J1-Pad36)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J7-Pad4)")
    (add_net "Net-(J7-Pad5)")
    (add_net "Net-(J7-Pad6)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J8-Pad4)")
    (add_net "Net-(J8-Pad5)")
    (add_net "Net-(J8-Pad6)")
    (add_net "Net-(JP1-Pad1)")
    (add_net RD)
    (add_net RESET)
    (add_net RTSA)
    (add_net RTSB)
    (add_net RXDA)
    (add_net RXDB)
    (add_net SPI0_CS)
    (add_net SPI0_IN)
    (add_net SPI0_OUT)
    (add_net SPI0_RX)
    (add_net SPI1_CS)
    (add_net SPI1_IN)
    (add_net SPI1_OUT)
    (add_net SPI1_RX)
    (add_net SPI2_CS)
    (add_net SPI2_IN)
    (add_net SPI2_RX)
    (add_net SPICLK)
    (add_net SPIDATA)
    (add_net SPI_RX)
    (add_net TXDA)
    (add_net TXDB)
    (add_net VCC)
    (add_net WR)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 212.344 145.288 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C5 (at -1.778 0.254 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 170.434 129.286)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value Conn_02x08_Odd_Even (at 1.27 20.11) (layer F.Fab))
    (fp_text user %R (at 1.27 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad10)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad10)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad10)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad10)"))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad10)"))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad10)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x40_P2.54mm_Horizontal (layer B.Cu) (tedit 59FED5CB)
    (at 155.702 152.4 270)
    (descr "Through hole angled pin header, 1x40, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x40 2.54mm single row")
    (fp_text reference J1 (at 4.385 2.27 270) (layer B.SilkS))
    (fp_text value Conn_01x40 (at 4.385 -101.33 270) (layer B.Fab))
    (fp_text user %R (at 2.77 -49.53) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 A7))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 A6))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 A5))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 A4))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 A3))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 A2))
    (pad 15 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 A1))
    (pad 16 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 A0))
    (pad 17 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 VCC))
    (pad 19 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 RESET))
    (pad 21 thru_hole oval (at 0 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 CLK))
    (pad 22 thru_hole oval (at 0 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 INT))
    (pad 23 thru_hole oval (at 0 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 0 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 WR))
    (pad 25 thru_hole oval (at 0 -60.96 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 RD))
    (pad 26 thru_hole oval (at 0 -63.5 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 IORQ))
    (pad 27 thru_hole oval (at 0 -66.04 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 D0))
    (pad 28 thru_hole oval (at 0 -68.58 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 D1))
    (pad 29 thru_hole oval (at 0 -71.12 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 D2))
    (pad 30 thru_hole oval (at 0 -73.66 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 D3))
    (pad 31 thru_hole oval (at 0 -76.2 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 D4))
    (pad 32 thru_hole oval (at 0 -78.74 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 D5))
    (pad 33 thru_hole oval (at 0 -81.28 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 D6))
    (pad 34 thru_hole oval (at 0 -83.82 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 D7))
    (pad 35 thru_hole oval (at 0 -86.36 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(J1-Pad35)"))
    (pad 36 thru_hole oval (at 0 -88.9 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J1-Pad36)"))
    (pad 37 thru_hole oval (at 0 -91.44 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 0 -93.98 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 -96.52 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 40 thru_hole oval (at 0 -99.06 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x40_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 198.628 127.254 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C1 (at -2.032 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 RESET))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 583F5ADB)
    (at 158.9278 120.2436)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 26.6446 -55.0545) (layer F.SilkS) hide)
    (fp_text value "" (at 2.3368 -73.0631 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 164.338 124.968 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C2 (at 1.016 2.286) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 185.42 124.46 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C3 (at 2.54 2.032) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 199.644 115.57 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C4 (at 1.27 2.286 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 221.996 106.172 90)
    (descr "Through hole angled pin header, 1x08, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x08 2.54mm single row")
    (fp_text reference J3 (at 4.385 -2.27 90) (layer F.SilkS))
    (fp_text value Conn_01x08_Male (at 4.385 20.05 90) (layer F.Fab))
    (fp_text user %R (at 2.77 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 SPI0_CS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 SPICLK))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 SPIDATA))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 SPI0_RX))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 VCC))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 SPI0_IN))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 SPI0_OUT))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 199.898 106.172 90)
    (descr "Through hole angled pin header, 1x08, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x08 2.54mm single row")
    (fp_text reference J4 (at 4.385 -2.27 90) (layer F.SilkS))
    (fp_text value Conn_01x08_Male (at 4.385 20.05 90) (layer F.Fab))
    (fp_text user %R (at 2.77 8.89) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 SPI1_OUT))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 SPI1_IN))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 VCC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 SPI1_RX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 SPIDATA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 SPICLK))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 SPI1_CS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 177.8 106.172 90)
    (descr "Through hole angled pin header, 1x08, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x08 2.54mm single row")
    (fp_text reference J5 (at 4.385 -2.27 90) (layer F.SilkS))
    (fp_text value Conn_01x08_Male (at 4.385 20.05 90) (layer F.Fab))
    (fp_text user %R (at 2.77 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 SPI2_CS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 SPICLK))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 SPIDATA))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 SPI2_RX))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 VCC))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 SPI2_IN))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 248.158 135.636)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J7 (at 3.048 -2.794) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 4.385 14.97) (layer F.Fab))
    (fp_text user %R (at 2.77 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J7-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 VCC))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J7-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J7-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J7-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 248.412 113.538)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J8 (at 2.54 -2.286) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 4.385 14.97) (layer F.Fab))
    (fp_text user %R (at 2.77 6.35 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J8-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(J8-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J8-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(J8-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 206.502 146.304)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 CLK))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 194.818 121.412 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 2.032 0 180) (layer F.SilkS))
    (fp_text value 4K7 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 RESET))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP8 (layer F.Cu) (tedit 5A14249F)
    (at 244.348 130.81 270)
    (descr "8-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at -1.524 -3.302 180) (layer F.SilkS))
    (fp_text value R_Pack04_SIP (at 10.16 2.4 90) (layer F.Fab))
    (fp_text user %R (at 8.89 0 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 17.78 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 CTSA))
    (pad 7 thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(J7-Pad6)"))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 TXDA))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(J7-Pad5)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 RXDA))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(J7-Pad4)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 RTSA))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(J7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP8 (layer F.Cu) (tedit 5A14249F)
    (at 244.348 108.966 270)
    (descr "8-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN2 (at -2.794 0.254 180) (layer F.SilkS))
    (fp_text value R_Pack04_SIP (at 10.16 2.4 90) (layer F.Fab))
    (fp_text user %R (at 8.89 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(J8-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 RTSB))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(J8-Pad4)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 RXDB))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(J8-Pad5)"))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 TXDB))
    (pad 7 thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(J8-Pad6)"))
    (pad 8 thru_hole oval (at 17.78 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 CTSB))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H4.3mm (layer F.Cu) (tedit 5A02FE31)
    (at 164.084 112.268)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.302 2.032) (layer F.SilkS))
    (fp_text value SW_SPST (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 RESET))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 RESET))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H4.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LCC:PLCC-44_THT-Socket (layer F.Cu) (tedit 5A02ECC8)
    (at 231.14 131.826)
    (descr "PLCC, 44 pins, through hole")
    (tags "plcc leaded")
    (fp_text reference U1 (at -1.27 -8.89) (layer F.SilkS))
    (fp_text value 26C92-PLCC44 (at -1.27 19.1) (layer F.Fab))
    (fp_text user %R (at -1.27 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -2.54 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 SPI0_IN))
    (pad 5 thru_hole circle (at -5.08 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 CTSB))
    (pad 43 thru_hole circle (at 2.54 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 SPI1_IN))
    (pad 41 thru_hole circle (at 5.08 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 SPI_RX))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 A0))
    (pad 4 thru_hole circle (at -5.08 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 A1))
    (pad 6 thru_hole circle (at -7.62 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 A2))
    (pad 44 thru_hole circle (at 0 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 VCC))
    (pad 42 thru_hole circle (at 2.54 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 SPI2_IN))
    (pad 8 thru_hole circle (at -7.62 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 CTSA))
    (pad 10 thru_hole circle (at -7.62 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 RD))
    (pad 12 thru_hole circle (at -7.62 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at -7.62 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 RTSB))
    (pad 16 thru_hole circle (at -7.62 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 SPI1_OUT))
    (pad 7 thru_hole circle (at -10.16 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 A3))
    (pad 9 thru_hole circle (at -10.16 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 WR))
    (pad 11 thru_hole circle (at -10.16 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 RXDB))
    (pad 13 thru_hole circle (at -10.16 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 TXDB))
    (pad 15 thru_hole circle (at -10.16 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 MUX1))
    (pad 17 thru_hole circle (at -10.16 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 SPIDATA))
    (pad 19 thru_hole circle (at -7.62 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 D3))
    (pad 21 thru_hole circle (at -5.08 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 D7))
    (pad 23 thru_hole circle (at -2.54 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 0 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 D6))
    (pad 27 thru_hole circle (at 2.54 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 D2))
    (pad 29 thru_hole circle (at 7.62 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 SPICLK))
    (pad 18 thru_hole circle (at -7.62 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 D1))
    (pad 20 thru_hole circle (at -5.08 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 D5))
    (pad 22 thru_hole circle (at -2.54 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole circle (at 0 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 INT))
    (pad 26 thru_hole circle (at 2.54 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 D4))
    (pad 28 thru_hole circle (at 5.08 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 D0))
    (pad 30 thru_hole circle (at 5.08 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 SPI0_OUT))
    (pad 32 thru_hole circle (at 5.08 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 RTSA))
    (pad 34 thru_hole circle (at 5.08 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask))
    (pad 36 thru_hole circle (at 5.08 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(JP1-Pad1)"))
    (pad 38 thru_hole circle (at 5.08 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 NRESET))
    (pad 40 thru_hole circle (at 5.08 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at 7.62 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 MUX0))
    (pad 33 thru_hole circle (at 7.62 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 TXDA))
    (pad 35 thru_hole circle (at 7.62 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 RXDA))
    (pad 37 thru_hole circle (at 7.62 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask))
    (pad 39 thru_hole circle (at 7.62 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad10)"))
    (model ${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-44_THT-Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 159.004 129.032)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.032) (layer F.SilkS))
    (fp_text value 74HCT138 (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 A4))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad13)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 A5))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad11)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 A6))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad9)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad7)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 IORQ))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 A7))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad3)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad15)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 180.34 128.778)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74HC153 (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 MUX1))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 SPI2_RX))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 SPI2_RX))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 SPI1_RX))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 SPI0_RX))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 MUX0))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 SPI_RX))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92 (layer F.Cu) (tedit 5A279852)
    (at 199.136 148.082)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U4 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value DS1233 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 15 RESET))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 195.326 110.49 270)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U5 (at 7.112 -2.794 180) (layer F.SilkS))
    (fp_text value 74HCT139 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 VCC))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 RESET))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 SPI2_CS))
    (pad 13 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 RESET))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 SPI1_CS))
    (pad 12 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 SPI0_CS))
    (pad 11 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 MUX1))
    (pad 10 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 MUX0))
    (pad 9 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 NRESET))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 202.692 128.524)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference X1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value CXO_DIP8 (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 227.838 118.872 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 TXDB))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(J1-Pad35)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 233.172 118.872 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J1-Pad36)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 RXDB))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "JP2/3: Connect Port B\nTo RC2014 RX/TX" (at 218.44 113.538) (layer F.SilkS))
  (gr_text "UART, Timer, SPI, Clock, Reset\nEtched Pixels (C) 2020 CC-NC" (at 210.566 121.412) (layer F.SilkS))
  (gr_text "I/O PORT" (at 171.704 125.73) (layer F.SilkS))
  (gr_text 7.3728MHz (at 206.248 132.588 270) (layer F.SilkS))
  (gr_text "26C92 (PLCC-44)" (at 230.124 124.968) (layer F.SilkS))
  (gr_text "80\n90\nA0\nB0\nC0\nD0\nE0\nF0" (at 176.022 138.176) (layer F.SilkS))
  (gr_text 4K7 (at 194.818 126.238) (layer F.SilkS))
  (gr_text 74HC139 (at 185.166 114.046) (layer F.SilkS))
  (gr_text 74HC153 (at 184.404 136.906 270) (layer F.SilkS))
  (gr_text 74HC138 (at 162.306 137.16 270) (layer F.SilkS))
  (gr_text "JP1: Clock" (at 206.248 142.494) (layer F.SilkS))
  (gr_text EPUART2 (at 196.85 138.938) (layer F.SilkS))
  (gr_text "SPI #0\nCS CLK MOSI MISO VCC GND IN OUT" (at 231.14 109.474) (layer F.SilkS))
  (gr_text "SPI #1\nCS CLK MOSI MISO VCC GND IN OUT" (at 208.534 109.474) (layer F.SilkS))
  (gr_text "SPI #2" (at 172.72 105.664) (layer F.SilkS))
  (gr_text RESET (at 167.132 119.634) (layer F.SilkS))
  (gr_text COM1 (at 249.428 131.064) (layer F.SilkS))
  (gr_text COM2 (at 249.174 109.22) (layer F.SilkS))
  (gr_text "Pin 1" (at 155.68168 146.60118 90) (layer F.SilkS))
  (gr_text "A15\nA14\nA13\nA12\nA11\nA10\nA9\nA8\nA7\nA6\nA5\nA4\nA3\nA2\nA1\nA0\nGnd\n5v\nM1\nReset\nClock\nINT\nMreq\nWr\nRo\nIORQ\nD0\nD1\nD2\nD3\nD4\nD5\nD6\nD7\nTx\nRx\nUSR1\nUSR2\nUSR3" (at 204.123143 151.13 90) (layer B.SilkS))
  (gr_line (start 253 108.685) (end 253 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 247.8184 103.505) (end 168.91 103.505) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 247.8184 108.685) (end 247.8184 103.505) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.8986 118.5164) (end 153.8986 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.91 103.505) (end 153.8986 118.5164) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.8986 153.3652) (end 253 153.3652) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.924 153.416) (xy 153.924 118.618) (xy 168.91 103.378) (xy 247.904 103.378) (xy 252.984 107.95)
        (xy 252.984 153.416)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.924 153.416) (xy 153.924 118.364) (xy 168.91 103.378) (xy 248.158 103.378) (xy 252.984 107.95)
        (xy 252.984 153.416)
      )
    )
  )
)
