(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6002)
    (drawings 34)
    (tracks 97)
    (zones 0)
    (modules 12)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu power)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (user_trace_width 1.27)
    (user_trace_width 1.778)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.8 0.5)
    (user_via 0.91 0.6)
    (user_via 1.05 0.7)
    (user_via 1.2 0.8)
    (user_via 1.35 0.9)
    (user_via 1.5 1)
    (user_via 1.8 1.2)
    (user_via 2.1 1.4)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.2)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /low)
  (net 4 /high)
  (net 5 /pressure)
  (net 6 /UDPI)
  (net 7 /LED_data)
  (net 8 /LED_CLK)
  (net 9 /AUX)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +5V)
    (add_net /AUX)
    (add_net /LED_CLK)
    (add_net /LED_data)
    (add_net /UDPI)
    (add_net /high)
    (add_net /low)
    (add_net /pressure)
    (add_net GND)
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 137.26 117.24)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 7.24 -2.24) (layer F.SilkS))
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 113.76 99.74)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at -6.26 -9.74) (layer F.SilkS))
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Symbol:OSHW-Logo2_9.8x8mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 135.5 108.4 270)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_9.8x8mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (module Potentiometer_SMD:Potentiometer_Bourns_3224J_Horizontal (layer F.Cu) (tedit 5A3D7171)
    (at 121.5 100 270)
    (descr "Potentiometer, horizontal, Bourns 3224J, https://www.bourns.com/docs/Product-Datasheets/3224.pdf")
    (tags "Potentiometer horizontal Bourns 3224J")
    (attr smd)
    (fp_text reference RV1 (at -9.6 0 180) (layer F.SilkS))
    (fp_text value 2-20k (at 0 3.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at 2 -1.15 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2 0 270) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 3 /low))
    (pad 3 smd rect (at 2 1.15 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3224J_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_SMD:Potentiometer_Bourns_3224J_Horizontal (layer F.Cu) (tedit 5A3D7171)
    (at 129.5 100 270)
    (descr "Potentiometer, horizontal, Bourns 3224J, https://www.bourns.com/docs/Product-Datasheets/3224.pdf")
    (tags "Potentiometer horizontal Bourns 3224J")
    (attr smd)
    (fp_text reference RV2 (at -9.4 0.4 180) (layer F.SilkS))
    (fp_text value 2-20k (at 0 3.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 2 1.15 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2 0 270) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 4 /high))
    (pad 1 smd rect (at 2 -1.15 270) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3224J_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm (layer F.Cu) (tedit 5DC5F6A8)
    (at 125.5 108.5 180)
    (descr "VQFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/20%20Lead%20VQFN%203x3x0_9mm_1_7EP%20U2B%20C04-21496a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (attr smd)
    (fp_text reference U2 (at -1.7 -2.9) (layer F.SilkS))
    (fp_text value ATtiny816 (at 0 2.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd custom (at -1.45 -0.8 180) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (net 9 /AUX)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.35 -0.05) (xy 0.299289 -0.05) (xy 0.35 0.000711) (xy 0.35 0.05) (xy -0.35 0.05)
) (width 0.1))
      ))
    (pad 2 smd roundrect (at -1.45 -0.4 180) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /LED_CLK))
    (pad 3 smd roundrect (at -1.45 0 180) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 4 smd roundrect (at -1.45 0.4 180) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 5 smd custom (at -1.45 0.8 180) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (net 5 /pressure)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.35 -0.05) (xy 0.35 -0.05) (xy 0.35 -0.000711) (xy 0.299289 0.05) (xy -0.35 0.05)
) (width 0.1))
      ))
    (pad 6 smd custom (at -0.8 1.45 180) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.299289) (xy 0.000711 -0.35) (xy 0.05 -0.35) (xy 0.05 0.35) (xy -0.05 0.35)
) (width 0.1))
      ))
    (pad 7 smd roundrect (at -0.4 1.45 180) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at 0 1.45 180) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at 0.4 1.45 180) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd custom (at 0.8 1.45 180) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.35) (xy -0.000711 -0.35) (xy 0.05 -0.299289) (xy 0.05 0.35) (xy -0.05 0.35)
) (width 0.1))
      ))
    (pad 11 smd custom (at 1.45 0.8 180) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.35 -0.05) (xy 0.35 -0.05) (xy 0.35 0.05) (xy -0.299289 0.05) (xy -0.35 -0.000711)
) (width 0.1))
      ))
    (pad 12 smd roundrect (at 1.45 0.4 180) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at 1.45 0 180) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /low))
    (pad 14 smd roundrect (at 1.45 -0.4 180) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /high))
    (pad 15 smd custom (at 1.45 -0.8 180) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.35 0.000711) (xy -0.299289 -0.05) (xy 0.35 -0.05) (xy 0.35 0.05) (xy -0.35 0.05)
) (width 0.1))
      ))
    (pad 16 smd custom (at 0.8 -1.45 180) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.35) (xy 0.05 -0.35) (xy 0.05 0.299289) (xy -0.000711 0.35) (xy -0.05 0.35)
) (width 0.1))
      ))
    (pad 17 smd roundrect (at 0.4 -1.45 180) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 18 smd roundrect (at 0 -1.45 180) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 19 smd roundrect (at -0.4 -1.45 180) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /UDPI))
    (pad 20 smd custom (at -0.8 -1.45 180) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (net 7 /LED_data)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.35) (xy 0.05 -0.35) (xy 0.05 0.35) (xy 0.000711 0.35) (xy -0.05 0.299289)
) (width 0.1))
      ))
    (pad 21 smd rect (at 0 0 180) (size 1.7 1.7) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad "" smd roundrect (at -0.425 -0.425 180) (size 0.69 0.69) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.425 0.425 180) (size 0.69 0.69) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 -0.425 180) (size 0.69 0.69) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 0.425 180) (size 0.69 0.69) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:NXP_Case_1351 (layer B.Cu) (tedit 5E8B7651)
    (at 125.5 108.5)
    (attr smd)
    (fp_text reference U1 (at -5.91 0 90) (layer B.SilkS))
    (fp_text value MPXVxxx (at 0 0 180) (layer B.Fab))
    (pad 8 smd rect (at -3.81 7.52475) (size 1.2 2.73) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -3.81 -7.52475) (size 1.2 2.73) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -1.27 7.52475) (size 1.2 2.73) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -1.27 -7.52475) (size 1.2 2.73) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 6 smd rect (at 1.27 7.52475) (size 1.2 2.73) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at 1.27 -7.52475) (size 1.2 2.73) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 3.81 7.52475) (size 1.2 2.73) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at 3.81 -7.52475) (size 1.2 2.73) (layers B.Cu B.Paste B.Mask)
      (net 5 /pressure))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130 110)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.6 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130 108)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.5 0) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.5 100 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.5 0.1 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130 106)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.5 0) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /pressure))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 59FED5CC)
    (at 125.5 117 270)
    (descr "surface-mounted straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x04 2.54mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 -6 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 6.14 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -3.81 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2.525 -3.81 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /LED_CLK))
    (pad 3 smd rect (at -2.525 -1.27 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.525 -1.27 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -2.525 1.27 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 9 /AUX))
    (pad 6 smd rect (at 2.525 1.27 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /LED_data))
    (pad 7 smd rect (at -2.525 3.81 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /UDPI))
    (pad 8 smd rect (at 2.525 3.81 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 8 (width 0.15) (layer Dwgs.User)
    (gr_text "8.000 mm" (at 125.5 86.7) (layer Dwgs.User))
    (feature1 (pts (xy 129.5 100) (xy 129.5 87.413579)))
    (feature2 (pts (xy 121.5 100) (xy 121.5 87.413579)))
    (crossbar (pts (xy 121.5 88) (xy 129.5 88)))
    (arrow1a (pts (xy 129.5 88) (xy 128.373496 88.586421)))
    (arrow1b (pts (xy 129.5 88) (xy 128.373496 87.413579)))
    (arrow2a (pts (xy 121.5 88) (xy 122.626504 88.586421)))
    (arrow2b (pts (xy 121.5 88) (xy 122.626504 87.413579)))
  )
  (dimension 10.5 (width 0.15) (layer Dwgs.User)
    (gr_text "10.500 mm" (at 116.25 90.7) (layer Dwgs.User))
    (feature1 (pts (xy 111 100) (xy 111 91.413579)))
    (feature2 (pts (xy 121.5 100) (xy 121.5 91.413579)))
    (crossbar (pts (xy 121.5 92) (xy 111 92)))
    (arrow1a (pts (xy 111 92) (xy 112.126504 91.413579)))
    (arrow1b (pts (xy 111 92) (xy 112.126504 92.586421)))
    (arrow2a (pts (xy 121.5 92) (xy 120.373496 91.413579)))
    (arrow2b (pts (xy 121.5 92) (xy 120.373496 92.586421)))
  )
  (dimension 6 (width 0.15) (layer Dwgs.User)
    (gr_text "6.000 mm" (at 147.3 97 90) (layer Dwgs.User))
    (feature1 (pts (xy 141 94) (xy 146.586421 94)))
    (feature2 (pts (xy 141 100) (xy 146.586421 100)))
    (crossbar (pts (xy 146 100) (xy 146 94)))
    (arrow1a (pts (xy 146 94) (xy 146.586421 95.126504)))
    (arrow1b (pts (xy 146 94) (xy 145.413579 95.126504)))
    (arrow2a (pts (xy 146 100) (xy 146.586421 98.873496)))
    (arrow2b (pts (xy 146 100) (xy 145.413579 98.873496)))
  )
  (dimension 10.5 (width 0.15) (layer Dwgs.User)
    (gr_text "10.500 mm" (at 134.75 90.7) (layer Dwgs.User))
    (feature1 (pts (xy 140 100) (xy 140 91.413579)))
    (feature2 (pts (xy 129.5 100) (xy 129.5 91.413579)))
    (crossbar (pts (xy 129.5 92) (xy 140 92)))
    (arrow1a (pts (xy 140 92) (xy 138.873496 92.586421)))
    (arrow1b (pts (xy 140 92) (xy 138.873496 91.413579)))
    (arrow2a (pts (xy 129.5 92) (xy 130.626504 92.586421)))
    (arrow2b (pts (xy 129.5 92) (xy 130.626504 91.413579)))
  )
  (gr_text 8 (at 120 120.5 90) (layer F.SilkS))
  (gr_text 1 (at 131.5 113.6 90) (layer F.SilkS))
  (gr_text "J1 - PINOUT\n1. +5V, 2. LED_CLK, \n3. GND, 4. GND, \n5. AUX, 6. LED_D, \n7. UPDI, 8. +5V " (at 116.6 103 270) (layer F.SilkS))
  (gr_text Hackaday.io/lnLog (at 126.6 119.8) (layer B.SilkS))
  (gr_text 2 (at 131.5 120 90) (layer F.SilkS))
  (gr_text "Enclosure\n1551MFLBK" (at 115.5 95.5) (layer F.SilkS))
  (gr_line (start 140.01 100.24) (end 136.76 100.24) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 111.01 94.99) (end 111.01 116.74) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 133.76 97.24) (end 133.76 93.99) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 111.01 116.74) (end 114.26 116.74) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 112.01 94.99) (end 112.01 93.99) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 117.26 119.74) (end 117.26 122.99) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 133.76 93.99) (end 112.01 93.99) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 139.01 121.99) (end 139.01 122.99) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 114.26 119.74) (end 117.26 119.740001) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 140.01 121.99) (end 140.01 100.24) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 117.26 122.99) (end 139.01 122.99) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 136.76 97.24) (end 133.76 97.24) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_text "ATTINY-816 Water \nLevel Indicator" (at 124.9 96.8) (layer B.SilkS))
  (gr_text HIGH (at 130.4 96) (layer F.SilkS))
  (gr_text LOW (at 122.9 95.9) (layer F.SilkS))
  (gr_text "MPXV4006GP\n0-6kPa\n0-600mm H2O" (at 136.6 101.5 270) (layer F.SilkS))
  (dimension 29 (width 0.15) (layer Dwgs.User)
    (gr_text "29.000 mm" (at 125.5 128.650001) (layer Dwgs.User))
    (feature1 (pts (xy 140 122) (xy 140 127.936422)))
    (feature2 (pts (xy 111 122) (xy 111 127.936422)))
    (crossbar (pts (xy 111 127.350001) (xy 140 127.350001)))
    (arrow1a (pts (xy 140 127.350001) (xy 138.873496 127.936422)))
    (arrow1b (pts (xy 140 127.350001) (xy 138.873496 126.76358)))
    (arrow2a (pts (xy 111 127.350001) (xy 112.126504 127.936422)))
    (arrow2b (pts (xy 111 127.350001) (xy 112.126504 126.76358)))
  )
  (dimension 29 (width 0.15) (layer Dwgs.User)
    (gr_text "29.000 mm" (at 145.8 108.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 135 123) (xy 145.086421 123)))
    (feature2 (pts (xy 135 94) (xy 145.086421 94)))
    (crossbar (pts (xy 144.5 94) (xy 144.5 123)))
    (arrow1a (pts (xy 144.5 123) (xy 143.913579 121.873496)))
    (arrow1b (pts (xy 144.5 123) (xy 145.086421 121.873496)))
    (arrow2a (pts (xy 144.5 94) (xy 143.913579 95.126504)))
    (arrow2b (pts (xy 144.5 94) (xy 145.086421 95.126504)))
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.933406 125.438755) (xy 110.033406 124.838755) (xy 110.083406 91.038755) (xy 146.983406 91.638755)
      )
    )
  )
)
