(kicad_pcb (version 20171130) (host pcbnew 5.1.5-1.fc31)
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 877)
    (zones 0)
    (modules 18)
    (nets 53)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/tmp/188"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 RESET)
  (net 4 A15)
  (net 5 A14)
  (net 6 A13)
  (net 7 A12)
  (net 8 A11)
  (net 9 A10)
  (net 10 A9)
  (net 11 A8)
  (net 12 A7)
  (net 13 A6)
  (net 14 A5)
  (net 15 A4)
  (net 16 A3)
  (net 17 A19)
  (net 18 A2)
  (net 19 A18)
  (net 20 A1)
  (net 21 A17)
  (net 22 A0)
  (net 23 A16)
  (net 24 CLK)
  (net 25 INT)
  (net 26 MREQ)
  (net 27 WR)
  (net 28 RD)
  (net 29 IORQ)
  (net 30 NMI)
  (net 31 AD0)
  (net 32 AD1)
  (net 33 AD2)
  (net 34 AD3)
  (net 35 AD4)
  (net 36 AD5)
  (net 37 AD6)
  (net 38 AD7)
  (net 39 "Net-(R2-Pad2)")
  (net 40 AS16)
  (net 41 AS17)
  (net 42 AS18)
  (net 43 AS19)
  (net 44 ALE)
  (net 45 CLK1.8)
  (net 46 "Net-(U1-Pad45)")
  (net 47 "Net-(U1-Pad46)")
  (net 48 "Net-(U1-Pad47)")
  (net 49 S2)
  (net 50 CLKIN)
  (net 51 "Net-(U3-Pad9)")
  (net 52 M1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A10)
    (add_net A11)
    (add_net A12)
    (add_net A13)
    (add_net A14)
    (add_net A15)
    (add_net A16)
    (add_net A17)
    (add_net A18)
    (add_net A19)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net A8)
    (add_net A9)
    (add_net AD0)
    (add_net AD1)
    (add_net AD2)
    (add_net AD3)
    (add_net AD4)
    (add_net AD5)
    (add_net AD6)
    (add_net AD7)
    (add_net ALE)
    (add_net AS16)
    (add_net AS17)
    (add_net AS18)
    (add_net AS19)
    (add_net CLK)
    (add_net CLK1.8)
    (add_net CLKIN)
    (add_net GND)
    (add_net INT)
    (add_net IORQ)
    (add_net M1)
    (add_net MREQ)
    (add_net NMI)
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U1-Pad47)")
    (add_net "Net-(U3-Pad9)")
    (add_net RD)
    (add_net RESET)
    (add_net S2)
    (add_net VCC)
    (add_net WR)
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x40_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A422)
    (at 187.2615 137.2235 270)
    (descr "Through hole straight socket strip, 2x40, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x40 2.54mm double row")
    (fp_text reference J1 (at -1.27 2.77 270) (layer B.SilkS))
    (fp_text value Conn_02x40_Odd_Even (at -1.27 -101.83 270) (layer B.Fab))
    (fp_text user %R (at -1.27 -49.53) (layer B.Fab))
    (pad 80 thru_hole oval (at -2.54 -99.06 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 79 thru_hole oval (at 0 -99.06 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 78 thru_hole oval (at -2.54 -96.52 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 77 thru_hole oval (at 0 -96.52 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 76 thru_hole oval (at -2.54 -93.98 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 75 thru_hole oval (at 0 -93.98 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 74 thru_hole oval (at -2.54 -91.44 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 73 thru_hole oval (at 0 -91.44 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 72 thru_hole oval (at -2.54 -88.9 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 71 thru_hole oval (at 0 -88.9 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 70 thru_hole oval (at -2.54 -86.36 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 69 thru_hole oval (at 0 -86.36 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 68 thru_hole oval (at -2.54 -83.82 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 67 thru_hole oval (at 0 -83.82 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 AD7))
    (pad 66 thru_hole oval (at -2.54 -81.28 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 65 thru_hole oval (at 0 -81.28 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 AD6))
    (pad 64 thru_hole oval (at -2.54 -78.74 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 63 thru_hole oval (at 0 -78.74 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 AD5))
    (pad 62 thru_hole oval (at -2.54 -76.2 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 61 thru_hole oval (at 0 -76.2 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 AD4))
    (pad 60 thru_hole oval (at -2.54 -73.66 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 59 thru_hole oval (at 0 -73.66 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 AD3))
    (pad 58 thru_hole oval (at -2.54 -71.12 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 57 thru_hole oval (at 0 -71.12 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 AD2))
    (pad 56 thru_hole oval (at -2.54 -68.58 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 55 thru_hole oval (at 0 -68.58 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 AD1))
    (pad 54 thru_hole oval (at -2.54 -66.04 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 53 thru_hole oval (at 0 -66.04 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 AD0))
    (pad 52 thru_hole oval (at -2.54 -63.5 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 NMI))
    (pad 51 thru_hole oval (at 0 -63.5 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 IORQ))
    (pad 50 thru_hole oval (at -2.54 -60.96 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 49 thru_hole oval (at 0 -60.96 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 RD))
    (pad 48 thru_hole oval (at -2.54 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 47 thru_hole oval (at 0 -58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 WR))
    (pad 46 thru_hole oval (at -2.54 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 45 thru_hole oval (at 0 -55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 MREQ))
    (pad 44 thru_hole oval (at -2.54 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 43 thru_hole oval (at 0 -53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 INT))
    (pad 42 thru_hole oval (at -2.54 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 41 thru_hole oval (at 0 -50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 CLK))
    (pad 40 thru_hole oval (at -2.54 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 RESET))
    (pad 38 thru_hole oval (at -2.54 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 M1))
    (pad 36 thru_hole oval (at -2.54 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 35 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 34 thru_hole oval (at -2.54 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 33 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 32 thru_hole oval (at -2.54 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 A16))
    (pad 31 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 A0))
    (pad 30 thru_hole oval (at -2.54 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 A17))
    (pad 29 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 A1))
    (pad 28 thru_hole oval (at -2.54 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 A18))
    (pad 27 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 A2))
    (pad 26 thru_hole oval (at -2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 A19))
    (pad 25 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 A3))
    (pad 24 thru_hole oval (at -2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 A4))
    (pad 22 thru_hole oval (at -2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 A5))
    (pad 20 thru_hole oval (at -2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 A6))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 A7))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 A8))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 A9))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 A10))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 A11))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 A12))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 A13))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 A14))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 A15))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x40_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module alan:80188_plcc (layer F.Cu) (tedit 0)
    (at 202.438 111.252)
    (descr "Module specifique pour 80188, pads ronds")
    (fp_text reference U1 (at 0 -2.54) (layer F.SilkS))
    (fp_text value 80C188 (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at -10.16 12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 A15))
    (pad 2 thru_hole circle (at -10.16 10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 38 AD7))
    (pad 3 thru_hole circle (at -7.62 12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 A14))
    (pad 4 thru_hole circle (at -7.62 10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 37 AD6))
    (pad 5 thru_hole circle (at -5.08 12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 6 A13))
    (pad 6 thru_hole circle (at -5.08 10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 36 AD5))
    (pad 7 thru_hole circle (at -2.54 12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 A12))
    (pad 8 thru_hole circle (at -2.54 10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 35 AD4))
    (pad 9 thru_hole circle (at 0 12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 10 thru_hole circle (at 0 10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 A11))
    (pad 11 thru_hole circle (at 2.54 12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 AD3))
    (pad 12 thru_hole circle (at 2.54 10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 A10))
    (pad 13 thru_hole circle (at 5.08 12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 AD2))
    (pad 14 thru_hole circle (at 5.08 10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 A9))
    (pad 15 thru_hole circle (at 7.62 12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 AD1))
    (pad 16 thru_hole circle (at 7.62 10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 A8))
    (pad 17 thru_hole circle (at 10.16 12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 AD0))
    (pad 18 thru_hole circle (at 12.7 10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 10.16 10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 12.7 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 21 thru_hole circle (at 10.16 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 45 CLK1.8))
    (pad 22 thru_hole circle (at 12.7 5.08) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 10.16 5.08) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at 12.7 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 RESET))
    (pad 25 thru_hole circle (at 10.16 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at 12.7 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 27 thru_hole circle (at 10.16 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at 12.7 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 29 thru_hole circle (at 10.16 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 30 thru_hole circle (at 12.7 -5.08) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at 10.16 -5.08) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at 12.7 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at 10.16 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at 12.7 -10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at 10.16 -12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 36 thru_hole circle (at 10.16 -10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 37 thru_hole circle (at 7.62 -12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 38 thru_hole circle (at 7.62 -10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 39 thru_hole circle (at 5.08 -12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 40 thru_hole circle (at 5.08 -10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 41 thru_hole circle (at 2.54 -12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 42 thru_hole circle (at 2.54 -10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 43 thru_hole circle (at 0 -12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 44 thru_hole circle (at 0 -10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 45 thru_hole circle (at -2.54 -12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 46 "Net-(U1-Pad45)"))
    (pad 46 thru_hole circle (at -2.54 -10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 47 "Net-(U1-Pad46)"))
    (pad 47 thru_hole circle (at -5.08 -12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 48 "Net-(U1-Pad47)"))
    (pad 48 thru_hole circle (at -5.08 -10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 49 thru_hole circle (at -7.62 -12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 39 "Net-(R2-Pad2)"))
    (pad 50 thru_hole circle (at -7.62 -10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 51 thru_hole circle (at -10.16 -12.7) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 52 thru_hole circle (at -12.7 -10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 53 thru_hole circle (at -10.16 -10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 54 thru_hole circle (at -12.7 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 49 S2))
    (pad 55 thru_hole circle (at -10.16 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 56 thru_hole circle (at -12.7 -5.08) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 CLK))
    (pad 57 thru_hole circle (at -10.16 -5.08) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 48 "Net-(U1-Pad47)"))
    (pad 58 thru_hole circle (at -12.7 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 59 thru_hole circle (at -10.16 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 50 CLKIN))
    (pad 60 thru_hole circle (at -12.7 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 61 thru_hole circle (at -10.16 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 44 ALE))
    (pad 62 thru_hole circle (at -12.7 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 RD))
    (pad 63 thru_hole circle (at -10.16 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 WR))
    (pad 64 thru_hole circle (at -12.7 5.08) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask))
    (pad 65 thru_hole circle (at -10.16 5.08) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 43 AS19))
    (pad 66 thru_hole circle (at -12.7 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 42 AS18))
    (pad 67 thru_hole circle (at -10.16 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 41 AS17))
    (pad 68 thru_hole circle (at -12.7 10.16) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 40 AS16))
  )
  (module Package_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 242.6335 109.6645 180)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.80238 -2.14122) (layer F.SilkS))
    (fp_text value 74HCT573 (at 3.81 25.19) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 ALE))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 AD0))
    (pad 12 thru_hole oval (at 7.62 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 A7))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 AD1))
    (pad 13 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 A6))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 AD2))
    (pad 14 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 A5))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 AD3))
    (pad 15 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 A4))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 AD4))
    (pad 16 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 A3))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 AD5))
    (pad 17 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 A2))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 AD6))
    (pad 18 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 A1))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 AD7))
    (pad 19 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 A0))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 264.8585 128.0795 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C1 (at 4.45262 0.87122 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 204.47 129.032)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C2 (at 1.17348 2.16408) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 237.744 113.7285)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C3 (at 3.29692 1.98374) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 228.6 88.9 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (fp_text reference C4 (at 1.3208 3.16484 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 270.891 113.284 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C5 (at -2.42316 0.49276 180) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 3.75 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 RESET))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 273.2405 98.3615 270)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 3.9243 -0.05842 180) (layer F.SilkS))
    (fp_text value BAT43 (at 3.81 2.12 90) (layer F.Fab))
    (fp_text user %R (at 4.11 0 90) (layer F.Fab))
    (fp_text user K (at 0 -1.8 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 RESET))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 277.622 98.2345 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.89382 -0.05588 180) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 RESET))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 282.194 105.918 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.78968 -0.06096 180) (layer F.SilkS))
    (fp_text value 3K3 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 277.622 109.728 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3.76936 -0.01524 180) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 INT))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 282.2575 109.7915 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 3.66522 -0.14478 180) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 NMI))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 273.177 93.091)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.87604 0.01016) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 M1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 224.79 83.439 270)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at -0.06096 -2.67716 180) (layer F.SilkS))
    (fp_text value 74HCT373 (at 3.81 25.19 90) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 ALE))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 7.62 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 A18))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 AS18))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 AS17))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 A17))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 A16))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 AS16))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 AS19))
    (pad 18 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 S2))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(U3-Pad9)"))
    (pad 19 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 IORQ))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 284.607 122.301 270)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U4 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value 74HCT00 (at 3.81 17.57 90) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(U3-Pad9)"))
    (pad 8 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U1-Pad46)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(U3-Pad9)"))
    (pad 9 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 NMI))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 A19))
    (pad 10 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 NMI))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 INT))
    (pad 11 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 MREQ))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 INT))
    (pad 12 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 IORQ))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(U1-Pad45)"))
    (pad 13 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 IORQ))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Oscillator:Oscillator_DIP-8 (layer F.Cu) (tedit 58CD3344)
    (at 255.524 109.9185 270)
    (descr "Oscillator, DIP8,http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf")
    (tags oscillator)
    (fp_text reference X1 (at 11.37158 -4.65328 180) (layer F.SilkS))
    (fp_text value 14.72MHz (at 3.81 3.74 90) (layer F.Fab))
    (fp_text user %R (at 3.81 -3.81 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 7.62 -7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 CLKIN))
    (pad 8 thru_hole circle (at 0 -7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_DIP-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Oscillator:Oscillator_DIP-8 (layer F.Cu) (tedit 58CD3344)
    (at 258.699 102.489)
    (descr "Oscillator, DIP8,http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf")
    (tags oscillator)
    (fp_text reference X2 (at 3.81 -11.26) (layer F.SilkS))
    (fp_text value 1.8MHz (at 3.81 3.74) (layer F.Fab))
    (fp_text user %R (at 3.81 -3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 CLK1.8))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_DIP-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text EP188 (at 199.136 94.996) (layer F.SilkS))
  (gr_text "v 0.2" (at 284.48 91.186) (layer F.SilkS))
  (gr_text "80C188 CPU Card For RC2014\n(C) 2019 Etched Pixels CC-NC" (at 264.9728 86.97976) (layer F.SilkS))
  (gr_line (start 199.136 81.28) (end 185.4835 94.869) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 288.0995 81.28) (end 199.136 81.28) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 288.0995 139.0015) (end 288.0995 81.28) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.4835 139.0015) (end 288.0995 139.0015) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.4835 139.0015) (end 185.4835 94.869) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.4835 94.8055) (xy 199.0725 81.28) (xy 288.0995 81.28) (xy 288.0995 139.0015) (xy 185.4835 139.0015)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.547 94.869) (xy 199.136 81.28) (xy 288.036 81.28) (xy 288.163 139.0015) (xy 185.547 139.0015)
      )
    )
  )
)
