Circuit: * C:\Users\Standa\Desktop\Projects\LCR\HW\Dev\Sim\StableOutputDriver\sim.asc

WARNING: Node NC_01 is floating.

WARNING: Less than two connections to node NC_01.  This node is used by C1.
WARNING: Less than two connections to node NC_02.  This node is used by V3.
WARNING: Less than two connections to node NC_03.  This node is used by V4.
Direct Newton iteration for .op point succeeded.
.step fm=10 temp=0°C
.step fm=10000 temp=0°C
.step fm=10 temp=25°C
.step fm=10000 temp=25°C
.step fm=10 temp=50°C
.step fm=10000 temp=50°C

Date: Sat Oct 19 09:54:16 2019
Total elapsed time: 11.282 seconds.

tnom = 27
temp = 50
method = modified trap
totiter = 2126
traniter = 2110
tranpoints = 1056
accept = 1052
rejected = 4
matrix size = 27
fillins = 9
solver = Normal
Matrix Compiler1: 1.68 KB object code size  1.0/0.4/[0.3]
Matrix Compiler2: 2.20 KB object code size  0.5/0.6/[0.4]

