<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.1">
<drawing>
<library>
<description>Generated from &lt;b&gt;GemaLight V3.0.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="CUS-12B_CUS-12B">
</package>
<package name="MAX1551EZK_T_SOT95P275X110-5N">
</package>
<package name="NEOPIXEL-ATTINY-85_ATTINY85_DIP254P762X533-8">
</package>
<package name="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTORHOLES">
</package>
<package name="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTORSMD">
</package>
<package name="SMALL-LED-LTST-S270KRKT_0603">
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTCOM_20MM_PTH">
<description>&lt;h3&gt;20mm (CR2032) Coin Cell Battery Holder - PTH&lt;/h3&gt;
&lt;p&gt;Basic 20mm coin cell holder. Posts can be inserted into 0.1" perf board! Holds the common CR2032 type batteries.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/CoinCellHolder-20mm.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTCOM_20MM_PTH_KIT">
<description>&lt;h3&gt;20mm (CR2032) Coin Cell Battery Holder - PTH&lt;/h3&gt;
&lt;p&gt;Basic 20mm coin cell holder. Posts can be inserted into 0.1" perf board! Holds the common CR2032 type batteries.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/CoinCellHolder-20mm.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTCON-6.8MM">
<description>Part#: MS621FE-FL11E</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTCON_9V">
<description>&lt;h3&gt;PCMOUNT 9V Battery Holder&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.memoryprotectiondevices.com/datasheets/BC9VPC-datasheet.pdf"&gt;Datasheet&lt;/a&gt; (MPD BC9VPC)&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTCON_12MM">
<description>&lt;h3&gt;12mm Coin Cell (CR1225) Battery Holder - SMD&lt;/h3&gt;
&lt;p&gt;Holds battery in place with friction. The metal housing connects to the positive side of the battery and the PCB pad underneath is connected to the negative side.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Prototyping/KEY-3000.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTCON_12MM_PTH">
<description>&lt;h3&gt;12mm Coin Cell Battery (CR1225) Holder - PTH&lt;/h3&gt;
&lt;p&gt;This is a through hole 12mm coin cell battery holder. Holds battery in place with friction. Metal housing is +, PCB pad underneath is -.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Prototyping/KEY-3001.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTCON_20MM">
<description>&lt;h3&gt;20mm Coin Cell Battery (CR2032) Holder - SMD (Single Pad)&lt;/h3&gt;
&lt;p&gt;Part number: CR2032-THM&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTCON_20MM_4LEGS">
<description>&lt;h3&gt;20mm Coin Cell Battery (CR2032) Holder - SMD (Dual Pad)&lt;/h3&gt;
&lt;p&gt;This holder fits 20mm Lithium coin cell batteries and holds the battery in place with friction. The metal housing connects to the positive (+) side of the battery and the PCB pad underneath is connected to the negative (-) side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/BAT-BLH-001.jpg"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTCON_20MM_4LEGS_OVERPASTE">
<description>&lt;h3&gt;20mm Coin Cell Battery (CR2032) Holder - SMD (Dual Pad) (Overpaste on pads)&lt;/h3&gt;
&lt;p&gt;This holder fits 20mm Lithium coin cell batteries and holds the battery in place with friction. The metal housing connects to the positive (+) side of the battery and the PCB pad underneath is connected to the negative (-) side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/BAT-BLH-001.jpg"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTCON_20MM_4LEGS_OVERPASTE_INNER">
<description>&lt;h3&gt;20mm Coin Cell Battery (CR2032) Holder - SMD (Dual Pad) (Overpaste on inner side of pads)&lt;/h3&gt;
&lt;p&gt;This holder fits 20mm Lithium coin cell batteries and holds the battery in place with friction. The metal housing connects to the positive (+) side of the battery and the PCB pad underneath is connected to the negative (-) side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/BAT-BLH-001.jpg"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTCON_24.5MM_PTH">
<description>&lt;h3&gt;24.5mm Coin Cell Battery (CR2450) Holder - PTH&lt;/h3&gt;
&lt;p&gt;Through hole 24.5 mm coin cell holder. Holds battery in place with friction. Metal housing is +, PCB pad underneath is -.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Batteries/Coin_Cell_Holder_245mm-3009.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTERY-AA">
<description>&lt;h3&gt;AA Battery Clips&lt;/h3&gt;
&lt;p&gt;PCB mount clips properly spaced to hold a AA battery&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/M60-2p9.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTERY-AA-HOLDER-KIT">
<description>&lt;h3&gt;AA Battery Holder&lt;/h3&gt;
&lt;p&gt;PTH Single-cell AA battery holder&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.digikey.com/product-detail/en/keystone-electronics/2460/36-2460-ND/280629"&gt;Product Link&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTERY-AA-KIT">
<description>&lt;h3&gt;AA Battery Clips (KIT Variant)&lt;/h3&gt;
&lt;p&gt;PCB mount clips properly spaced to hold a AA battery&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/M60-2p9.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTERY-AAA">
<description>&lt;h3&gt;AAA Battery Clips&lt;/h3&gt;
&lt;p&gt;PCB mount clips properly spaced to hold a AAA battery.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/M60-2p9.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTERY-AAA-KIT">
<description>&lt;h3&gt;AAA Battery Clips (KIT Variant)&lt;/h3&gt;
&lt;p&gt;PCB mount clips properly spaced to hold a AAA battery.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/M60-2p9.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-BATTERIES-20MM_BATTERY_18650-HOLDER">
<description>&lt;h3&gt;18650 Lithium Ion Cell Battery Holders&lt;/h3&gt;
&lt;p&gt;PCB mount clips properly spaced to hold a 18650 Lithium Ion Cell battery.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Prototyping/54.PDF"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SPARKFUN-CAPACITORS_0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-CAPACITORS_0603:1">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-CAPACITORS_CAP-PTH-SMALL-KIT">
<description>&lt;h3&gt;CAP-PTH-SMALL-KIT&lt;/h3&gt;
Commonly used for small ceramic capacitors. Like our 0.1uF (http://www.sparkfun.com/products/8375) or 22pF caps (http://www.sparkfun.com/products/8571).&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="SPARKFUN-CONNECTORS_1X01_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-CONNECTORS_PAD.02X.02">
<description>&lt;h3&gt;Electrically Conductive Pad 0.02" Square&lt;/h3&gt;
Used as a test point connection for pogo pins or other debugging tools. 
&lt;p&gt;Specifications:
&lt;li&gt;Area: 0.02" x 0.02"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;TEST_POINT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-CONNECTORS_PAD.03X.03">
<description>&lt;h3&gt;Electrically Conductive Pad 0.03" Circle&lt;/h3&gt;
Used as a test point connection for pogo pins or other debugging tools. 
&lt;p&gt;Specifications:
&lt;li&gt;Area: 0.03" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;TEST_POINT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-CONNECTORS_PAD.03X.04">
<description>&lt;h3&gt;Electrically Conductive Pad 0.04" Circle&lt;/h3&gt;
Used as a test point connection for pogo pins or other debugging tools. 
&lt;p&gt;Specifications:
&lt;li&gt;Area: 0.04" x 0.04"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;TEST_POINT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-CONNECTORS_PAD.03X.05">
<description>&lt;h3&gt;Electrically Conductive Pad 0.05" Circle&lt;/h3&gt;
Used as a test point connection for pogo pins or other debugging tools. 
&lt;p&gt;Specifications:
&lt;li&gt;Area: 0.05" x 0.05"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;TEST_POINT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-CONNECTORS_TP_15TH">
<description>&lt;h3&gt;Electrically Conductive Via 0.015" Drill&lt;/h3&gt;
Used as a test point connection for pogo pins or other debugging tools. 
&lt;p&gt;Specifications:
&lt;li&gt;Area:0.015"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;TEST_POINT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-RESISTORS_0603:2">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-RESISTORS_AXIAL-0.1">
<description>&lt;h3&gt;AXIAL-0.1&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.1" pitch between holes.&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-RESISTORS_AXIAL-0.1-KIT">
<description>&lt;h3&gt;AXIAL-0.1-KIT&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.1" pitch between holes.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of the AXIAL-0.1 package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-RESISTORS_AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-RESISTORS_AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
<package name="SPARKFUN-SWITCHES_TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-SWITCHES_TACTILE_SWITCH_PTH_6.0MM_KIT">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-SWITCHES_TACTILE_SWITCH_PTH_12MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 12mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-5050)&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-SWITCHES_TACTILE_SWITCH_PTH_RIGHT_ANGLE">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, Right-angle&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/SW016.JPG"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-SWITCHES_TACTILE_SWITCH_PTH_RIGHT_ANGLE_KIT">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, Right-angle&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/SW016.JPG"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_4.5MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 4.5mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://spec_sheets.e-switch.com/specs/P010338.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_4.6X2.8MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 4.6 x 2.8mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ck-components.com/media/1479/kmr2.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_5.2MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 5.2mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/Buttons/SMD-Button.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_6.0X3.5MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 6.0 x 3.5 mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/1101.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_6.2MM_TALL">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 6.2mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.apem.com/files/apem/brochures/ADTS6-ADTSM-KTSC6.pdf"&gt;Datasheet&lt;/a&gt; (ADTSM63NVTR)&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_12MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 12mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Components/Switches/N301102.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_RIGHT_ANGLE">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, Right-angle&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;</description>
</package>
<package name="SUBMINIATRE-SLIDE-SWITCH-JS102011SAQN_TOGGLESWITCHJS122011JAQN">
<description>TOGGLESwitchJS102011SAQN</description>
</package>
<package name="ZX62D-B-5PA8_ZX62D-B-5PA8">
<description>&lt;b&gt;Micro USB Type B Connector&lt;/b&gt; - Standard, Shell Through Hole&lt;br&gt;
&lt;br&gt;
Source: &lt;a href="http://www.hirose.co.jp/cataloge_hp/ed_ZX_20140804.pdf"&gt;http://www.hirose.co.jp/cataloge_hp/ed_ZX_20140804.pdf&lt;/a&gt;</description>
</package>
</packages>
<symbols>
<symbol name="CUS-12B_SW_SPDT_POL">
<description>&lt;h3&gt;SPST Switch w/ Polarity Mark&lt;/h3&gt;
&lt;p&gt;Used by 3PDT switch. Drawn as three separate gates for schematic clarity.&lt;/p&gt;</description>
<pin name="O" direction="pas"/>
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="MAX1551EZK_T_MAX1551EZK+T">
<pin name="!POK"/>
<pin name="BAT" direction="pwr"/>
<pin name="DC"/>
<pin name="GND" direction="pwr"/>
<pin name="USB" direction="pwr"/>
</symbol>
<symbol name="NEOPIXEL-ATTINY-85_ATTINY85_ATTINY85-20PU">
<pin name="(PCINT3/XTAL1/CLKI/~OC1B/ADC3)_PB3"/>
<pin name="(PCINT4/XTAL2/CLKO/OC1B/ADC2)_PB4"/>
<pin name="(PCINT5/~RESET/ADC0/DW)_PB5"/>
<pin name="GND" direction="pas"/>
<pin name="PB0_(MOSI/DI/SDA/AIN0/OC0A/~OC1A/AREF/PCINT0)"/>
<pin name="PB1_(MISO/DO/AIN1/OC0B/OC1A/PCINT1)"/>
<pin name="PB2_(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTOR">
<pin name="DATA"/>
<pin name="GND0"/>
<pin name="GND1"/>
<pin name="VCC"/>
</symbol>
<symbol name="SMALL-LED-LTST-S270KRKT_LTST-S270KRKT">
<pin name="A2" direction="pas"/>
<pin name="K2" direction="pas"/>
</symbol>
<symbol name="SPARKFUN-BATTERIES-20MM_BATTERY">
<description>&lt;h3&gt;Battery (Single-Cell)&lt;/h3&gt;</description>
<pin name="+" direction="pwr"/>
<pin name="-" direction="pwr"/>
</symbol>
<symbol name="SPARKFUN-CAPACITORS_CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SPARKFUN-CONNECTORS_TEST-POINT">
<pin name="1"/>
</symbol>
<symbol name="SPARKFUN-RESISTORS_RESISTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SPARKFUN-SWITCHES_SWITCH-MOMENTARY-2">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="ZX62D-B-5PA8_MICRO-USB">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="ZX62D-B-5PA8_MICRO-USB-SHIELD">
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="S4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CUS-12B_CUS-12B" prefix="SW">
<gates>
<gate name="$" symbol="CUS-12B_SW_SPDT_POL"/>
</gates>
<devices>
<device name="" package="CUS-12B_CUS-12B">
<connects>
<connect gate="$" pin="O" pad="P$1"/>
<connect gate="$" pin="P" pad="P$2"/>
<connect gate="$" pin="S" pad="P$3"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Switch, Slide, Smd "/>
<attribute name="MF" value="Copal"/>
<attribute name="MP" value="CUS-12B"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1551EZK_T_MAX1551EZK+T" prefix="U">
<gates>
<gate name="A" symbol="MAX1551EZK_T_MAX1551EZK+T"/>
</gates>
<devices>
<device name="" package="MAX1551EZK_T_SOT95P275X110-5N">
<connects>
<connect gate="A" pin="!POK" pad="3"/>
<connect gate="A" pin="BAT" pad="5"/>
<connect gate="A" pin="DC" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="USB" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Charger IC Lithium-Ion TSOT-23-5 "/>
<attribute name="MF" value="Maxim Integrated"/>
<attribute name="MP" value="MAX1551EZK+"/>
<attribute name="PACKAGE" value="SOT-23-5 Maxim"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NEOPIXEL-ATTINY-85_ATTINY85_ATTINY85-20PU" prefix="U">
<description>8-bit Microcontroller with In-System Programmable Flash</description>
<gates>
<gate name="A" symbol="NEOPIXEL-ATTINY-85_ATTINY85_ATTINY85-20PU"/>
</gates>
<devices>
<device name="" package="NEOPIXEL-ATTINY-85_ATTINY85_DIP254P762X533-8">
<connects>
<connect gate="A" pin="(PCINT3/XTAL1/CLKI/~OC1B/ADC3)_PB3" pad="2"/>
<connect gate="A" pin="(PCINT4/XTAL2/CLKO/OC1B/ADC2)_PB4" pad="3"/>
<connect gate="A" pin="(PCINT5/~RESET/ADC0/DW)_PB5" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="PB0_(MOSI/DI/SDA/AIN0/OC0A/~OC1A/AREF/PCINT0)" pad="5"/>
<connect gate="A" pin="PB1_(MISO/DO/AIN1/OC0B/OC1A/PCINT1)" pad="6"/>
<connect gate="A" pin="PB2_(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATTINY85-20PU"/>
<attribute name="OC_FARNELL" value="1455162"/>
<attribute name="OC_NEWARK" value="68T3808"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTOR" uservalue="yes">
<description>Neo pixel solder connector for strip</description>
<gates>
<gate name="G$1" symbol="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTOR"/>
</gates>
<devices>
<device name="" package="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTORHOLES">
<connects>
<connect gate="G$1" pin="DATA" pad="DATA"/>
<connect gate="G$1" pin="GND0" pad="GND0"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NEOSTRIPCONNECTORSMD" package="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTORSMD">
<connects>
<connect gate="G$1" pin="DATA" pad="DATA"/>
<connect gate="G$1" pin="GND0" pad="GND0"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMALL-LED-LTST-S270KRKT_LTST-S270KRKT" prefix="D">
<description>http://octopart.com/ltst-c190tbkt-lite-on-550003</description>
<gates>
<gate name="G$1" symbol="SMALL-LED-LTST-S270KRKT_LTST-S270KRKT"/>
</gates>
<devices>
<device name="" package="SMALL-LED-LTST-S270KRKT_0603">
<connects>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="K2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value=" Red 631nm LED Indication - Discrete 2V 0603 (1608 Metric) "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="160-1479-1-ND"/>
<attribute name="MF" value="Lite-On Inc."/>
<attribute name="MP" value="LTST-S270KRKT"/>
<attribute name="PACKAGE" value="0603 Lite-On Inc."/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-BATTERIES-20MM_BATTERY" prefix="BT" uservalue="yes">
<description>&lt;h3&gt;Battery - Single Cell&lt;/h3&gt;
&lt;p&gt;A variety of battery chemistries, sizes, and footprints.&lt;/p&gt;
&lt;p&gt;Device List:
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;20MM_PTH - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/783"&gt;Coin Cell Battery Holder - 20mm (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;20MM_PTH_KIT- &lt;/b&gt; &lt;a href="http://www.sparkfun.com/products/783"&gt;Coin Cell battery Holder - 20 mm (PTH) &lt;/a&gt;kit version with special mask&lt;/li&gt;
&lt;li&gt;&lt;b&gt;6.8MM_PTH - &lt;/b&gt; &lt;a href="https://www.digikey.com/product-detail/en/seiko-instruments/MS621FE-FL11E/728-1057-ND/1889208?WT.srch=1&amp;gclid=CNOQ5a6LzdQCFZS2wAodXCkE0g"&gt;Coin Cell Battery Holder - 6.8MM(SMD)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;12MM_SMD - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/10592"&gt;Coin Cell Battery Holder - 12mm (SMD)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;12MM_PTH - &lt;/b&gt;&lt;a href="https://www.sparkfun.com/products/7948"&gt;Coin Cell Battery Holder - 12mm (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;20MM_SMD - &lt;/b&gt; 20mm Coin Cell Battery Holder (SMD) (2 legs)&lt;/li&gt;
&lt;ul&gt;&lt;li&gt;Used on the &lt;a href="https://www.sparkfun.com/products/11734"&gt;Big Time Watch Kit&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;li&gt;&lt;b&gt;20MM_SMD_4LEGS - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/11892"&gt;Coin Cell Battery Holder - 20mm (SMD)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;20MM_SMD_4LEGS_OVERPASTE - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/11892"&gt;Coin Cell Battery Holder - 20mm (SMD)&lt;/a&gt; (Over-paste on the legs)&lt;/li&gt;
&lt;li&gt;&lt;b&gt;24.5MM_PTH - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/8863"&gt;Coin Cell Battery Holder - 24.5mm (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;9V - &lt;/b&gt; 9V Battery Holder - PC Mount &lt;/li&gt;
&lt;ul&gt;&lt;li&gt;Used on the &lt;a href="https://www.sparkfun.com/products/11177"&gt;SparkFun SparkPunk Sound Kit &lt;/a&gt; and &lt;a href="https://www.sparkfun.com/products/12707"&gt;SparkFun SparkPunk Sequencer Kit &lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;li&gt;&lt;b&gt;18650 - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/13113"&gt;Battery Holder - 18650 (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;AA - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/7949"&gt;Battery Holder - 1xAA (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;AAA - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/12718"&gt;Battery Holder - 1xAAA (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;AA_KIT - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/7949"&gt;Battery Holder - 1xAA (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;ul&gt;&lt;li&gt;Special kit package - pads only have exposed copper on one side of the board.&lt;/li&gt;&lt;/ul&gt;
&lt;li&gt;&lt;b&gt;AAA_KIT - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/12718"&gt;Battery Holder - 1xAAA (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;ul&gt;&lt;li&gt;Special kit package - pads only have exposed copper on one side of the board.&lt;/li&gt;&lt;/ul&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-BATTERIES-20MM_BATTERY"/>
</gates>
<devices>
<device name="-6.8MM_SMD" package="SPARKFUN-BATTERIES-20MM_BATTCON-6.8MM">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-13734"/>
<attribute name="VALUE" value="6.8MM_COIN_CELL"/>
</technology>
</technologies>
</device>
<device name="-9V" package="SPARKFUN-BATTERIES-20MM_BATTCON_9V">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-10855"/>
</technology>
</technologies>
</device>
<device name="-12MM_PTH" package="SPARKFUN-BATTERIES-20MM_BATTCON_12MM_PTH">
<connects>
<connect gate="G$1" pin="+" pad="VCC@1"/>
<connect gate="G$1" pin="-" pad="GND"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-08315"/>
<attribute name="SF_SKU" value="PRT-07948"/>
</technology>
</technologies>
</device>
<device name="-12MM_SMD" package="SPARKFUN-BATTERIES-20MM_BATTCON_12MM">
<connects>
<connect gate="G$1" pin="+" pad="PWR@2"/>
<connect gate="G$1" pin="-" pad="GND"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-08044"/>
<attribute name="SF_SKU" value="PRT-10592"/>
</technology>
</technologies>
</device>
<device name="-20MM_PTH" package="SPARKFUN-BATTERIES-20MM_BATTCOM_20MM_PTH">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-09031"/>
<attribute name="SF_SKU" value="PRT-00783"/>
</technology>
</technologies>
</device>
<device name="-20MM_PTH_KIT" package="SPARKFUN-BATTERIES-20MM_BATTCOM_20MM_PTH_KIT">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-20MM_SMD" package="SPARKFUN-BATTERIES-20MM_BATTCON_20MM">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-11519"/>
</technology>
</technologies>
</device>
<device name="-20MM_SMD_4LEGS" package="SPARKFUN-BATTERIES-20MM_BATTCON_20MM_4LEGS">
<connects>
<connect gate="G$1" pin="+" pad="POSITIVE@1 POSITIVE@2 POSITIVE@3 POSITIVE@4"/>
<connect gate="G$1" pin="-" pad="GND"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-10373"/>
<attribute name="SF_SKU" value="PRT-11892"/>
</technology>
</technologies>
</device>
<device name="-20MM_SMD_4LEGS_OVERPASTE" package="SPARKFUN-BATTERIES-20MM_BATTCON_20MM_4LEGS_OVERPASTE">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="PRT-11892 "/>
<attribute name="SF_SKU" value="BATT-10373"/>
</technology>
</technologies>
</device>
<device name="-20MM_SMD_4LEGS_OVERPASTE_INNER" package="SPARKFUN-BATTERIES-20MM_BATTCON_20MM_4LEGS_OVERPASTE_INNER">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-24.5MM_PTH" package="SPARKFUN-BATTERIES-20MM_BATTCON_24.5MM_PTH">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_SKU" value="PRT-08863"/>
</technology>
</technologies>
</device>
<device name="-18650" package="SPARKFUN-BATTERIES-20MM_BATTERY_18650-HOLDER">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-12327"/>
<attribute name="SF_SKU" value="PRT-13113"/>
</technology>
</technologies>
</device>
<device name="-AA" package="SPARKFUN-BATTERIES-20MM_BATTERY-AA">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-08316"/>
<attribute name="SF_SKU" value="PRT-07949"/>
</technology>
</technologies>
</device>
<device name="-AA-HOLDER_KIT" package="SPARKFUN-BATTERIES-20MM_BATTERY-AA-HOLDER-KIT">
<connects>
<connect gate="G$1" pin="+" pad="P"/>
<connect gate="G$1" pin="-" pad="N"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AAA" package="SPARKFUN-BATTERIES-20MM_BATTERY-AAA">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-08571"/>
<attribute name="SF_SKU" value="PRT-12718"/>
</technology>
</technologies>
</device>
<device name="-AAA_KIT" package="SPARKFUN-BATTERIES-20MM_BATTERY-AAA-KIT">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-08571"/>
<attribute name="SF_SKU" value="PRT-12718"/>
</technology>
</technologies>
</device>
<device name="-AA_KIT" package="SPARKFUN-BATTERIES-20MM_BATTERY-AA-KIT">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-08316"/>
<attribute name="SF_SKU" value="PRT-07949"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-CAPACITORS_0.1UF" prefix="C">
<description>&lt;h3&gt;0.1µF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-CAPACITORS_CAP"/>
</gates>
<devices>
<device name="-0402-16V-10%" package="SPARKFUN-CAPACITORS_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-12416"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="-0603-25V-(+80/-20%)" package="SPARKFUN-CAPACITORS_0603:1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="-0603-25V-5%" package="SPARKFUN-CAPACITORS_0603:1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="-0603-100V-10%" package="SPARKFUN-CAPACITORS_0603:1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08390"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="-KIT-EZ-50V-20%" package="SPARKFUN-CAPACITORS_CAP-PTH-SMALL-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08370"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-CONNECTORS_TEST-POINT" prefix="TP">
<description>&lt;h3&gt;SparkFun Test Points&lt;/h3&gt;
&lt;p&gt;Bare copper test points for troubleshooting or In-Circuit-Testing. These are used by our Production team for verifying production board runs using pogo-pins on test beds.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13284”&gt;SparkFun LSM9DS1 Breakout&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13714”&gt;SparkFun PSOC&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13879"&gt;SparkFun Load Cell Amplifier&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-CONNECTORS_TEST-POINT"/>
</gates>
<devices>
<device name="2" package="SPARKFUN-CONNECTORS_PAD.02X.02">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3" package="SPARKFUN-CONNECTORS_PAD.03X.03">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3X4" package="SPARKFUN-CONNECTORS_PAD.03X.04">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3X5" package="SPARKFUN-CONNECTORS_PAD.03X.05">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PTH" package="SPARKFUN-CONNECTORS_1X01_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TP_15TH_THRU" package="SPARKFUN-CONNECTORS_TP_15TH">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-RESISTORS_100OHM" prefix="R">
<description>&lt;h3&gt;100Ω resistor&lt;/h3&gt;
&lt;p&gt;A resistor is a passive two-terminal electrical component that implements electrical resistance as a circuit element. Resistors act to reduce current flow, and, at the same time, act to lower voltage levels within circuits. - Wikipedia&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-RESISTORS_RESISTOR"/>
</gates>
<devices>
<device name="-0603-1/4W-5%" package="SPARKFUN-RESISTORS_0603:2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-12438"/>
<attribute name="VALUE" value="100"/>
</technology>
</technologies>
</device>
<device name="-0603-1/10W-1%" package="SPARKFUN-RESISTORS_0603:2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-07863"/>
<attribute name="VALUE" value="100"/>
</technology>
</technologies>
</device>
<device name="-HORIZ-1/4W-1%" package="SPARKFUN-RESISTORS_AXIAL-0.3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-12181"/>
<attribute name="VALUE" value="100"/>
</technology>
</technologies>
</device>
<device name="-HORIZ_KIT-1/4W-1%" package="SPARKFUN-RESISTORS_AXIAL-0.3EZ">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-12181"/>
<attribute name="VALUE" value="100"/>
</technology>
</technologies>
</device>
<device name="-VERT-1/4W-1%" package="SPARKFUN-RESISTORS_AXIAL-0.1">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-12181"/>
<attribute name="VALUE" value="100"/>
</technology>
</technologies>
</device>
<device name="-VERT_KIT-1/4W-1%" package="SPARKFUN-RESISTORS_AXIAL-0.1-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-12181"/>
<attribute name="VALUE" value="100"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-SWITCHES_MOMENTARY-SWITCH-SPST" prefix="S">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;h4&gt;Variants&lt;/h4&gt;
&lt;h5&gt;PTH-12MM - 12mm square, through-hole&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9190"&gt;Momentary Pushbutton Switch - 12mm Square&lt;/a&gt; (COM-09190)&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;PTH-6.0MM, PTH-6.0MM-KIT - 6.0mm square, through-hole&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/97"&gt;Mini Pushbutton Switch&lt;/a&gt; (COM-00097)&lt;/li&gt;
&lt;li&gt;KIT package intended for soldering kit's - only one side of pads' copper is exposed.&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;PTH-RIGHT-ANGLE-KIT - Right-angle, through-hole&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10791"&gt;Right Angle Tactile Button&lt;/a&gt; - Used on &lt;a href="https://www.sparkfun.com/products/11734"&gt;
SparkFun BigTime Watch Kit&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-12MM - 12mm square, surface-mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12993"&gt;Tactile Button - SMD (12mm)&lt;/a&gt; (COM-12993)&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/11888"&gt;SparkFun PicoBoard&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-4.5MM - 4.5mm Square Trackball Switch&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13169"&gt;SparkFun Blackberry Trackballer Breakout&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-4.6MMX2.8MM -  4.60mm x 2.80mm, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13664"&gt;SparkFun SAMD21 Mini Breakout&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-5.2MM, SMD-5.2-REDUNDANT - 5.2mm square, surface-mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8720"&gt;Mini Pushbutton Switch - SMD&lt;/a&gt; (COM-08720)&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/11114"&gt;Arduino Pro Mini&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;REDUNDANT package connects both switch circuits together&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-6.0X3.5MM - 6.0 x 3.5mm, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8229"&gt;Momentary Reset Switch SMD&lt;/a&gt; (COM-08229)&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-6.2MM-TALL - 6.2mm square, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12992"&gt;Tactile Button - SMD (6mm)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/12651"&gt;SparkFun Digital Sandbox&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-RIGHT-ANGLE - Right-angle, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13036"&gt;SparkFun Block for Intel® Edison - Arduino&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-SWITCHES_SWITCH-MOMENTARY-2"/>
</gates>
<devices>
<device name="-PTH-6.0MM" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_PTH_6.0MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</technology>
</technologies>
</device>
<device name="-PTH-6.0MM-KIT" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_PTH_6.0MM_KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097 "/>
</technology>
</technologies>
</device>
<device name="-PTH-12MM" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_PTH_12MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-09185"/>
<attribute name="SF_SKU" value="COM-09190"/>
</technology>
</technologies>
</device>
<device name="-PTH-RIGHT-ANGLE" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_PTH_RIGHT_ANGLE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10672"/>
<attribute name="SF_SKU" value="COM-10791"/>
</technology>
</technologies>
</device>
<device name="-PTH-RIGHT-ANGLE-KIT" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_PTH_RIGHT_ANGLE_KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10672"/>
<attribute name="SF_SKU" value="COM-10791"/>
</technology>
</technologies>
</device>
<device name="-SMD-4.5MM" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_4.5MM">
<connects>
<connect gate="G$1" pin="1" pad="2 3"/>
<connect gate="G$1" pin="2" pad="1 4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-09213"/>
</technology>
</technologies>
</device>
<device name="-SMD-4.6X2.8MM" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_4.6X2.8MM">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="3 4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-13065"/>
</technology>
</technologies>
</device>
<device name="-SMD-5.2-REDUNDANT" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_5.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="3 4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="SF_SKU" value="COM-08720"/>
</technology>
</technologies>
</device>
<device name="-SMD-5.2-TALL-REDUNDANT" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_5.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="3 4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-14139"/>
</technology>
</technologies>
</device>
<device name="-SMD-5.2MM" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_5.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="SF_SKU" value="COM-08720"/>
</technology>
</technologies>
</device>
<device name="-SMD-5.2MM-TALL" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_5.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-14139"/>
</technology>
</technologies>
</device>
<device name="-SMD-6.0X3.5MM" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_6.0X3.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-00815"/>
<attribute name="SF_SKU" value="COM-08229"/>
</technology>
</technologies>
</device>
<device name="-SMD-6.2MM-TALL" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_6.2MM_TALL">
<connects>
<connect gate="G$1" pin="1" pad="A2"/>
<connect gate="G$1" pin="2" pad="B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</technology>
</technologies>
</device>
<device name="-SMD-12MM" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_12MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-11967"/>
<attribute name="SF_SKU" value="COM-12993"/>
</technology>
</technologies>
</device>
<device name="-SMD-RIGHT-ANGLE" package="SPARKFUN-SWITCHES_TACTILE_SWITCH_SMD_RIGHT_ANGLE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-12265"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUBMINIATRE-SLIDE-SWITCH-JS102011SAQN_SLIDESWITCH">
<gates>
</gates>
<devices>
<device name="" package="SUBMINIATRE-SLIDE-SWITCH-JS102011SAQN_TOGGLESWITCHJS122011JAQN">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZX62D-B-5PA8_ZX62D-B-5PA8" prefix="X">
<description>&lt;b&gt;Micro USB Type B Connector&lt;/b&gt; - Standard, Shell Through Hole&lt;br&gt;
&lt;br&gt;
Source: &lt;a href="http://www.hirose.co.jp/cataloge_hp/ed_ZX_20140804.pdf"&gt;http://www.hirose.co.jp/cataloge_hp/ed_ZX_20140804.pdf&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ZX62D-B-5PA8_MICRO-USB"/>
<gate name="S" symbol="ZX62D-B-5PA8_MICRO-USB-SHIELD"/>
</gates>
<devices>
<device name="" package="ZX62D-B-5PA8_ZX62D-B-5PA8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="S" pin="S1" pad="S1"/>
<connect gate="S" pin="S2" pad="S2"/>
<connect gate="S" pin="S3" pad="S3"/>
<connect gate="S" pin="S4" pad="S4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Hirose"/>
<attribute name="MPN" value="ZX62D-B-5PA8"/>
<attribute name="OC_FARNELL" value="2300438"/>
<attribute name="OC_NEWARK" value="69W0712"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
