(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 39)
    (tracks 142)
    (zones 0)
    (modules 9)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1525)
    (trace_clearance 0.2)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1525)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.25 0.825)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0201)
    (solder_mask_min_width 0.152)
    (pad_to_paste_clearance -0.0001)
    (aux_axis_origin 0 0)
    (visible_elements FFF9FF7F)
    (pcbplotparams
      (layerselection 0x00010_7ffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/"))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 /PC14)
  (net 4 /PC15)
  (net 5 /NRST)
  (net 6 /PA0)
  (net 7 /PA1)
  (net 8 /PA2)
  (net 9 /PA3)
  (net 10 /PA4)
  (net 11 /PA5)
  (net 12 /PA6)
  (net 13 /PA7)
  (net 14 /PB0)
  (net 15 /PB1)
  (net 16 /PA8)
  (net 17 /PA9)
  (net 18 /PA10)
  (net 19 /SWD)
  (net 20 /SWC)
  (net 21 /PA11)
  (net 22 /PA12)
  (net 23 /PB5)
  (net 24 /PB6)
  (net 25 /PB7)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /NRST)
    (add_net /PA0)
    (add_net /PA1)
    (add_net /PA10)
    (add_net /PA11)
    (add_net /PA12)
    (add_net /PA2)
    (add_net /PA3)
    (add_net /PA4)
    (add_net /PA5)
    (add_net /PA6)
    (add_net /PA7)
    (add_net /PA8)
    (add_net /PA9)
    (add_net /PB0)
    (add_net /PB1)
    (add_net /PB5)
    (add_net /PB6)
    (add_net /PB7)
    (add_net /PC14)
    (add_net /PC15)
    (add_net /SWC)
    (add_net /SWD)
    (add_net GND)
    (add_net VCC)
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 160.741947 78.039547 315)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.43 315) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 1 smd roundrect (at -0.787501 0 315) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (pad 2 smd roundrect (at 0.787501 0 315) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:Molex_2x3_Contact (layer B.Cu) (tedit 59513E8F)
    (at 156.4259 74.9754)
    (attr smd)
    (fp_text reference J5 (at 0 4.4) (layer B.SilkS))
    (fp_text value CONN_02X03 (at -0.05 -4.15) (layer B.Fab))
    (pad 1 smd rect (at -1.6 1.925) (size 1.3 1.85) (layers B.Cu B.Paste B.Mask)
      (net 5 /NRST) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 2 smd rect (at -1.6 -1.925) (size 1.3 1.85) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 3 smd rect (at 0 1.925) (size 1.3 1.85) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 4 smd rect (at 0 -1.925) (size 1.3 1.85) (layers B.Cu B.Paste B.Mask)
      (net 20 /SWC) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 5 smd rect (at 1.6 1.925) (size 1.3 1.85) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 6 smd rect (at 1.6 -1.925) (size 1.3 1.85) (layers B.Cu B.Paste B.Mask)
      (net 19 /SWD) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 151.638 69.7865)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at -0.015901 0.155299) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.3111 72.136 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm (layer F.Cu) (tedit 5B4E85CE)
    (at 156.2735 75.0189)
    (descr "QFN, 32 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_32_05-08-1693.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U1 (at 0 -3.82) (layer F.SilkS))
    (fp_text value STM32L071KBUx (at 0 3.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 33 smd roundrect (at 0 0) (size 3.45 3.45) (layers F.Cu F.Mask) (roundrect_rratio 0.072464)
      (net 2 GND))
    (pad "" smd roundrect (at -1.15 -1.15) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.15 0) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.15 1.15) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 -1.15) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 0) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 1.15) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.15 -1.15) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.15 0) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.15 1.15) (size 0.93 0.93) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -2.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /PC14))
    (pad 2 smd roundrect (at -2.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /PC15))
    (pad 3 smd roundrect (at -2.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /NRST))
    (pad 4 smd roundrect (at -2.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 5 smd roundrect (at -2.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (pad 6 smd roundrect (at -2.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /PA0))
    (pad 7 smd roundrect (at -2.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /PA1))
    (pad 8 smd roundrect (at -2.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /PA2))
    (pad 9 smd roundrect (at -1.75 2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /PA3))
    (pad 10 smd roundrect (at -1.25 2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /PA4))
    (pad 11 smd roundrect (at -0.75 2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /PA5))
    (pad 12 smd roundrect (at -0.25 2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /PA6))
    (pad 13 smd roundrect (at 0.25 2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /PA7))
    (pad 14 smd roundrect (at 0.75 2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /PB0))
    (pad 15 smd roundrect (at 1.25 2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /PB1))
    (pad 16 smd roundrect (at 1.75 2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 17 smd roundrect (at 2.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (pad 18 smd roundrect (at 2.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /PA8))
    (pad 19 smd roundrect (at 2.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /PA9))
    (pad 20 smd roundrect (at 2.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /PA10))
    (pad 21 smd roundrect (at 2.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /PA11))
    (pad 22 smd roundrect (at 2.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /PA12))
    (pad 23 smd roundrect (at 2.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /SWD))
    (pad 24 smd roundrect (at 2.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (pad 25 smd roundrect (at 1.75 -2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /SWC))
    (pad 26 smd roundrect (at 1.25 -2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 27 smd roundrect (at 0.75 -2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /PB5))
    (pad 28 smd roundrect (at 0.25 -2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /PB6))
    (pad 29 smd roundrect (at -0.25 -2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /PB7))
    (pad 30 smd roundrect (at -0.75 -2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 31 smd roundrect (at -1.25 -2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 32 smd roundrect (at -1.75 -2.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x07_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 150.495 72.4662)
    (descr "Through hole straight pin header, 1x07, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x07 1.27mm single row")
    (fp_text reference J1 (at 0 -1.695) (layer F.SilkS))
    (fp_text value Conn_01x07_Male (at 0 9.315) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 /PC14))
    (pad 3 thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 /PC15))
    (pad 4 thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 /NRST))
    (pad 5 thru_hole oval (at 0 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 /PA0))
    (pad 6 thru_hole oval (at 0 6.35) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 /PA1))
    (pad 7 thru_hole oval (at 0 7.62) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 /PA2))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x07_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x07_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 152.6413 80.0608 90)
    (descr "Through hole straight pin header, 1x07, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x07 1.27mm single row")
    (fp_text reference J2 (at 0 -1.695 90) (layer F.SilkS))
    (fp_text value Conn_01x07_Male (at 0 9.315 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 /PB1))
    (pad 6 thru_hole oval (at 0 6.35 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 /PB0))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 /PA7))
    (pad 4 thru_hole oval (at 0 3.81 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 /PA6))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 /PA5))
    (pad 2 thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 /PA4))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 /PA3))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x07_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x05_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 161.7599 76.6445 180)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (fp_text reference J3 (at 0 -1.695 180) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 6.775 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 /PA8))
    (pad 2 thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 /PA9))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 /PA10))
    (pad 4 thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 21 /PA11))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 22 /PA12))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x04_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 158.1912 69.9516 270)
    (descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x04 1.27mm single row")
    (fp_text reference J4 (at 0 -1.695 270) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 0 5.505 270) (layer F.Fab))
    (fp_text user %R (at 0 1.905) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 23 /PB5))
    (pad 2 thru_hole oval (at 0 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 24 /PB6))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 25 /PB7))
    (pad 4 thru_hole oval (at 0 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x04_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text A11 (at 160.2232 72.8472) (layer B.SilkS))
  (gr_text 2020 (at 162.2679 80.0481 90) (layer B.SilkS))
  (gr_text 8/19 (at 160.6296 69.8246) (layer B.SilkS))
  (gr_text jkl (at 150.4823 69.5579) (layer B.SilkS))
  (gr_text tArmDuino32 (at 156.464 75.1586) (layer B.SilkS))
  (gr_text RST (at 152.0317 76.3778) (layer B.SilkS))
  (gr_text C15 (at 152.146 75.1078) (layer B.SilkS))
  (gr_text C14 (at 152.1968 73.6981) (layer B.SilkS))
  (gr_text A0 (at 151.892 77.5462) (layer B.SilkS))
  (gr_text A1 (at 151.5618 78.867) (layer B.SilkS))
  (gr_text A2 (at 151.511 80.8482) (layer B.SilkS))
  (gr_text A3 (at 152.7556 78.8035) (layer B.SilkS))
  (gr_text A4 (at 154.0256 79.0194) (layer B.SilkS))
  (gr_text A5 (at 155.2194 78.9432) (layer B.SilkS))
  (gr_text A6 (at 156.4386 78.9178) (layer B.SilkS))
  (gr_text A7 (at 157.6324 78.867) (layer B.SilkS))
  (gr_text B0 (at 158.9913 78.9051) (layer B.SilkS))
  (gr_text B1 (at 160.4391 78.867) (layer B.SilkS))
  (gr_text A8 (at 160.528 76.5429) (layer B.SilkS))
  (gr_text A9 (at 160.5026 75.2475) (layer B.SilkS))
  (gr_text A10 (at 160.2232 74.0156) (layer B.SilkS))
  (gr_text VCC (at 150.6601 71.247) (layer B.SilkS))
  (gr_text B7 (at 155.6385 71.2851) (layer B.SilkS))
  (gr_text A12 (at 160.1978 71.4502) (layer B.SilkS))
  (gr_text B5 (at 158.3309 71.3613) (layer B.SilkS))
  (gr_text B6 (at 156.9212 71.3867) (layer B.SilkS))
  (gr_text GND (at 153.1493 71.12) (layer B.SilkS))
  (gr_line (start 158.5259 68.6) (end 163 68.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.5259 69.1) (end 158.5259 68.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.3259 69.1) (end 158.5259 69.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.3259 68.6) (end 154.3259 69.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.5259 81.5) (end 163 81.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.5259 81) (end 158.5259 81.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.3259 81.5) (end 154.3259 81) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.3259 81) (end 158.5259 81) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.5 81.5) (end 149.5 68.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.3259 81.5) (end 149.5 81.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163 68.6) (end 163 81.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.5 68.6) (end 154.3259 68.6) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.7203 68.834) (xy 162.7505 68.834) (xy 162.7759 81.28) (xy 149.7457 81.2673)
      )
    )
  )
)
