<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="48.26" y2="0" width="0" layer="20"/>
<wire x1="48.26" y1="0" x2="50.8" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="50.8" y1="2.54" x2="50.8" y2="20.32" width="0" layer="20"/>
<wire x1="50.8" y1="20.32" x2="48.26" y2="22.86" width="0" layer="20" curve="90"/>
<wire x1="48.26" y1="22.86" x2="2.54" y2="22.86" width="0" layer="20"/>
<wire x1="2.54" y1="22.86" x2="0" y2="20.32" width="0" layer="20" curve="90"/>
<wire x1="0" y1="20.32" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<text>RST</text>
<text>3V</text>
<text>BM</text>
<text>GND</text>
<text>EN</text>
<text>GND</text>
<hole x="48.26" y="20.32" drill="2.54"/>
<hole x="48.26" y="2.54" drill="2.54"/>
<text>RST</text>
<text>_</text>
<text>+</text>
<text>+</text>
<text>_</text>
<text>NOTE
POL!</text>
<text>B</text>
<text>A</text>
<text>Proto 1</text>
</plain>
<libraries>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="MOUNTINGHOLE_2.5_PLATED">
</package>
<package name="1X16_ROUND">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X12_ROUND">
</package>
</packages>
</library>
<library name="My-Caps-SMT-Ceramic">
<packages>
<package name="CAPC2012X145N">
</package>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="My-Resistors-SMT">
<packages>
<package name="0603-SPARKFUN">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="My-Inductors-SMT">
<packages>
<package name="IND_SRU1048-1R5Y">
</package>
<package name="IND_TAIYO_BRC2518_TAY">
</package>
<package name="IND_BLM18_0603-M">
</package>
</packages>
</library>
<library name="My-Switches">
<packages>
<package name="SWITCH_11MA1QS1">
</package>
<package name="KMR2">
</package>
</packages>
</library>
<library name="BatterySqueezer-Misc">
<packages>
<package name="RNM0015A">
</package>
<package name="CUI_PJ-202A">
</package>
<package name="JSTPH2">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_2_NO_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="REV" value="C"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MH2" library="microbuilder" package="MOUNTINGHOLE_2.5_PLATED" value="MOUNTINGHOLE2.5">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNI" value="DNI"/>
</element>
<element name="MH1" library="microbuilder" package="MOUNTINGHOLE_2.5_PLATED" value="MOUNTINGHOLE2.5">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="DNI" value="DNI"/>
</element>
<element name="JP2" library="microbuilder" package="1X16_ROUND" value="">
<attribute name="DNI" value="DNI"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="microbuilder" package="1X12_ROUND" value="">
<attribute name="DNI" value="DNI"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="BatterySqueezer-Misc" package="JSTPH2" value="">
<attribute name="DESCRIPTION" value="Connector Header Surface Mount, Right Angle 2 position 0.079&quot; (2.00mm) "/>
<attribute name="DPN" value="455-1749-1-ND"/>
<attribute name="MANUFACTURER" value=" JST Sales America Inc"/>
<attribute name="MPN" value="S2B-PH-SM4-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="My-Resistors-SMT" package="0603-SPARKFUN" value="10k">
<attribute name="DESCRIPTION" value="10 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Moisture Resistant Thick Film"/>
<attribute name="DPN" value="CR0603-FX-1002ELFCT-ND"/>
<attribute name="MANUFACTURER" value="Bourns Inc. "/>
<attribute name="MPN" value="CR0603-FX-1002ELF"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R1" library="My-Resistors-SMT" package="0603-SPARKFUN" value="150k">
<attribute name="DESCRIPTION" value="150 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Moisture Resistant Thick Film"/>
<attribute name="DPN" value="118-CR0603-FX-1503ELFCT-ND"/>
<attribute name="MANUFACTURER" value="Bourns Inc. "/>
<attribute name="MPN" value="CR0603-FX-1503ELF "/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150k"/>
</element>
<element name="U1" library="BatterySqueezer-Misc" package="RNM0015A" value="TPS63070RNMR">
<attribute name="DESCRIPTION" value="Buck-Boost Switching Regulator IC Positive Adjustable 2.5V 1 Output 3.6A (Switch) 15-PowerVFQFN"/>
<attribute name="DPN" value="296-44874-1-ND"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MPN" value="TPS63070RNMR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="My-Inductors-SMT" package="IND_SRU1048-1R5Y" value="1.5uH">
<attribute name="DESCRIPTION" value=" 1.5µH Shielded Wirewound Inductor 7A 4.3mOhm Nonstandard "/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/bourns-inc/SRU1048-1R5Y/SRU1048-1R5YCT-ND/2353040?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="DPN" value="SRU1048-1R5YCT-ND"/>
<attribute name="MANUFACTURER" value="Bourns"/>
<attribute name="MPN" value="SRU1048-1R5Y"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="Nonstandard Bourns"/>
<attribute name="VALUE" value="1.5uH"/>
</element>
<element name="C8" library="My-Caps-SMT-Ceramic" package="0603" value="0.1uF">
<attribute name="DESCRIPTION" value="0.1µF ±10% 25V Ceramic Capacitor X7R 0603 (1608 Metric)"/>
<attribute name="DPN" value="1276-1006-1-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MPN" value="CL10B104KA8NNNC"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 (1608 Metric) "/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="0.1uF"/>
<attribute name="VOLTAGE" value="25V"/>
</element>
<element name="C11" library="My-Caps-SMT-Ceramic" package="CAPC2012X145N" value="22uF">
<attribute name="DESCRIPTION" value=" 22µF ±20% 35V Ceramic Capacitor X5R 0805 _2012 Metric_ "/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/tdk-corporation/C2012X5R1V226M125AC/445-14428-1-ND/3956094?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="DPN" value="445-14428-1-ND"/>
<attribute name="MANUFACTURER" value="TDK"/>
<attribute name="MPN" value="C2012X5R1V226M125AC"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2012 TDK"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="My-Caps-SMT-Ceramic" package="CAPC2012X145N" value="22uF">
<attribute name="DESCRIPTION" value=" 22µF ±20% 35V Ceramic Capacitor X5R 0805 _2012 Metric_ "/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/tdk-corporation/C2012X5R1V226M125AC/445-14428-1-ND/3956094?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="DPN" value="445-14428-1-ND"/>
<attribute name="MANUFACTURER" value="TDK"/>
<attribute name="MPN" value="C2012X5R1V226M125AC"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2012 TDK"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="My-Caps-SMT-Ceramic" package="0603" value="10uF">
<attribute name="DESCRIPTION" value="10µF ±20% 6.3V Ceramic Capacitor X5R 0603 (1608 Metric)"/>
<attribute name="DPN" value="587-5869-1-ND"/>
<attribute name="MANUFACTURER" value="Taiyo Yuden"/>
<attribute name="MPN" value="JMK107ABJ106MA-T"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 (1608 Metric) "/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="6.3V"/>
</element>
<element name="C2" library="My-Caps-SMT-Ceramic" package="0603" value="47uF">
<attribute name="DESCRIPTION" value="CAP CER 47UF 6.3V X5R 1206"/>
<attribute name="DPN" value="1276-1167-1-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MPN" value="CL31A476MQHNNNE"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 (1608 Metric) "/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="6.3V"/>
</element>
<element name="R6" library="My-Resistors-SMT" package="0603-SPARKFUN" value="100k">
<attribute name="DESCRIPTION" value="100 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Moisture Resistant Thick Film"/>
<attribute name="DPN" value="CR0603-FX-1003ELFCT-ND"/>
<attribute name="MANUFACTURER" value="Bourns Inc. "/>
<attribute name="MPN" value="CR0603-FX-1003ELF"/>
<attribute name="NAME"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="My-Switches" package="KMR2" value="SPDT/NO">
<attribute name="DESCRIPTION" value="Tactile Switch SPST-NO Top Actuated Surface Mount "/>
<attribute name="DPN" value="CKN10247CT-ND"/>
<attribute name="MANUFACTURER" value="C&amp;K"/>
<attribute name="MPN" value="KMR241NG LFS"/>
<attribute name="VALUE" value="SPDT/NO"/>
</element>
<element name="J1" library="BatterySqueezer-Misc" package="CUI_PJ-202A" value="PJ-202A">
<attribute name="DESCRIPTION" value="Power Barrel Connector Jack 2.10mm ID (0.083&quot;), 5.50mm OD (0.217&quot;) Through Hole, Right Angle "/>
<attribute name="DNI" value="DNI"/>
<attribute name="DPN" value="CP-202A-ND"/>
<attribute name="MANUFACTURER" value="CUI INC"/>
<attribute name="MPN" value="PJ-202A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="My-Resistors-SMT" package="0603-SPARKFUN" value="475k">
<attribute name="DESCRIPTION" value="475 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Moisture Resistant Thick Film"/>
<attribute name="DPN" value="CR0603-FX-4753ELFCT-ND"/>
<attribute name="MANUFACTURER" value="Bourns Inc. "/>
<attribute name="MPN" value="CR0603-FX-4753ELF"/>
<attribute name="NAME"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="475k"/>
</element>
<element name="R7" library="My-Resistors-SMT" package="0603-SPARKFUN" value="150k">
<attribute name="DESCRIPTION" value="150 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Moisture Resistant Thick Film"/>
<attribute name="DPN" value="118-CR0603-FX-1503ELFCT-ND"/>
<attribute name="MANUFACTURER" value="Bourns Inc. "/>
<attribute name="MPN" value="CR0603-FX-1503ELF "/>
<attribute name="NAME"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150k"/>
</element>
<element name="L2" library="My-Inductors-SMT" package="IND_TAIYO_BRC2518_TAY" value="1uH">
<attribute name="DESCRIPTION" value="1µH Unshielded Wirewound Inductor 1.65A 50mOhm 1007 (2518 Metric)"/>
<attribute name="DPN" value="587-2437-1-ND"/>
<attribute name="MANUFACTURER" value="TAIYO YUDEN"/>
<attribute name="MPN" value="BRC2518T1R0M"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="My-Inductors-SMT" package="IND_BLM18_0603-M" value="180 OHM">
<attribute name="DESCRIPTION" value="180 Ohms @ 100MHz 1 Power Line Ferrite Bead 0603 (1608 Metric) 1.5A 90mOhm "/>
<attribute name="DPN" value="490-5263-1-ND"/>
<attribute name="MANUFACTURER" value="MURATA"/>
<attribute name="MPN" value="BLM18PG181SN1D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="My-Caps-SMT-Ceramic" package="0603" value="1uF">
<attribute name="DESCRIPTION" value="1µF ±10% 10V Ceramic Capacitor X7R 0603 (1608 Metric)"/>
<attribute name="DPN" value="1276-1945-1-ND"/>
<attribute name="MANUFACTURER" value="  Samsung Electro-Mechanics "/>
<attribute name="MPN" value="CL10B105KP8NFNC"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1uF"/>
<attribute name="VOLTAGE" value="10V"/>
</element>
<element name="C6" library="My-Caps-SMT-Ceramic" package="0603" value="10uF">
<attribute name="DESCRIPTION" value="10µF ±20% 6.3V Ceramic Capacitor X5R 0603 (1608 Metric)"/>
<attribute name="DPN" value="587-5869-1-ND"/>
<attribute name="MANUFACTURER" value="Taiyo Yuden"/>
<attribute name="MPN" value="JMK107ABJ106MA-T"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 (1608 Metric) "/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="6.3V"/>
</element>
<element name="SW2" library="My-Switches" package="SWITCH_11MA1QS1" value="SPDT">
<attribute name="DESCRIPTION" value="Slide Switch SPDT Through Hole, Right Angle "/>
<attribute name="DPN" value="CKN9560-ND"/>
<attribute name="MANUFACTURER" value="C&amp;K"/>
<attribute name="MPN" value="OS102011MA1QS1"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="My-Resistors-SMT" package="0603-SPARKFUN" value="100k">
<attribute name="DESCRIPTION" value="100 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Moisture Resistant Thick Film"/>
<attribute name="DPN" value="CR0603-FX-1003ELFCT-ND"/>
<attribute name="MANUFACTURER" value="Bourns Inc. "/>
<attribute name="MPN" value="CR0603-FX-1003ELF"/>
<attribute name="NAME"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NO_SILK" value="JUMPER_NC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NO_SILK" value="JUMPER_NO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="My-Caps-SMT-Ceramic" package="0603" value="10uF">
<attribute name="DESCRIPTION" value=" Multilayer Ceramic Capacitors - 10UF 35V X5R 0603 "/>
<attribute name="DPN" value="490-13248-1-ND"/>
<attribute name="MANUFACTURER" value="Murata"/>
<attribute name="MPN" value="GRM188R6YA106MA73D"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="35V"/>
</element>
<element name="C3" library="My-Caps-SMT-Ceramic" package="0603" value="47uF">
<attribute name="DESCRIPTION" value="CAP CER 47UF 6.3V X5R 1206"/>
<attribute name="DPN" value="1276-1167-1-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MPN" value="CL31A476MQHNNNE"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 (1608 Metric) "/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="6.3V"/>
</element>
<element name="C5" library="My-Caps-SMT-Ceramic" package="0603" value="0.1uF">
<attribute name="DESCRIPTION" value="0.1µF ±10% 25V Ceramic Capacitor X7R 0603 (1608 Metric)"/>
<attribute name="DPN" value="1276-1006-1-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MPN" value="CL10B104KA8NNNC"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 (1608 Metric) "/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="0.1uF"/>
<attribute name="VOLTAGE" value="25V"/>
</element>
<element name="R2" library="My-Resistors-SMT" package="0603-SPARKFUN" value="100k">
<attribute name="DESCRIPTION" value="100 kOhms ±1% 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Moisture Resistant Thick Film"/>
<attribute name="DPN" value="CR0603-FX-1003ELFCT-ND"/>
<attribute name="MANUFACTURER" value="Bourns Inc. "/>
<attribute name="MPN" value="CR0603-FX-1003ELF"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="My-Caps-SMT-Ceramic" package="0603" value="0.1uF">
<attribute name="DESCRIPTION" value="0.1µF ±10% 25V Ceramic Capacitor X7R 0603 (1608 Metric)"/>
<attribute name="DPN" value="1276-1006-1-ND"/>
<attribute name="MANUFACTURER" value="Samsung Electro-Mechanics"/>
<attribute name="MPN" value="CL10B104KA8NNNC"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 (1608 Metric) "/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25V"/>
</element>
<element name="C10" library="My-Caps-SMT-Ceramic" package="CAPC2012X145N" value="22uF">
<attribute name="DESCRIPTION" value=" 22µF ±20% 35V Ceramic Capacitor X5R 0805 _2012 Metric_ "/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/tdk-corporation/C2012X5R1V226M125AC/445-14428-1-ND/3956094?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="DPN" value="445-14428-1-ND"/>
<attribute name="MANUFACTURER" value="TDK"/>
<attribute name="MPN" value="C2012X5R1V226M125AC"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2012 TDK"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="My-Caps-SMT-Ceramic" package="CAPC2012X145N" value="22uF">
<attribute name="DESCRIPTION" value=" 22µF ±20% 35V Ceramic Capacitor X5R 0805 _2012 Metric_ "/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/tdk-corporation/C2012X5R1V226M125AC/445-14428-1-ND/3956094?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="DPN" value="445-14428-1-ND"/>
<attribute name="MANUFACTURER" value="TDK"/>
<attribute name="MPN" value="C2012X5R1V226M125AC"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2012 TDK"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP2" pad="13"/>
<contactref element="JP2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="X1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="C8" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="10"/>
<contactref element="SW1" pad="2"/>
<contactref element="SW1" pad="4"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="R7" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="SW2" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="15"/>
<contactref element="C7" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="JP2" pad="15"/>
<contactref element="C6" pad="2"/>
<contactref element="L3" pad="1"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="VCEL">
<contactref element="R3" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="X1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="13"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="PB22/I6/SERCOM5.2">
</signal>
<signal name="PB23/I7/SERCOM5.3">
</signal>
<signal name="PB03/I3/AIN11/SERCOM5.1">
</signal>
<signal name="BATMON">
<contactref element="R4" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VAUX">
<contactref element="C8" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="TPS_L1">
<contactref element="U1" pad="11"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="TPS_L2">
<contactref element="L1" pad="2"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="TPS_VOUT">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="7"/>
<contactref element="C2" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="L2" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="TPS_FB">
<contactref element="U1" pad="5"/>
<contactref element="R5" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="PS">
<contactref element="U1" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="RST">
<contactref element="JP2" pad="16"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="L1L3">
<contactref element="L2" pad="1"/>
<contactref element="L3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="EN_MAIN">
<contactref element="JP3" pad="2"/>
<contactref element="SW2" pad="1"/>
</signal>
<signal name="EN_TPS">
<contactref element="SW2" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="BATMON_OP">
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
